CMSIS-Core (Cortex-M): Using TrustZone for ARMv8-M

| CMSIS-Core (Cortex-M) Version 5.0.2 CMSIS-Core support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Using TrustZone for ARMv8-M

The optional ARMv8-M security extension is similar to ARM TrustZone technology used in Cortex-A processors, but is optimized for ultra-low power embedded applications. TrustZone for ARMv8-M enables of multiple software security domains that restrict access to secure memory and I/O only for trusted software.

TrustZone for ARMv8-M:

- preserves low interrupt latencies for both Secure and Non-secure domains.
- does not impose code overhead, cycle overhead or the complexity of a virtualization based solution.
- introduces the Secure Gateway (SG) processor instruction for calls to the secure domain.

Notations

This manual uses the following notations to identify functions and hardware resources that are related to TrustZone for ARMv8-M:

- prefix TZ or __TZ indicates a function that is available only in ARMv8-M TrustZone enabled devices.
- postfix _NS indicates a hardware resource that belongs to the Non-secure state.
- postfix _S indicates a hardware resource that belongs to the Secure state.

# Simplified Use Case with TrustZone

An ARMv8-M TrustZone enabled device has restricted access for data, code, and I/O access to trusted software that runs in the Secure state. Typical applications are secure IoT nodes, firmware IP protection, or multi-party embedded software deployments.

The figure Simplified Use Case shows and embedded application that is split into a User Project (executed in Non-secure state) and a Firmware Project (executed in Secure state).

- System Start: after power on or reset, an ARMv8-M system starts code execution in the Secure state. The access rights for the Non-secure state is configured.
- User Application: control can be transferred to Non-secure state to execute user code. This code can only call functions in the secure state that are marked for execution with the SG (secure gate) instruction and memory attributes. Any attempt to access memory or peripherals that are assigned to the Secure state triggers a security exception.
- Firmware callbacks: code running in the Secure state can execute code in the Non-secure state using call-back function pointers. For example, a communication stack (protected firmware) could use an I/O driver that is configured in user space.

Simplified Use Case

Program execution in the Secure state is further protected by TrustZone hardware from software failures. For example, an ARMv8-M system may implement two independent SYSTICK timers which allows to stop code execution in Non-secure state in case of timing violations. Also function pointer callbacks from Secure state to Non-secure state protected by a special CPU instruction and the address bit 0 which prevents anciently executing code in Non-secure state.

## Program Examples

This CMSIS software pack contains the following program examples that show the usage of TrustZone for ARMv8-M on Cortex-M33 devices:

Example | Description
--- | ---
TrustZone for ARMv8-M No RTOS | bare-metal secure/non-secure programming without RTOS (shows the Simplified Use Case).
TrustZone for ARMv8-M RTOS | secure/non-secure RTOS example with thread context management
TrustZone for ARMv8-M RTOS Security Tests | secure/non-secure RTOS example with security test cases and system recovery

Other sample application that reflects this Simplified Use Case is the ARMv8MBL Secure/Non-Secure example that is available in the Software Pack Keil - ARM V2M-MPS2 Board Support PACK for Cortex-M System Design Kit Devices (Keil:V2M-MPS2_CMx_BSP.1.2.0.pack or higher).

# Programmers Model with TrustZone

The figure Secure Memory Map shows the memory view for the Secure state. In the Secure state all memory and peripherals can be accessed. The System Control and Debug area provides access to secure peripherals and non-secure peripherals that are mirrored at a memory alias.

The secure peripherals are only accessible during program execution in Secure state. The Secure Attribute Unit (SAU) configures the non-secure memory, peripheral, and interrupt access. Also available are a secure MPU (memory protection unit), secure SCB (system control block), and secure SysTick timer.

The system supports two separate interrupt vector tables for secure and non-secure code execution. This interrupt assignment is controlled during Secure state code execution via the NVIC (nested vector interrupt controller).

Secure Memory Map

The figure Non-Secure Memory Map shows the memory view for the Non-secure state. This memory view is identical to the traditional Cortex-M memory map. Access to any secure memory or peripheral space triggers the secure exception that executes a handler in Secure state.

The System Partition Header File partition_<device>.h defines the initial setup of the Non-Secure Memory Map during system start in the Secure state (refer to functions SystemInit and TZ_SAU_Setup).

Non-Secure Memory Map

The figure Registers shows the register view of the ARMv8-M system with TrustZone. As the general purpose registers are can be accessed from any state (secure or non-secure), function calls between the states use these registers for parameter and return values.

The register R13 is the stack pointer alias, and the actual stack pointer (PSP_NS, MSP_NS, PSP_S, MSP_S) accessed depends on state (Secure or Non-secure) and mode (handler=exception/interrupt execution or thread=normal code execution).

In ARMv8-M Mainline, each stack pointer has a limit register (PSPLIM_NS, MSPLIM_NS, PSPLIM_S, MSPLIM_S) that traps stack overflows with the UsageFault exception (register UFSR bit STKOF=1).

An ARMv8-M system with TrustZone has an independent CONTROL register for each state (Secure or Non-secure). The interrupt/exception control registers (PRIMASK, FAULTMASK, BASEPRI) are banked between the states (Secure or Non-secure), however the interrupt priority for the Non-Secure state can be lowered (SCB_AIRCR register bit PRIS) so that secure interrupts have always higher priority.

The core registers of the current state (Secure or Non-secure) are accessed using the standard Core Register Access functions. In Secure state all non-secure registers are accessible using the Core Register Access Functions related to TrustZone for ARMv8-M.

Registers

# CMSIS Files for TrustZone

The CMSIS-Core files are extended by the System Partition Header File partition_<device>.h which defines the initial system configuration and during SystemInit in Secure state.

CMSIS with extensions for TrustZone

Note
  Refer to Using CMSIS in Embedded Applications for a general description of the CMSIS-Core (Cortex-M) files.

## RTOS Thread Context Management

To provide a consistent RTOS thread context management for ARMv8-M TrustZone across the various real-time operating systems (RTOS), the CMSIS-Core (Cortex-M) includes header file TZ_context.h with API definitions. An non-secure application which uses an RTOS and calls secure library modules requires the management of the secure stack space. Since secure state registers cannot be accessed by the RTOS that runs in non-secure state secure functions implement the thread context switch.

As the non-secure state and secure state parts of an application are separated, the API for managing the secure stack space should be standardized. Otherwise the secure library modules would force the non-secure state application to use a matching RTOS implementation.

RTOS Thread Context Management for ARMv8-M TrustZone

To allocate the context memory for threads, an RTOS kernel that runs in non-secure state calls the interface functions defined by the header file TZ_context.h. The TZ_context functions itself are part of the secure state application. An minimum implementation is provided as part of RTOS2 and should handle the secure stack for the thread execution. However it is also possible to implement the context memory management system with additional features such as access control to secure state memory regions using an MPU.

The API functions of TZ_context are described in the chapter Reference under TrustZone for ARMv8-M - RTOS Context Management.

Refer to Program Examples for RTOS examples that provide a template implementation for TZ_context.c.