CMSIS-DAP: Configure I/O Ports and Debug Unit

| CMSIS-DAP Version 1.2.0 (Proposal) Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Content
Configure I/O Ports and Debug Unit
Firmware Configuration

DAP_config.h configures I/O ports and Debug Unit hardware parameters. More...

## Content
| CMSIS-DAP Debug Unit Information
| Provides definitions about the hardware and configuration of the Debug Unit.
| CMSIS-DAP Hardware I/O Pin Access
| Standard I/O Pins of the CMSIS-DAP Hardware Debug Port support standard JTAG mode and Serial Wire Debug (SWD) mode.
| CMSIS-DAP Hardware Status LEDs
| CMSIS-DAP Hardware may provide LEDs that indicate the status of the CMSIS-DAP Debug Unit.
| CMSIS-DAP Initialization
| CMSIS-DAP Hardware I/O and LED Pins are initialized with the function DAP_SETUP.

## Description

DAP_config.h configures I/O ports and Debug Unit hardware parameters.

The CMSIS-DAP Firmware configuration file DAP_config.h provides the interface functions and configuration parameters for the hardware of the CMSIS-DAP Debug Unit.