CMSIS-Core (Cortex-A): CNTP_CTL_Type Union Reference

| CMSIS-Core (Cortex-A) Version 1.0.0 CMSIS-Core support for Cortex-A processor-based devices

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
CNTP_CTL_Type Union Reference
Generic Physical Timer Functions

Physical Timer Control register.

## Data Fields
struct {
uint32_t ENABLE:1
| bit: 0 Enables the timer. More...
uint32_t IMASK:1
| bit: 1 Timer output signal mask bit. More...
uint32_t ISTATUS:1
| bit: 2 The status of the timer. More...
uint32_t _reserved0:29
| bit: 3..31 Reserved More...
} | b
| Structure used for bit access. More...
uint32_t | w
| Type used for word access. More...
struct {
uint32_t ENABLE:1
| bit: 0 Enables the timer. More...
uint32_t IMASK:1
| bit: 1 Timer output signal mask bit. More...
uint32_t ISTATUS:1
| bit: 2 The status of the timer. More...
} | b
| Structure used for bit access. More...

## Field Documentation

uint32_t CNTP_CTL_Type::_reserved0

struct { ... } CNTP_CTL_Type::b

struct { ... } CNTP_CTL_Type::b

uint32_t CNTP_CTL_Type::ENABLE

Enables the timer.

Permitted values are:

- 0 - Timer disabled.
- 1 - Timer enabled.

uint32_t CNTP_CTL_Type::IMASK

Timer output signal mask bit.

Permitted values are:

- 0 - Timer output signal is not masked.
- 1 - Timer output signal is masked.

uint32_t CNTP_CTL_Type::ISTATUS

The status of the timer.

This bit indicates whether the timer condition is asserted:

- 0 - Timer condition is not asserted.
- 1 - Timer condition is asserted.

uint32_t CNTP_CTL_Type::w