CMSIS-RTOS2: RTX Migration Guide

| CMSIS-RTOS2 Version 2.1.1 Real-Time Operating System: API and RTX Reference Implementation

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
RTX Migration Guide

RTX5 supplies both API layers: CMSIS-RTOS v1 and CMSIS-RTOS v2. This allows a gradient transition from version 1 to 2. A modified v1 header and a special v1 compatibility module enable existing code to run on a v2 implementation with almost no modifications.

Only a few incompatibilities and limitations exist:

- Kernel startup
  The function `osKernelRunning` has been deprecated. "main" was usually a running thread in v1 implementations, which is not the case in v2 anymore. It was also possible to not even initialize and start the Kernel, but just to assume that "main" was a running thread. Portable code would typically initialize the Kernel (osKernelInitialize) and then start the Kernel (osKernelStart) or skip that part if `osKernelRunning` indicated that it is already running.
  The example code below shows how to overcome this situation.
- The function `osWait` is deprecated.
- Error code incompatibility
  CMSIS-RTOS v1 used two different error codes for invalid parameters: `osErrorParameter` and `osErrorValue`. The new version only uses a common osErrorParameter code. Therefore, code relying on osErrorValue is not compatible. The following functions are affected:
  - osThreadSetPriority returns osErrorParameter instead of osErrorValue when priority is out of range
  - osMemoryPoolFree (previously `osPoolFree`) returns osErrorParameter instead of osErrorValue when block to be returned is invalid
- The osDelay return code has changed from osErrorTimeout to osOK.

The level of migration depends on the project's phase in its life cycle:

- The first level of migration is to migrate to RTX5 without changing the API level.
- The second level in the transition is to use v2 API functions and v1 API functions in mixed variation.
- The third level is the full transition to the API v2. It is non-trivial and requires some additional development effort to migrate all API v1 calls to v2.

# Level 1 Migration - Upgrade to RTX5 on API v1

Upgrade to RTX Version 5 from any 4.x version using the API v1 compatibility layer. Configure an existing project as follows:

- Open Manage Run-Time Environment window
- Expand CMSIS software component.
- Expand RTOS (API), uncheck Keil RTX, and select Keil RTX5.
- Expand RTOS2 (API) and select Keil RTX5.
- Resolve missing components.

Component Selection for RTX5

- Click OK.
- Expand CMSIS group in the Project window:
- Open RTX_Config.h and adapt the configuration to suit the application including (refer to Configure RTX v5):
  - System Configuration->Global Dynamic Memory size
  - Kernel Tick Frequency
  - Thread Configuration->Default Thread Stack size
- Rename function `int main (void)` to `void app_main (void *arg)`.
- Create a new function `int main (void)` which implements at least:
  - System initialization and configuration
  - Update SystemCoreClock
  - Initialize CMSIS-RTOS kernel
  - Creates new thread app_main
  - Start RTOS scheduler

Example - Application Main Thread

/* Renamed main() function */
void app_main (void const *argument) {
// contents of old "main"
}
osThreadDef(app_main, osPriorityNormal, 1, 0);
int main (void) {
// System Initialization
SystemCoreClockUpdate();
// ...
osKernelInitialize();
osThreadCreate(osThread(app_main), NULL);
osKernelStart();
for (;;);
}

Note
  In RTOS API v1 all timings were specified in milliseconds. RTX5 defines all times in kernel ticks. To match both it is recommended to set the Kernel Tick Frequency to 1000 Hz in the System Configuration.

To validate the correct operation of your RTOS after migration you can temporarily integrate the RTOS Validation component into your project.

# Level 2 Migration - Use API v2 and v1 alongside in RTX5

Implementing new features in your project is ideally done using the new API. Both API versions are offered in RTX5 and can exist along-side.

The component selection is identical to Migration Level 1.

Include "cmsis_os2.h" in all modules where access to API v2 functions is required.

#include "cmsis_os.h" // ARM::CMSIS:RTOS:Keil RTX5
#include "cmsis_os2.h" // ARM::CMSIS:RTOS2:Keil RTX5

The following snippet shows how threads - created with both API versions - live along-side:

/*----------------------------------------------------------------------------
* Thread 4 'phaseD': Phase D output - API v2 thread
*---------------------------------------------------------------------------*/
void phaseD (void *argument) {
for (;;) {
osThreadFlagsWait(0x0001, osFlagsWaitAny, osWaitForever); /* wait for an event flag 0x0001 */
Switch_On (LED_D);
signal_func(tid_phaseA); /* call common signal function */
Switch_Off(LED_D);
}
}
/*----------------------------------------------------------------------------
* Thread 5 'clock': Signal Clock - API v1 thread
*---------------------------------------------------------------------------*/
void clock (void const *argument) {
for (;;) {
osSignalWait(0x0100, osWaitForever); /* Wait for event send by API v2 function osThreadFlagsSet() */
Switch_On (LED_CLK);
osDelay(80); /* delay ticks */
Switch_Off(LED_CLK);
}
}
/* Define the API v1 thread */
osThreadDef(clock, osPriorityNormal, 1, 0);
/*----------------------------------------------------------------------------
* Main: Initialize and start RTX Kernel
*---------------------------------------------------------------------------*/
void app_main (void *argument) {
; //...
/* Create the API v2 thread */
tid_phaseD = osThreadNew(phaseD, NULL, NULL);
/* Create the API v1 thread */
tid_clock = osThreadCreate(osThread(clock), NULL);
osThreadFlagsSet(tid_phaseA, 0x0001); /* set signal to phaseA thread */
osDelay(osWaitForever);
while(1);
}

The full example "RTX5 Migration" is part of the CMSIS5 pack and available from the pack installer.

# Level 3 Migration - Full transition to API v2

Migrating fully to APIv2 reduces the overhead of the translation layer and simplifies the project. There is some effort to replace and re-test all API Version 1 calls. The following steps are recommended as a rough guide-line:

- Open Manage Run-Time Environment window:
- Expand CMSIS Software Component:
- Expand RTOS (API) Software Component and de-select Keil RTX5
- Click OK
- Exchange all occurrences of
  #include "cmsis_os.h"
  with
  #include "cmsis_os2.h"
- Identify all references to the API v1 and replace with the appropriate calls in v2. You might want to use the Error List window in uVision to identify the related code passages quickly.

Note
  See Detailed API Function Differences for details in differences.

Generally there are no longer os*Def macros to declare OS objects.

Note
  - Signal Events have been replaced. Use the functions listed under Thread Flags and Event Flags instead.
  - The Mail Queue RTOS v1 functions have been deprecated. Use the functionality of the Message Queue instead. Differences are listed under Message Queue.