BLE_API v2.1.3

Data Fields
BLE_Adv_Param Struct Reference
BLE Common » BLE Structure Definition

BLE advertising parameter. More...

`#include <ble_cmd.h>`

## Data Fields
BleAdvType | advType
uint16_t | advIntervalMin
uint16_t | advIntervalMax
BLE_Addr_Param | advDirectAddrParam
BleAdvChannelMap | advChannelMap
BleAdvFilterPolicy | advFilterPolicy

## Detailed Description

BLE advertising parameter.

## Field Documentation

## ◆ advChannelMap

BleAdvChannelMap BLE_Adv_Param::advChannelMap

Advertising channel map

## ◆ advDirectAddrParam

BLE_Addr_Param BLE_Adv_Param::advDirectAddrParam

The BLE address and BLE address type for directed advertising

Note
  MUST set advDirectAddrParam if BLE advertising type is set to ADV_TYPE_ADV_DIRECT_IND.

## ◆ advFilterPolicy

BleAdvFilterPolicy BLE_Adv_Param::advFilterPolicy

Advertising filter policy

## ◆ advIntervalMax

uint16_t BLE_Adv_Param::advIntervalMax

Maximum advertising interval.

Note
  Advertising interval = value * 0.625ms
  Advertising interval range = ADV_INTERVAL_MIN ~ ADV_INTERVAL_MAX

## ◆ advIntervalMin

uint16_t BLE_Adv_Param::advIntervalMin

Minimum advertising interval.

Note
  Advertising interval = value * 0.625ms
  Advertising interval range = ADV_INTERVAL_MIN ~ ADV_INTERVAL_MAX

## ◆ advType

BleAdvType BLE_Adv_Param::advType

BLE advertising type

The documentation for this struct was generated from the following file:

- Source/Include/ble_cmd.h