BLE_API v2.1.3

Variables
RF Power Definition
Porting » MCU Porting Related

## Variables
const int8_t(* | TXPOWER_TABLE )[6]
uint8_t | size_TXPOWER_TABLE

## Detailed Description

RF Power definition.

## Variable Documentation

## ◆ size_TXPOWER_TABLE

uint8_t size_TXPOWER_TABLE
| extern

The size of defined BLE TX power level table

Note
  TXPOWER_TABLE is defined in "porting_rfpower.c.

## ◆ TXPOWER_TABLE

const int8_t(* TXPOWER_TABLE)[6]
| extern

BLE TX power level table

Attention
  BLE TX power level table can be modified but please noted that the default TX power setting is set to index 0.

Note
  TXPOWER_TABLE is defined in "porting_rfpower.c.