BLE_API v2.1.3

Data Fields
BLE_Event_ConnParam Struct Reference
BLE Common » BLE Structure Definition

BLE Event Connection Parameter. More...

`#include <ble_cmd.h>`

## Data Fields
BleConnStatus | status
uint8_t | hostId
BleConnRole | connRole
BLE_Addr_Param | peerAddr
uint16_t | connInterval
uint16_t | connLatency
uint16_t | connSupervisionTimeout

## Detailed Description

BLE Event Connection Parameter.

## Field Documentation

## ◆ connInterval

uint16_t BLE_Event_ConnParam::connInterval

The current link connection interval value.

## ◆ connLatency

uint16_t BLE_Event_ConnParam::connLatency

The current link connection latency value.

## ◆ connRole

BleConnRole BLE_Event_ConnParam::connRole

Connection role

## ◆ connSupervisionTimeout

uint16_t BLE_Event_ConnParam::connSupervisionTimeout

The current link connection supervision timeout value.

## ◆ hostId

uint8_t BLE_Event_ConnParam::hostId

Host id.

## ◆ peerAddr

BLE_Addr_Param BLE_Event_ConnParam::peerAddr

Remote device address type and address.

## ◆ status

BleConnStatus BLE_Event_ConnParam::status

BLE connection event status.

The documentation for this struct was generated from the following file:

- Source/Include/ble_cmd.h