BLE_API v2.1.3

Data Fields
BLE_DataLength_Param Struct Reference
BLE Common » BLE Structure Definition

BLE Data Length. More...

`#include <ble_cmd.h>`

## Data Fields
uint16_t | txMaxOctets
uint16_t | rxMaxOctets

## Detailed Description

BLE Data Length.

## Field Documentation

## ◆ rxMaxOctets

uint16_t BLE_DataLength_Param::rxMaxOctets

Preferred maximum number of payload octets that the Controller for transmission in a single Link Layer packet on this connection.

## ◆ txMaxOctets

uint16_t BLE_DataLength_Param::txMaxOctets

Preferred maximum number of payload octets that the Controller for reception in a single Link Layer packet on this connection.

The documentation for this struct was generated from the following file:

- Source/Include/ble_cmd.h