BLE_API v2.1.3

BLE Advertising Type Definition
BLE Common » BLE Command Definition » BLE Advertising Definition

## BleAdvType
Define advertising type.
typedef uint8_t | BleAdvType
#define | ADV_TYPE_ADV_IND 0x00
#define | ADV_TYPE_ADV_DIRECT_IND 0x01
#define | ADV_TYPE_SCAN_IND 0x02
#define | ADV_TYPE_ADV_NONCONN_IND 0x03
#define | ADV_TYPE_SCAN_RSP 0x04

## Detailed Description

BLE advertising type definition.

## Macro Definition Documentation

## ◆ ADV_TYPE_ADV_DIRECT_IND

#define ADV_TYPE_ADV_DIRECT_IND 0x01

Connectable directed advertising.

## ◆ ADV_TYPE_ADV_IND

#define ADV_TYPE_ADV_IND 0x00

Connectable and scannable undirected advertising.

## ◆ ADV_TYPE_ADV_NONCONN_IND

#define ADV_TYPE_ADV_NONCONN_IND 0x03

Non-Connectable undirected advertising.

## ◆ ADV_TYPE_SCAN_IND

#define ADV_TYPE_SCAN_IND 0x02

Scanable undirected advertising.

## ◆ ADV_TYPE_SCAN_RSP

#define ADV_TYPE_SCAN_RSP 0x04

Scan Response.