BLE_API v2.1.3

Variables
BLE GAP UUID Definitions
BLE Services » BLE Defined-Services » BLE GAP Service Definitions

## Variables
const uint16_t | ATTR_UUID_GAP_PRIMARY_SERVICE []
const uint16_t | ATTR_UUID_GAP_CHARC_DEVICE_NAME []
const uint16_t | ATTR_UUID_GAP_CHARC_APPEARANCE []
const uint16_t | ATTR_UUID_GAP_CHARC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS []

## Detailed Description

Here shows the definitions of the BLE GAP UUID Definitions.

## Variable Documentation

## ◆ ATTR_UUID_GAP_CHARC_APPEARANCE

const uint16_t ATTR_UUID_GAP_CHARC_APPEARANCE[]
| extern

GAP characteristic appearance UUID.

## ◆ ATTR_UUID_GAP_CHARC_DEVICE_NAME

const uint16_t ATTR_UUID_GAP_CHARC_DEVICE_NAME[]
| extern

GAP characteristic device name UUID.

## ◆ ATTR_UUID_GAP_CHARC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS

const uint16_t ATTR_UUID_GAP_CHARC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS[]
| extern

GAP characteristic peripheral preferred connection parameters UUID.

## ◆ ATTR_UUID_GAP_PRIMARY_SERVICE

const uint16_t ATTR_UUID_GAP_PRIMARY_SERVICE[]
| extern

GAP service UUID.