BLE_API v2.1.3

Data Fields
BLE_Event_ScanReportParam Struct Reference
BLE Common » BLE Structure Definition

BLE Event Scan Report Parameter. More...

`#include <ble_cmd.h>`

## Data Fields
BleAdvType | rptType
BLE_Addr_Param | rptPeerAddr
uint8_t | rptDataLength
uint8_t | rptData [31]
int8_t | rptRssi

## Detailed Description

BLE Event Scan Report Parameter.

## Field Documentation

## ◆ rptData

uint8_t BLE_Event_ScanReportParam::rptData[31]

Received advertising or scan response data.

## ◆ rptDataLength

uint8_t BLE_Event_ScanReportParam::rptDataLength

Received advertising or scan response data length.

## ◆ rptPeerAddr

BLE_Addr_Param BLE_Event_ScanReportParam::rptPeerAddr

Remote device address type and address.

## ◆ rptRssi

int8_t BLE_Event_ScanReportParam::rptRssi

Received Signal Strength Indication in dBm.

## ◆ rptType

BleAdvType BLE_Event_ScanReportParam::rptType

BLE advertising type.

The documentation for this struct was generated from the following file:

- Source/Include/ble_cmd.h