BLE_API v2.1.3

Data Fields
BLE_Conn_Param Struct Reference
BLE Common » BLE Structure Definition

BLE connection parameter. More...

`#include <ble_cmd.h>`

## Data Fields
uint16_t | connIntervalMin
uint16_t | connIntervalMax
uint16_t | connLatency
uint16_t | connSupervisionTimeout

## Detailed Description

BLE connection parameter.

## Field Documentation

## ◆ connIntervalMax

uint16_t BLE_Conn_Param::connIntervalMax

Maximum connection interval.

Note
  Connection interval = value * 1.25ms
  Connection interval range = CONN_INTERVAL_MIN ~ CONN_INTERVAL_MAX

## ◆ connIntervalMin

uint16_t BLE_Conn_Param::connIntervalMin

Minimum connection interval.

Note
  Connection interval = value * 1.25ms
  Connection interval range = CONN_INTERVAL_MIN ~ CONN_INTERVAL_MAX

## ◆ connLatency

uint16_t BLE_Conn_Param::connLatency

Slave latency for the connection in number of connection event.

Note
  Latency range = CONN_LATENCY_MIN to CONN_LATENCY_MAX

## ◆ connSupervisionTimeout

uint16_t BLE_Conn_Param::connSupervisionTimeout

Connection supervision timeout.

Note
  Supervision timeout = value * 10ms
  Supervision timeout range = CONN_SUBTIMEOUT_MIN ~ CONN_SUBTIMEOUT_MAX

The documentation for this struct was generated from the following file:

- Source/Include/ble_cmd.h