BLE_API v2.1.3

Macros
BLE GAP Service and Characteristic Definitions
BLE Services » BLE Defined-Services » BLE GAP Service Definitions

## Macros
#define | ATT_GAP_SERVICE
const ATTRIBUTE_BLE | ATT_GAP_PRIMARY_SERVICE
const ATTRIBUTE_BLE | ATT_GAP_CHARACTERISTIC_DEVICE_NAME
const ATTRIBUTE_BLE | ATT_GAP_DEVICE_NAME
const ATTRIBUTE_BLE | ATT_GAP_CHARACTERISTIC_APPEARANCE
const ATTRIBUTE_BLE | ATT_GAP_APPEARANCE
const ATTRIBUTE_BLE | ATT_GAP_CHARACTERISTIC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
const ATTRIBUTE_BLE | ATT_GAP_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS

## Detailed Description

Here shows the definitions of the GAP service and characteristic.

## Macro Definition Documentation

## ◆ ATT_GAP_SERVICE

#define ATT_GAP_SERVICE

Value:
&ATT_GAP_PRIMARY_SERVICE, \
&ATT_GAP_CHARACTERISTIC_DEVICE_NAME, \
&ATT_GAP_DEVICE_NAME, \
&ATT_GAP_CHARACTERISTIC_APPEARANCE, \
&ATT_GAP_APPEARANCE, \
&ATT_GAP_CHARACTERISTIC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS, \
&ATT_GAP_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS, \
ATT_GAP_APPEARANCE
const ATTRIBUTE_BLE ATT_GAP_APPEARANCE
ATT_GAP_DEVICE_NAME
const ATTRIBUTE_BLE ATT_GAP_DEVICE_NAME
ATT_GAP_CHARACTERISTIC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
const ATTRIBUTE_BLE ATT_GAP_CHARACTERISTIC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
ATT_GAP_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
const ATTRIBUTE_BLE ATT_GAP_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
ATT_GAP_CHARACTERISTIC_DEVICE_NAME
const ATTRIBUTE_BLE ATT_GAP_CHARACTERISTIC_DEVICE_NAME
ATT_GAP_PRIMARY_SERVICE
const ATTRIBUTE_BLE ATT_GAP_PRIMARY_SERVICE
ATT_GAP_CHARACTERISTIC_APPEARANCE
const ATTRIBUTE_BLE ATT_GAP_CHARACTERISTIC_APPEARANCE

GAP Service Definition

## Variable Documentation

## ◆ ATT_GAP_APPEARANCE

const ATTRIBUTE_BLE ATT_GAP_APPEARANCE
| extern

GAP appearance value.

## ◆ ATT_GAP_CHARACTERISTIC_APPEARANCE

const ATTRIBUTE_BLE ATT_GAP_CHARACTERISTIC_APPEARANCE
| extern

GAP characteristic appearance.

## ◆ ATT_GAP_CHARACTERISTIC_DEVICE_NAME

const ATTRIBUTE_BLE ATT_GAP_CHARACTERISTIC_DEVICE_NAME
| extern

GAP characteristic device name.

## ◆ ATT_GAP_CHARACTERISTIC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS

const ATTRIBUTE_BLE ATT_GAP_CHARACTERISTIC_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
| extern

GAP characteristic peripheral preferred connection parameters.

## ◆ ATT_GAP_DEVICE_NAME

const ATTRIBUTE_BLE ATT_GAP_DEVICE_NAME
| extern

GAP device name value.

## ◆ ATT_GAP_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS

const ATTRIBUTE_BLE ATT_GAP_PERIPHERAL_PREFERRED_CONNECTION_PARAMETERS
| extern

GAP peripheral preferred connection parameters value.

## ◆ ATT_GAP_PRIMARY_SERVICE

const ATTRIBUTE_BLE ATT_GAP_PRIMARY_SERVICE
| extern

GAP primary Service.