BLE_API v2.1.3

BLE Scan Interval Minimum and Maximum Definition
BLE Common » BLE Command Definition » BLE Scan Definition

## BleScanInterval
Define BLE scan interval minimum and maximum.
typedef uint8_t | BleScanIntervalRange
#define | SCAN_INTERVAL_MIN 0x0004
#define | SCAN_INTERVAL_MAX 0x4000

## Detailed Description

BLE scan Interval range definition.

## Macro Definition Documentation

## ◆ SCAN_INTERVAL_MAX

#define SCAN_INTERVAL_MAX 0x4000

The unit of scan interval is 0.625ms
Maximum scan interval is 10.24s = (0x4000 * 0.625) ms

## ◆ SCAN_INTERVAL_MIN

#define SCAN_INTERVAL_MIN 0x0004

The unit of scan interval is 0.625ms
Minimum scan interval is 2.5ms = (0x0004 * 0.625) ms