BLE_API v2.1.3

Variables
BLE Based UUID Definitions
BLE Services » BLE Service Based Definitions

## Variables
const uint16_t | ATTR_UUID_INVALID []
const uint16_t | ATTR_UUID_TYPE_PRIMARY_SERVICE []
const uint16_t | ATTR_UUID_TYPE_SECONDARY_SERVICE []
const uint16_t | ATTR_UUID_TYPE_INCLUDE []
const uint16_t | ATTR_UUID_TYPE_CHARACTERISTIC []
const uint16_t | ATTR_UUID_TYPE_CHARC_EXTENDED_PROPERTIES []
const uint16_t | ATTR_UUID_TYPE_CHARC_USER_DESCRIPTION []
const uint16_t | ATTR_UUID_TYPE_CLIENT_CHARC_CONFIGURATION []
const uint16_t | ATTR_UUID_TYPE_SERVER_CHARC_CONFIGURATION []
const uint16_t | ATTR_UUID_TYPE_CHARC_PRESENTATION_FORMAT []
const uint16_t | ATTR_UUID_TYPE_CHARC_AGGREGATE_FORMAT []
const uint16_t | ATTR_UUID_TYPE_VALID_RANGE []
const uint16_t | ATTR_UUID_TYPE_EXTERNAL_REPORT_REFERENCE []
const uint16_t | ATTR_UUID_TYPE_REPORT_REFERENCE []

## Detailed Description

Here shows the definitions of the BLE based UUID Definitions.

## Variable Documentation

## ◆ ATTR_UUID_INVALID

const uint16_t ATTR_UUID_INVALID[]
| extern

Invalid UUID.

## ◆ ATTR_UUID_TYPE_CHARACTERISTIC

const uint16_t ATTR_UUID_TYPE_CHARACTERISTIC[]
| extern

Characteristic UUID.

## ◆ ATTR_UUID_TYPE_CHARC_AGGREGATE_FORMAT

const uint16_t ATTR_UUID_TYPE_CHARC_AGGREGATE_FORMAT[]
| extern

Characteristic aggregate format UUID.

## ◆ ATTR_UUID_TYPE_CHARC_EXTENDED_PROPERTIES

const uint16_t ATTR_UUID_TYPE_CHARC_EXTENDED_PROPERTIES[]
| extern

Characteristic extended properties UUID.

## ◆ ATTR_UUID_TYPE_CHARC_PRESENTATION_FORMAT

const uint16_t ATTR_UUID_TYPE_CHARC_PRESENTATION_FORMAT[]
| extern

Characteristic presentation format UUID.

## ◆ ATTR_UUID_TYPE_CHARC_USER_DESCRIPTION

const uint16_t ATTR_UUID_TYPE_CHARC_USER_DESCRIPTION[]
| extern

Characteristic user description UUID.

## ◆ ATTR_UUID_TYPE_CLIENT_CHARC_CONFIGURATION

const uint16_t ATTR_UUID_TYPE_CLIENT_CHARC_CONFIGURATION[]
| extern

Client characteristic configuration descriptor UUID.

## ◆ ATTR_UUID_TYPE_EXTERNAL_REPORT_REFERENCE

const uint16_t ATTR_UUID_TYPE_EXTERNAL_REPORT_REFERENCE[]
| extern

External report reference UUID.

## ◆ ATTR_UUID_TYPE_INCLUDE

const uint16_t ATTR_UUID_TYPE_INCLUDE[]
| extern

Included Service UUID.

## ◆ ATTR_UUID_TYPE_PRIMARY_SERVICE

const uint16_t ATTR_UUID_TYPE_PRIMARY_SERVICE[]
| extern

Primary Service UUID.

## ◆ ATTR_UUID_TYPE_REPORT_REFERENCE

const uint16_t ATTR_UUID_TYPE_REPORT_REFERENCE[]
| extern

Report reference UUID.

## ◆ ATTR_UUID_TYPE_SECONDARY_SERVICE

const uint16_t ATTR_UUID_TYPE_SECONDARY_SERVICE[]
| extern

Secondary Service UUID.

## ◆ ATTR_UUID_TYPE_SERVER_CHARC_CONFIGURATION

const uint16_t ATTR_UUID_TYPE_SERVER_CHARC_CONFIGURATION[]
| extern

Client characteristic configuration UUID.

## ◆ ATTR_UUID_TYPE_VALID_RANGE

const uint16_t ATTR_UUID_TYPE_VALID_RANGE[]
| extern

Valid range UUID.