BLE_API v2.1.3

Macros | Typedefs
BLE GATT Client Characteristic Configuration Value Definition
BLE Common » BLE Command Definition

## Macros
#define | BLEGATT_CCCD_NONE 0x0000
#define | BLEGATT_CCCD_NOTIFICATION 0x0001
#define | BLEGATT_CCCD_INDICATION 0x0002
#define | BLEGATT_CCCD_NOTIFY_INDICATE 0x0003

## Typedefs
typedef uint16_t | BleGattCCCDValue

## Detailed Description

BLE GATT client characteristic configuration value definition.

## Macro Definition Documentation

## ◆ BLEGATT_CCCD_INDICATION

#define BLEGATT_CCCD_INDICATION 0x0002

The Characteristic shall be indicated.

## ◆ BLEGATT_CCCD_NONE

#define BLEGATT_CCCD_NONE 0x0000

Disabled notification/ indication.

## ◆ BLEGATT_CCCD_NOTIFICATION

#define BLEGATT_CCCD_NOTIFICATION 0x0001

The Characteristic shall be notified.

## ◆ BLEGATT_CCCD_NOTIFY_INDICATE

#define BLEGATT_CCCD_NOTIFY_INDICATE 0x0003

The Characteristic shall be both notified and indicated.