BLE_API v2.1.3

BLE Advertising Interval Minimum and Maximum Definition
BLE Common » BLE Command Definition » BLE Advertising Definition

## BleAdvInterval
Define BLE advertising interval minimum and maximum.
typedef uint8_t | BleAdvIntervalRange
#define | ADV_INTERVAL_MIN 0x0020
#define | ADV_INTERVAL_MAX 0x4000

## Detailed Description

BLE advertising interval range definition.

## Macro Definition Documentation

## ◆ ADV_INTERVAL_MAX

#define ADV_INTERVAL_MAX 0x4000

The unit of advertising interval is 0.625ms
Maximum advertising interval is 10.24s = (0x4000 * 0.625) ms

## ◆ ADV_INTERVAL_MIN

#define ADV_INTERVAL_MIN 0x0020

The unit of advertising interval is 0.625ms
Minimum advertising interval is 20ms = (0x20 * 0.625) ms