BLE_API v2.1.3

Macros | Typedefs
BLE GATT Characteristic Value Write Definition
BLE Common » BLE Command Definition

## Macros
#define | BLEGATT_WRITE 0x00
#define | BLEGATT_WRITE_WITHOUT_RSP 0x01

## Typedefs
typedef uint8_t | BleGattWrite

## Detailed Description

There are five sub-procedures that can be used to write a Characteristic Value.

## Macro Definition Documentation

## ◆ BLEGATT_WRITE

#define BLEGATT_WRITE 0x00

GATT write (Write request).

## ◆ BLEGATT_WRITE_WITHOUT_RSP

#define BLEGATT_WRITE_WITHOUT_RSP 0x01

GATT write without response (Write command).