BLE_API v2.1.3

Variables
BLE HRS UUID Definitions
BLE Services » BLE Defined-Services » BLE HRS Definitions

## Variables
const uint16_t | ATTR_UUID_HRS_PRIMARY_SERVICE []
const uint16_t | ATTR_UUID_HRS_CHARC_HEART_RATE_MEASUREMENT []
const uint16_t | ATTR_UUID_HRS_CHARC_BODY_SENSOR_LOCATION []

## Detailed Description

Here shows the definitions of the BLE HRS UUID Definitions.

## Variable Documentation

## ◆ ATTR_UUID_HRS_CHARC_BODY_SENSOR_LOCATION

const uint16_t ATTR_UUID_HRS_CHARC_BODY_SENSOR_LOCATION[]
| extern

Heart Rate body sensor location characteristic UUID.

## ◆ ATTR_UUID_HRS_CHARC_HEART_RATE_MEASUREMENT

const uint16_t ATTR_UUID_HRS_CHARC_HEART_RATE_MEASUREMENT[]
| extern

Heart Rate measurement characteristic UUID.

## ◆ ATTR_UUID_HRS_PRIMARY_SERVICE

const uint16_t ATTR_UUID_HRS_PRIMARY_SERVICE[]
| extern

Heart Rate Service UUID.