BLE_API v2.1.3

Variables
BLE UDF01S UUID Definitions
BLE Services » BLE Defined-Services » BLE UDF01S Definitions

## Variables
const uint16_t | ATTR_UUID_UDF01S_PRIMARY_SERVICE []
const uint16_t | ATTR_UUID_UDF01S_CHARC_UDATR01 []
const uint16_t | ATTR_UUID_UDF01S_CHARC_UDATN01 []
const uint16_t | ATTR_UUID_UDF01S_CHARC_UDATRW01 []

## Detailed Description

Here shows the definitions of the BLE UDF01S UUID Definitions.

## Variable Documentation

## ◆ ATTR_UUID_UDF01S_CHARC_UDATN01

const uint16_t ATTR_UUID_UDF01S_CHARC_UDATN01[]
| extern

UDF01S characteristic UDATN01 UUID.

## ◆ ATTR_UUID_UDF01S_CHARC_UDATR01

const uint16_t ATTR_UUID_UDF01S_CHARC_UDATR01[]
| extern

UDF01S characteristic UDATR01 UUID.

## ◆ ATTR_UUID_UDF01S_CHARC_UDATRW01

const uint16_t ATTR_UUID_UDF01S_CHARC_UDATRW01[]
| extern

UDF01S characteristic UDATRW01 UUID.

## ◆ ATTR_UUID_UDF01S_PRIMARY_SERVICE

const uint16_t ATTR_UUID_UDF01S_PRIMARY_SERVICE[]
| extern

UDF01S service UUID.