BLE_API v2.1.3

Variables
BLE BAS UUID Definitions
BLE Services » BLE Defined-Services » BLE BAS Definitions

## Variables
const uint16_t | ATTR_UUID_BAS_PRIMARY_SERVICE []
const uint16_t | ATTR_UUID_BAS_CHARC_BATTERY_LEVEL []

## Detailed Description

Here shows the definitions of the BLE BAS UUID Definitions.

## Variable Documentation

## ◆ ATTR_UUID_BAS_CHARC_BATTERY_LEVEL

const uint16_t ATTR_UUID_BAS_CHARC_BATTERY_LEVEL[]
| extern

BAS characteristic BATTERY_LEVEL UUID.

## ◆ ATTR_UUID_BAS_PRIMARY_SERVICE

const uint16_t ATTR_UUID_BAS_PRIMARY_SERVICE[]
| extern

BAS service UUID.