BLE_API v2.1.3

Macros
BLE Gap Flags Mode
BLE GAP Definition

## Macros
#define | GAP_FLAGS_LIMITED_DISCOVERABLE_MODE 0x01
#define | GAP_FLAGS_GENERAL_DISCOVERABLE_MODE 0x02
#define | GAP_FLAGS_BR_EDR_NOT_SUPPORTED 0x04
#define | GAP_FLAGS_SIMUL_DEV_CAP_CONTROLLER 0x08
#define | GAP_FLAGS_SIMUL_DEV_CAP_HOST 0x10
#define | BLE_GAP_FLAGS_LIMITED_DISCOVERABLE_MODE (GAP_FLAGS_LIMITED_DISCOVERABLE_MODE|GAP_FLAGS_BR_EDR_NOT_SUPPORTED)
#define | BLE_GAP_FLAGS_GENERAL_DISCOVERABLE_MODE (GAP_FLAGS_GENERAL_DISCOVERABLE_MODE|GAP_FLAGS_BR_EDR_NOT_SUPPORTED)

## Detailed Description

BLE Gap flags mode.

## Macro Definition Documentation

## ◆ BLE_GAP_FLAGS_GENERAL_DISCOVERABLE_MODE

#define BLE_GAP_FLAGS_GENERAL_DISCOVERABLE_MODE (GAP_FLAGS_GENERAL_DISCOVERABLE_MODE|GAP_FLAGS_BR_EDR_NOT_SUPPORTED)

LE general discoverable mode, BR/EDR not supported.

## ◆ BLE_GAP_FLAGS_LIMITED_DISCOVERABLE_MODE

#define BLE_GAP_FLAGS_LIMITED_DISCOVERABLE_MODE (GAP_FLAGS_LIMITED_DISCOVERABLE_MODE|GAP_FLAGS_BR_EDR_NOT_SUPPORTED)

LE limited discoverable mode, BR/EDR not supported.

## ◆ GAP_FLAGS_BR_EDR_NOT_SUPPORTED

#define GAP_FLAGS_BR_EDR_NOT_SUPPORTED 0x04

BR/EDR not supported.

## ◆ GAP_FLAGS_GENERAL_DISCOVERABLE_MODE

#define GAP_FLAGS_GENERAL_DISCOVERABLE_MODE 0x02

LE general discoverable mode

## ◆ GAP_FLAGS_LIMITED_DISCOVERABLE_MODE

#define GAP_FLAGS_LIMITED_DISCOVERABLE_MODE 0x01

LE limited discoverable mode

## ◆ GAP_FLAGS_SIMUL_DEV_CAP_CONTROLLER

#define GAP_FLAGS_SIMUL_DEV_CAP_CONTROLLER 0x08

Simultaneous LE and BR/EDR to same device capable (Controller).

## ◆ GAP_FLAGS_SIMUL_DEV_CAP_HOST

#define GAP_FLAGS_SIMUL_DEV_CAP_HOST 0x10

Simultaneous LE and BR/EDR to same device capable (Host).