BLE_API v2.1.3

Functions
MCU SPI I/O Re-mapping Function
Porting » MCU Porting Related » MCU Miscellaneous Porting » MCU Miscellaneous Porting Function

## Functions
void | setRF_SpiIoMapping (void)

## Detailed Description

Here shows the MCU SPI I/O re-mapping function.

## Function Documentation

## ◆ setRF_SpiIoMapping()

void setRF_SpiIoMapping | ( | void |  | ) |

MCU SPI IO mapping. Must do this after Power ON and MCU GPIO initialed.