BLE_API v2.1.3

Macros
The Exponent of Flash Programming Size Definition
Porting » MCU Porting Related » MCU Flash Porting Definition » MCU Flash Detail Porting Definition » Flash Page Size | Porting » MCU Porting Related » MCU Flash Porting Definition » MCU Flash Detail Porting Definition » Flash Page Size » Flash Programming Size

Defined supported the exponent of flash programming size. More...

## Macros
#define | FLASH_PROGRAM_SIZE_FOR_EXPONENT_0 0
#define | FLASH_PROGRAM_SIZE_FOR_EXPONENT_1 1
#define | FLASH_PROGRAM_SIZE_FOR_EXPONENT_2 2

## Detailed Description

Defined supported the exponent of flash programming size.

## Macro Definition Documentation

## ◆ FLASH_PROGRAM_SIZE_FOR_EXPONENT_0

#define FLASH_PROGRAM_SIZE_FOR_EXPONENT_0 0

FLASH_PROGRAM_SIZE = 2^exponent = 2^0 = 1

## ◆ FLASH_PROGRAM_SIZE_FOR_EXPONENT_1

#define FLASH_PROGRAM_SIZE_FOR_EXPONENT_1 1

FLASH_PROGRAM_SIZE = 2^exponent = 2^1 = 2

## ◆ FLASH_PROGRAM_SIZE_FOR_EXPONENT_2

#define FLASH_PROGRAM_SIZE_FOR_EXPONENT_2 2

FLASH_PROGRAM_SIZE = 2^exponent = 2^2 = 4