BLE_API v2.1.3

Macros
BLE Customer Characteristic UUID Definitions
BLE Services » BLE UUIDs » BLE GATT Characteristic UUID Definitions

## Macros
#define | GATT_CSTM_CHARC_UDATR01 0xFA01
#define | GATT_CSTM_CHARC_UDATN01 0xFA02
#define | GATT_CSTM_CHARC_UDATRW01 0xFA03
#define | GATT_CSTM_CHARC_UDATR02 0xFA04
#define | GATT_CSTM_CHARC_UDATN02 0xFA05
#define | GATT_CSTM_CHARC_UDATRW02 0xFA06
#define | GATT_CSTM_CHARC_UDATR03 0xFA07
#define | GATT_CSTM_CHARC_UDATN03 0xFA08
#define | GATT_CSTM_CHARC_UDATRW03 0xFA09

## Detailed Description

BLE customer characteristic UUID definitions.

## Macro Definition Documentation

## ◆ GATT_CSTM_CHARC_UDATN01

#define GATT_CSTM_CHARC_UDATN01 0xFA02

User Data Notification 01 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATN02

#define GATT_CSTM_CHARC_UDATN02 0xFA05

User Data Notification 02 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATN03

#define GATT_CSTM_CHARC_UDATN03 0xFA08

User Data Notification 03 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATR01

#define GATT_CSTM_CHARC_UDATR01 0xFA01

User Data Read 01 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATR02

#define GATT_CSTM_CHARC_UDATR02 0xFA04

User Data Read 02 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATR03

#define GATT_CSTM_CHARC_UDATR03 0xFA07

User Data Read 03 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATRW01

#define GATT_CSTM_CHARC_UDATRW01 0xFA03

User Data Read Write 01 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATRW02

#define GATT_CSTM_CHARC_UDATRW02 0xFA06

User Data Read Write 02 Characteristic UUID.

## ◆ GATT_CSTM_CHARC_UDATRW03

#define GATT_CSTM_CHARC_UDATRW03 0xFA09

User Data Read Write 03 Characteristic UUID.