BLE_API v2.1.3

Macros
MCU Wake-Up Required Time from Sleep Mode
RF PHY » RF PHY Definition.

## Macros
#define | MCU_WAKEUP_RETENSIONTIME_MAX 16
#define | MCU_WAKEUP_RETENSIONTIME_MIN 1

## Detailed Description

This parameter adjusts the retention time required for the MCU to wake up from sleep mode, plus some necessary parameters set via SPI operation. The unit of the MCU wake-up retention time is 125us.

Note
  The range of MCU wake-up retention time is 125us to 2ms.

## Macro Definition Documentation

## ◆ MCU_WAKEUP_RETENSIONTIME_MAX

#define MCU_WAKEUP_RETENSIONTIME_MAX 16

2ms = 16*125us

## ◆ MCU_WAKEUP_RETENSIONTIME_MIN

#define MCU_WAKEUP_RETENSIONTIME_MIN 1

125us = 1*125us