BLE_API v2.1.3

BLE Connection Supervision Timeout Range Definition
BLE Common » BLE Command Definition » BLE Connection Parameter Definition

## BleConnSupTimeout
Define BLE connection supervision timeout minimum and maximum.
typedef uint8_t | BleConnectionSupTimeoutRange
#define | CONN_SUBTIMEOUT_MIN 0x000A
#define | CONN_SUBTIMEOUT_MAX 0x0C80

## Detailed Description

BLE connection supervision timeout range definition.

## Macro Definition Documentation

## ◆ CONN_SUBTIMEOUT_MAX

#define CONN_SUBTIMEOUT_MAX 0x0C80

The unit of connection supervision timeout is 10ms
Maximum connection supervision timeout is 32s = (0x0C80 * 10) ms

## ◆ CONN_SUBTIMEOUT_MIN

#define CONN_SUBTIMEOUT_MIN 0x000A

The unit of connection supervision timeout is 10ms
Minimum connection supervision timeout is 100ms = (0x000A * 10) ms