BLE_API v2.1.3

Data Fields
BLEATT_HRS_Handles Struct Reference
BLE Services » BLE Defined-Services » BLE HRS Definitions » BLE HRS Application Definitions » BLE HRS Structure Definitions

`#include <ble_service_hrs.h>`

## Data Fields
uint16_t | hdl_heart_rate_measurement
uint16_t | hdl_heart_rate_measurement_cccd
uint16_t | hdl_body_sensor_location

## Detailed Description

HRS Handles Definition

## Field Documentation

## ◆ hdl_body_sensor_location

uint16_t BLEATT_HRS_Handles::hdl_body_sensor_location

Handle of Body sensor location.

## ◆ hdl_heart_rate_measurement

uint16_t BLEATT_HRS_Handles::hdl_heart_rate_measurement

Handle of Heart rate measurement.

## ◆ hdl_heart_rate_measurement_cccd

uint16_t BLEATT_HRS_Handles::hdl_heart_rate_measurement_cccd

Handle of Heart rate measurement client characteristic configuration descriptor.

The documentation for this struct was generated from the following file:

- Source/Service/HRS/ble_service_hrs.h