BLE_API v2.1.3

Functions
BLE DTM Function For MP
BLE Common » BLE Command Function

## Functions
BleStackStatus | setRF_MPTestContTx (uint8_t channel)

## Detailed Description

This file shows the BLE DTM functions for MP. (ble_rftone.h)

## Function Documentation

## ◆ setRF_MPTestContTx()

BleStackStatus setRF_MPTestContTx | ( | uint8_t | channel | ) |

Function for Enable Continuous TX for MP Test.

Note
  This function is defined in "ble_rftone.h"