BLE_API v2.1.3

Data Fields
BLEATT_HRS_Data Struct Reference
BLE Services » BLE Defined-Services » BLE HRS Definitions » BLE HRS Application Definitions » BLE HRS Structure Definitions

`#include <ble_service_hrs.h>`

## Data Fields
uint8_t | heart_rate_measurement [4]
uint16_t | heart_rate_measurement_cccd
uint8_t | body_sensor_location

## Detailed Description

HRS Data Definition

Note
  User defined.

## Field Documentation

## ◆ body_sensor_location

uint8_t BLEATT_HRS_Data::body_sensor_location

Body sensor location value

## ◆ heart_rate_measurement

uint8_t BLEATT_HRS_Data::heart_rate_measurement[4]

Heart rate measurement value: [0]: HRS Flag; [1]: Heart Rate Data [3][2]: Heart Rate RR-Interval

## ◆ heart_rate_measurement_cccd

uint16_t BLEATT_HRS_Data::heart_rate_measurement_cccd

Heart rate measurement cccd value

The documentation for this struct was generated from the following file:

- Source/Service/HRS/ble_service_hrs.h