BLE_API v2.1.3

### - a -

- addr : BLE_Addr_Param
- addrType : BLE_Addr_Param
- advChannelMap : BLE_Adv_Param
- advDirectAddrParam : BLE_Adv_Param
- advFilterPolicy : BLE_Adv_Param
- advIntervalMax : BLE_Adv_Param
- advIntervalMin : BLE_Adv_Param
- advType : BLE_Adv_Param
- appearance : BLEATT_GAP_Data
- att_handler : Att_Error_Rsp_Data
- attCallFunc : ATTRIBUTE_BLE
- attDbParsedResultparam : BLE_Event_AttDbParsedParam

### - b -

- battery_level : BLEATT_BAS_Data
- battery_level_cccd : BLEATT_BAS_Data
- body_sensor_location : BLEATT_HRS_Data
- bondingFlags : BLE_BondingFlags_Param

### - c -

- cfgClientCharc : ATTRIBUTE_BLE_Hdl_Para
- cfgServerCharc : ATTRIBUTE_BLE_Hdl_Para
- clientDB : ATTR_DB_Role_by_ID
- cmdAccess : BLE_Event_AttParam
- connInterval : BLE_Event_ConnParam , BLE_Event_ConnUpdateParam
- connIntervalMax : BLE_Conn_Param
- connIntervalMin : BLE_Conn_Param
- connLatency : BLE_Conn_Param , BLE_Event_ConnParam , BLE_Event_ConnUpdateParam
- connRole : BLE_Event_ConnParam
- connSupervisionTimeout : BLE_Conn_Param , BLE_Event_ConnParam , BLE_Event_ConnUpdateParam

### - d -

- data : BLE_Event_AttParam , BLEATT_BAS_Info , BLEATT_FOTA_Info , BLEATT_GATT_Info , BLEATT_HRS_Info , BLEATT_UDF01S_Info
- dataLenparam : BLE_Event_DataLengthParam
- description : Charac_Presentation_Format
- device_name : BLEATT_GAP_Data
- device_name_len : BLEATT_GAP_Data
- disconnectReason : BLE_Event_DisconnParam

### - e -

- error_code : Att_Error_Rsp_Data
- exponent : Charac_Presentation_Format

### - f -

- firmware_rev_format : BLEATT_DIS_Data
- firmware_rev_str : BLEATT_DIS_Data
- format : Charac_Presentation_Format
- fota_command_cccd : BLEATT_FOTA_Data
- fota_data_cccd : BLEATT_FOTA_Data

### - g -

- gattRole : BLE_Event_AttParam

### - h -

- handles : BLEATT_BAS_Info , BLEATT_DIS_Info , BLEATT_FOTA_Info , BLEATT_GAP_Info , BLEATT_GATT_Info , BLEATT_HRS_Info , BLEATT_UDF01S_Info
- hardware_rev_format : BLEATT_DIS_Data
- hardware_rev_str : BLEATT_DIS_Data
- hdl_appearance : BLEATT_GAP_Handles
- hdl_battery_level : BLEATT_BAS_Handles
- hdl_battery_level_cccd : BLEATT_BAS_Handles
- hdl_body_sensor_location : BLEATT_HRS_Handles
- hdl_device_name : BLEATT_GAP_Handles
- hdl_firmware_revision_string : BLEATT_DIS_Handles
- hdl_firmware_revision_string_format : BLEATT_DIS_Handles
- hdl_fota_command : BLEATT_FOTA_Handles
- hdl_fota_command_cccd : BLEATT_FOTA_Handles
- hdl_fota_command_user_description : BLEATT_FOTA_Handles
- hdl_fota_data : BLEATT_FOTA_Handles
- hdl_fota_data_cccd : BLEATT_FOTA_Handles
- hdl_fota_data_user_description : BLEATT_FOTA_Handles
- hdl_hardware_revision_string : BLEATT_DIS_Handles
- hdl_hardware_revision_string_format : BLEATT_DIS_Handles
- hdl_heart_rate_measurement : BLEATT_HRS_Handles
- hdl_heart_rate_measurement_cccd : BLEATT_HRS_Handles
- hdl_manufacturer_name_string : BLEATT_DIS_Handles
- hdl_manufacturer_name_string_format : BLEATT_DIS_Handles
- hdl_model_number_string : BLEATT_DIS_Handles
- hdl_model_number_string_format : BLEATT_DIS_Handles
- hdl_peripheral_preferred_connParam : BLEATT_GAP_Handles
- hdl_pnp_id : BLEATT_DIS_Handles
- hdl_serial_number_string : BLEATT_DIS_Handles
- hdl_serial_number_string_format : BLEATT_DIS_Handles
- hdl_service_changed : BLEATT_GATT_Handles
- hdl_service_changed_cccd : BLEATT_GATT_Handles
- hdl_software_revision_string : BLEATT_DIS_Handles
- hdl_software_revision_string_format : BLEATT_DIS_Handles
- hdl_system_id : BLEATT_DIS_Handles
- hdl_udatn01 : BLEATT_UDF01S_Handles
- hdl_udatn01_cccd : BLEATT_UDF01S_Handles
- hdl_udatr01 : BLEATT_UDF01S_Handles
- hdl_udatrw01 : BLEATT_UDF01S_Handles
- hdlNum : BLE_Event_AttParam
- heart_rate_measurement : BLEATT_HRS_Data
- heart_rate_measurement_cccd : BLEATT_HRS_Data
- hostId : BLE_Event_AttDbParsed_Param , BLE_Event_AttParam , BLE_Event_AuthStatusParam , BLE_Event_ConnParam , BLE_Event_ConnUpdateParam , BLE_Event_DataLengthParam , BLE_Event_DisconnParam , BLE_Event_MtuParam , BLE_Event_PassKeyConfirmParam , BLE_Event_PhyParam , BLE_Event_PhyUpdateParam , BLE_Event_RssiParam , BLE_Event_StkGenMethodParam , Service_Basic_Info

### - i -

- index : Service_Basic_Info
- ioCapsParam : BLE_IOCaps_Param

### - l -

- length : BLE_Event_AttParam , String_Format
- lenValue : ATTRIBUTE_BLE

### - m -

- manufacturer_id : SystemId_Format
- manufacturer_name_format : BLEATT_DIS_Data
- manufacturer_name_str : BLEATT_DIS_Data
- mapClientDB : ATTR_DB_Mapping_by_ID
- mapServerDB : ATTR_DB_Mapping_by_ID
- model_number_format : BLEATT_DIS_Data
- model_number_str : BLEATT_DIS_Data
- mtuSize : BLE_Event_MtuParam

### - n -

- name_space : Charac_Presentation_Format
- numHDL : ATTRIBUTE_BLE_Hdl_Para

### - o -

- organizationally_unique_id : SystemId_Format

### - p -

- peerAddr : BLE_Event_ConnParam
- peripheral_conn_param : BLEATT_GAP_Data
- permFormatDB : ATTRIBUTE_BLE
- phy : BLE_Event_PhyParam , BLE_Event_PhyUpdateParam
- pnp_id : BLEATT_DIS_Data
- product_id : PnPId_Format
- product_version : PnPId_Format
- propertyValue : ATTRIBUTE_BLE , ATTRIBUTE_BLE_Hdl_Para

### - r -

- request_opcode : Att_Error_Rsp_Data
- result : BLE_Event_AttDbParsed_Param
- role : BLEATT_BAS_Info , BLEATT_DIS_Info , BLEATT_FOTA_Info , BLEATT_GAP_Info , BLEATT_GATT_Info , BLEATT_HRS_Info , BLEATT_UDF01S_Info , Service_Basic_Info
- rptData : BLE_Event_ScanReportParam
- rptDataLength : BLE_Event_ScanReportParam
- rptPeerAddr : BLE_Event_ScanReportParam
- rptRssi : BLE_Event_ScanReportParam
- rptType : BLE_Event_ScanReportParam
- rssi : BLE_Event_RssiParam
- rxMaxOctets : BLE_DataLength_Param
- rxPhy : BLE_Phy_Param

### - s -

- scanFilterPolicy : BLE_Scan_Param
- scanInterval : BLE_Scan_Param
- scanType : BLE_Scan_Param
- scanWindow : BLE_Scan_Param
- serial_number_format : BLEATT_DIS_Data
- serial_number_str : BLEATT_DIS_Data
- serverDB : ATTR_DB_Role_by_ID
- service_changed_cccd : BLEATT_GATT_Data
- sizeMapClientDB : ATTR_DB_Mapping_by_ID_size
- sizeMapServerDB : ATTR_DB_Mapping_by_ID_size
- software_rev_format : BLEATT_DIS_Data
- software_rev_str : BLEATT_DIS_Data
- status : BLE_Event_AdvCompleteParam , BLE_Event_AuthStatusParam , BLE_Event_ConnParam , BLE_Event_ConnUpdateParam , BLE_Event_CreateConnParam , BLE_Event_PhyUpdateParam
- stkGenMethod : BLE_Event_StkGenMethodParam
- str : String_Format
- system_id : BLEATT_DIS_Data

### - t -

- txMaxOctets : BLE_DataLength_Param
- txPhy : BLE_Phy_Param

### - u -

- udatn01_cccd : BLEATT_UDF01S_Data
- unit : Charac_Presentation_Format
- uuidType : ATTRIBUTE_BLE
- uuidValue : ATTRIBUTE_BLE

### - v -

- value : ATTRIBUTE_BLE_Hdl_Para
- vendor_id : PnPId_Format
- vendor_id_source : PnPId_Format