BLE_API v2.1.3

BLE Scan Window Minimum and Maximum Definition
BLE Common » BLE Command Definition » BLE Scan Definition

## BleScanWindow
Define BLE Scan window minimum and maximum.
typedef uint8_t | BleScanWindowRange
#define | SCAN_WINDOW_MIN 0x0004
#define | SCAN_WINDOW_MAX 0x4000

## Detailed Description

BLE scan window range definition.

## Macro Definition Documentation

## ◆ SCAN_WINDOW_MAX

#define SCAN_WINDOW_MAX 0x4000

The unit of scan window is 0.625ms
Maximum scan window is 10.24s = (0x4000 * 0.625) ms

## ◆ SCAN_WINDOW_MIN

#define SCAN_WINDOW_MIN 0x0004

The unit of scan window is 0.625ms
Minimum scan window is 2.5ms = (0x0004 * 0.625) ms