BLE_API v2.1.3

Macros
BLE FOTA Service and Characteristic Definitions
BLE Services » BLE Defined-Services » BLE FOTA Definitions

## Macros
#define | ATT_FOTA_SERVICE
const ATTRIBUTE_BLE | ATT_FOTA_PRIMARY_SERVICE
const ATTRIBUTE_BLE | ATT_FOTA_CHARACTERISTIC_DATA
const ATTRIBUTE_BLE | ATT_FOTA_DATA
const ATTRIBUTE_BLE | ATT_FOTA_DATA_CLIENT_CHARC_CONFIGURATION
const ATTRIBUTE_BLE | ATT_FOTA_DATA_USER_DESCRIPTION
const ATTRIBUTE_BLE | ATT_FOTA_CHARACTERISTIC_COMMAND
const ATTRIBUTE_BLE | ATT_FOTA_COMMAND
const ATTRIBUTE_BLE | ATT_FOTA_COMMAND_CLIENT_CHARC_CONFIGURATION
const ATTRIBUTE_BLE | ATT_FOTA_COMMAND_USER_DESCRIPTION

## Detailed Description

Here shows the definitions of the FOTA service and characteristic.

## Macro Definition Documentation

## ◆ ATT_FOTA_SERVICE

#define ATT_FOTA_SERVICE

Value:
&ATT_FOTA_PRIMARY_SERVICE, \
&ATT_FOTA_CHARACTERISTIC_DATA, \
&ATT_FOTA_DATA, \
&ATT_FOTA_DATA_CLIENT_CHARC_CONFIGURATION, \
&ATT_FOTA_DATA_USER_DESCRIPTION, \
&ATT_FOTA_CHARACTERISTIC_COMMAND, \
&ATT_FOTA_COMMAND, \
&ATT_FOTA_COMMAND_CLIENT_CHARC_CONFIGURATION, \
&ATT_FOTA_COMMAND_USER_DESCRIPTION,
ATT_FOTA_CHARACTERISTIC_COMMAND
const ATTRIBUTE_BLE ATT_FOTA_CHARACTERISTIC_COMMAND
ATT_FOTA_PRIMARY_SERVICE
const ATTRIBUTE_BLE ATT_FOTA_PRIMARY_SERVICE
ATT_FOTA_COMMAND_CLIENT_CHARC_CONFIGURATION
const ATTRIBUTE_BLE ATT_FOTA_COMMAND_CLIENT_CHARC_CONFIGURATION
ATT_FOTA_DATA_USER_DESCRIPTION
const ATTRIBUTE_BLE ATT_FOTA_DATA_USER_DESCRIPTION
ATT_FOTA_DATA
const ATTRIBUTE_BLE ATT_FOTA_DATA
ATT_FOTA_COMMAND_USER_DESCRIPTION
const ATTRIBUTE_BLE ATT_FOTA_COMMAND_USER_DESCRIPTION
ATT_FOTA_DATA_CLIENT_CHARC_CONFIGURATION
const ATTRIBUTE_BLE ATT_FOTA_DATA_CLIENT_CHARC_CONFIGURATION
ATT_FOTA_COMMAND
const ATTRIBUTE_BLE ATT_FOTA_COMMAND
ATT_FOTA_CHARACTERISTIC_DATA
const ATTRIBUTE_BLE ATT_FOTA_CHARACTERISTIC_DATA

FOTA Service Definition

## Variable Documentation

## ◆ ATT_FOTA_CHARACTERISTIC_COMMAND

const ATTRIBUTE_BLE ATT_FOTA_CHARACTERISTIC_COMMAND
| extern

FOTA characteristic COMMAND.

## ◆ ATT_FOTA_CHARACTERISTIC_DATA

const ATTRIBUTE_BLE ATT_FOTA_CHARACTERISTIC_DATA
| extern

FOTA characteristic DATA.

## ◆ ATT_FOTA_COMMAND

const ATTRIBUTE_BLE ATT_FOTA_COMMAND
| extern

FOTA COMMAND value.

## ◆ ATT_FOTA_COMMAND_CLIENT_CHARC_CONFIGURATION

const ATTRIBUTE_BLE ATT_FOTA_COMMAND_CLIENT_CHARC_CONFIGURATION
| extern

FOTA COMMAND client characteristic configuration descriptor.

## ◆ ATT_FOTA_COMMAND_USER_DESCRIPTION

const ATTRIBUTE_BLE ATT_FOTA_COMMAND_USER_DESCRIPTION
| extern

FOTA COMMAND user description.

## ◆ ATT_FOTA_DATA

const ATTRIBUTE_BLE ATT_FOTA_DATA
| extern

FOTA DATA value.

## ◆ ATT_FOTA_DATA_CLIENT_CHARC_CONFIGURATION

const ATTRIBUTE_BLE ATT_FOTA_DATA_CLIENT_CHARC_CONFIGURATION
| extern

FOTA DATA client characteristic configuration descriptor.

## ◆ ATT_FOTA_DATA_USER_DESCRIPTION

const ATTRIBUTE_BLE ATT_FOTA_DATA_USER_DESCRIPTION
| extern

FOTA DATA user description.

## ◆ ATT_FOTA_PRIMARY_SERVICE

const ATTRIBUTE_BLE ATT_FOTA_PRIMARY_SERVICE
| extern

FOTA primary service.