| MINI51DE_BSP V3.02.003 The Board Support Package for Mini51DE Series MCU

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - u -

- u32_I2C_SW_Delay : i2c_software_gpio.c
- u32I2C_ByteSize : i2c_software_gpio_with_timer.c
- u32I2C_ByteSizeCount : i2c_software_gpio_with_timer.c
- u8I2C_Buffer : i2c_software_gpio_with_timer.c
- UART : Mini51Series.h
- UART0 : Mini51Series.h
- UART_ALT_CSR_ADDR_MATCH_Msk : Mini51Series.h
- UART_ALT_CSR_ADDR_MATCH_Pos : Mini51Series.h
- UART_ALT_CSR_RS485_AAD_Msk : Mini51Series.h
- UART_ALT_CSR_RS485_AAD_Pos : Mini51Series.h
- UART_ALT_CSR_RS485_ADD_EN_Msk : Mini51Series.h
- UART_ALT_CSR_RS485_ADD_EN_Pos : Mini51Series.h
- UART_ALT_CSR_RS485_AUD_Msk : Mini51Series.h
- UART_ALT_CSR_RS485_AUD_Pos : Mini51Series.h
- UART_ALT_CSR_RS485_NMM_Msk : Mini51Series.h
- UART_ALT_CSR_RS485_NMM_Pos : Mini51Series.h
- UART_BASE : Mini51Series.h
- UART_BAUD_BRD_Msk : Mini51Series.h
- UART_BAUD_BRD_Pos : Mini51Series.h
- UART_BAUD_DIV_X_EN_Msk : Mini51Series.h
- UART_BAUD_DIV_X_EN_Pos : Mini51Series.h
- UART_BAUD_DIV_X_ONE_Msk : Mini51Series.h
- UART_BAUD_DIV_X_ONE_Pos : Mini51Series.h
- UART_BAUD_DIVIDER_X_Msk : Mini51Series.h
- UART_BAUD_DIVIDER_X_Pos : Mini51Series.h
- UART_BAUD_MODE0 : uart.h
- UART_BAUD_MODE0_DIVIDER : uart.h
- UART_BAUD_MODE2 : uart.h
- UART_BAUD_MODE2_DIVIDER : uart.h
- UART_CLEAR_RTS() : uart.h
- UART_ClearIntFlag() : uart.h
- UART_Close() : uart.h
- UART_DISABLE_INT : uart.h
- UART_DisableFlowCtrl() : uart.h
- UART_DisableInt() : uart.h
- UART_ENABLE_INT : uart.h
- UART_EnableFlowCtrl() : uart.h
- UART_EnableInt() : uart.h
- UART_FCR_RFITL_14BYTES : uart.h
- UART_FCR_RFITL_1BYTE : uart.h
- UART_FCR_RFITL_4BYTES : uart.h
- UART_FCR_RFITL_8BYTES : uart.h
- UART_FCR_RFITL_Msk : Mini51Series.h
- UART_FCR_RFITL_Pos : Mini51Series.h
- UART_FCR_RFR_Msk : Mini51Series.h
- UART_FCR_RFR_Pos : Mini51Series.h
- UART_FCR_RTS_TRI_LEV_14BYTES : uart.h
- UART_FCR_RTS_TRI_LEV_1BYTE : uart.h
- UART_FCR_RTS_TRI_LEV_4BYTES : uart.h
- UART_FCR_RTS_TRI_LEV_8BYTES : uart.h
- UART_FCR_RTS_TRI_LEV_Msk : Mini51Series.h
- UART_FCR_RTS_TRI_LEV_Pos : Mini51Series.h
- UART_FCR_RX_DIS_Msk : Mini51Series.h
- UART_FCR_RX_DIS_Pos : Mini51Series.h
- UART_FCR_TFR_Msk : Mini51Series.h
- UART_FCR_TFR_Pos : Mini51Series.h
- UART_FSR_BIF_Msk : Mini51Series.h
- UART_FSR_BIF_Pos : Mini51Series.h
- UART_FSR_FEF_Msk : Mini51Series.h
- UART_FSR_FEF_Pos : Mini51Series.h
- UART_FSR_PEF_Msk : Mini51Series.h
- UART_FSR_PEF_Pos : Mini51Series.h
- UART_FSR_RS485_ADD_DETF_Msk : Mini51Series.h
- UART_FSR_RS485_ADD_DETF_Pos : Mini51Series.h
- UART_FSR_RX_EMPTY_Msk : Mini51Series.h
- UART_FSR_RX_EMPTY_Pos : Mini51Series.h
- UART_FSR_RX_FULL_Msk : Mini51Series.h
- UART_FSR_RX_FULL_Pos : Mini51Series.h
- UART_FSR_RX_OVER_IF_Msk : Mini51Series.h
- UART_FSR_RX_OVER_IF_Pos : Mini51Series.h
- UART_FSR_RX_POINTER_Msk : Mini51Series.h
- UART_FSR_RX_POINTER_Pos : Mini51Series.h
- UART_FSR_TE_FLAG_Msk : Mini51Series.h
- UART_FSR_TE_FLAG_Pos : Mini51Series.h
- UART_FSR_TX_EMPTY_Msk : Mini51Series.h
- UART_FSR_TX_EMPTY_Pos : Mini51Series.h
- UART_FSR_TX_FULL_Msk : Mini51Series.h
- UART_FSR_TX_FULL_Pos : Mini51Series.h
- UART_FSR_TX_OVER_IF_Msk : Mini51Series.h
- UART_FSR_TX_OVER_IF_Pos : Mini51Series.h
- UART_FSR_TX_POINTER_Msk : Mini51Series.h
- UART_FSR_TX_POINTER_Pos : Mini51Series.h
- UART_FUN_SEL_FUN_SEL_Msk : Mini51Series.h
- UART_FUN_SEL_FUN_SEL_Pos : Mini51Series.h
- UART_FUNC_SEL_IrDA : uart.h
- UART_FUNC_SEL_RS485 : uart.h
- UART_FUNC_SEL_UART : uart.h
- UART_GET_INT_FLAG : uart.h
- UART_GET_RX_EMPTY : uart.h
- UART_GET_RX_FULL : uart.h
- UART_GET_TX_EMPTY : uart.h
- UART_GET_TX_FULL : uart.h
- UART_IER_AUTO_CTS_EN_Msk : Mini51Series.h
- UART_IER_AUTO_CTS_EN_Pos : Mini51Series.h
- UART_IER_AUTO_RTS_EN_Msk : Mini51Series.h
- UART_IER_AUTO_RTS_EN_Pos : Mini51Series.h
- UART_IER_BUF_ERR_IEN_Msk : Mini51Series.h
- UART_IER_BUF_ERR_IEN_Pos : Mini51Series.h
- UART_IER_MODEM_IEN_Msk : Mini51Series.h
- UART_IER_MODEM_IEN_Pos : Mini51Series.h
- UART_IER_RDA_IEN_Msk : Mini51Series.h
- UART_IER_RDA_IEN_Pos : Mini51Series.h
- UART_IER_RLS_IEN_Msk : Mini51Series.h
- UART_IER_RLS_IEN_Pos : Mini51Series.h
- UART_IER_RTO_IEN_Msk : Mini51Series.h
- UART_IER_RTO_IEN_Pos : Mini51Series.h
- UART_IER_THRE_IEN_Msk : Mini51Series.h
- UART_IER_THRE_IEN_Pos : Mini51Series.h
- UART_IER_TIME_OUT_EN_Msk : Mini51Series.h
- UART_IER_TIME_OUT_EN_Pos : Mini51Series.h
- UART_IER_WAKE_EN_Msk : Mini51Series.h
- UART_IER_WAKE_EN_Pos : Mini51Series.h
- UART_IRCR_INV_RX_Msk : Mini51Series.h
- UART_IRCR_INV_RX_Pos : Mini51Series.h
- UART_IRCR_INV_TX_Msk : Mini51Series.h
- UART_IRCR_INV_TX_Pos : Mini51Series.h
- UART_IRCR_TX_SELECT_Msk : Mini51Series.h
- UART_IRCR_TX_SELECT_Pos : Mini51Series.h
- UART_IRQn : Mini51Series.h
- UART_IS_RX_FULL : uart.h
- UART_IS_RX_READY : uart.h
- UART_IS_TX_EMPTY : uart.h
- UART_IS_TX_FULL : uart.h
- UART_ISR_BUF_ERR_IF_Msk : Mini51Series.h
- UART_ISR_BUF_ERR_IF_Pos : Mini51Series.h
- UART_ISR_BUF_ERR_INT_Msk : Mini51Series.h
- UART_ISR_BUF_ERR_INT_Pos : Mini51Series.h
- UART_ISR_MODEM_IF_Msk : Mini51Series.h
- UART_ISR_MODEM_IF_Pos : Mini51Series.h
- UART_ISR_MODEM_INT_Msk : Mini51Series.h
- UART_ISR_MODEM_INT_Pos : Mini51Series.h
- UART_ISR_RDA_IF_Msk : Mini51Series.h
- UART_ISR_RDA_IF_Pos : Mini51Series.h
- UART_ISR_RDA_INT_Msk : Mini51Series.h
- UART_ISR_RDA_INT_Pos : Mini51Series.h
- UART_ISR_RLS_IF_Msk : Mini51Series.h
- UART_ISR_RLS_IF_Pos : Mini51Series.h
- UART_ISR_RLS_INT_Msk : Mini51Series.h
- UART_ISR_RLS_INT_Pos : Mini51Series.h
- UART_ISR_THRE_IF_Msk : Mini51Series.h
- UART_ISR_THRE_IF_Pos : Mini51Series.h
- UART_ISR_THRE_INT_Msk : Mini51Series.h
- UART_ISR_THRE_INT_Pos : Mini51Series.h
- UART_ISR_TOUT_IF_Msk : Mini51Series.h
- UART_ISR_TOUT_IF_Pos : Mini51Series.h
- UART_ISR_TOUT_INT_Msk : Mini51Series.h
- UART_ISR_TOUT_INT_Pos : Mini51Series.h
- UART_LCR_BCB_Msk : Mini51Series.h
- UART_LCR_BCB_Pos : Mini51Series.h
- UART_LCR_EPE_Msk : Mini51Series.h
- UART_LCR_EPE_Pos : Mini51Series.h
- UART_LCR_NSB_Msk : Mini51Series.h
- UART_LCR_NSB_Pos : Mini51Series.h
- UART_LCR_PBE_Msk : Mini51Series.h
- UART_LCR_PBE_Pos : Mini51Series.h
- UART_LCR_SPE_Msk : Mini51Series.h
- UART_LCR_SPE_Pos : Mini51Series.h
- UART_LCR_WLS_Msk : Mini51Series.h
- UART_LCR_WLS_Pos : Mini51Series.h
- UART_MCR_LEV_RTS_Msk : Mini51Series.h
- UART_MCR_LEV_RTS_Pos : Mini51Series.h
- UART_MCR_RTS_Msk : Mini51Series.h
- UART_MCR_RTS_Pos : Mini51Series.h
- UART_MCR_RTS_ST_Msk : Mini51Series.h
- UART_MCR_RTS_ST_Pos : Mini51Series.h
- UART_MODULE : clk.h
- UART_MSR_CTS_ST_Msk : Mini51Series.h
- UART_MSR_CTS_ST_Pos : Mini51Series.h
- UART_MSR_DCTSF_Msk : Mini51Series.h
- UART_MSR_DCTSF_Pos : Mini51Series.h
- UART_MSR_LEV_CTS_Msk : Mini51Series.h
- UART_MSR_LEV_CTS_Pos : Mini51Series.h
- UART_Open() : uart.h
- UART_PARITY_EVEN : uart.h
- UART_PARITY_MARK : uart.h
- UART_PARITY_NONE : uart.h
- UART_PARITY_ODD : uart.h
- UART_PARITY_SPACE : uart.h
- UART_RBR_RBR_Msk : Mini51Series.h
- UART_RBR_RBR_Pos : Mini51Series.h
- UART_Read() : uart.h
- UART_READ : uart.h
- UART_RS485_CLEAR_ADDR_FLAG : uart.h
- UART_RS485_GET_ADDR_FLAG : uart.h
- UART_RST : sys.h
- UART_RTS_IS_HIGH_LEV_TRG : uart.h
- UART_RTS_IS_LOW_LEV_TRG : uart.h
- UART_SelectIrDAMode() : uart.h
- UART_SelectRS485Mode() : uart.h
- UART_SET_RTS() : uart.h
- UART_SetLine_Config() : uart.h
- UART_SetTimeoutCnt() : uart.h
- UART_STOP_BIT_1 : uart.h
- UART_STOP_BIT_1_5 : uart.h
- UART_STOP_BIT_2 : uart.h
- UART_THR_THR_Msk : Mini51Series.h
- UART_THR_THR_Pos : Mini51Series.h
- UART_TOR_DLY_Msk : Mini51Series.h
- UART_TOR_DLY_Pos : Mini51Series.h
- UART_TOR_TOIC_Msk : Mini51Series.h
- UART_TOR_TOIC_Pos : Mini51Series.h
- UART_WAIT_TX_EMPTY : uart.h
- UART_WORD_LEN_5 : uart.h
- UART_WORD_LEN_6 : uart.h
- UART_WORD_LEN_7 : uart.h
- UART_WORD_LEN_8 : uart.h
- UART_Write() : uart.h
- UART_WRITE : uart.h