| MINI51DE_BSP V3.02.003 The Board Support Package for Mini51DE Series MCU

### - s -

- SPI : Mini51Series.h
- SPI0 : Mini51Series.h
- SPI_ABORT_3WIRE_TRANSFER : spi.h
- SPI_BASE : Mini51Series.h
- SPI_CLR_3WIRE_START_INT_FLAG : spi.h
- SPI_CLR_UNIT_TRANS_INT_FLAG : spi.h
- SPI_CNTRL2_BCn_Msk : Mini51Series.h
- SPI_CNTRL2_BCn_Pos : Mini51Series.h
- SPI_CNTRL2_NOSLVSEL_Msk : Mini51Series.h
- SPI_CNTRL2_NOSLVSEL_Pos : Mini51Series.h
- SPI_CNTRL2_SLV_ABORT_Msk : Mini51Series.h
- SPI_CNTRL2_SLV_ABORT_Pos : Mini51Series.h
- SPI_CNTRL2_SLV_START_INTSTS_Msk : Mini51Series.h
- SPI_CNTRL2_SLV_START_INTSTS_Pos : Mini51Series.h
- SPI_CNTRL2_SS_INT_OPT_Msk : Mini51Series.h
- SPI_CNTRL2_SS_INT_OPT_Pos : Mini51Series.h
- SPI_CNTRL2_SSTA_INTEN_Msk : Mini51Series.h
- SPI_CNTRL2_SSTA_INTEN_Pos : Mini51Series.h
- SPI_CNTRL_CLKP_Msk : Mini51Series.h
- SPI_CNTRL_CLKP_Pos : Mini51Series.h
- SPI_CNTRL_FIFO_Msk : Mini51Series.h
- SPI_CNTRL_FIFO_Pos : Mini51Series.h
- SPI_CNTRL_GO_BUSY_Msk : Mini51Series.h
- SPI_CNTRL_GO_BUSY_Pos : Mini51Series.h
- SPI_CNTRL_IE_Msk : Mini51Series.h
- SPI_CNTRL_IE_Pos : Mini51Series.h
- SPI_CNTRL_IF_Msk : Mini51Series.h
- SPI_CNTRL_IF_Pos : Mini51Series.h
- SPI_CNTRL_LSB_Msk : Mini51Series.h
- SPI_CNTRL_LSB_Pos : Mini51Series.h
- SPI_CNTRL_REORDER_Msk : Mini51Series.h
- SPI_CNTRL_REORDER_Pos : Mini51Series.h
- SPI_CNTRL_RX_EMPTY_Msk : Mini51Series.h
- SPI_CNTRL_RX_EMPTY_Pos : Mini51Series.h
- SPI_CNTRL_RX_FULL_Msk : Mini51Series.h
- SPI_CNTRL_RX_FULL_Pos : Mini51Series.h
- SPI_CNTRL_RX_NEG_Msk : Mini51Series.h
- SPI_CNTRL_RX_NEG_Pos : Mini51Series.h
- SPI_CNTRL_SLAVE_Msk : Mini51Series.h
- SPI_CNTRL_SLAVE_Pos : Mini51Series.h
- SPI_CNTRL_SP_CYCLE_Msk : Mini51Series.h
- SPI_CNTRL_SP_CYCLE_Pos : Mini51Series.h
- SPI_CNTRL_TX_BIT_LEN_Msk : Mini51Series.h
- SPI_CNTRL_TX_BIT_LEN_Pos : Mini51Series.h
- SPI_CNTRL_TX_EMPTY_Msk : Mini51Series.h
- SPI_CNTRL_TX_EMPTY_Pos : Mini51Series.h
- SPI_CNTRL_TX_FULL_Msk : Mini51Series.h
- SPI_CNTRL_TX_FULL_Pos : Mini51Series.h
- SPI_CNTRL_TX_NEG_Msk : Mini51Series.h
- SPI_CNTRL_TX_NEG_Pos : Mini51Series.h
- SPI_DISABLE_3WIRE_MODE : spi.h
- SPI_DISABLE_BYTE_REORDER : spi.h
- SPI_DIVIDER_DIVIDER_Msk : Mini51Series.h
- SPI_DIVIDER_DIVIDER_Pos : Mini51Series.h
- SPI_ENABLE_3WIRE_MODE : spi.h
- SPI_ENABLE_BYTE_REORDER : spi.h
- SPI_FIFO_CTL_RX_CLR_Msk : Mini51Series.h
- SPI_FIFO_CTL_RX_CLR_Pos : Mini51Series.h
- SPI_FIFO_CTL_RX_INTEN_Msk : Mini51Series.h
- SPI_FIFO_CTL_RX_INTEN_Pos : Mini51Series.h
- SPI_FIFO_CTL_RX_THRESHOLD_Msk : Mini51Series.h
- SPI_FIFO_CTL_RX_THRESHOLD_Pos : Mini51Series.h
- SPI_FIFO_CTL_RXOV_INTEN_Msk : Mini51Series.h
- SPI_FIFO_CTL_RXOV_INTEN_Pos : Mini51Series.h
- SPI_FIFO_CTL_TIMEOUT_INTEN_Msk : Mini51Series.h
- SPI_FIFO_CTL_TIMEOUT_INTEN_Pos : Mini51Series.h
- SPI_FIFO_CTL_TX_CLR_Msk : Mini51Series.h
- SPI_FIFO_CTL_TX_CLR_Pos : Mini51Series.h
- SPI_FIFO_CTL_TX_INTEN_Msk : Mini51Series.h
- SPI_FIFO_CTL_TX_INTEN_Pos : Mini51Series.h
- SPI_FIFO_CTL_TX_THRESHOLD_Msk : Mini51Series.h
- SPI_FIFO_CTL_TX_THRESHOLD_Pos : Mini51Series.h
- SPI_FIFO_RX_INTEN_MASK : spi.h
- SPI_FIFO_RXOV_INTEN_MASK : spi.h
- SPI_FIFO_TIMEOUT_INTEN_MASK : spi.h
- SPI_FIFO_TX_INTEN_MASK : spi.h
- SPI_GET_RX_FIFO_COUNT : spi.h
- SPI_GET_RX_FIFO_EMPTY_FLAG : spi.h
- SPI_GET_TX_FIFO_EMPTY_FLAG : spi.h
- SPI_GET_TX_FIFO_FULL_FLAG : spi.h
- SPI_IE_MASK : spi.h
- SPI_IS_BUSY : spi.h
- SPI_MASTER : spi.h
- SPI_MODE_0 : spi.h
- SPI_MODE_1 : spi.h
- SPI_MODE_2 : spi.h
- SPI_MODE_3 : spi.h
- SPI_MODULE : clk.h
- SPI_READ_RX : spi.h
- SPI_RST : sys.h
- SPI_RX_RX_Msk : Mini51Series.h
- SPI_RX_RX_Pos : Mini51Series.h
- SPI_SET_LSB_FIRST : spi.h
- SPI_SET_MSB_FIRST : spi.h
- SPI_SET_SUSPEND_CYCLE : spi.h
- SPI_SLAVE : spi.h
- SPI_SS : spi.h
- SPI_SS_ACTIVE_HIGH : spi.h
- SPI_SS_ACTIVE_LOW : spi.h
- SPI_SSR_AUTOSS_Msk : Mini51Series.h
- SPI_SSR_AUTOSS_Pos : Mini51Series.h
- SPI_SSR_LTRIG_FLAG_Msk : Mini51Series.h
- SPI_SSR_LTRIG_FLAG_Pos : Mini51Series.h
- SPI_SSR_SS_LTRIG_Msk : Mini51Series.h
- SPI_SSR_SS_LTRIG_Pos : Mini51Series.h
- SPI_SSR_SS_LVL_Msk : Mini51Series.h
- SPI_SSR_SS_LVL_Pos : Mini51Series.h
- SPI_SSR_SSR_Msk : Mini51Series.h
- SPI_SSR_SSR_Pos : Mini51Series.h
- SPI_SSTA_INTEN_MASK : spi.h
- SPI_STATUS_IF_Msk : Mini51Series.h
- SPI_STATUS_IF_Pos : Mini51Series.h
- SPI_STATUS_RX_EMPTY_Msk : Mini51Series.h
- SPI_STATUS_RX_EMPTY_Pos : Mini51Series.h
- SPI_STATUS_RX_FIFO_COUNT_Msk : Mini51Series.h
- SPI_STATUS_RX_FIFO_COUNT_Pos : Mini51Series.h
- SPI_STATUS_RX_FULL_Msk : Mini51Series.h
- SPI_STATUS_RX_FULL_Pos : Mini51Series.h
- SPI_STATUS_RX_INTSTS_Msk : Mini51Series.h
- SPI_STATUS_RX_INTSTS_Pos : Mini51Series.h
- SPI_STATUS_RX_OVERRUN_Msk : Mini51Series.h
- SPI_STATUS_RX_OVERRUN_Pos : Mini51Series.h
- SPI_STATUS_SLV_START_INTSTS_Msk : Mini51Series.h
- SPI_STATUS_SLV_START_INTSTS_Pos : Mini51Series.h
- SPI_STATUS_TIMEOUT_Msk : Mini51Series.h
- SPI_STATUS_TIMEOUT_Pos : Mini51Series.h
- SPI_STATUS_TX_EMPTY_Msk : Mini51Series.h
- SPI_STATUS_TX_EMPTY_Pos : Mini51Series.h
- SPI_STATUS_TX_FIFO_COUNT_Msk : Mini51Series.h
- SPI_STATUS_TX_FIFO_COUNT_Pos : Mini51Series.h
- SPI_STATUS_TX_FULL_Msk : Mini51Series.h
- SPI_STATUS_TX_FULL_Pos : Mini51Series.h
- SPI_STATUS_TX_INTSTS_Msk : Mini51Series.h
- SPI_STATUS_TX_INTSTS_Pos : Mini51Series.h
- SPI_TRIGGER : spi.h
- SPI_TX_TX_Msk : Mini51Series.h
- SPI_TX_TX_Pos : Mini51Series.h
- SPI_WRITE_TX : spi.h
- SRAM_BASE : Mini51Series.h
- SYS : Mini51Series.h
- SYS_BODCR_BOD_DISABLE : sys.h
- SYS_BODCR_BOD_INTERRUPT_EN : sys.h
- SYS_BODCR_BOD_INTF_Msk : Mini51Series.h
- SYS_BODCR_BOD_INTF_Pos : Mini51Series.h
- SYS_BODCR_BOD_LPM_Msk : Mini51Series.h
- SYS_BODCR_BOD_LPM_Pos : Mini51Series.h
- SYS_BODCR_BOD_OUT_Msk : Mini51Series.h
- SYS_BODCR_BOD_OUT_Pos : Mini51Series.h
- SYS_BODCR_BOD_RST_EN : sys.h
- SYS_BODCR_BOD_RSTEN_Msk : Mini51Series.h
- SYS_BODCR_BOD_RSTEN_Pos : Mini51Series.h
- SYS_BODCR_BOD_VL_2_2V : sys.h
- SYS_BODCR_BOD_VL_2_7V : sys.h
- SYS_BODCR_BOD_VL_3_7V : sys.h
- SYS_BODCR_BOD_VL_4_4V : sys.h
- SYS_BODCR_BOD_VL_EXT_Msk : Mini51Series.h
- SYS_BODCR_BOD_VL_EXT_Pos : Mini51Series.h
- SYS_BODCR_BOD_VL_Msk : Mini51Series.h
- SYS_BODCR_BOD_VL_Pos : Mini51Series.h
- SYS_CLEAR_BOD_INT_FLAG : sys.h
- SYS_CLEAR_BOD_LPM : sys.h
- SYS_CLEAR_RST_SOURCE : sys.h
- SYS_DISABLE_BOD : sys.h
- SYS_DISABLE_BOD_RST : sys.h
- SYS_DISABLE_POR : sys.h
- SYS_ENABLE_BOD : sys.h
- SYS_ENABLE_BOD_RST : sys.h
- SYS_ENABLE_POR : sys.h
- SYS_GET_BOD_INT_FLAG : sys.h
- SYS_GET_BOD_OUTPUT : sys.h
- SYS_IPRSTC1_CHIP_RST_Msk : Mini51Series.h
- SYS_IPRSTC1_CHIP_RST_Pos : Mini51Series.h
- SYS_IPRSTC1_CPU_RST_Msk : Mini51Series.h
- SYS_IPRSTC1_CPU_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_ACMP_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_ACMP_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_ADC_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_ADC_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_GPIO_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_GPIO_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_I2C_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_I2C_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_PWM_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_PWM_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_SPI_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_SPI_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_TMR0_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_TMR0_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_TMR1_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_TMR1_RST_Pos : Mini51Series.h
- SYS_IPRSTC2_UART_RST_Msk : Mini51Series.h
- SYS_IPRSTC2_UART_RST_Pos : Mini51Series.h
- SYS_IRCTRIMCTL_TRIM_LOOP_Msk : Mini51Series.h
- SYS_IRCTRIMCTL_TRIM_LOOP_Pos : Mini51Series.h
- SYS_IRCTRIMCTL_TRIM_SEL_Msk : Mini51Series.h
- SYS_IRCTRIMCTL_TRIM_SEL_Pos : Mini51Series.h
- SYS_IRCTRIMIEN_32K_ERR_IEN_Msk : Mini51Series.h
- SYS_IRCTRIMIEN_32K_ERR_IEN_Pos : Mini51Series.h
- SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk : Mini51Series.h
- SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos : Mini51Series.h
- SYS_IRCTRIMINT_32K_ERR_INT_Msk : Mini51Series.h
- SYS_IRCTRIMINT_32K_ERR_INT_Pos : Mini51Series.h
- SYS_IRCTRIMINT_FREQ_LOCK_Msk : Mini51Series.h
- SYS_IRCTRIMINT_FREQ_LOCK_Pos : Mini51Series.h
- SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk : Mini51Series.h
- SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos : Mini51Series.h
- SYS_IS_BOD_RST : sys.h
- SYS_IS_CPU_RST : sys.h
- SYS_IS_POR_RST : sys.h
- SYS_IS_RSTPIN_RST : sys.h
- SYS_IS_SYSTEM_RST : sys.h
- SYS_IS_WDT_RST : sys.h
- SYS_MFP_ALT_Msk : sys.h
- SYS_MFP_MFP_Msk : sys.h
- SYS_MFP_P00_CTS : sys.h
- SYS_MFP_P00_GPIO : sys.h
- SYS_MFP_P00_Msk : sys.h
- SYS_MFP_P00_TXD : sys.h
- SYS_MFP_P01_GPIO : sys.h
- SYS_MFP_P01_Msk : sys.h
- SYS_MFP_P01_RTS : sys.h
- SYS_MFP_P01_RXD : sys.h
- SYS_MFP_P01_SPISS : sys.h
- SYS_MFP_P04_GPIO : sys.h
- SYS_MFP_P04_Msk : sys.h
- SYS_MFP_P04_PWM5 : sys.h
- SYS_MFP_P04_SPISS : sys.h
- SYS_MFP_P05_GPIO : sys.h
- SYS_MFP_P05_MOSI : sys.h
- SYS_MFP_P05_Msk : sys.h
- SYS_MFP_P06_GPIO : sys.h
- SYS_MFP_P06_MISO : sys.h
- SYS_MFP_P06_Msk : sys.h
- SYS_MFP_P07_GPIO : sys.h
- SYS_MFP_P07_Msk : sys.h
- SYS_MFP_P07_SPICLK : sys.h
- SYS_MFP_P10_AIN1 : sys.h
- SYS_MFP_P10_CPP0 : sys.h
- SYS_MFP_P10_GPIO : sys.h
- SYS_MFP_P10_Msk : sys.h
- SYS_MFP_P12_AIN2 : sys.h
- SYS_MFP_P12_CPP0 : sys.h
- SYS_MFP_P12_GPIO : sys.h
- SYS_MFP_P12_Msk : sys.h
- SYS_MFP_P12_RXD : sys.h
- SYS_MFP_P13_AIN3 : sys.h
- SYS_MFP_P13_CPP0 : sys.h
- SYS_MFP_P13_GPIO : sys.h
- SYS_MFP_P13_Msk : sys.h
- SYS_MFP_P13_TXD : sys.h
- SYS_MFP_P14_AIN4 : sys.h
- SYS_MFP_P14_CPN0 : sys.h
- SYS_MFP_P14_GPIO : sys.h
- SYS_MFP_P14_Msk : sys.h
- SYS_MFP_P15_AIN5 : sys.h
- SYS_MFP_P15_CPP0 : sys.h
- SYS_MFP_P15_GPIO : sys.h
- SYS_MFP_P15_Msk : sys.h
- SYS_MFP_P22_GPIO : sys.h
- SYS_MFP_P22_Msk : sys.h
- SYS_MFP_P22_PWM0 : sys.h
- SYS_MFP_P23_GPIO : sys.h
- SYS_MFP_P23_Msk : sys.h
- SYS_MFP_P23_PWM1 : sys.h
- SYS_MFP_P24_GPIO : sys.h
- SYS_MFP_P24_Msk : sys.h
- SYS_MFP_P24_PWM2 : sys.h
- SYS_MFP_P25_GPIO : sys.h
- SYS_MFP_P25_Msk : sys.h
- SYS_MFP_P25_PWM3 : sys.h
- SYS_MFP_P26_CPO1 : sys.h
- SYS_MFP_P26_GPIO : sys.h
- SYS_MFP_P26_Msk : sys.h
- SYS_MFP_P26_PWM4 : sys.h
- SYS_MFP_P30_AIN6 : sys.h
- SYS_MFP_P30_CPN1 : sys.h
- SYS_MFP_P30_GPIO : sys.h
- SYS_MFP_P30_Msk : sys.h
- SYS_MFP_P31_AIN7 : sys.h
- SYS_MFP_P31_CPP1 : sys.h
- SYS_MFP_P31_GPIO : sys.h
- SYS_MFP_P31_Msk : sys.h
- SYS_MFP_P32_CPP1 : sys.h
- SYS_MFP_P32_GPIO : sys.h
- SYS_MFP_P32_INT0 : sys.h
- SYS_MFP_P32_Msk : sys.h
- SYS_MFP_P32_STADC : sys.h
- SYS_MFP_P32_T0EX : sys.h
- SYS_MFP_P34_CPP1 : sys.h
- SYS_MFP_P34_GPIO : sys.h
- SYS_MFP_P34_Msk : sys.h
- SYS_MFP_P34_SDA : sys.h
- SYS_MFP_P34_T0 : sys.h
- SYS_MFP_P35_CPP1 : sys.h
- SYS_MFP_P35_GPIO : sys.h
- SYS_MFP_P35_Msk : sys.h
- SYS_MFP_P35_SCL : sys.h
- SYS_MFP_P35_T1 : sys.h
- SYS_MFP_P36_CKO : sys.h
- SYS_MFP_P36_CPO0 : sys.h
- SYS_MFP_P36_GPIO : sys.h
- SYS_MFP_P36_Msk : sys.h
- SYS_MFP_P36_T1EX : sys.h
- SYS_MFP_P46_GPIO : sys.h
- SYS_MFP_P46_ICE_CLK : sys.h
- SYS_MFP_P46_Msk : sys.h
- SYS_MFP_P47_GPIO : sys.h
- SYS_MFP_P47_ICE_DAT : sys.h
- SYS_MFP_P47_Msk : sys.h
- SYS_MFP_P50_GPIO : sys.h
- SYS_MFP_P50_Msk : sys.h
- SYS_MFP_P50_XTAL1 : sys.h
- SYS_MFP_P51_GPIO : sys.h
- SYS_MFP_P51_Msk : sys.h
- SYS_MFP_P51_XTAL2 : sys.h
- SYS_MFP_P52_GPIO : sys.h
- SYS_MFP_P52_INT1 : sys.h
- SYS_MFP_P52_Msk : sys.h
- SYS_MFP_P53_AIN0 : sys.h
- SYS_MFP_P53_GPIO : sys.h
- SYS_MFP_P53_Msk : sys.h
- SYS_MFP_P54_GPIO : sys.h
- SYS_MFP_P54_Msk : sys.h
- SYS_MFP_P55_GPIO : sys.h
- SYS_MFP_P55_Msk : sys.h
- SYS_MFP_TYPE_Msk : sys.h
- SYS_P0_MFP_P0_ALT0_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT0_Pos : Mini51Series.h
- SYS_P0_MFP_P0_ALT1_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT1_Pos : Mini51Series.h
- SYS_P0_MFP_P0_ALT4_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT4_Pos : Mini51Series.h
- SYS_P0_MFP_P0_ALT5_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT5_Pos : Mini51Series.h
- SYS_P0_MFP_P0_ALT6_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT6_Pos : Mini51Series.h
- SYS_P0_MFP_P0_ALT7_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT7_Pos : Mini51Series.h
- SYS_P0_MFP_P0_ALT_Msk : Mini51Series.h
- SYS_P0_MFP_P0_ALT_Pos : Mini51Series.h
- SYS_P0_MFP_P0_MFP_Msk : Mini51Series.h
- SYS_P0_MFP_P0_MFP_Pos : Mini51Series.h
- SYS_P0_MFP_P0_TYPE_Msk : Mini51Series.h
- SYS_P0_MFP_P0_TYPE_Pos : Mini51Series.h
- SYS_P1_MFP_P1_ALT0_Msk : Mini51Series.h
- SYS_P1_MFP_P1_ALT0_Pos : Mini51Series.h
- SYS_P1_MFP_P1_ALT2_Msk : Mini51Series.h
- SYS_P1_MFP_P1_ALT2_Pos : Mini51Series.h
- SYS_P1_MFP_P1_ALT3_Msk : Mini51Series.h
- SYS_P1_MFP_P1_ALT3_Pos : Mini51Series.h
- SYS_P1_MFP_P1_ALT4_Msk : Mini51Series.h
- SYS_P1_MFP_P1_ALT4_Pos : Mini51Series.h
- SYS_P1_MFP_P1_ALT5_Msk : Mini51Series.h
- SYS_P1_MFP_P1_ALT5_Pos : Mini51Series.h
- SYS_P1_MFP_P1_ALT_Msk : Mini51Series.h
- SYS_P1_MFP_P1_ALT_Pos : Mini51Series.h
- SYS_P1_MFP_P1_MFP_Msk : Mini51Series.h
- SYS_P1_MFP_P1_MFP_Pos : Mini51Series.h
- SYS_P1_MFP_P1_TYPE_Msk : Mini51Series.h
- SYS_P1_MFP_P1_TYPE_Pos : Mini51Series.h
- SYS_P2_MFP_P2_ALT2_Msk : Mini51Series.h
- SYS_P2_MFP_P2_ALT2_Pos : Mini51Series.h
- SYS_P2_MFP_P2_ALT3_Msk : Mini51Series.h
- SYS_P2_MFP_P2_ALT3_Pos : Mini51Series.h
- SYS_P2_MFP_P2_ALT4_Msk : Mini51Series.h
- SYS_P2_MFP_P2_ALT4_Pos : Mini51Series.h
- SYS_P2_MFP_P2_ALT5_Msk : Mini51Series.h
- SYS_P2_MFP_P2_ALT5_Pos : Mini51Series.h
- SYS_P2_MFP_P2_ALT6_Msk : Mini51Series.h
- SYS_P2_MFP_P2_ALT6_Pos : Mini51Series.h
- SYS_P2_MFP_P2_ALT_Msk : Mini51Series.h
- SYS_P2_MFP_P2_ALT_Pos : Mini51Series.h
- SYS_P2_MFP_P2_MFP_Msk : Mini51Series.h
- SYS_P2_MFP_P2_MFP_Pos : Mini51Series.h
- SYS_P2_MFP_P2_TYPE_Msk : Mini51Series.h
- SYS_P2_MFP_P2_TYPE_Pos : Mini51Series.h
- SYS_P3_MFP_P32CPP1_Msk : Mini51Series.h
- SYS_P3_MFP_P32CPP1_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT0_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT0_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT1_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT1_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT2_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT2_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT4_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT4_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT5_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT5_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT6_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT6_Pos : Mini51Series.h
- SYS_P3_MFP_P3_ALT_Msk : Mini51Series.h
- SYS_P3_MFP_P3_ALT_Pos : Mini51Series.h
- SYS_P3_MFP_P3_MFP_Msk : Mini51Series.h
- SYS_P3_MFP_P3_MFP_Pos : Mini51Series.h
- SYS_P3_MFP_P3_TYPE_Msk : Mini51Series.h
- SYS_P3_MFP_P3_TYPE_Pos : Mini51Series.h
- SYS_P4_MFP_P4_ALT6_Msk : Mini51Series.h
- SYS_P4_MFP_P4_ALT6_Pos : Mini51Series.h
- SYS_P4_MFP_P4_ALT7_Msk : Mini51Series.h
- SYS_P4_MFP_P4_ALT7_Pos : Mini51Series.h
- SYS_P4_MFP_P4_ALT_Msk : Mini51Series.h
- SYS_P4_MFP_P4_ALT_Pos : Mini51Series.h
- SYS_P4_MFP_P4_MFP_Msk : Mini51Series.h
- SYS_P4_MFP_P4_MFP_Pos : Mini51Series.h
- SYS_P4_MFP_P4_TYPE_Msk : Mini51Series.h
- SYS_P4_MFP_P4_TYPE_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT0_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT0_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT1_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT1_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT2_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT2_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT3_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT3_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT4_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT4_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT5_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT5_Pos : Mini51Series.h
- SYS_P5_MFP_P5_ALT_Msk : Mini51Series.h
- SYS_P5_MFP_P5_ALT_Pos : Mini51Series.h
- SYS_P5_MFP_P5_MFP_Msk : Mini51Series.h
- SYS_P5_MFP_P5_MFP_Pos : Mini51Series.h
- SYS_P5_MFP_P5_TYPE_Msk : Mini51Series.h
- SYS_P5_MFP_P5_TYPE_Pos : Mini51Series.h
- SYS_PDID_PDID_Msk : Mini51Series.h
- SYS_PDID_PDID_Pos : Mini51Series.h
- SYS_RegLockAddr_RegUnLock_Msk : Mini51Series.h
- SYS_RegLockAddr_RegUnLock_Pos : Mini51Series.h
- SYS_RSTSRC_RSTS_BOD_Msk : Mini51Series.h
- SYS_RSTSRC_RSTS_BOD_Pos : Mini51Series.h
- SYS_RSTSRC_RSTS_CPU_Msk : Mini51Series.h
- SYS_RSTSRC_RSTS_CPU_Pos : Mini51Series.h
- SYS_RSTSRC_RSTS_MCU_Msk : Mini51Series.h
- SYS_RSTSRC_RSTS_MCU_Pos : Mini51Series.h
- SYS_RSTSRC_RSTS_POR_Msk : Mini51Series.h
- SYS_RSTSRC_RSTS_POR_Pos : Mini51Series.h
- SYS_RSTSRC_RSTS_RESET_Msk : Mini51Series.h
- SYS_RSTSRC_RSTS_RESET_Pos : Mini51Series.h
- SYS_RSTSRC_RSTS_WDT_Msk : Mini51Series.h
- SYS_RSTSRC_RSTS_WDT_Pos : Mini51Series.h
- SYS_SET_BOD_LEVEL : sys.h
- SYS_SET_BOD_LPM : sys.h