| MINI51DE_BSP V3.02.003 The Board Support Package for Mini51DE Series MCU

### - i -

- I2C_ClearTimeoutFlag() : i2c.h
- I2C_Close() : i2c.h
- I2C_DisableInt() : i2c.h
- I2C_DisableTimeout() : i2c.h
- I2C_DisableWakeup() : i2c.h
- I2C_EnableInt() : i2c.h
- I2C_EnableTimeout() : i2c.h
- I2C_EnableWakeup() : i2c.h
- I2C_GetBusClockFreq() : i2c.h
- I2C_GetData() : i2c.h
- I2C_GetIntFlag() : i2c.h
- I2C_GetStatus() : i2c.h
- I2C_Open() : i2c.h
- I2C_SetBusClockFreq() : i2c.h
- I2C_SetData() : i2c.h
- I2C_SetSlaveAddr() : i2c.h
- I2C_SetSlaveAddrMask() : i2c.h
- I2C_SW_Get() : i2c_software_gpio.h, i2c_software_gpio.c
- I2C_SW_Get_byte() : i2c_software_gpio.c
- I2C_SW_I_Count() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Get() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Get_Byte() : i2c_software_gpio_with_timer.c
- I2C_SW_I_IsBZ() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Open() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Send() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Send_Byte() : i2c_software_gpio_with_timer.c
- I2C_SW_I_Send_Start() : i2c_software_gpio_with_timer.c
- I2C_SW_I_Send_Stop() : i2c_software_gpio_with_timer.c
- I2C_SW_Open() : i2c_software_gpio.h, i2c_software_gpio.c
- I2C_SW_Send() : i2c_software_gpio.h, i2c_software_gpio.c
- I2C_SW_Send_byte() : i2c_software_gpio.c
- I2C_Trigger() : i2c.h
- IsDebugFifoEmpty() : retarget.c