| MINI51DE_BSP V3.02.003 The Board Support Package for Mini51DE Series MCU

Functions
sys.c File Reference

MINI51 series SYS driver source file. More...

`#include "Mini51Series.h"`
Include dependency graph for sys.c:

Go to the source code of this file.

## Functions
void | SYS_ClearResetSrc (uint32_t u32Src)
| This function clear the selected system reset source. More...
uint32_t | SYS_GetBODStatus (void)
| This function get Brown-out detector output status. More...
uint32_t | SYS_GetResetSrc (void)
| This function get the system reset source register value. More...
uint32_t | SYS_IsRegLocked (void)
| This function check register write-protection bit setting. More...
void | SYS_LockReg (void)
| This function enable register write-protection function. More...
void | SYS_UnlockReg (void)
| This function disable register write-protection function. More...
uint32_t | SYS_ReadPDID (void)
| This function get product ID. More...
void | SYS_ResetChip (void)
| This function reset chip. More...
void | SYS_ResetCPU (void)
| This function reset CPU. More...
void | SYS_ResetModule (uint32_t u32ModuleIndex)
| This function reset selected modules. More...
void | SYS_EnableBOD (int32_t i32Mode, uint32_t u32BODLevel)
| This function configure BOD function. Configure BOD reset or interrupt mode and set Brown-out voltage level. Enable Brown-out function. More...
void | SYS_DisableBOD (void)
| This function disable BOD function. More...

## Detailed Description

MINI51 series SYS driver source file.

Version
  V1.00

Revision
  13

Date
  15/09/25 9:24a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file sys.c.