| MINI51DE_BSP V3.02.003 The Board Support Package for Mini51DE Series MCU

Data Fields
PWM_T Struct Reference

`#include <Mini51Series.h>`

## Data Fields
__IO uint32_t | PPR
__IO uint32_t | CSR
__IO uint32_t | PCR
__IO uint32_t | CNR [6]
__IO uint32_t | CMR [6]
__IO uint32_t | PIER
__IO uint32_t | PIIR
__IO uint32_t | POE
__IO uint32_t | PFBCON
__IO uint32_t | PDZIR
__IO uint32_t | TRGCON0
__IO uint32_t | TRGCON1
__IO uint32_t | TRGSTS0
__IO uint32_t | TRGSTS1
__IO uint32_t | PHCHG
__IO uint32_t | PHCHGNXT
__IO uint32_t | PHCHGMASK
__IO uint32_t | INTACCUCTL

## Detailed Description

    @addtogroup PWM Pulse Width Modulation Controller(PWM)
    Memory Mapped Structure for PWM Controller

Definition at line 2751 of file Mini51Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Mini51Series/Include/Mini51Series.h