| MINI55_BSP V3.01.003 The Board Support Package for Mini55 Series MCU

Macros | Functions
pwm.h File Reference

MINI55 series PWM driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | PWM_CHANNEL_NUM (6)
#define | PWM_CLK_DIV_1 (4UL)
#define | PWM_CLK_DIV_2 (0UL)
#define | PWM_CLK_DIV_4 (1UL)
#define | PWM_CLK_DIV_8 (2UL)
#define | PWM_CLK_DIV_16 (3UL)
#define | PWM_EDGE_ALIGNED (0UL)
#define | PWM_CENTER_ALIGNED (PWM_CTL_CNTTYPE_Msk)
#define | PWM_TRIGGER_ADC_CNTR_IS_0 PWM_ADCTCTL0_ZPTRGEN0_Msk
#define | PWM_TRIGGER_ADC_CNTR_IS_CMR_D PWM_ADCTCTL0_CDTRGEN0_Msk
#define | PWM_TRIGGER_ADC_CNTR_IS_CNR PWM_ADCTCTL0_CPTRGEN0_Msk
#define | PWM_TRIGGER_ADC_CNTR_IS_CMR_U PWM_ADCTCTL0_CUTRGEN0_Msk
#define | PWM_FB0_EINT0 (PWM_BRKCTL_BRK0EN_Msk)
#define | PWM_FB0_ACMP1 (PWM_BRKCTL_BRK0EN_Msk | PWM_BRKCTL_BRK1SEL_Msk)
#define | PWM_FB1_EINT1 (PWM_BRKCTL_BRK1EN_Msk)
#define | PWM_FB1_ACMP0 (PWM_BRKCTL_BRK1EN_Msk | PWM_BRKCTL_BRK0SEL_Msk)
#define | PWM_PERIOD_INT_UNDERFLOW (0)
#define | PWM_PERIOD_INT_MATCH_CNR (PWM_INTEN_PINTTYPE_Msk)
#define | PWM_CH0 0x0
#define | PWM_CH1 0x1
#define | PWM_CH2 0x2
#define | PWM_CH3 0x3
#define | PWM_CH4 0x4
#define | PWM_CH5 0x5
#define | PWM_ENABLE_COMPLEMENTARY_MODE(pwm)
| This macro enable complementary mode. More...
#define | PWM_DISABLE_COMPLEMENTARY_MODE(pwm)
| This macro disable complementary mode, and enable independent mode. More...
#define | PWM_ENABLE_GROUP_MODE(pwm)
| This macro enable group mode. More...
#define | PWM_DISABLE_GROUP_MODE(pwm)
| This macro disable group mode. More...
#define | PWM_ENABLE_SYNC_MODE(pwm)
| This macro enable synchronous mode. More...
#define | PWM_DISABLE_SYNC_MODE(pwm)
| This macro disable synchronous mode, and enable independent mode. More...
#define | PWM_ENABLE_OUTPUT_INVERTER(pwm, u32ChannelMask)
| This macro enable output inverter of specified channel(s) More...
#define | PWM_SET_PRESCALER(pwm, u32ChannelNum, u32Prescaler)
| This macro set the prescaler of the selected channel. More...
#define | PWM_SET_DIVIDER(pwm, u32ChannelNum, u32Divider)
| This macro set the divider of the selected channel. More...
#define | PWM_SET_CMR(pwm, u32ChannelNum, u32CMR)
| This macro set the duty of the selected channel. More...
#define | PWM_SET_CNR(pwm, u32ChannelNum, u32CNR)
| This macro set the period of the selected channel. More...
#define | PWM_SET_ALIGNED_TYPE(pwm, u32ChannelMask, u32AlignedType)
| This macro set the PWM aligned type. More...

## Functions
uint32_t | PWM_ConfigOutputChannel (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Frequency, uint32_t u32DutyCycle)
| This function config PWM generator and get the nearest frequency in edge aligned auto-reload mode. More...
void | PWM_Start (PWM_T *pwm, uint32_t u32ChannelMask)
| This function start PWM module. More...
void | PWM_Stop (PWM_T *pwm, uint32_t u32ChannelMask)
| This function stop PWM module. More...
void | PWM_ForceStop (PWM_T *pwm, uint32_t u32ChannelMask)
| This function stop PWM generation immediately by clear channel enable bit. More...
void | PWM_EnableADCTrigger (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| This function enable selected channel to trigger ADC. More...
void | PWM_DisableADCTrigger (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable selected channel to trigger ADC. More...
void | PWM_ClearADCTriggerFlag (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| This function clear selected channel trigger ADC flag. More...
uint32_t | PWM_GetADCTriggerFlag (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| This function get selected channel trigger ADC flag. More...
void | PWM_EnableFaultBrake (PWM_T *pwm, uint32_t u32ChannelMask, uint32_t u32LevelMask, uint32_t u32BrakeSource)
| This function enable fault brake of selected channels. More...
void | PWM_ClearFaultBrakeFlag (PWM_T *pwm, uint32_t u32BrakeSource)
| This function clear fault brake flag. More...
void | PWM_EnableOutput (PWM_T *pwm, uint32_t u32ChannelMask)
| This function enables PWM output generation of selected channels. More...
void | PWM_DisableOutput (PWM_T *pwm, uint32_t u32ChannelMask)
| This function disables PWM output generation of selected channels. More...
void | PWM_EnableDeadZone (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Duration)
| This function enable Dead zone of selected channel. More...
void | PWM_DisableDeadZone (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable Dead zone of selected channel. More...
void | PWM_EnableDutyInt (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32IntDutyType)
| This function enable duty interrupt of selected channel. More...
void | PWM_DisableDutyInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable duty interrupt of selected channel. More...
void | PWM_ClearDutyIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function clears duty interrupt flag of selected channel. More...
uint32_t | PWM_GetDutyIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get duty interrupt flag of selected channel. More...
void | PWM_EnableFaultBrakeInt (PWM_T *pwm, uint32_t u32BrakeSource)
| This function enable fault brake interrupt. More...
void | PWM_DisableFaultBrakeInt (PWM_T *pwm, uint32_t u32BrakeSource)
| This function disable fault brake interrupt. More...
void | PWM_ClearFaultBrakeIntFlag (PWM_T *pwm, uint32_t u32BrakeSource)
| This function clear fault brake interrupt of selected source. More...
uint32_t | PWM_GetFaultBrakeIntFlag (PWM_T *pwm, uint32_t u32BrakeSource)
| This function get fault brake interrupt of selected source. More...
void | PWM_EnablePeriodInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function enable Period interrupt of selected channel. More...
void | PWM_DisablePeriodInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable Period interrupt of selected channel. More...
void | PWM_ClearPeriodIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function clears Period interrupt flag of selected channel. More...
uint32_t | PWM_GetPeriodIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get Period interrupt flag of selected channel. More...
void | PWM_EnableCenterInt (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32IntPeriodType)
| This function enable Central interrupt of selected channel. More...
void | PWM_DisableCenterInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable Central interrupt of selected channel. More...
void | PWM_ClearCenterIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function clear Central interrupt of selected channel. More...
uint32_t | PWM_GetCenterIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get Central interrupt of selected channel. More...
void | PWM_EnableRiseInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function enable Rise interrupt of selected channel. More...
void | PWM_DisableRiseInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable Rise interrupt of selected channel. More...
void | PWM_ClearRiseIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function clears Rise interrupt flag of selected channel. More...
uint32_t | PWM_GetRiseIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get Rise interrupt flag of selected channel. More...

## Detailed Description

MINI55 series PWM driver header file.

Version
  V1.00

Revision
  11

Date
  15/07/07 6:26p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file pwm.h.