| MINI55_BSP V3.01.003 The Board Support Package for Mini55 Series MCU

Data Fields
UART_T Struct Reference

`#include <Mini55Series.h>`

## Data Fields
__IO uint32_t | DAT
__IO uint32_t | INTEN
__IO uint32_t | FIFO
__IO uint32_t | LINE
__IO uint32_t | MODEM
__IO uint32_t | MODEMSTS
__IO uint32_t | FIFOSTS
__IO uint32_t | INTSTS
__IO uint32_t | TOUT
__IO uint32_t | BAUD
__IO uint32_t | IRDA
__IO uint32_t | ALTCTL
__IO uint32_t | FUNCSEL

## Detailed Description

    @addtogroup UART Universal Asynchronous Receiver/Transmitter Controller(UART)
    Memory Mapped Structure for UART Controller

Definition at line 6170 of file Mini55Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Mini55Series/Include/Mini55Series.h