| MINI58_BSP V3.01.003 The Board Support Package for Mini58 Series MCU

Functions
adc.c File Reference

Mini58 series ADC driver source file. More...

`#include "Mini58Series.h"`
Include dependency graph for adc.c:

Go to the source code of this file.

## Functions
void | ADC_Open (ADC_T *adc, uint32_t u32InputMode, uint32_t u32OpMode, uint32_t u32ChMask)
| This API configures ADC module to be ready for convert the input from selected channel. More...
void | ADC_Close (ADC_T *adc)
| Disable ADC module. More...
void | ADC_EnableHWTrigger (ADC_T *adc, uint32_t u32Source, uint32_t u32Param)
| Configure the hardware trigger condition and enable hardware trigger. More...
void | ADC_DisableHWTrigger (ADC_T *adc)
| Disable hardware trigger ADC function. More...
void | ADC_SetExtraSampleTime (ADC_T *adc, uint32_t u32ChNum, uint32_t u32SampleTime)
| Set ADC sample time for designated channel. More...
void | ADC_EnableInt (ADC_T *adc, uint32_t u32Mask)
| Enable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_DisableInt (ADC_T *adc, uint32_t u32Mask)
| Disable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_SeqModeEnable (ADC_T *adc, uint32_t u32SeqTYPE, uint32_t u32ModeSel)
| ADC PWM Sequential Mode Control. More...
void | ADC_SeqModeTriggerSrc (ADC_T *adc, uint32_t u32SeqModeTriSrc1, uint32_t u32SeqModeTriSrc2)
| ADC PWM Sequential Mode PWM Trigger Source and type. More...

## Detailed Description

Mini58 series ADC driver source file.

Version
  V1.00

Revision
  4

Date
  15/07/21 3:15p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2022 Nuvoton Technology Corp. All rights reserved.

Definition in file adc.c.