| MINI58_BSP V3.01.003 The Board Support Package for Mini58 Series MCU

Data Structures | Macros | Typedefs | Enumerations
Mini58Series.h File Reference

Mini58 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini58 series MCU. More...

`#include "core_cm0.h"`
`#include "system_Mini58Series.h"`
`#include <stdint.h>`
`#include "sys.h"`
`#include "clk.h"`
`#include "acmp.h"`
`#include "adc.h"`
`#include "fmc.h"`
`#include "gpio.h"`
`#include "i2c.h"`
`#include "pwm.h"`
`#include "spi.h"`
`#include "timer.h"`
`#include "uart.h"`
`#include "wdt.h"`
`#include "wwdt.h"`
Include dependency graph for Mini58Series.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | ACMP_T
struct | ADC_T
struct | CLK_T
struct | FMC_T
struct | GPIO_T
struct | GPIO_DB_T
struct | I2C_T
struct | INTR_T
struct | PWM_T
struct | SPI_T
struct | SYS_T
struct | TIMER_T
struct | UART_T
struct | WDT_T
struct | WWDT_T

## Macros
#define | __CM0_REV 0x0201
#define | __NVIC_PRIO_BITS 2
#define | __Vendor_SysTickConfig 0
#define | __MPU_PRESENT 0
#define | __FPU_PRESENT 0
#define | FLASH_BASE ((uint32_t)0x00000000)
| Flash base address. More...
#define | SRAM_BASE ((uint32_t)0x20000000)
| SRAM base address. More...
#define | APB1PERIPH_BASE ((uint32_t)0x40000000)
| APB1 base address. More...
#define | APB2PERIPH_BASE ((uint32_t)0x40100000)
| APB2 base address. More...
#define | AHBPERIPH_BASE ((uint32_t)0x50000000)
| AHB base address. More...
#define | WDT_BASE (APB1PERIPH_BASE + 0x04000)
| WDT register base address. More...
#define | WWDT_BASE (APB1PERIPH_BASE + 0x04100)
| WWDT register base address. More...
#define | TIMER0_BASE (APB1PERIPH_BASE + 0x10000)
| TIMER0 register base address. More...
#define | TIMER1_BASE (APB1PERIPH_BASE + 0x10020)
| TIMER1 register base address. More...
#define | I2C0_BASE (APB1PERIPH_BASE + 0x20000)
| I2C0 register base address. More...
#define | I2C1_BASE (APB2PERIPH_BASE + 0x20000)
| I2C1 register base address. More...
#define | SPI_BASE (APB1PERIPH_BASE + 0x30000)
| SPI register base address. More...
#define | PWM_BASE (APB1PERIPH_BASE + 0x40000)
| PWM register base address. More...
#define | UART0_BASE (APB1PERIPH_BASE + 0x50000)
| UART0 register base address. More...
#define | UART1_BASE (APB2PERIPH_BASE + 0x50000)
| UART1 register base address. More...
#define | ACMP_BASE (APB1PERIPH_BASE + 0xD0000)
| ACMP register base address. More...
#define | ADC_BASE (APB1PERIPH_BASE + 0xE0000)
| ADC register base address. More...
#define | SYS_BASE (AHBPERIPH_BASE + 0x00000)
| SYS register base address. More...
#define | CLK_BASE (AHBPERIPH_BASE + 0x00200)
| CLK register base address. More...
#define | INTR_BASE (AHBPERIPH_BASE + 0x00300)
| INT register base address. More...
#define | P0_BASE (AHBPERIPH_BASE + 0x04000)
| GPIO Port 0 register base address. More...
#define | P1_BASE (AHBPERIPH_BASE + 0x04040)
| GPIO Port 1 register base address. More...
#define | P2_BASE (AHBPERIPH_BASE + 0x04080)
| GPIO Port 2 register base address. More...
#define | P3_BASE (AHBPERIPH_BASE + 0x040C0)
| GPIO Port 3 register base address. More...
#define | P4_BASE (AHBPERIPH_BASE + 0x04100)
| GPIO Port 4 register base address. More...
#define | P5_BASE (AHBPERIPH_BASE + 0x04140)
| GPIO Port 5 register base address. More...
#define | GPIO_DBNCECON_BASE (AHBPERIPH_BASE + 0x04180)
| GPIO De-bounce register vase. More...
#define | GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO pin data register base address. More...
#define | GPIOBIT0_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO Port 0 bit access register base address. More...
#define | GPIOBIT1_BASE (AHBPERIPH_BASE + 0x04220)
| GPIO Port 1 bit access register base address. More...
#define | GPIOBIT2_BASE (AHBPERIPH_BASE + 0x04240)
| GPIO Port 2 bit access register base address. More...
#define | GPIOBIT3_BASE (AHBPERIPH_BASE + 0x04260)
| GPIO Port 3 bit access register base address. More...
#define | GPIOBIT4_BASE (AHBPERIPH_BASE + 0x04280)
| GPIO Port 4 bit access register base address. More...
#define | GPIOBIT5_BASE (AHBPERIPH_BASE + 0x042A0)
| GPIO Port 5 bit access register base address. More...
#define | FMC_BASE (AHBPERIPH_BASE + 0x0C000)
| FMC register base address. More...
#define | WDT ((WDT_T *) WDT_BASE)
| Pointer to WDT register structure. More...
#define | WWDT ((WWDT_T *) WWDT_BASE)
| Pointer to WWDT register structure. More...
#define | TIMER0 ((TIMER_T *) TIMER0_BASE)
| Pointer to Timer 0 register structure. More...
#define | TIMER1 ((TIMER_T *) TIMER1_BASE)
| Pointer to Timer 1 register structure. More...
#define | I2C ((I2C_T *) I2C0_BASE)
| Pointer to I2C0 register structure. More...
#define | I2C0 ((I2C_T *) I2C0_BASE)
| Pointer to I2C0 register structure. More...
#define | I2C1 ((I2C_T *) I2C1_BASE)
| Pointer to I2C1 register structure. More...
#define | SPI ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | SPI0 ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | PWM ((PWM_T *) PWM_BASE)
| Pointer to PWM register structure. More...
#define | UART ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure. More...
#define | UART0 ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure. More...
#define | UART1 ((UART_T *) UART1_BASE)
| Pointer to UART1 register structure. More...
#define | ADC ((ADC_T *) ADC_BASE)
| Pointer to ADC register structure. More...
#define | ACMP ((ACMP_T *) ACMP_BASE)
| Pointer to ACMP register structure. More...
#define | SYS ((SYS_T *) SYS_BASE)
| Pointer to SYS register structure. More...
#define | CLK ((CLK_T *) CLK_BASE)
| Pointer to CLK register structure. More...
#define | INTR ((INTR_T *) INTR_BASE)
| Pointer to INT register structure. More...
#define | P0 ((GPIO_T *) P0_BASE)
| Pointer to GPIO port 0 register structure. More...
#define | P1 ((GPIO_T *) P1_BASE)
| Pointer to GPIO port 1 register structure. More...
#define | P2 ((GPIO_T *) P2_BASE)
| Pointer to GPIO port 2 register structure. More...
#define | P3 ((GPIO_T *) P3_BASE)
| Pointer to GPIO port 3 register structure. More...
#define | P4 ((GPIO_T *) P4_BASE)
| Pointer to GPIO port 4 register structure. More...
#define | P5 ((GPIO_T *) P5_BASE)
| Pointer to GPIO port 5 register structure. More...
#define | GPIO ((GPIO_DB_T *) GPIO_DBNCECON_BASE)
| Pointer to GPIO de-bounce register structure. More...
#define | FMC ((FMC_T *) FMC_BASE)
| Pointer to FMC register structure. More...
#define | M8(addr) (*((vu8 *) (addr)))
| Get a 8-bit unsigned value from specified address. More...
#define | M16(addr) (*((vu16 *) (addr)))
| Get a 16-bit unsigned value from specified address. More...
#define | M32(addr) (*((vu32 *) (addr)))
| Get a 32-bit unsigned value from specified address. More...
#define | outpw(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inpw(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outps(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inps(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outpb(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inpb(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | outp32(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inp32(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outp16(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inp16(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outp8(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inp8(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | NULL (0)
| NULL pointer. More...
#define | TRUE (1)
| Boolean true, define to use in API parameters or return value. More...
#define | FALSE (0)
| Boolean false, define to use in API parameters or return value. More...
#define | ENABLE (1)
| Enable, define to use in API parameters. More...
#define | DISABLE (0)
| Disable, define to use in API parameters. More...
#define | BIT0 (0x00000001)
| Bit 0 mask of an 32 bit integer. More...
#define | BIT1 (0x00000002)
| Bit 1 mask of an 32 bit integer. More...
#define | BIT2 (0x00000004)
| Bit 2 mask of an 32 bit integer. More...
#define | BIT3 (0x00000008)
| Bit 3 mask of an 32 bit integer. More...
#define | BIT4 (0x00000010)
| Bit 4 mask of an 32 bit integer. More...
#define | BIT5 (0x00000020)
| Bit 5 mask of an 32 bit integer. More...
#define | BIT6 (0x00000040)
| Bit 6 mask of an 32 bit integer. More...
#define | BIT7 (0x00000080)
| Bit 7 mask of an 32 bit integer. More...
#define | BIT8 (0x00000100)
| Bit 8 mask of an 32 bit integer. More...
#define | BIT9 (0x00000200)
| Bit 9 mask of an 32 bit integer. More...
#define | BIT10 (0x00000400)
| Bit 10 mask of an 32 bit integer. More...
#define | BIT11 (0x00000800)
| Bit 11 mask of an 32 bit integer. More...
#define | BIT12 (0x00001000)
| Bit 12 mask of an 32 bit integer. More...
#define | BIT13 (0x00002000)
| Bit 13 mask of an 32 bit integer. More...
#define | BIT14 (0x00004000)
| Bit 14 mask of an 32 bit integer. More...
#define | BIT15 (0x00008000)
| Bit 15 mask of an 32 bit integer. More...
#define | BIT16 (0x00010000)
| Bit 16 mask of an 32 bit integer. More...
#define | BIT17 (0x00020000)
| Bit 17 mask of an 32 bit integer. More...
#define | BIT18 (0x00040000)
| Bit 18 mask of an 32 bit integer. More...
#define | BIT19 (0x00080000)
| Bit 19 mask of an 32 bit integer. More...
#define | BIT20 (0x00100000)
| Bit 20 mask of an 32 bit integer. More...
#define | BIT21 (0x00200000)
| Bit 21 mask of an 32 bit integer. More...
#define | BIT22 (0x00400000)
| Bit 22 mask of an 32 bit integer. More...
#define | BIT23 (0x00800000)
| Bit 23 mask of an 32 bit integer. More...
#define | BIT24 (0x01000000)
| Bit 24 mask of an 32 bit integer. More...
#define | BIT25 (0x02000000)
| Bit 25 mask of an 32 bit integer. More...
#define | BIT26 (0x04000000)
| Bit 26 mask of an 32 bit integer. More...
#define | BIT27 (0x08000000)
| Bit 27 mask of an 32 bit integer. More...
#define | BIT28 (0x10000000)
| Bit 28 mask of an 32 bit integer. More...
#define | BIT29 (0x20000000)
| Bit 29 mask of an 32 bit integer. More...
#define | BIT30 (0x40000000)
| Bit 30 mask of an 32 bit integer. More...
#define | BIT31 (0x80000000)
| Bit 31 mask of an 32 bit integer. More...
#define | BYTE0_Msk (0x000000FF)
| Mask to get bit0~bit7 from a 32 bit integer. More...
#define | BYTE1_Msk (0x0000FF00)
| Mask to get bit8~bit15 from a 32 bit integer. More...
#define | BYTE2_Msk (0x00FF0000)
| Mask to get bit16~bit23 from a 32 bit integer. More...
#define | BYTE3_Msk (0xFF000000)
| Mask to get bit24~bit31 from a 32 bit integer. More...
#define | GET_BYTE0(u32Param) ((u32Param & BYTE0_Msk) )
#define | GET_BYTE1(u32Param) ((u32Param & BYTE1_Msk) >> 8)
#define | GET_BYTE2(u32Param) ((u32Param & BYTE2_Msk) >> 16)
#define | GET_BYTE3(u32Param) ((u32Param & BYTE3_Msk) >> 24)
#define | ACMP_CTL_ACMPEN_Pos (0)
#define | ACMP_CTL_ACMPEN_Msk (0x1ul << ACMP_CTL_ACMPEN_Pos)
#define | ACMP_CTL_ACMPIE_Pos (1)
#define | ACMP_CTL_ACMPIE_Msk (0x1ul << ACMP_CTL_ACMPIE_Pos)
#define | ACMP_CTL_HYSSEL_Pos (2)
#define | ACMP_CTL_HYSSEL_Msk (0x1ul << ACMP_CTL_HYSSEL_Pos)
#define | ACMP_CTL_NEGSEL_Pos (4)
#define | ACMP_CTL_NEGSEL_Msk (0x1ul << ACMP_CTL_NEGSEL_Pos)
#define | ACMP_CTL_RTRGEN_Pos (8)
#define | ACMP_CTL_RTRGEN_Msk (0x1ul << ACMP_CTL_RTRGEN_Pos)
#define | ACMP_CTL_FTRGEN_Pos (9)
#define | ACMP_CTL_FTRGEN_Msk (0x1ul << ACMP_CTL_FTRGEN_Pos)
#define | ACMP_CTL_FILTSEL_Pos (20)
#define | ACMP_CTL_FILTSEL_Msk (0xful << ACMP_CTL_FILTSEL_Pos)
#define | ACMP_CTL_POSSEL_Pos (29)
#define | ACMP_CTL_POSSEL_Msk (0x3ul << ACMP_CTL_POSSEL_Pos)
#define | ACMP_STATUS_ACMPIF0_Pos (0)
#define | ACMP_STATUS_ACMPIF0_Msk (0x1ul << ACMP_STATUS_ACMPIF0_Pos)
#define | ACMP_STATUS_ACMPIF1_Pos (1)
#define | ACMP_STATUS_ACMPIF1_Msk (0x1ul << ACMP_STATUS_ACMPIF1_Pos)
#define | ACMP_STATUS_ACMPO0_Pos (2)
#define | ACMP_STATUS_ACMPO0_Msk (0x1ul << ACMP_STATUS_ACMPO0_Pos)
#define | ACMP_STATUS_ACMPO1_Pos (3)
#define | ACMP_STATUS_ACMPO1_Msk (0x1ul << ACMP_STATUS_ACMPO1_Pos)
#define | ACMP_VREF_CRVCTL_Pos (0)
#define | ACMP_VREF_CRVCTL_Msk (0xful << ACMP_VREF_CRVCTL_Pos)
#define | ACMP_VREF_IREFSEL_Pos (7)
#define | ACMP_VREF_IREFSEL_Msk (0x1ul << ACMP_VREF_IREFSEL_Pos)
#define | ADC_DAT_RESULT_Pos (0)
#define | ADC_DAT_RESULT_Msk (0x3fful << ADC_DAT_RESULT_Pos)
#define | ADC_DAT_OV_Pos (16)
#define | ADC_DAT_OV_Msk (0x1ul << ADC_DAT_OV_Pos)
#define | ADC_DAT_VALID_Pos (17)
#define | ADC_DAT_VALID_Msk (0x1ul << ADC_DAT_VALID_Pos)
#define | ADC_CTL_ADCEN_Pos (0)
#define | ADC_CTL_ADCEN_Msk (0x1ul << ADC_CTL_ADCEN_Pos)
#define | ADC_CTL_ADCIEN_Pos (1)
#define | ADC_CTL_ADCIEN_Msk (0x1ul << ADC_CTL_ADCIEN_Pos)
#define | ADC_CTL_HWTRGSEL_Pos (4)
#define | ADC_CTL_HWTRGSEL_Msk (0x3ul << ADC_CTL_HWTRGSEL_Pos)
#define | ADC_CTL_HWTRGCOND_Pos (6)
#define | ADC_CTL_HWTRGCOND_Msk (0x1ul << ADC_CTL_HWTRGCOND_Pos)
#define | ADC_CTL_HWTRGEN_Pos (8)
#define | ADC_CTL_HWTRGEN_Msk (0x1ul << ADC_CTL_HWTRGEN_Pos)
#define | ADC_CTL_SWTRG_Pos (11)
#define | ADC_CTL_SWTRG_Msk (0x1ul << ADC_CTL_SWTRG_Pos)
#define | ADC_CHEN_CHEN0_Pos (0)
#define | ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)
#define | ADC_CHEN_CHEN1_Pos (1)
#define | ADC_CHEN_CHEN1_Msk (0x1ul << ADC_CHEN_CHEN1_Pos)
#define | ADC_CHEN_CHEN2_Pos (2)
#define | ADC_CHEN_CHEN2_Msk (0x1ul << ADC_CHEN_CHEN2_Pos)
#define | ADC_CHEN_CHEN3_Pos (3)
#define | ADC_CHEN_CHEN3_Msk (0x1ul << ADC_CHEN_CHEN3_Pos)
#define | ADC_CHEN_CHEN4_Pos (4)
#define | ADC_CHEN_CHEN4_Msk (0x1ul << ADC_CHEN_CHEN4_Pos)
#define | ADC_CHEN_CHEN5_Pos (5)
#define | ADC_CHEN_CHEN5_Msk (0x1ul << ADC_CHEN_CHEN5_Pos)
#define | ADC_CHEN_CHEN6_Pos (6)
#define | ADC_CHEN_CHEN6_Msk (0x1ul << ADC_CHEN_CHEN6_Pos)
#define | ADC_CHEN_CHEN7_Pos (7)
#define | ADC_CHEN_CHEN7_Msk (0x1ul << ADC_CHEN_CHEN7_Pos)
#define | ADC_CHEN_CH7SEL_Pos (8)
#define | ADC_CHEN_CH7SEL_Msk (0x1ul << ADC_CHEN_CH7SEL_Pos)
#define | ADC_CMP0_ADCMPEN_Pos (0)
#define | ADC_CMP0_ADCMPEN_Msk (0x1ul << ADC_CMP0_ADCMPEN_Pos)
#define | ADC_CMP0_ADCMPIE_Pos (1)
#define | ADC_CMP0_ADCMPIE_Msk (0x1ul << ADC_CMP0_ADCMPIE_Pos)
#define | ADC_CMP0_CMPCOND_Pos (2)
#define | ADC_CMP0_CMPCOND_Msk (0x1ul << ADC_CMP0_CMPCOND_Pos)
#define | ADC_CMP0_CMPCH_Pos (3)
#define | ADC_CMP0_CMPCH_Msk (0x7ul << ADC_CMP0_CMPCH_Pos)
#define | ADC_CMP0_CMPMCNT_Pos (8)
#define | ADC_CMP0_CMPMCNT_Msk (0xful << ADC_CMP0_CMPMCNT_Pos)
#define | ADC_CMP0_CMPDAT_Pos (16)
#define | ADC_CMP0_CMPDAT_Msk (0x3fful << ADC_CMP0_CMPDAT_Pos)
#define | ADC_CMP1_ADCMPEN_Pos (0)
#define | ADC_CMP1_ADCMPEN_Msk (0x1ul << ADC_CMP1_ADCMPEN_Pos)
#define | ADC_CMP1_ADCMPIE_Pos (1)
#define | ADC_CMP1_ADCMPIE_Msk (0x1ul << ADC_CMP1_ADCMPIE_Pos)
#define | ADC_CMP1_CMPCOND_Pos (2)
#define | ADC_CMP1_CMPCOND_Msk (0x1ul << ADC_CMP1_CMPCOND_Pos)
#define | ADC_CMP1_CMPCH_Pos (3)
#define | ADC_CMP1_CMPCH_Msk (0x7ul << ADC_CMP1_CMPCH_Pos)
#define | ADC_CMP1_CMPMCNT_Pos (8)
#define | ADC_CMP1_CMPMCNT_Msk (0xful << ADC_CMP1_CMPMCNT_Pos)
#define | ADC_CMP1_CMPDAT_Pos (16)
#define | ADC_CMP1_CMPDAT_Msk (0x3fful << ADC_CMP1_CMPDAT_Pos)
#define | ADC_STATUS_ADIF_Pos (0)
#define | ADC_STATUS_ADIF_Msk (0x1ul << ADC_STATUS_ADIF_Pos)
#define | ADC_STATUS_ADCMPF0_Pos (1)
#define | ADC_STATUS_ADCMPF0_Msk (0x1ul << ADC_STATUS_ADCMPF0_Pos)
#define | ADC_STATUS_ADCMPF1_Pos (2)
#define | ADC_STATUS_ADCMPF1_Msk (0x1ul << ADC_STATUS_ADCMPF1_Pos)
#define | ADC_STATUS_BUSY_Pos (3)
#define | ADC_STATUS_BUSY_Msk (0x1ul << ADC_STATUS_BUSY_Pos)
#define | ADC_STATUS_CHANNEL_Pos (4)
#define | ADC_STATUS_CHANNEL_Msk (0x7ul << ADC_STATUS_CHANNEL_Pos)
#define | ADC_STATUS_VALID_Pos (8)
#define | ADC_STATUS_VALID_Msk (0x1ul << ADC_STATUS_VALID_Pos)
#define | ADC_STATUS_OV_Pos (16)
#define | ADC_STATUS_OV_Msk (0x1ul << ADC_STATUS_OV_Pos)
#define | ADC_TRGDLY_DELAY_Pos (0)
#define | ADC_TRGDLY_DELAY_Msk (0xfful << ADC_TRGDLY_DELAY_Pos)
#define | ADC_EXTSMPT_EXTSMPT_Pos (0)
#define | ADC_EXTSMPT_EXTSMPT_Msk (0xful << ADC_EXTSMPT_EXTSMPT_Pos)
#define | ADC_SEQCTL_SEQEN_Pos (0)
#define | ADC_SEQCTL_SEQEN_Msk (0x1ul << ADC_SEQCTL_SEQEN_Pos)
#define | ADC_SEQCTL_SEQTYPE_Pos (1)
#define | ADC_SEQCTL_SEQTYPE_Msk (0x1ul << ADC_SEQCTL_SEQTYPE_Pos)
#define | ADC_SEQCTL_MODESEL_Pos (2)
#define | ADC_SEQCTL_MODESEL_Msk (0x3ul << ADC_SEQCTL_MODESEL_Pos)
#define | ADC_SEQCTL_TRG1CTL_Pos (8)
#define | ADC_SEQCTL_TRG1CTL_Msk (0xful << ADC_SEQCTL_TRG1CTL_Pos)
#define | ADC_SEQCTL_TRG2CTL_Pos (16)
#define | ADC_SEQCTL_TRG2CTL_Msk (0xful << ADC_SEQCTL_TRG2CTL_Pos)
#define | ADC_SEQDAT1_RESULT_Pos (0)
#define | ADC_SEQDAT1_RESULT_Msk (0x3fful << ADC_SEQDAT1_RESULT_Pos)
#define | ADC_SEQDAT1_OV_Pos (16)
#define | ADC_SEQDAT1_OV_Msk (0x1ul << ADC_SEQDAT1_OV_Pos)
#define | ADC_SEQDAT1_VALID_Pos (17)
#define | ADC_SEQDAT1_VALID_Msk (0x1ul << ADC_SEQDAT1_VALID_Pos)
#define | ADC_SEQDAT2_RESULT_Pos (0)
#define | ADC_SEQDAT2_RESULT_Msk (0x3fful << ADC_SEQDAT2_RESULT_Pos)
#define | ADC_SEQDAT2_OV_Pos (16)
#define | ADC_SEQDAT2_OV_Msk (0x1ul << ADC_SEQDAT2_OV_Pos)
#define | ADC_SEQDAT2_VALID_Pos (17)
#define | ADC_SEQDAT2_VALID_Msk (0x1ul << ADC_SEQDAT2_VALID_Pos)
#define | CLK_PWRCTL_XTLEN_Pos (0)
#define | CLK_PWRCTL_XTLEN_Msk (0x3ul << CLK_PWRCTL_XTLEN_Pos)
#define | CLK_PWRCTL_HIRCEN_Pos (2)
#define | CLK_PWRCTL_HIRCEN_Msk (0x1ul << CLK_PWRCTL_HIRCEN_Pos)
#define | CLK_PWRCTL_LIRCEN_Pos (3)
#define | CLK_PWRCTL_LIRCEN_Msk (0x1ul << CLK_PWRCTL_LIRCEN_Pos)
#define | CLK_PWRCTL_PDWKDLY_Pos (4)
#define | CLK_PWRCTL_PDWKDLY_Msk (0x1ul << CLK_PWRCTL_PDWKDLY_Pos)
#define | CLK_PWRCTL_PDWKIEN_Pos (5)
#define | CLK_PWRCTL_PDWKIEN_Msk (0x1ul << CLK_PWRCTL_PDWKIEN_Pos)
#define | CLK_PWRCTL_PDWKIF_Pos (6)
#define | CLK_PWRCTL_PDWKIF_Msk (0x1ul << CLK_PWRCTL_PDWKIF_Pos)
#define | CLK_PWRCTL_PDEN_Pos (7)
#define | CLK_PWRCTL_PDEN_Msk (0x1ul << CLK_PWRCTL_PDEN_Pos)
#define | CLK_PWRCTL_PDLXT_Pos (9)
#define | CLK_PWRCTL_PDLXT_Msk (0x1ul << CLK_PWRCTL_PDLXT_Pos)
#define | CLK_AHBCLK_ISPCKEN_Pos (2)
#define | CLK_AHBCLK_ISPCKEN_Msk (0x1ul << CLK_AHBCLK_ISPCKEN_Pos)
#define | CLK_APBCLK_WDTCKEN_Pos (0)
#define | CLK_APBCLK_WDTCKEN_Msk (0x1ul << CLK_APBCLK_WDTCKEN_Pos)
#define | CLK_APBCLK_TMR0CKEN_Pos (2)
#define | CLK_APBCLK_TMR0CKEN_Msk (0x1ul << CLK_APBCLK_TMR0CKEN_Pos)
#define | CLK_APBCLK_TMR1CKEN_Pos (3)
#define | CLK_APBCLK_TMR1CKEN_Msk (0x1ul << CLK_APBCLK_TMR1CKEN_Pos)
#define | CLK_APBCLK_CLKOCKEN_Pos (6)
#define | CLK_APBCLK_CLKOCKEN_Msk (0x1ul << CLK_APBCLK_CLKOCKEN_Pos)
#define | CLK_APBCLK_I2C0CKEN_Pos (8)
#define | CLK_APBCLK_I2C0CKEN_Msk (0x1ul << CLK_APBCLK_I2C0CKEN_Pos)
#define | CLK_APBCLK_I2C1CKEN_Pos (9)
#define | CLK_APBCLK_I2C1CKEN_Msk (0x1ul << CLK_APBCLK_I2C1CKEN_Pos)
#define | CLK_APBCLK_SPICKEN_Pos (12)
#define | CLK_APBCLK_SPICKEN_Msk (0x1ul << CLK_APBCLK_SPICKEN_Pos)
#define | CLK_APBCLK_UART0CKEN_Pos (16)
#define | CLK_APBCLK_UART0CKEN_Msk (0x1ul << CLK_APBCLK_UART0CKEN_Pos)
#define | CLK_APBCLK_UART1CKEN_Pos (17)
#define | CLK_APBCLK_UART1CKEN_Msk (0x1ul << CLK_APBCLK_UART1CKEN_Pos)
#define | CLK_APBCLK_PWMCH01CKEN_Pos (20)
#define | CLK_APBCLK_PWMCH01CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH01CKEN_Pos)
#define | CLK_APBCLK_PWMCH23CKEN_Pos (21)
#define | CLK_APBCLK_PWMCH23CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH23CKEN_Pos)
#define | CLK_APBCLK_PWMCH45CKEN_Pos (22)
#define | CLK_APBCLK_PWMCH45CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH45CKEN_Pos)
#define | CLK_APBCLK_ADCCKEN_Pos (28)
#define | CLK_APBCLK_ADCCKEN_Msk (0x1ul << CLK_APBCLK_ADCCKEN_Pos)
#define | CLK_APBCLK_ACMPCKEN_Pos (30)
#define | CLK_APBCLK_ACMPCKEN_Msk (0x1ul << CLK_APBCLK_ACMPCKEN_Pos)
#define | CLK_STATUS_XTLSTB_Pos (0)
#define | CLK_STATUS_XTLSTB_Msk (0x1ul << CLK_STATUS_XTLSTB_Pos)
#define | CLK_STATUS_PLLSTB_Pos (2)
#define | CLK_STATUS_PLLSTB_Msk (0x1ul << CLK_STATUS_PLLSTB_Pos)
#define | CLK_STATUS_LIRCSTB_Pos (3)
#define | CLK_STATUS_LIRCSTB_Msk (0x1ul << CLK_STATUS_LIRCSTB_Pos)
#define | CLK_STATUS_HIRCSTB_Pos (4)
#define | CLK_STATUS_HIRCSTB_Msk (0x1ul << CLK_STATUS_HIRCSTB_Pos)
#define | CLK_STATUS_CLKSFAIL_Pos (7)
#define | CLK_STATUS_CLKSFAIL_Msk (0x1ul << CLK_STATUS_CLKSFAIL_Pos)
#define | CLK_CLKSEL0_HCLKSEL_Pos (0)
#define | CLK_CLKSEL0_HCLKSEL_Msk (0x7ul << CLK_CLKSEL0_HCLKSEL_Pos)
#define | CLK_CLKSEL0_STCLKSEL_Pos (3)
#define | CLK_CLKSEL0_STCLKSEL_Msk (0x7ul << CLK_CLKSEL0_STCLKSEL_Pos)
#define | CLK_CLKSEL1_WDTSEL_Pos (0)
#define | CLK_CLKSEL1_WDTSEL_Msk (0x3ul << CLK_CLKSEL1_WDTSEL_Pos)
#define | CLK_CLKSEL1_ADCSEL_Pos (2)
#define | CLK_CLKSEL1_ADCSEL_Msk (0x3ul << CLK_CLKSEL1_ADCSEL_Pos)
#define | CLK_CLKSEL1_SPISEL_Pos (4)
#define | CLK_CLKSEL1_SPISEL_Msk (0x3ul << CLK_CLKSEL1_SPISEL_Pos)
#define | CLK_CLKSEL1_TMR0SEL_Pos (8)
#define | CLK_CLKSEL1_TMR0SEL_Msk (0x7ul << CLK_CLKSEL1_TMR0SEL_Pos)
#define | CLK_CLKSEL1_TMR1SEL_Pos (12)
#define | CLK_CLKSEL1_TMR1SEL_Msk (0x7ul << CLK_CLKSEL1_TMR1SEL_Pos)
#define | CLK_CLKSEL1_UARTSEL_Pos (24)
#define | CLK_CLKSEL1_UARTSEL_Msk (0x3ul << CLK_CLKSEL1_UARTSEL_Pos)
#define | CLK_CLKSEL1_PWMCH01SEL_Pos (28)
#define | CLK_CLKSEL1_PWMCH01SEL_Msk (0x3ul << CLK_CLKSEL1_PWMCH01SEL_Pos)
#define | CLK_CLKSEL1_PWMCH23SEL_Pos (30)
#define | CLK_CLKSEL1_PWMCH23SEL_Msk (0x3ul << CLK_CLKSEL1_PWMCH23SEL_Pos)
#define | CLK_CLKDIV_HCLKDIV_Pos (0)
#define | CLK_CLKDIV_HCLKDIV_Msk (0xful << CLK_CLKDIV_HCLKDIV_Pos)
#define | CLK_CLKDIV_UARTDIV_Pos (8)
#define | CLK_CLKDIV_UARTDIV_Msk (0xful << CLK_CLKDIV_UARTDIV_Pos)
#define | CLK_CLKDIV_ADCDIV_Pos (16)
#define | CLK_CLKDIV_ADCDIV_Msk (0xfful << CLK_CLKDIV_ADCDIV_Pos)
#define | CLK_CLKSEL2_CLKOSEL_Pos (2)
#define | CLK_CLKSEL2_CLKOSEL_Msk (0x3ul << CLK_CLKSEL2_CLKOSEL_Pos)
#define | CLK_CLKSEL2_PWMCH45SEL_Pos (4)
#define | CLK_CLKSEL2_PWMCH45SEL_Msk (0x3ul << CLK_CLKSEL2_PWMCH45SEL_Pos)
#define | CLK_CLKSEL2_WWDTSEL_Pos (16)
#define | CLK_CLKSEL2_WWDTSEL_Msk (0x3ul << CLK_CLKSEL2_WWDTSEL_Pos)
#define | CLK_PLLCTL_FBDIV_Pos (0)
#define | CLK_PLLCTL_FBDIV_Msk (0x1fful << CLK_PLLCTL_FBDIV_Pos)
#define | CLK_PLLCTL_INDIV_Pos (9)
#define | CLK_PLLCTL_INDIV_Msk (0x1ful << CLK_PLLCTL_INDIV_Pos)
#define | CLK_PLLCTL_OUTDIV_Pos (14)
#define | CLK_PLLCTL_OUTDIV_Msk (0x3ul << CLK_PLLCTL_OUTDIV_Pos)
#define | CLK_PLLCTL_PD_Pos (16)
#define | CLK_PLLCTL_PD_Msk (0x1ul << CLK_PLLCTL_PD_Pos)
#define | CLK_PLLCTL_BP_Pos (17)
#define | CLK_PLLCTL_BP_Msk (0x1ul << CLK_PLLCTL_BP_Pos)
#define | CLK_PLLCTL_OE_Pos (18)
#define | CLK_PLLCTL_OE_Msk (0x1ul << CLK_PLLCTL_OE_Pos)
#define | CLK_PLLCTL_PLLSRC_Pos (19)
#define | CLK_PLLCTL_PLLSRC_Msk (0x1ul << CLK_PLLCTL_PLLSRC_Pos)
#define | CLK_CLKOCTL_FREQSEL_Pos (0)
#define | CLK_CLKOCTL_FREQSEL_Msk (0xful << CLK_CLKOCTL_FREQSEL_Pos)
#define | CLK_CLKOCTL_CLKOEN_Pos (4)
#define | CLK_CLKOCTL_CLKOEN_Msk (0x1ul << CLK_CLKOCTL_CLKOEN_Pos)
#define | CLK_CLKOCTL_DIV1EN_Pos (5)
#define | CLK_CLKOCTL_DIV1EN_Msk (0x1ul << CLK_CLKOCTL_DIV1EN_Pos)
#define | FMC_ISPCTL_ISPEN_Pos (0)
#define | FMC_ISPCTL_ISPEN_Msk (0x1ul << FMC_ISPCTL_ISPEN_Pos)
#define | FMC_ISPCTL_BS_Pos (1)
#define | FMC_ISPCTL_BS_Msk (0x1ul << FMC_ISPCTL_BS_Pos)
#define | FMC_ISPCTL_SPUEN_Pos (2)
#define | FMC_ISPCTL_SPUEN_Msk (0x1ul << FMC_ISPCTL_SPUEN_Pos)
#define | FMC_ISPCTL_APUEN_Pos (3)
#define | FMC_ISPCTL_APUEN_Msk (0x1ul << FMC_ISPCTL_APUEN_Pos)
#define | FMC_ISPCTL_CFGUEN_Pos (4)
#define | FMC_ISPCTL_CFGUEN_Msk (0x1ul << FMC_ISPCTL_CFGUEN_Pos)
#define | FMC_ISPCTL_LDUEN_Pos (5)
#define | FMC_ISPCTL_LDUEN_Msk (0x1ul << FMC_ISPCTL_LDUEN_Pos)
#define | FMC_ISPCTL_ISPFF_Pos (6)
#define | FMC_ISPCTL_ISPFF_Msk (0x1ul << FMC_ISPCTL_ISPFF_Pos)
#define | FMC_ISPADDR_ISPADDR_Pos (0)
#define | FMC_ISPADDR_ISPADDR_Msk (0xfffffffful << FMC_ISPADDR_ISPADDR_Pos)
#define | FMC_ISPDAT_ISPDAT_Pos (0)
#define | FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)
#define | FMC_ISPCMD_CMD_Pos (0)
#define | FMC_ISPCMD_CMD_Msk (0x7ful << FMC_ISPCMD_CMD_Pos)
#define | FMC_ISPTRG_ISPGO_Pos (0)
#define | FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)
#define | FMC_DFBA_DFBA_Pos (0)
#define | FMC_DFBA_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)
#define | FMC_FATCTL_FOM_Pos (4)
#define | FMC_FATCTL_FOM_Msk (0x7ul << FMC_FATCTL_FOM_Pos)
#define | FMC_ISPSTS_ISPBUSY_Pos (0)
#define | FMC_ISPSTS_ISPBUSY_Msk (0x1ul << FMC_ISPSTS_ISPBUSY_Pos)
#define | FMC_ISPSTS_CBS_Pos (1)
#define | FMC_ISPSTS_CBS_Msk (0x3ul << FMC_ISPSTS_CBS_Pos)
#define | FMC_ISPSTS_ISPFF_Pos (6)
#define | FMC_ISPSTS_ISPFF_Msk (0x1ul << FMC_ISPSTS_ISPFF_Pos)
#define | FMC_ISPSTS_VECMAP_Pos (9)
#define | FMC_ISPSTS_VECMAP_Msk (0xffful << FMC_ISPSTS_VECMAP_Pos)
#define | FMC_ISPSTS_SCODE_Pos (31)
#define | FMC_ISPSTS_SCODE_Msk (0x1ul << FMC_ISPSTS_SCODE_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_INTSRC_INTSRC8_Pos (8)
#define | GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)
#define | GP_INTSRC_INTSRC9_Pos (9)
#define | GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)
#define | GP_INTSRC_INTSRC10_Pos (10)
#define | GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)
#define | GP_INTSRC_INTSRC11_Pos (11)
#define | GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)
#define | GP_INTSRC_INTSRC12_Pos (12)
#define | GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)
#define | GP_INTSRC_INTSRC13_Pos (13)
#define | GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)
#define | GP_INTSRC_INTSRC14_Pos (14)
#define | GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)
#define | GP_INTSRC_INTSRC15_Pos (15)
#define | GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_INTSRC_INTSRC8_Pos (8)
#define | GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)
#define | GP_INTSRC_INTSRC9_Pos (9)
#define | GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)
#define | GP_INTSRC_INTSRC10_Pos (10)
#define | GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)
#define | GP_INTSRC_INTSRC11_Pos (11)
#define | GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)
#define | GP_INTSRC_INTSRC12_Pos (12)
#define | GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)
#define | GP_INTSRC_INTSRC13_Pos (13)
#define | GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)
#define | GP_INTSRC_INTSRC14_Pos (14)
#define | GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)
#define | GP_INTSRC_INTSRC15_Pos (15)
#define | GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_INTSRC_INTSRC8_Pos (8)
#define | GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)
#define | GP_INTSRC_INTSRC9_Pos (9)
#define | GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)
#define | GP_INTSRC_INTSRC10_Pos (10)
#define | GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)
#define | GP_INTSRC_INTSRC11_Pos (11)
#define | GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)
#define | GP_INTSRC_INTSRC12_Pos (12)
#define | GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)
#define | GP_INTSRC_INTSRC13_Pos (13)
#define | GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)
#define | GP_INTSRC_INTSRC14_Pos (14)
#define | GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)
#define | GP_INTSRC_INTSRC15_Pos (15)
#define | GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_INTSRC_INTSRC8_Pos (8)
#define | GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)
#define | GP_INTSRC_INTSRC9_Pos (9)
#define | GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)
#define | GP_INTSRC_INTSRC10_Pos (10)
#define | GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)
#define | GP_INTSRC_INTSRC11_Pos (11)
#define | GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)
#define | GP_INTSRC_INTSRC12_Pos (12)
#define | GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)
#define | GP_INTSRC_INTSRC13_Pos (13)
#define | GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)
#define | GP_INTSRC_INTSRC14_Pos (14)
#define | GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)
#define | GP_INTSRC_INTSRC15_Pos (15)
#define | GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_INTSRC_INTSRC8_Pos (8)
#define | GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)
#define | GP_INTSRC_INTSRC9_Pos (9)
#define | GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)
#define | GP_INTSRC_INTSRC10_Pos (10)
#define | GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)
#define | GP_INTSRC_INTSRC11_Pos (11)
#define | GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)
#define | GP_INTSRC_INTSRC12_Pos (12)
#define | GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)
#define | GP_INTSRC_INTSRC13_Pos (13)
#define | GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)
#define | GP_INTSRC_INTSRC14_Pos (14)
#define | GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)
#define | GP_INTSRC_INTSRC15_Pos (15)
#define | GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_INTSRC_INTSRC8_Pos (8)
#define | GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)
#define | GP_INTSRC_INTSRC9_Pos (9)
#define | GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)
#define | GP_INTSRC_INTSRC10_Pos (10)
#define | GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)
#define | GP_INTSRC_INTSRC11_Pos (11)
#define | GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)
#define | GP_INTSRC_INTSRC12_Pos (12)
#define | GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)
#define | GP_INTSRC_INTSRC13_Pos (13)
#define | GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)
#define | GP_INTSRC_INTSRC14_Pos (14)
#define | GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)
#define | GP_INTSRC_INTSRC15_Pos (15)
#define | GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)
#define | GP_DBCTL_DBCLKSEL_Pos (0)
#define | GP_DBCTL_DBCLKSEL_Msk (0xful << GP_DBCTL_DBCLKSEL_Pos)
#define | GP_DBCTL_DBCLKSRC_Pos (4)
#define | GP_DBCTL_DBCLKSRC_Msk (0x1ul << GP_DBCTL_DBCLKSRC_Pos)
#define | GP_DBCTL_ICLKON_Pos (5)
#define | GP_DBCTL_ICLKON_Msk (0x1ul << GP_DBCTL_ICLKON_Pos)
#define | I2C_CTL_AA_Pos (2)
#define | I2C_CTL_AA_Msk (0x1ul << I2C_CTL_AA_Pos)
#define | I2C_CTL_SI_Pos (3)
#define | I2C_CTL_SI_Msk (0x1ul << I2C_CTL_SI_Pos)
#define | I2C_CTL_STO_Pos (4)
#define | I2C_CTL_STO_Msk (0x1ul << I2C_CTL_STO_Pos)
#define | I2C_CTL_STA_Pos (5)
#define | I2C_CTL_STA_Msk (0x1ul << I2C_CTL_STA_Pos)
#define | I2C_CTL_I2CEN_Pos (6)
#define | I2C_CTL_I2CEN_Msk (0x1ul << I2C_CTL_I2CEN_Pos)
#define | I2C_CTL_INTEN_Pos (7)
#define | I2C_CTL_INTEN_Msk (0x1ul << I2C_CTL_INTEN_Pos)
#define | I2C_ADDR0_GC_Pos (0)
#define | I2C_ADDR0_GC_Msk (0x1ul << I2C_ADDR0_GC_Pos)
#define | I2C_ADDR0_ADDR_Pos (1)
#define | I2C_ADDR0_ADDR_Msk (0x7ful << I2C_ADDR0_ADDR_Pos)
#define | I2C_DAT_DAT_Pos (0)
#define | I2C_DAT_DAT_Msk (0xfful << I2C_DAT_DAT_Pos)
#define | I2C_STATUS_STATUS_Pos (0)
#define | I2C_STATUS_STATUS_Msk (0xfful << I2C_STATUS_STATUS_Pos)
#define | I2C_CLKDIV_DIVIDER_Pos (0)
#define | I2C_CLKDIV_DIVIDER_Msk (0xfful << I2C_CLKDIV_DIVIDER_Pos)
#define | I2C_TOCTL_TOIF_Pos (0)
#define | I2C_TOCTL_TOIF_Msk (0x1ul << I2C_TOCTL_TOIF_Pos)
#define | I2C_TOCTL_TOCURIEN_Pos (1)
#define | I2C_TOCTL_TOCURIEN_Msk (0x1ul << I2C_TOCTL_TOCURIEN_Pos)
#define | I2C_TOCTL_TOCEN_Pos (2)
#define | I2C_TOCTL_TOCEN_Msk (0x1ul << I2C_TOCTL_TOCEN_Pos)
#define | I2C_ADDR1_GC_Pos (0)
#define | I2C_ADDR1_GC_Msk (0x1ul << I2C_ADDR1_GC_Pos)
#define | I2C_ADDR1_ADDR_Pos (1)
#define | I2C_ADDR1_ADDR_Msk (0x7ful << I2C_ADDR1_ADDR_Pos)
#define | I2C_ADDR2_GC_Pos (0)
#define | I2C_ADDR2_GC_Msk (0x1ul << I2C_ADDR2_GC_Pos)
#define | I2C_ADDR2_ADDR_Pos (1)
#define | I2C_ADDR2_ADDR_Msk (0x7ful << I2C_ADDR2_ADDR_Pos)
#define | I2C_ADDR3_GC_Pos (0)
#define | I2C_ADDR3_GC_Msk (0x1ul << I2C_ADDR3_GC_Pos)
#define | I2C_ADDR3_ADDR_Pos (1)
#define | I2C_ADDR3_ADDR_Msk (0x7ful << I2C_ADDR3_ADDR_Pos)
#define | I2C_ADDRMSK0_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK0_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK0_ADDRMSK_Pos)
#define | I2C_ADDRMSK1_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK1_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK1_ADDRMSK_Pos)
#define | I2C_ADDRMSK2_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK2_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK2_ADDRMSK_Pos)
#define | I2C_ADDRMSK3_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK3_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK3_ADDRMSK_Pos)
#define | I2C_CTL1_WKEN_Pos (0)
#define | I2C_CTL1_WKEN_Msk (0x1ul << I2C_CTL1_WKEN_Pos)
#define | I2C_CTL1_TWOLVFIFO_Pos (1)
#define | I2C_CTL1_TWOLVFIFO_Msk (0x1ul << I2C_CTL1_TWOLVFIFO_Pos)
#define | I2C_CTL1_NSTRETCH_Pos (2)
#define | I2C_CTL1_NSTRETCH_Msk (0x1ul << I2C_CTL1_NSTRETCH_Pos)
#define | I2C_CTL1_OVIEN_Pos (3)
#define | I2C_CTL1_OVIEN_Msk (0x1ul << I2C_CTL1_OVIEN_Pos)
#define | I2C_CTL1_URIEN_Pos (4)
#define | I2C_CTL1_URIEN_Msk (0x1ul << I2C_CTL1_URIEN_Pos)
#define | I2C_STATUS1_WKIF_Pos (0)
#define | I2C_STATUS1_WKIF_Msk (0x1ul << I2C_STATUS1_WKIF_Pos)
#define | I2C_STATUS1_FULL_Pos (1)
#define | I2C_STATUS1_FULL_Msk (0x1ul << I2C_STATUS1_FULL_Pos)
#define | I2C_STATUS1_EMPTY_Pos (2)
#define | I2C_STATUS1_EMPTY_Msk (0x1ul << I2C_STATUS1_EMPTY_Pos)
#define | I2C_STATUS1_OVIF_Pos (3)
#define | I2C_STATUS1_OVIF_Msk (0x1ul << I2C_STATUS1_OVIF_Pos)
#define | I2C_STATUS1_URIF_Pos (4)
#define | I2C_STATUS1_URIF_Msk (0x1ul << I2C_STATUS1_URIF_Pos)
#define | INT_IRQ0_SRC_BOD_INT_Pos (0)
#define | INT_IRQ0_SRC_BOD_INT_Msk (0x1ul << INT_IRQ0_SRC_BOD_INT_Pos)
#define | INT_IRQ1_SRC_WDT_INT_Pos (0)
#define | INT_IRQ1_SRC_WDT_INT_Msk (0x1ul << INT_IRQ1_SRC_WDT_INT_Pos)
#define | INT_IRQ1_SRC_WWDT_INT_Pos (1)
#define | INT_IRQ1_SRC_WWDT_INT_Msk (0x1ul << INT_IRQ1_SRC_WWDT_INT_Pos)
#define | INT_IRQ2_SRC_EINT0_Pos (0)
#define | INT_IRQ2_SRC_EINT0_Msk (0x1ul << INT_IRQ2_SRC_EINT0_Pos)
#define | INT_IRQ3_SRC_EINT1_Pos (0)
#define | INT_IRQ3_SRC_EINT1_Msk (0x1ul << INT_IRQ_SRC3_EINT1_Pos)
#define | INT_IRQ4_SRC_GP0_INT_Pos (0)
#define | INT_IRQ4_SRC_GP0_INT_Msk (0x1ul << INT_IRQ4_SRC_GP0_INT_Pos)
#define | INT_IRQ4_SRC_GP1_INT_Pos (1)
#define | INT_IRQ4_SRC_GP1_INT_Msk (0x1ul << INT_IRQ4_SRC_GP1_INT_Pos)
#define | INT_IRQ5_SRC_GP2_INT_Pos (0)
#define | INT_IRQ5_SRC_GP2_INT_Msk (0x1ul << INT_IRQ5_SRC_GP2_INT_Pos)
#define | INT_IRQ5_SRC_GP3_INT_Pos (1)
#define | INT_IRQ5_SRC_GP3_INT_Msk (0x1ul << INT_IRQ5_SRC_GP3_INT_Pos)
#define | INT_IRQ5_SRC_GP4_INT_Pos (2)
#define | INT_IRQ5_SRC_GP4_INT_Msk (0x1ul << INT_IRQ5_SRC_GP4_INT_Pos)
#define | INT_IRQ6_SRC_PWM_INT_Pos (0)
#define | INT_IRQ6_SRC_PWM_INT_Msk (0x1ul << INT_IRQ6_SRC_PWM_INT_Pos)
#define | INT_IRQ7_SRC_BRAKE_INT_Pos (0)
#define | INT_IRQ7_SRC_BRAKE_INT_Msk (0x1ul << INT_IRQ_SRC_BRAKE_INT_Pos)
#define | INT_IRQ8_SRC_TMR0_INT_Pos (0)
#define | INT_IRQ8_SRC_TMR0_INT_Msk (0x1ul << INT_IRQ8_SRC_TMR0_INT_Pos)
#define | INT_IRQ9_SRC_TMR1_INT_Pos (0)
#define | INT_IRQ9_SRC_TMR1_INT_Msk (0x1ul << INT_IRQ9_SRC_TMR1_INT_Pos)
#define | INT_IRQ12_SRC_UART0_INT_Pos (0)
#define | INT_IRQ12_SRC_UART0_INT_Msk (0x1ul << INT_IRQ12_SRC_UART0_INT_Pos)
#define | INT_IRQ13_SRC_UART1_INT_Pos (0)
#define | INT_IRQ13_SRC_UART1_INT_Msk (0x1ul << INT_IRQ13_SRC_UART1_INT_Pos)
#define | INT_IRQ14_SRC_SPI_INT_Pos (0)
#define | INT_IRQ14_SRC_SPI_INT_Msk (0x1ul << INT_IRQ14_SRC_SPI_INT_Pos)
#define | INT_IRQ16_SRC_GP5_INT_Pos (0)
#define | INT_IRQ16_SRC_GP5_INT_Msk (0x1ul << INT_IRQ16_SRC_GP5_INT_Pos)
#define | INT_IRQ17_SRC_HIRC_TRIM_INT_Pos (0)
#define | INT_IRQ17_SRC_HIRC_TRIM_INT_Msk (0x1ul << INT_IRQ17_SRC_HIRC_TRIM_INT_Pos)
#define | INT_IRQ18_SRC_I2C0_INT_Pos (0)
#define | INT_IRQ18_SRC_I2C0_INT_Msk (0x1ul << INT_IRQ18_SRC_I2C0_INT_Pos)
#define | INT_IRQ19_SRC_I2C1_INT_Pos (0)
#define | INT_IRQ19_SRC_I2C1_INT_Msk (0x1ul << INT_IRQ19_SRC_I2C1_INT_Pos)
#define | INT_IRQ25_SRC_ACMP_INT_Pos (0)
#define | INT_IRQ25_SRC_ACMP_INT_Msk (0x1ul << INT_IRQ25_SRC_ACMP_INT_Pos)
#define | INT_IRQ28_SRC_PWRWU_INT_Pos (0)
#define | INT_IRQ28_SRC_PWRWU_INT_Msk (0x1ul << INT_IRQ28_SRC_PWRWU_INT_Pos)
#define | INT_IRQ29_SRC_ADC_INT_Pos (0)
#define | INT_IRQ29_SRC_ADC_INT_Msk (0x1ul << INT_IRQ29_SRC_ADC_INT_Pos)
#define | INT_CON_NMI_SEL_Pos (0)
#define | INT_CON_NMI_SEL_Msk (0x1ful << INT_CON_NMI_SEL_Pos)
#define | INT_CON_NMI_SEL_EN_Pos (8)
#define | INT_CON_NMI_SEL_EN_Msk (0x1ul << INT_CON_NMI_SEL_EN_Pos)
#define | INT_IRQ_MCU_IRQ_Pos (0)
#define | INT_IRQ_MCU_IRQ_Msk (0xfffffffful << INT_IRQ_MCU_IRQ_Pos)
#define | PWM_CLKPSC_CLKPSC01_Pos (0)
#define | PWM_CLKPSC_CLKPSC01_Msk (0xfful << PWM_CLKPSC_CLKPSC01_Pos)
#define | PWM_CLKPSC_CLKPSC23_Pos (8)
#define | PWM_CLKPSC_CLKPSC23_Msk (0xfful << PWM_CLKPSC_CLKPSC23_Pos)
#define | PWM_CLKPSC_CLKPSC45_Pos (16)
#define | PWM_CLKPSC_CLKPSC45_Msk (0xfful << PWM_CLKPSC_CLKPSC45_Pos)
#define | PWM_CLKDIV_CLKDIV0_Pos (0)
#define | PWM_CLKDIV_CLKDIV0_Msk (0x7ul << PWM_CLKDIV_CLKDIV0_Pos)
#define | PWM_CLKDIV_CLKDIV1_Pos (4)
#define | PWM_CLKDIV_CLKDIV1_Msk (0x7ul << PWM_CLKDIV_CLKDIV1_Pos)
#define | PWM_CLKDIV_CLKDIV2_Pos (8)
#define | PWM_CLKDIV_CLKDIV2_Msk (0x7ul << PWM_CLKDIV_CLKDIV2_Pos)
#define | PWM_CLKDIV_CLKDIV3_Pos (12)
#define | PWM_CLKDIV_CLKDIV3_Msk (0x7ul << PWM_CLKDIV_CLKDIV3_Pos)
#define | PWM_CLKDIV_CLKDIV4_Pos (16)
#define | PWM_CLKDIV_CLKDIV4_Msk (0x7ul << PWM_CLKDIV_CLKDIV4_Pos)
#define | PWM_CLKDIV_CLKDIV5_Pos (20)
#define | PWM_CLKDIV_CLKDIV5_Msk (0x7ul << PWM_CLKDIV_CLKDIV5_Pos)
#define | PWM_CTL_CNTEN0_Pos (0)
#define | PWM_CTL_CNTEN0_Msk (0x1ul << PWM_CTL_CNTEN0_Pos)
#define | PWM_CTL_DBGTRIOFF_Pos (1)
#define | PWM_CTL_DBGTRIOFF_Msk (0x1ul << PWM_CTL_DBGTRIOFF_Pos)
#define | PWM_CTL_PINV0_Pos (2)
#define | PWM_CTL_PINV0_Msk (0x1ul << PWM_CTL_PINV0_Pos)
#define | PWM_CTL_CNTMODE0_Pos (3)
#define | PWM_CTL_CNTMODE0_Msk (0x1ul << PWM_CTL_CNTMODE0_Pos)
#define | PWM_CTL_CNTEN1_Pos (4)
#define | PWM_CTL_CNTEN1_Msk (0x1ul << PWM_CTL_CNTEN1_Pos)
#define | PWM_CTL_HCUPDT_Pos (5)
#define | PWM_CTL_HCUPDT_Msk (0x1ul << PWM_CTL_HCUPDT_Pos)
#define | PWM_CTL_PINV1_Pos (6)
#define | PWM_CTL_PINV1_Msk (0x1ul << PWM_CTL_PINV1_Pos)
#define | PWM_CTL_CNTMODE1_Pos (7)
#define | PWM_CTL_CNTMODE1_Msk (0x1ul << PWM_CTL_CNTMODE1_Pos)
#define | PWM_CTL_CNTEN2_Pos (8)
#define | PWM_CTL_CNTEN2_Msk (0x1ul << PWM_CTL_CNTEN2_Pos)
#define | PWM_CTL_PINV2_Pos (10)
#define | PWM_CTL_PINV2_Msk (0x1ul << PWM_CTL_PINV2_Pos)
#define | PWM_CTL_CNTMODE2_Pos (11)
#define | PWM_CTL_CNTMODE2_Msk (0x1ul << PWM_CTL_CNTMODE2_Pos)
#define | PWM_CTL_CNTEN3_Pos (12)
#define | PWM_CTL_CNTEN3_Msk (0x1ul << PWM_CTL_CNTEN3_Pos)
#define | PWM_CTL_PINV3_Pos (14)
#define | PWM_CTL_PINV3_Msk (0x1ul << PWM_CTL_PINV3_Pos)
#define | PWM_CTL_CNTMODE3_Pos (15)
#define | PWM_CTL_CNTMODE3_Msk (0x1ul << PWM_CTL_CNTMODE3_Pos)
#define | PWM_CTL_CNTEN4_Pos (16)
#define | PWM_CTL_CNTEN4_Msk (0x1ul << PWM_CTL_CNTEN4_Pos)
#define | PWM_CTL_PINV4_Pos (18)
#define | PWM_CTL_PINV4_Msk (0x1ul << PWM_CTL_PINV4_Pos)
#define | PWM_CTL_CNTMODE4_Pos (19)
#define | PWM_CTL_CNTMODE4_Msk (0x1ul << PWM_CTL_CNTMODE4_Pos)
#define | PWM_CTL_CNTEN5_Pos (20)
#define | PWM_CTL_CNTEN5_Msk (0x1ul << PWM_CTL_CNTEN5_Pos)
#define | PWM_CTL_ASYMEN_Pos (21)
#define | PWM_CTL_ASYMEN_Msk (0x1ul << PWM_CTL_ASYMEN_Pos)
#define | PWM_CTL_PINV5_Pos (22)
#define | PWM_CTL_PINV5_Msk (0x1ul << PWM_CTL_PINV5_Pos)
#define | PWM_CTL_CNTMODE5_Pos (23)
#define | PWM_CTL_CNTMODE5_Msk (0x1ul << PWM_CTL_CNTMODE5_Pos)
#define | PWM_CTL_DTCNT01_Pos (24)
#define | PWM_CTL_DTCNT01_Msk (0x1ul << PWM_CTL_DTCNT01_Pos)
#define | PWM_CTL_DTCNT23_Pos (25)
#define | PWM_CTL_DTCNT23_Msk (0x1ul << PWM_CTL_DTCNT23_Pos)
#define | PWM_CTL_DTCNT45_Pos (26)
#define | PWM_CTL_DTCNT45_Msk (0x1ul << PWM_CTL_DTCNT45_Pos)
#define | PWM_CTL_CNTCLR_Pos (27)
#define | PWM_CTL_CNTCLR_Msk (0x1ul << PWM_CTL_CNTCLR_Pos)
#define | PWM_CTL_MODE_Pos (28)
#define | PWM_CTL_MODE_Msk (0x3ul << PWM_CTL_MODE_Pos)
#define | PWM_CTL_GROUPEN_Pos (30)
#define | PWM_CTL_GROUPEN_Msk (0x1ul << PWM_CTL_GROUPEN_Pos)
#define | PWM_CTL_CNTTYPE_Pos (31)
#define | PWM_CTL_CNTTYPE_Msk (0x1ul << PWM_CTL_CNTTYPE_Pos)
#define | PWM_PERIOD0_PERIOD0_Pos (0)
#define | PWM_PERIOD0_PERIOD0_Msk (0xfffful << PWM_PERIOD0_PERIOD0_Pos)
#define | PWM_PERIOD0_PERIOD1_Pos (0)
#define | PWM_PERIOD0_PERIOD1_Msk (0xfffful << PWM_PERIOD0_PERIOD1_Pos)
#define | PWM_PERIOD0_PERIOD2_Pos (0)
#define | PWM_PERIOD0_PERIOD2_Msk (0xfffful << PWM_PERIOD0_PERIOD2_Pos)
#define | PWM_PERIOD0_PERIOD3_Pos (0)
#define | PWM_PERIOD0_PERIOD3_Msk (0xfffful << PWM_PERIOD0_PERIOD3_Pos)
#define | PWM_PERIOD0_PERIOD4_Pos (0)
#define | PWM_PERIOD0_PERIOD4_Msk (0xfffful << PWM_PERIOD0_PERIOD4_Pos)
#define | PWM_PERIOD0_PERIOD5_Pos (0)
#define | PWM_PERIOD0_PERIOD5_Msk (0xfffful << PWM_PERIOD0_PERIOD5_Pos)
#define | PWM_PERIOD1_PERIOD0_Pos (0)
#define | PWM_PERIOD1_PERIOD0_Msk (0xfffful << PWM_PERIOD1_PERIOD0_Pos)
#define | PWM_PERIOD1_PERIOD1_Pos (0)
#define | PWM_PERIOD1_PERIOD1_Msk (0xfffful << PWM_PERIOD1_PERIOD1_Pos)
#define | PWM_PERIOD1_PERIOD2_Pos (0)
#define | PWM_PERIOD1_PERIOD2_Msk (0xfffful << PWM_PERIOD1_PERIOD2_Pos)
#define | PWM_PERIOD1_PERIOD3_Pos (0)
#define | PWM_PERIOD1_PERIOD3_Msk (0xfffful << PWM_PERIOD1_PERIOD3_Pos)
#define | PWM_PERIOD1_PERIOD4_Pos (0)
#define | PWM_PERIOD1_PERIOD4_Msk (0xfffful << PWM_PERIOD1_PERIOD4_Pos)
#define | PWM_PERIOD1_PERIOD5_Pos (0)
#define | PWM_PERIOD1_PERIOD5_Msk (0xfffful << PWM_PERIOD1_PERIOD5_Pos)
#define | PWM_PERIOD2_PERIOD0_Pos (0)
#define | PWM_PERIOD2_PERIOD0_Msk (0xfffful << PWM_PERIOD2_PERIOD0_Pos)
#define | PWM_PERIOD2_PERIOD1_Pos (0)
#define | PWM_PERIOD2_PERIOD1_Msk (0xfffful << PWM_PERIOD2_PERIOD1_Pos)
#define | PWM_PERIOD2_PERIOD2_Pos (0)
#define | PWM_PERIOD2_PERIOD2_Msk (0xfffful << PWM_PERIOD2_PERIOD2_Pos)
#define | PWM_PERIOD2_PERIOD3_Pos (0)
#define | PWM_PERIOD2_PERIOD3_Msk (0xfffful << PWM_PERIOD2_PERIOD3_Pos)
#define | PWM_PERIOD2_PERIOD4_Pos (0)
#define | PWM_PERIOD2_PERIOD4_Msk (0xfffful << PWM_PERIOD2_PERIOD4_Pos)
#define | PWM_PERIOD2_PERIOD5_Pos (0)
#define | PWM_PERIOD2_PERIOD5_Msk (0xfffful << PWM_PERIOD2_PERIOD5_Pos)
#define | PWM_PERIOD3_PERIOD0_Pos (0)
#define | PWM_PERIOD3_PERIOD0_Msk (0xfffful << PWM_PERIOD3_PERIOD0_Pos)
#define | PWM_PERIOD3_PERIOD1_Pos (0)
#define | PWM_PERIOD3_PERIOD1_Msk (0xfffful << PWM_PERIOD3_PERIOD1_Pos)
#define | PWM_PERIOD3_PERIOD2_Pos (0)
#define | PWM_PERIOD3_PERIOD2_Msk (0xfffful << PWM_PERIOD3_PERIOD2_Pos)
#define | PWM_PERIOD3_PERIOD3_Pos (0)
#define | PWM_PERIOD3_PERIOD3_Msk (0xfffful << PWM_PERIOD3_PERIOD3_Pos)
#define | PWM_PERIOD3_PERIOD4_Pos (0)
#define | PWM_PERIOD3_PERIOD4_Msk (0xfffful << PWM_PERIOD3_PERIOD4_Pos)
#define | PWM_PERIOD3_PERIOD5_Pos (0)
#define | PWM_PERIOD3_PERIOD5_Msk (0xfffful << PWM_PERIOD3_PERIOD5_Pos)
#define | PWM_PERIOD4_PERIOD0_Pos (0)
#define | PWM_PERIOD4_PERIOD0_Msk (0xfffful << PWM_PERIOD4_PERIOD0_Pos)
#define | PWM_PERIOD4_PERIOD1_Pos (0)
#define | PWM_PERIOD4_PERIOD1_Msk (0xfffful << PWM_PERIOD4_PERIOD1_Pos)
#define | PWM_PERIOD4_PERIOD2_Pos (0)
#define | PWM_PERIOD4_PERIOD2_Msk (0xfffful << PWM_PERIOD4_PERIOD2_Pos)
#define | PWM_PERIOD4_PERIOD3_Pos (0)
#define | PWM_PERIOD4_PERIOD3_Msk (0xfffful << PWM_PERIOD4_PERIOD3_Pos)
#define | PWM_PERIOD4_PERIOD4_Pos (0)
#define | PWM_PERIOD4_PERIOD4_Msk (0xfffful << PWM_PERIOD4_PERIOD4_Pos)
#define | PWM_PERIOD4_PERIOD5_Pos (0)
#define | PWM_PERIOD4_PERIOD5_Msk (0xfffful << PWM_PERIOD4_PERIOD5_Pos)
#define | PWM_PERIOD5_PERIOD0_Pos (0)
#define | PWM_PERIOD5_PERIOD0_Msk (0xfffful << PWM_PERIOD5_PERIOD0_Pos)
#define | PWM_PERIOD5_PERIOD1_Pos (0)
#define | PWM_PERIOD5_PERIOD1_Msk (0xfffful << PWM_PERIOD5_PERIOD1_Pos)
#define | PWM_PERIOD5_PERIOD2_Pos (0)
#define | PWM_PERIOD5_PERIOD2_Msk (0xfffful << PWM_PERIOD5_PERIOD2_Pos)
#define | PWM_PERIOD5_PERIOD3_Pos (0)
#define | PWM_PERIOD5_PERIOD3_Msk (0xfffful << PWM_PERIOD5_PERIOD3_Pos)
#define | PWM_PERIOD5_PERIOD4_Pos (0)
#define | PWM_PERIOD5_PERIOD4_Msk (0xfffful << PWM_PERIOD5_PERIOD4_Pos)
#define | PWM_PERIOD5_PERIOD5_Pos (0)
#define | PWM_PERIOD5_PERIOD5_Msk (0xfffful << PWM_PERIOD5_PERIOD5_Pos)
#define | PWM_CMPDAT0_CMP0_Pos (0)
#define | PWM_CMPDAT0_CMP0_Msk (0xfffful << PWM_CMPDAT0_CMP0_Pos)
#define | PWM_CMPDAT0_CMP1_Pos (0)
#define | PWM_CMPDAT0_CMP1_Msk (0xfffful << PWM_CMPDAT0_CMP1_Pos)
#define | PWM_CMPDAT0_CMP2_Pos (0)
#define | PWM_CMPDAT0_CMP2_Msk (0xfffful << PWM_CMPDAT0_CMP2_Pos)
#define | PWM_CMPDAT0_CMP3_Pos (0)
#define | PWM_CMPDAT0_CMP3_Msk (0xfffful << PWM_CMPDAT0_CMP3_Pos)
#define | PWM_CMPDAT0_CMP4_Pos (0)
#define | PWM_CMPDAT0_CMP4_Msk (0xfffful << PWM_CMPDAT0_CMP4_Pos)
#define | PWM_CMPDAT0_CMP5_Pos (0)
#define | PWM_CMPDAT0_CMP5_Msk (0xfffful << PWM_CMPDAT0_CMP5_Pos)
#define | PWM_CMPDAT0_CMPD0_Pos (16)
#define | PWM_CMPDAT0_CMPD0_Msk (0xfffful << PWM_CMPDAT0_CMPD0_Pos)
#define | PWM_CMPDAT0_CMPD1_Pos (16)
#define | PWM_CMPDAT0_CMPD1_Msk (0xfffful << PWM_CMPDAT0_CMPD1_Pos)
#define | PWM_CMPDAT0_CMPD2_Pos (16)
#define | PWM_CMPDAT0_CMPD2_Msk (0xfffful << PWM_CMPDAT0_CMPD2_Pos)
#define | PWM_CMPDAT0_CMPD3_Pos (16)
#define | PWM_CMPDAT0_CMPD3_Msk (0xfffful << PWM_CMPDAT0_CMPD3_Pos)
#define | PWM_CMPDAT0_CMPD4_Pos (16)
#define | PWM_CMPDAT0_CMPD4_Msk (0xfffful << PWM_CMPDAT0_CMPD4_Pos)
#define | PWM_CMPDAT0_CMPD5_Pos (16)
#define | PWM_CMPDAT0_CMPD5_Msk (0xfffful << PWM_CMPDAT0_CMPD5_Pos)
#define | PWM_CMPDAT1_CMP0_Pos (0)
#define | PWM_CMPDAT1_CMP0_Msk (0xfffful << PWM_CMPDAT1_CMP0_Pos)
#define | PWM_CMPDAT1_CMP1_Pos (0)
#define | PWM_CMPDAT1_CMP1_Msk (0xfffful << PWM_CMPDAT1_CMP1_Pos)
#define | PWM_CMPDAT1_CMP2_Pos (0)
#define | PWM_CMPDAT1_CMP2_Msk (0xfffful << PWM_CMPDAT1_CMP2_Pos)
#define | PWM_CMPDAT1_CMP3_Pos (0)
#define | PWM_CMPDAT1_CMP3_Msk (0xfffful << PWM_CMPDAT1_CMP3_Pos)
#define | PWM_CMPDAT1_CMP4_Pos (0)
#define | PWM_CMPDAT1_CMP4_Msk (0xfffful << PWM_CMPDAT1_CMP4_Pos)
#define | PWM_CMPDAT1_CMP5_Pos (0)
#define | PWM_CMPDAT1_CMP5_Msk (0xfffful << PWM_CMPDAT1_CMP5_Pos)
#define | PWM_CMPDAT1_CMPD0_Pos (16)
#define | PWM_CMPDAT1_CMPD0_Msk (0xfffful << PWM_CMPDAT1_CMPD0_Pos)
#define | PWM_CMPDAT1_CMPD1_Pos (16)
#define | PWM_CMPDAT1_CMPD1_Msk (0xfffful << PWM_CMPDAT1_CMPD1_Pos)
#define | PWM_CMPDAT1_CMPD2_Pos (16)
#define | PWM_CMPDAT1_CMPD2_Msk (0xfffful << PWM_CMPDAT1_CMPD2_Pos)
#define | PWM_CMPDAT1_CMPD3_Pos (16)
#define | PWM_CMPDAT1_CMPD3_Msk (0xfffful << PWM_CMPDAT1_CMPD3_Pos)
#define | PWM_CMPDAT1_CMPD4_Pos (16)
#define | PWM_CMPDAT1_CMPD4_Msk (0xfffful << PWM_CMPDAT1_CMPD4_Pos)
#define | PWM_CMPDAT1_CMPD5_Pos (16)
#define | PWM_CMPDAT1_CMPD5_Msk (0xfffful << PWM_CMPDAT1_CMPD5_Pos)
#define | PWM_CMPDAT2_CMP0_Pos (0)
#define | PWM_CMPDAT2_CMP0_Msk (0xfffful << PWM_CMPDAT2_CMP0_Pos)
#define | PWM_CMPDAT2_CMP1_Pos (0)
#define | PWM_CMPDAT2_CMP1_Msk (0xfffful << PWM_CMPDAT2_CMP1_Pos)
#define | PWM_CMPDAT2_CMP2_Pos (0)
#define | PWM_CMPDAT2_CMP2_Msk (0xfffful << PWM_CMPDAT2_CMP2_Pos)
#define | PWM_CMPDAT2_CMP3_Pos (0)
#define | PWM_CMPDAT2_CMP3_Msk (0xfffful << PWM_CMPDAT2_CMP3_Pos)
#define | PWM_CMPDAT2_CMP4_Pos (0)
#define | PWM_CMPDAT2_CMP4_Msk (0xfffful << PWM_CMPDAT2_CMP4_Pos)
#define | PWM_CMPDAT2_CMP5_Pos (0)
#define | PWM_CMPDAT2_CMP5_Msk (0xfffful << PWM_CMPDAT2_CMP5_Pos)
#define | PWM_CMPDAT2_CMPD0_Pos (16)
#define | PWM_CMPDAT2_CMPD0_Msk (0xfffful << PWM_CMPDAT2_CMPD0_Pos)
#define | PWM_CMPDAT2_CMPD1_Pos (16)
#define | PWM_CMPDAT2_CMPD1_Msk (0xfffful << PWM_CMPDAT2_CMPD1_Pos)
#define | PWM_CMPDAT2_CMPD2_Pos (16)
#define | PWM_CMPDAT2_CMPD2_Msk (0xfffful << PWM_CMPDAT2_CMPD2_Pos)
#define | PWM_CMPDAT2_CMPD3_Pos (16)
#define | PWM_CMPDAT2_CMPD3_Msk (0xfffful << PWM_CMPDAT2_CMPD3_Pos)
#define | PWM_CMPDAT2_CMPD4_Pos (16)
#define | PWM_CMPDAT2_CMPD4_Msk (0xfffful << PWM_CMPDAT2_CMPD4_Pos)
#define | PWM_CMPDAT2_CMPD5_Pos (16)
#define | PWM_CMPDAT2_CMPD5_Msk (0xfffful << PWM_CMPDAT2_CMPD5_Pos)
#define | PWM_CMPDAT3_CMP0_Pos (0)
#define | PWM_CMPDAT3_CMP0_Msk (0xfffful << PWM_CMPDAT3_CMP0_Pos)
#define | PWM_CMPDAT3_CMP1_Pos (0)
#define | PWM_CMPDAT3_CMP1_Msk (0xfffful << PWM_CMPDAT3_CMP1_Pos)
#define | PWM_CMPDAT3_CMP2_Pos (0)
#define | PWM_CMPDAT3_CMP2_Msk (0xfffful << PWM_CMPDAT3_CMP2_Pos)
#define | PWM_CMPDAT3_CMP3_Pos (0)
#define | PWM_CMPDAT3_CMP3_Msk (0xfffful << PWM_CMPDAT3_CMP3_Pos)
#define | PWM_CMPDAT3_CMP4_Pos (0)
#define | PWM_CMPDAT3_CMP4_Msk (0xfffful << PWM_CMPDAT3_CMP4_Pos)
#define | PWM_CMPDAT3_CMP5_Pos (0)
#define | PWM_CMPDAT3_CMP5_Msk (0xfffful << PWM_CMPDAT3_CMP5_Pos)
#define | PWM_CMPDAT3_CMPD0_Pos (16)
#define | PWM_CMPDAT3_CMPD0_Msk (0xfffful << PWM_CMPDAT3_CMPD0_Pos)
#define | PWM_CMPDAT3_CMPD1_Pos (16)
#define | PWM_CMPDAT3_CMPD1_Msk (0xfffful << PWM_CMPDAT3_CMPD1_Pos)
#define | PWM_CMPDAT3_CMPD2_Pos (16)
#define | PWM_CMPDAT3_CMPD2_Msk (0xfffful << PWM_CMPDAT3_CMPD2_Pos)
#define | PWM_CMPDAT3_CMPD3_Pos (16)
#define | PWM_CMPDAT3_CMPD3_Msk (0xfffful << PWM_CMPDAT3_CMPD3_Pos)
#define | PWM_CMPDAT3_CMPD4_Pos (16)
#define | PWM_CMPDAT3_CMPD4_Msk (0xfffful << PWM_CMPDAT3_CMPD4_Pos)
#define | PWM_CMPDAT3_CMPD5_Pos (16)
#define | PWM_CMPDAT3_CMPD5_Msk (0xfffful << PWM_CMPDAT3_CMPD5_Pos)
#define | PWM_CMPDAT4_CMP0_Pos (0)
#define | PWM_CMPDAT4_CMP0_Msk (0xfffful << PWM_CMPDAT4_CMP0_Pos)
#define | PWM_CMPDAT4_CMP1_Pos (0)
#define | PWM_CMPDAT4_CMP1_Msk (0xfffful << PWM_CMPDAT4_CMP1_Pos)
#define | PWM_CMPDAT4_CMP2_Pos (0)
#define | PWM_CMPDAT4_CMP2_Msk (0xfffful << PWM_CMPDAT4_CMP2_Pos)
#define | PWM_CMPDAT4_CMP3_Pos (0)
#define | PWM_CMPDAT4_CMP3_Msk (0xfffful << PWM_CMPDAT4_CMP3_Pos)
#define | PWM_CMPDAT4_CMP4_Pos (0)
#define | PWM_CMPDAT4_CMP4_Msk (0xfffful << PWM_CMPDAT4_CMP4_Pos)
#define | PWM_CMPDAT4_CMP5_Pos (0)
#define | PWM_CMPDAT4_CMP5_Msk (0xfffful << PWM_CMPDAT4_CMP5_Pos)
#define | PWM_CMPDAT4_CMPD0_Pos (16)
#define | PWM_CMPDAT4_CMPD0_Msk (0xfffful << PWM_CMPDAT4_CMPD0_Pos)
#define | PWM_CMPDAT4_CMPD1_Pos (16)
#define | PWM_CMPDAT4_CMPD1_Msk (0xfffful << PWM_CMPDAT4_CMPD1_Pos)
#define | PWM_CMPDAT4_CMPD2_Pos (16)
#define | PWM_CMPDAT4_CMPD2_Msk (0xfffful << PWM_CMPDAT4_CMPD2_Pos)
#define | PWM_CMPDAT4_CMPD3_Pos (16)
#define | PWM_CMPDAT4_CMPD3_Msk (0xfffful << PWM_CMPDAT4_CMPD3_Pos)
#define | PWM_CMPDAT4_CMPD4_Pos (16)
#define | PWM_CMPDAT4_CMPD4_Msk (0xfffful << PWM_CMPDAT4_CMPD4_Pos)
#define | PWM_CMPDAT4_CMPD5_Pos (16)
#define | PWM_CMPDAT4_CMPD5_Msk (0xfffful << PWM_CMPDAT4_CMPD5_Pos)
#define | PWM_CMPDAT5_CMP0_Pos (0)
#define | PWM_CMPDAT5_CMP0_Msk (0xfffful << PWM_CMPDAT5_CMP0_Pos)
#define | PWM_CMPDAT5_CMP1_Pos (0)
#define | PWM_CMPDAT5_CMP1_Msk (0xfffful << PWM_CMPDAT5_CMP1_Pos)
#define | PWM_CMPDAT5_CMP2_Pos (0)
#define | PWM_CMPDAT5_CMP2_Msk (0xfffful << PWM_CMPDAT5_CMP2_Pos)
#define | PWM_CMPDAT5_CMP3_Pos (0)
#define | PWM_CMPDAT5_CMP3_Msk (0xfffful << PWM_CMPDAT5_CMP3_Pos)
#define | PWM_CMPDAT5_CMP4_Pos (0)
#define | PWM_CMPDAT5_CMP4_Msk (0xfffful << PWM_CMPDAT5_CMP4_Pos)
#define | PWM_CMPDAT5_CMP5_Pos (0)
#define | PWM_CMPDAT5_CMP5_Msk (0xfffful << PWM_CMPDAT5_CMP5_Pos)
#define | PWM_CMPDAT5_CMPD0_Pos (16)
#define | PWM_CMPDAT5_CMPD0_Msk (0xfffful << PWM_CMPDAT5_CMPD0_Pos)
#define | PWM_CMPDAT5_CMPD1_Pos (16)
#define | PWM_CMPDAT5_CMPD1_Msk (0xfffful << PWM_CMPDAT5_CMPD1_Pos)
#define | PWM_CMPDAT5_CMPD2_Pos (16)
#define | PWM_CMPDAT5_CMPD2_Msk (0xfffful << PWM_CMPDAT5_CMPD2_Pos)
#define | PWM_CMPDAT5_CMPD3_Pos (16)
#define | PWM_CMPDAT5_CMPD3_Msk (0xfffful << PWM_CMPDAT5_CMPD3_Pos)
#define | PWM_CMPDAT5_CMPD4_Pos (16)
#define | PWM_CMPDAT5_CMPD4_Msk (0xfffful << PWM_CMPDAT5_CMPD4_Pos)
#define | PWM_CMPDAT5_CMPD5_Pos (16)
#define | PWM_CMPDAT5_CMPD5_Msk (0xfffful << PWM_CMPDAT5_CMPD5_Pos)
#define | PWM_INTEN_ZIEN0_Pos (0)
#define | PWM_INTEN_ZIEN0_Msk (0x1ul << PWM_INTEN_ZIEN0_Pos)
#define | PWM_INTEN_ZIEN1_Pos (1)
#define | PWM_INTEN_ZIEN1_Msk (0x1ul << PWM_INTEN_ZIEN1_Pos)
#define | PWM_INTEN_ZIEN2_Pos (2)
#define | PWM_INTEN_ZIEN2_Msk (0x1ul << PWM_INTEN_ZIEN2_Pos)
#define | PWM_INTEN_ZIEN3_Pos (3)
#define | PWM_INTEN_ZIEN3_Msk (0x1ul << PWM_INTEN_ZIEN3_Pos)
#define | PWM_INTEN_ZIEN4_Pos (4)
#define | PWM_INTEN_ZIEN4_Msk (0x1ul << PWM_INTEN_ZIEN4_Pos)
#define | PWM_INTEN_ZIEN5_Pos (5)
#define | PWM_INTEN_ZIEN5_Msk (0x1ul << PWM_INTEN_ZIEN5_Pos)
#define | PWM_INTEN_CMPDIEN0_Pos (8)
#define | PWM_INTEN_CMPDIEN0_Msk (0x1ul << PWM_INTEN_CMPDIEN0_Pos)
#define | PWM_INTEN_CMPDIEN1_Pos (9)
#define | PWM_INTEN_CMPDIEN1_Msk (0x1ul << PWM_INTEN_CMPDIEN1_Pos)
#define | PWM_INTEN_CMPDIEN2_Pos (10)
#define | PWM_INTEN_CMPDIEN2_Msk (0x1ul << PWM_INTEN_CMPDIEN2_Pos)
#define | PWM_INTEN_CMPDIEN3_Pos (11)
#define | PWM_INTEN_CMPDIEN3_Msk (0x1ul << PWM_INTEN_CMPDIEN3_Pos)
#define | PWM_INTEN_CMPDIEN4_Pos (12)
#define | PWM_INTEN_CMPDIEN4_Msk (0x1ul << PWM_INTEN_CMPDIEN4_Pos)
#define | PWM_INTEN_CMPDIEN5_Pos (13)
#define | PWM_INTEN_CMPDIEN5_Msk (0x1ul << PWM_INTEN_CMPDIEN5_Pos)
#define | PWM_INTEN_BRKIEN_Pos (16)
#define | PWM_INTEN_BRKIEN_Msk (0x1ul << PWM_INTEN_BRKIEN_Pos)
#define | PWM_INTEN_PINTTYPE_Pos (17)
#define | PWM_INTEN_PINTTYPE_Msk (0x1ul << PWM_INTEN_PINTTYPE_Pos)
#define | PWM_INTEN_PIEN0_Pos (18)
#define | PWM_INTEN_PIEN0_Msk (0x1ul << PWM_INTEN_PIEN0_Pos)
#define | PWM_INTEN_PIEN1_Pos (19)
#define | PWM_INTEN_PIEN1_Msk (0x1ul << PWM_INTEN_PIEN1_Pos)
#define | PWM_INTEN_PIEN2_Pos (20)
#define | PWM_INTEN_PIEN2_Msk (0x1ul << PWM_INTEN_PIEN2_Pos)
#define | PWM_INTEN_PIEN3_Pos (21)
#define | PWM_INTEN_PIEN3_Msk (0x1ul << PWM_INTEN_PIEN3_Pos)
#define | PWM_INTEN_PIEN4_Pos (22)
#define | PWM_INTEN_PIEN4_Msk (0x1ul << PWM_INTEN_PIEN4_Pos)
#define | PWM_INTEN_PIEN5_Pos (23)
#define | PWM_INTEN_PIEN5_Msk (0x1ul << PWM_INTEN_PIEN5_Pos)
#define | PWM_INTEN_CMPUIEN0_Pos (24)
#define | PWM_INTEN_CMPUIEN0_Msk (0x1ul << PWM_INTEN_CMPUIEN0_Pos)
#define | PWM_INTEN_CMPUIEN1_Pos (25)
#define | PWM_INTEN_CMPUIEN1_Msk (0x1ul << PWM_INTEN_CMPUIEN1_Pos)
#define | PWM_INTEN_CMPUIEN2_Pos (26)
#define | PWM_INTEN_CMPUIEN2_Msk (0x1ul << PWM_INTEN_CMPUIEN2_Pos)
#define | PWM_INTEN_CMPUIEN3_Pos (27)
#define | PWM_INTEN_CMPUIEN3_Msk (0x1ul << PWM_INTEN_CMPUIEN3_Pos)
#define | PWM_INTEN_CMPUIEN4_Pos (28)
#define | PWM_INTEN_CMPUIEN4_Msk (0x1ul << PWM_INTEN_CMPUIEN4_Pos)
#define | PWM_INTEN_CMPUIEN5_Pos (29)
#define | PWM_INTEN_CMPUIEN5_Msk (0x1ul << PWM_INTEN_CMPUIEN5_Pos)
#define | PWM_INTSTS_ZIF0_Pos (0)
#define | PWM_INTSTS_ZIF0_Msk (0x1ul << PWM_INTSTS_ZIF0_Pos)
#define | PWM_INTSTS_ZIF1_Pos (1)
#define | PWM_INTSTS_ZIF1_Msk (0x1ul << PWM_INTSTS_ZIF1_Pos)
#define | PWM_INTSTS_ZIF2_Pos (2)
#define | PWM_INTSTS_ZIF2_Msk (0x1ul << PWM_INTSTS_ZIF2_Pos)
#define | PWM_INTSTS_ZIF3_Pos (3)
#define | PWM_INTSTS_ZIF3_Msk (0x1ul << PWM_INTSTS_ZIF3_Pos)
#define | PWM_INTSTS_ZIF4_Pos (4)
#define | PWM_INTSTS_ZIF4_Msk (0x1ul << PWM_INTSTS_ZIF4_Pos)
#define | PWM_INTSTS_ZIF5_Pos (5)
#define | PWM_INTSTS_ZIF5_Msk (0x1ul << PWM_INTSTS_ZIF5_Pos)
#define | PWM_INTSTS_CMPDIF0_Pos (8)
#define | PWM_INTSTS_CMPDIF0_Msk (0x1ul << PWM_INTSTS_CMPDIF0_Pos)
#define | PWM_INTSTS_CMPDIF1_Pos (9)
#define | PWM_INTSTS_CMPDIF1_Msk (0x1ul << PWM_INTSTS_CMPDIF1_Pos)
#define | PWM_INTSTS_CMPDIF2_Pos (10)
#define | PWM_INTSTS_CMPDIF2_Msk (0x1ul << PWM_INTSTS_CMPDIF2_Pos)
#define | PWM_INTSTS_CMPDIF3_Pos (11)
#define | PWM_INTSTS_CMPDIF3_Msk (0x1ul << PWM_INTSTS_CMPDIF3_Pos)
#define | PWM_INTSTS_CMPDIF4_Pos (12)
#define | PWM_INTSTS_CMPDIF4_Msk (0x1ul << PWM_INTSTS_CMPDIF4_Pos)
#define | PWM_INTSTS_CMPDIF5_Pos (13)
#define | PWM_INTSTS_CMPDIF5_Msk (0x1ul << PWM_INTSTS_CMPDIF5_Pos)
#define | PWM_INTSTS_BRKIF0_Pos (16)
#define | PWM_INTSTS_BRKIF0_Msk (0x1ul << PWM_INTSTS_BRKIF0_Pos)
#define | PWM_INTSTS_BRKIF1_Pos (17)
#define | PWM_INTSTS_BRKIF1_Msk (0x1ul << PWM_INTSTS_BRKIF1_Pos)
#define | PWM_INTSTS_PIF0_Pos (18)
#define | PWM_INTSTS_PIF0_Msk (0x1ul << PWM_INTSTS_PIF0_Pos)
#define | PWM_INTSTS_PIF1_Pos (19)
#define | PWM_INTSTS_PIF1_Msk (0x1ul << PWM_INTSTS_PIF1_Pos)
#define | PWM_INTSTS_PIF2_Pos (20)
#define | PWM_INTSTS_PIF2_Msk (0x1ul << PWM_INTSTS_PIF2_Pos)
#define | PWM_INTSTS_PIF3_Pos (21)
#define | PWM_INTSTS_PIF3_Msk (0x1ul << PWM_INTSTS_PIF3_Pos)
#define | PWM_INTSTS_PIF4_Pos (22)
#define | PWM_INTSTS_PIF4_Msk (0x1ul << PWM_INTSTS_PIF4_Pos)
#define | PWM_INTSTS_PIF5_Pos (23)
#define | PWM_INTSTS_PIF5_Msk (0x1ul << PWM_INTSTS_PIF5_Pos)
#define | PWM_INTSTS_CMPUIF0_Pos (24)
#define | PWM_INTSTS_CMPUIF0_Msk (0x1ul << PWM_INTSTS_CMPUIF0_Pos)
#define | PWM_INTSTS_CMPUIF1_Pos (25)
#define | PWM_INTSTS_CMPUIF1_Msk (0x1ul << PWM_INTSTS_CMPUIF1_Pos)
#define | PWM_INTSTS_CMPUIF2_Pos (26)
#define | PWM_INTSTS_CMPUIF2_Msk (0x1ul << PWM_INTSTS_CMPUIF2_Pos)
#define | PWM_INTSTS_CMPUIF3_Pos (27)
#define | PWM_INTSTS_CMPUIF3_Msk (0x1ul << PWM_INTSTS_CMPUIF3_Pos)
#define | PWM_INTSTS_CMPUIF4_Pos (28)
#define | PWM_INTSTS_CMPUIF4_Msk (0x1ul << PWM_INTSTS_CMPUIF4_Pos)
#define | PWM_INTSTS_CMPUIF5_Pos (29)
#define | PWM_INTSTS_CMPUIF5_Msk (0x1ul << PWM_INTSTS_CMPUIF5_Pos)
#define | PWM_POEN_POEN0_Pos (0)
#define | PWM_POEN_POEN0_Msk (0x1ul << PWM_POEN_POEN0_Pos)
#define | PWM_POEN_POEN1_Pos (1)
#define | PWM_POEN_POEN1_Msk (0x1ul << PWM_POEN_POEN1_Pos)
#define | PWM_POEN_POEN2_Pos (2)
#define | PWM_POEN_POEN2_Msk (0x1ul << PWM_POEN_POEN2_Pos)
#define | PWM_POEN_POEN3_Pos (3)
#define | PWM_POEN_POEN3_Msk (0x1ul << PWM_POEN_POEN3_Pos)
#define | PWM_POEN_POEN4_Pos (4)
#define | PWM_POEN_POEN4_Msk (0x1ul << PWM_POEN_POEN4_Pos)
#define | PWM_POEN_POEN5_Pos (5)
#define | PWM_POEN_POEN5_Msk (0x1ul << PWM_POEN_POEN5_Pos)
#define | PWM_BRKCTL_BRK0EN_Pos (0)
#define | PWM_BRKCTL_BRK0EN_Msk (0x1ul << PWM_BRKCTL_BRK0EN_Pos)
#define | PWM_BRKCTL_BRK1EN_Pos (1)
#define | PWM_BRKCTL_BRK1EN_Msk (0x1ul << PWM_BRKCTL_BRK1EN_Pos)
#define | PWM_BRKCTL_BRK0SEL_Pos (2)
#define | PWM_BRKCTL_BRK0SEL_Msk (0x1ul << PWM_BRKCTL_BRK0SEL_Pos)
#define | PWM_BRKCTL_BRK1SEL_Pos (3)
#define | PWM_BRKCTL_BRK1SEL_Msk (0x1ul << PWM_BRKCTL_BRK1SEL_Pos)
#define | PWM_BRKCTL_BRKSTS_Pos (7)
#define | PWM_BRKCTL_BRKSTS_Msk (0x1ul << PWM_BRKCTL_BRKSTS_Pos)
#define | PWM_BRKCTL_BRKACT_Pos (8)
#define | PWM_BRKCTL_BRKACT_Msk (0x1ul << PWM_BRKCTL_BRKACT_Pos)
#define | PWM_BRKCTL_SWBRK_Pos (9)
#define | PWM_BRKCTL_SWBRK_Msk (0x1ul << PWM_BRKCTL_SWBRK_Pos)
#define | PWM_BRKCTL_BKOD0_Pos (24)
#define | PWM_BRKCTL_BKOD0_Msk (0x1ul << PWM_BRKCTL_BKOD0_Pos)
#define | PWM_BRKCTL_BKOD1_Pos (25)
#define | PWM_BRKCTL_BKOD1_Msk (0x1ul << PWM_BRKCTL_BKOD1_Pos)
#define | PWM_BRKCTL_BKOD2_Pos (26)
#define | PWM_BRKCTL_BKOD2_Msk (0x1ul << PWM_BRKCTL_BKOD2_Pos)
#define | PWM_BRKCTL_BKOD3_Pos (27)
#define | PWM_BRKCTL_BKOD3_Msk (0x1ul << PWM_BRKCTL_BKOD3_Pos)
#define | PWM_BRKCTL_BKOD4_Pos (28)
#define | PWM_BRKCTL_BKOD4_Msk (0x1ul << PWM_BRKCTL_BKOD4_Pos)
#define | PWM_BRKCTL_BKOD5_Pos (29)
#define | PWM_BRKCTL_BKOD5_Msk (0x1ul << PWM_BRKCTL_BKOD5_Pos)
#define | PWM_BRKCTL_D6BKOD_Pos (30)
#define | PWM_BRKCTL_D6BKOD_Msk (0x1ul << PWM_BRKCTL_D6BKOD_Pos)
#define | PWM_BRKCTL_D7BKOD_Pos (31)
#define | PWM_BRKCTL_D7BKOD_Msk (0x1ul << PWM_BRKCTL_D7BKOD_Pos)
#define | PWM_DTCTL_DTI01_Pos (0)
#define | PWM_DTCTL_DTI01_Msk (0xfful << PWM_DTCTL_DTI01_Pos)
#define | PWM_DTCTL_DTI23_Pos (8)
#define | PWM_DTCTL_DTI23_Msk (0xfful << PWM_DTCTL_DTI23_Pos)
#define | PWM_DTCTL_DTI45_Pos (16)
#define | PWM_DTCTL_DTI45_Msk (0xfful << PWM_DTCTL_DTI45_Pos)
#define | PWM_ADCTCTL0_CUTRGEN0_Pos (0)
#define | PWM_ADCTCTL0_CUTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN0_Pos)
#define | PWM_ADCTCTL0_CPTRGEN0_Pos (1)
#define | PWM_ADCTCTL0_CPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN0_Pos)
#define | PWM_ADCTCTL0_CDTRGEN0_Pos (2)
#define | PWM_ADCTCTL0_CDTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN0_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN0_Pos (3)
#define | PWM_ADCTCTL0_ZPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN0_Pos)
#define | PWM_ADCTCTL0_CUTRGEN1_Pos (8)
#define | PWM_ADCTCTL0_CUTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN1_Pos)
#define | PWM_ADCTCTL0_CPTRGEN1_Pos (9)
#define | PWM_ADCTCTL0_CPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN1_Pos)
#define | PWM_ADCTCTL0_CDTRGEN1_Pos (10)
#define | PWM_ADCTCTL0_CDTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN1_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN1_Pos (11)
#define | PWM_ADCTCTL0_ZPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN1_Pos)
#define | PWM_ADCTCTL0_CUTRGEN2_Pos (16)
#define | PWM_ADCTCTL0_CUTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN2_Pos)
#define | PWM_ADCTCTL0_CPTRGEN2_Pos (17)
#define | PWM_ADCTCTL0_CPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN2_Pos)
#define | PWM_ADCTCTL0_CDTRGEN2_Pos (18)
#define | PWM_ADCTCTL0_CDTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN2_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN2_Pos (19)
#define | PWM_ADCTCTL0_ZPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN2_Pos)
#define | PWM_ADCTCTL0_CUTRGEN3_Pos (24)
#define | PWM_ADCTCTL0_CUTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN3_Pos)
#define | PWM_ADCTCTL0_CPTRGEN3_Pos (25)
#define | PWM_ADCTCTL0_CPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN3_Pos)
#define | PWM_ADCTCTL0_CDTRGEN3_Pos (26)
#define | PWM_ADCTCTL0_CDTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN3_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN3_Pos (27)
#define | PWM_ADCTCTL0_ZPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN3_Pos)
#define | PWM_ADCTCTL1_CUTRGEN4_Pos (0)
#define | PWM_ADCTCTL1_CUTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN4_Pos)
#define | PWM_ADCTCTL1_CPTRGEN4_Pos (1)
#define | PWM_ADCTCTL1_CPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN4_Pos)
#define | PWM_ADCTCTL1_CDTRGEN4_Pos (2)
#define | PWM_ADCTCTL1_CDTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN4_Pos)
#define | PWM_ADCTCTL1_ZPTRGEN4_Pos (3)
#define | PWM_ADCTCTL1_ZPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN4_Pos)
#define | PWM_ADCTCTL1_CUTRGEN5_Pos (8)
#define | PWM_ADCTCTL1_CUTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN5_Pos)
#define | PWM_ADCTCTL1_CPTRGEN5_Pos (9)
#define | PWM_ADCTCTL1_CPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN5_Pos)
#define | PWM_ADCTCTL1_CDTRGEN5_Pos (10)
#define | PWM_ADCTCTL1_CDTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN5_Pos)
#define | PWM_ADCTCTL1_ZPTRGEN5_Pos (11)
#define | PWM_ADCTCTL1_ZPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN5_Pos)
#define | PWM_ADCTSTS0_CUTRGF0_Pos (0)
#define | PWM_ADCTSTS0_CUTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF0_Pos)
#define | PWM_ADCTSTS0_CPTRGF0_Pos (1)
#define | PWM_ADCTSTS0_CPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF0_Pos)
#define | PWM_ADCTSTS0_CDTRGF0_Pos (2)
#define | PWM_ADCTSTS0_CDTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF0_Pos)
#define | PWM_ADCTSTS0_ZPTRGF0_Pos (3)
#define | PWM_ADCTSTS0_ZPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF0_Pos)
#define | PWM_ADCTSTS0_CUTRGF1_Pos (8)
#define | PWM_ADCTSTS0_CUTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF1_Pos)
#define | PWM_ADCTSTS0_CPTRGF1_Pos (9)
#define | PWM_ADCTSTS0_CPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF1_Pos)
#define | PWM_ADCTSTS0_CDTRGF1_Pos (10)
#define | PWM_ADCTSTS0_CDTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF1_Pos)
#define | PWM_ADCTSTS0_ZPTRGF1_Pos (11)
#define | PWM_ADCTSTS0_ZPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF1_Pos)
#define | PWM_ADCTSTS0_CUTRGF2_Pos (16)
#define | PWM_ADCTSTS0_CUTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF2_Pos)
#define | PWM_ADCTSTS0_CPTRGF2_Pos (17)
#define | PWM_ADCTSTS0_CPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF2_Pos)
#define | PWM_ADCTSTS0_CDTRGF2_Pos (18)
#define | PWM_ADCTSTS0_CDTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF2_Pos)
#define | PWM_ADCTSTS0_ZPTRGF2_Pos (19)
#define | PWM_ADCTSTS0_ZPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF2_Pos)
#define | PWM_ADCTSTS0_CUTRGF3_Pos (24)
#define | PWM_ADCTSTS0_CUTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF3_Pos)
#define | PWM_ADCTSTS0_CPTRGF3_Pos (25)
#define | PWM_ADCTSTS0_CPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF3_Pos)
#define | PWM_ADCTSTS0_CDTRGF3_Pos (26)
#define | PWM_ADCTSTS0_CDTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF3_Pos)
#define | PWM_ADCTSTS0_ZPTRGF3_Pos (27)
#define | PWM_ADCTSTS0_ZPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF3_Pos)
#define | PWM_ADCTSTS1_CUTRGF4_Pos (0)
#define | PWM_ADCTSTS1_CUTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF4_Pos)
#define | PWM_ADCTSTS1_CPTRGF4_Pos (1)
#define | PWM_ADCTSTS1_CPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF4_Pos)
#define | PWM_ADCTSTS1_CDTRGF4_Pos (2)
#define | PWM_ADCTSTS1_CDTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF4_Pos)
#define | PWM_ADCTSTS1_ZPTRGF4_Pos (3)
#define | PWM_ADCTSTS1_ZPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF4_Pos)
#define | PWM_ADCTSTS1_CUTRGF5_Pos (8)
#define | PWM_ADCTSTS1_CUTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF5_Pos)
#define | PWM_ADCTSTS1_CPTRGF5_Pos (9)
#define | PWM_ADCTSTS1_CPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF5_Pos)
#define | PWM_ADCTSTS1_CDTRGF5_Pos (10)
#define | PWM_ADCTSTS1_CDTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF5_Pos)
#define | PWM_ADCTSTS1_ZPTRGF5_Pos (11)
#define | PWM_ADCTSTS1_ZPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF5_Pos)
#define | PWM_PHCHG_MSKDAT0_Pos (0)
#define | PWM_PHCHG_MSKDAT0_Msk (0x1ul << PWM_PHCHG_MSKDAT0_Pos)
#define | PWM_PHCHG_MSKDAT1_Pos (1)
#define | PWM_PHCHG_MSKDAT1_Msk (0x1ul << PWM_PHCHG_MSKDAT1_Pos)
#define | PWM_PHCHG_MSKDAT2_Pos (2)
#define | PWM_PHCHG_MSKDAT2_Msk (0x1ul << PWM_PHCHG_MSKDAT2_Pos)
#define | PWM_PHCHG_MSKDAT3_Pos (3)
#define | PWM_PHCHG_MSKDAT3_Msk (0x1ul << PWM_PHCHG_MSKDAT3_Pos)
#define | PWM_PHCHG_MSKDAT4_Pos (4)
#define | PWM_PHCHG_MSKDAT4_Msk (0x1ul << PWM_PHCHG_MSKDAT4_Pos)
#define | PWM_PHCHG_MSKDAT5_Pos (5)
#define | PWM_PHCHG_MSKDAT5_Msk (0x1ul << PWM_PHCHG_MSKDAT5_Pos)
#define | PWM_PHCHG_MSKDAT6_Pos (6)
#define | PWM_PHCHG_MSKDAT6_Msk (0x1ul << PWM_PHCHG_MSKDAT6_Pos)
#define | PWM_PHCHG_MSKDAT7_Pos (7)
#define | PWM_PHCHG_MSKDAT7_Msk (0x1ul << PWM_PHCHG_MSKDAT7_Pos)
#define | PWM_PHCHG_MSKEN0_Pos (8)
#define | PWM_PHCHG_MSKEN0_Msk (0x1ul << PWM_PHCHG_MSKEN0_Pos)
#define | PWM_PHCHG_MSKEN1_Pos (9)
#define | PWM_PHCHG_MSKEN1_Msk (0x1ul << PWM_PHCHG_MSKEN1_Pos)
#define | PWM_PHCHG_MSKEN2_Pos (10)
#define | PWM_PHCHG_MSKEN2_Msk (0x1ul << PWM_PHCHG_MSKEN2_Pos)
#define | PWM_PHCHG_MSKEN3_Pos (11)
#define | PWM_PHCHG_MSKEN3_Msk (0x1ul << PWM_PHCHG_MSKEN3_Pos)
#define | PWM_PHCHG_MSKEN4_Pos (12)
#define | PWM_PHCHG_MSKEN4_Msk (0x1ul << PWM_PHCHG_MSKEN4_Pos)
#define | PWM_PHCHG_MSKEN5_Pos (13)
#define | PWM_PHCHG_MSKEN5_Msk (0x1ul << PWM_PHCHG_MSKEN5_Pos)
#define | PWM_PHCHG_AUTOCLR0_Pos (14)
#define | PWM_PHCHG_AUTOCLR0_Msk (0x1ul << PWM_PHCHG_AUTOCLR0_Pos)
#define | PWM_PHCHG_AUTOCLR1_Pos (15)
#define | PWM_PHCHG_AUTOCLR1_Msk (0x1ul << PWM_PHCHG_AUTOCLR1_Pos)
#define | PWM_PHCHG_AOFFEN01_Pos (16)
#define | PWM_PHCHG_AOFFEN01_Msk (0x1ul << PWM_PHCHG_AOFFEN01_Pos)
#define | PWM_PHCHG_AOFFEN11_Pos (17)
#define | PWM_PHCHG_AOFFEN11_Msk (0x1ul << PWM_PHCHG_AOFFEN11_Pos)
#define | PWM_PHCHG_AOFFEN21_Pos (18)
#define | PWM_PHCHG_AOFFEN21_Msk (0x1ul << PWM_PHCHG_AOFFEN21_Pos)
#define | PWM_PHCHG_AOFFEN31_Pos (19)
#define | PWM_PHCHG_AOFFEN31_Msk (0x1ul << PWM_PHCHG_AOFFEN31_Pos)
#define | PWM_PHCHG_A1POSSEL_Pos (20)
#define | PWM_PHCHG_A1POSSEL_Msk (0x3ul << PWM_PHCHG_A1POSSEL_Pos)
#define | PWM_PHCHG_TMR1TEN_Pos (22)
#define | PWM_PHCHG_TMR1TEN_Msk (0x1ul << PWM_PHCHG_TMR1TEN_Pos)
#define | PWM_PHCHG_ACMP1TEN_Pos (23)
#define | PWM_PHCHG_ACMP1TEN_Msk (0x1ul << PWM_PHCHG_ACMP1TEN_Pos)
#define | PWM_PHCHG_AOFFEN00_Pos (24)
#define | PWM_PHCHG_AOFFEN00_Msk (0x1ul << PWM_PHCHG_AOFFEN00_Pos)
#define | PWM_PHCHG_AOFFEN10_Pos (25)
#define | PWM_PHCHG_AOFFEN10_Msk (0x1ul << PWM_PHCHG_AOFFEN10_Pos)
#define | PWM_PHCHG_AOFFEN20_Pos (26)
#define | PWM_PHCHG_AOFFEN20_Msk (0x1ul << PWM_PHCHG_AOFFEN20_Pos)
#define | PWM_PHCHG_AOFFEN30_Pos (27)
#define | PWM_PHCHG_AOFFEN30_Msk (0x1ul << PWM_PHCHG_AOFFEN30_Pos)
#define | PWM_PHCHG_A0POSSEL_Pos (28)
#define | PWM_PHCHG_A0POSSEL_Msk (0x3ul << PWM_PHCHG_A0POSSEL_Pos)
#define | PWM_PHCHG_TMR0TEN_Pos (30)
#define | PWM_PHCHG_TMR0TEN_Msk (0x1ul << PWM_PHCHG_TMR0TEN_Pos)
#define | PWM_PHCHG_ACMP0TEN_Pos (31)
#define | PWM_PHCHG_ACMP0TEN_Msk (0x1ul << PWM_PHCHG_ACMP0TEN_Pos)
#define | PWM_PHCHGNXT_MSKDAT0_Pos (0)
#define | PWM_PHCHGNXT_MSKDAT0_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT0_Pos)
#define | PWM_PHCHGNXT_MSKDAT1_Pos (1)
#define | PWM_PHCHGNXT_MSKDAT1_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT1_Pos)
#define | PWM_PHCHGNXT_MSKDAT2_Pos (2)
#define | PWM_PHCHGNXT_MSKDAT2_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT2_Pos)
#define | PWM_PHCHGNXT_MSKDAT3_Pos (3)
#define | PWM_PHCHGNXT_MSKDAT3_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT3_Pos)
#define | PWM_PHCHGNXT_MSKDAT4_Pos (4)
#define | PWM_PHCHGNXT_MSKDAT4_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT4_Pos)
#define | PWM_PHCHGNXT_MSKDAT5_Pos (5)
#define | PWM_PHCHGNXT_MSKDAT5_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT5_Pos)
#define | PWM_PHCHGNXT_MSKDAT6_Pos (6)
#define | PWM_PHCHGNXT_MSKDAT6_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT6_Pos)
#define | PWM_PHCHGNXT_MSKDAT7_Pos (7)
#define | PWM_PHCHGNXT_MSKDAT7_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT7_Pos)
#define | PWM_PHCHGNXT_MSKEN0_Pos (8)
#define | PWM_PHCHGNXT_MSKEN0_Msk (0x1ul << PWM_PHCHGNXT_MSKEN0_Pos)
#define | PWM_PHCHGNXT_MSKEN1_Pos (9)
#define | PWM_PHCHGNXT_MSKEN1_Msk (0x1ul << PWM_PHCHGNXT_MSKEN1_Pos)
#define | PWM_PHCHGNXT_MSKEN2_Pos (10)
#define | PWM_PHCHGNXT_MSKEN2_Msk (0x1ul << PWM_PHCHGNXT_MSKEN2_Pos)
#define | PWM_PHCHGNXT_MSKEN3_Pos (11)
#define | PWM_PHCHGNXT_MSKEN3_Msk (0x1ul << PWM_PHCHGNXT_MSKEN3_Pos)
#define | PWM_PHCHGNXT_MSKEN4_Pos (12)
#define | PWM_PHCHGNXT_MSKEN4_Msk (0x1ul << PWM_PHCHGNXT_MSKEN4_Pos)
#define | PWM_PHCHGNXT_MSKEN5_Pos (13)
#define | PWM_PHCHGNXT_MSKEN5_Msk (0x1ul << PWM_PHCHGNXT_MSKEN5_Pos)
#define | PWM_PHCHGNXT_AUTOCLR0_Pos (14)
#define | PWM_PHCHGNXT_AUTOCLR0_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR0_Pos)
#define | PWM_PHCHGNXT_AUTOCLR1_Pos (15)
#define | PWM_PHCHGNXT_AUTOCLR1_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR1_Pos)
#define | PWM_PHCHGNXT_AOFFEN01_Pos (16)
#define | PWM_PHCHGNXT_AOFFEN01_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN01_Pos)
#define | PWM_PHCHGNXT_AOFFEN11_Pos (17)
#define | PWM_PHCHGNXT_AOFFEN11_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN11_Pos)
#define | PWM_PHCHGNXT_AOFFEN21_Pos (18)
#define | PWM_PHCHGNXT_AOFFEN21_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN21_Pos)
#define | PWM_PHCHGNXT_AOFFEN31_Pos (19)
#define | PWM_PHCHGNXT_AOFFEN31_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN31_Pos)
#define | PWM_PHCHGNXT_A1POSSEL_Pos (20)
#define | PWM_PHCHGNXT_A1POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A1POSSEL_Pos)
#define | PWM_PHCHGNXT_TMR1TEN_Pos (22)
#define | PWM_PHCHGNXT_TMR1TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR1TEN_Pos)
#define | PWM_PHCHGNXT_ACMP1TEN_Pos (23)
#define | PWM_PHCHGNXT_ACMP1TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP1TEN_Pos)
#define | PWM_PHCHGNXT_AOFFEN00_Pos (24)
#define | PWM_PHCHGNXT_AOFFEN00_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN00_Pos)
#define | PWM_PHCHGNXT_AOFFEN10_Pos (25)
#define | PWM_PHCHGNXT_AOFFEN10_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN10_Pos)
#define | PWM_PHCHGNXT_AOFFEN20_Pos (26)
#define | PWM_PHCHGNXT_AOFFEN20_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN20_Pos)
#define | PWM_PHCHGNXT_AOFFEN30_Pos (27)
#define | PWM_PHCHGNXT_AOFFEN30_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN30_Pos)
#define | PWM_PHCHGNXT_A0POSSEL_Pos (28)
#define | PWM_PHCHGNXT_A0POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A0POSSEL_Pos)
#define | PWM_PHCHGNXT_TMR0TEN_Pos (30)
#define | PWM_PHCHGNXT_TMR0TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR0TEN_Pos)
#define | PWM_PHCHGNXT_ACMP0TEN_Pos (31)
#define | PWM_PHCHGNXT_ACMP0TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP0TEN_Pos)
#define | PWM_PHCHGMSK_MASKEND6_Pos (6)
#define | PWM_PHCHGMSK_MASKEND6_Msk (0x1ul << PWM_PHCHGMSK_MASKEND6_Pos)
#define | PWM_PHCHGMSK_MASKEND7_Pos (7)
#define | PWM_PHCHGMSK_MASKEND7_Msk (0x1ul << PWM_PHCHGMSK_MASKEND7_Pos)
#define | PWM_PHCHGMSK_POSCTL0_Pos (8)
#define | PWM_PHCHGMSK_POSCTL0_Msk (0x1ul << PWM_PHCHGMSK_POSCTL0_Pos)
#define | PWM_PHCHGMSK_POSCTL1_Pos (9)
#define | PWM_PHCHGMSK_POSCTL1_Msk (0x1ul << PWM_PHCHGMSK_POSCTL1_Pos)
#define | PWM_IFA_IFAEN_Pos (0)
#define | PWM_IFA_IFAEN_Msk (0x1ul << PWM_IFA_IFAEN_Pos)
#define | PWM_IFA_IFCNT_Pos (4)
#define | PWM_IFA_IFCNT_Msk (0xful << PWM_IFA_IFCNT_Pos)
#define | PWM_PCACTL_PCAEN_Pos (0)
#define | PWM_PCACTL_PCAEN_Msk (0x1ul << PWM_PCACTL_PCAEN_Pos)
#define | PWM_MSKALIGN_MSKDAT0_Pos (0)
#define | PWM_MSKALIGN_MSKDAT0_Msk (0x1ul << PWM_MSKALIGN_MSKDAT0_Pos)
#define | PWM_MSKALIGN_MSKDAT1_Pos (1)
#define | PWM_MSKALIGN_MSKDAT1_Msk (0x1ul << PWM_MSKALIGN_MSKDAT1_Pos)
#define | PWM_MSKALIGN_MSKDAT2_Pos (2)
#define | PWM_MSKALIGN_MSKDAT2_Msk (0x1ul << PWM_MSKALIGN_MSKDAT2_Pos)
#define | PWM_MSKALIGN_MSKDAT3_Pos (3)
#define | PWM_MSKALIGN_MSKDAT3_Msk (0x1ul << PWM_MSKALIGN_MSKDAT3_Pos)
#define | PWM_MSKALIGN_MSKDAT4_Pos (4)
#define | PWM_MSKALIGN_MSKDAT4_Msk (0x1ul << PWM_MSKALIGN_MSKDAT4_Pos)
#define | PWM_MSKALIGN_MSKDAT5_Pos (5)
#define | PWM_MSKALIGN_MSKDAT5_Msk (0x1ul << PWM_MSKALIGN_MSKDAT5_Pos)
#define | PWM_MSKALIGN_MSKEN0_Pos (8)
#define | PWM_MSKALIGN_MSKEN0_Msk (0x1ul << PWM_MSKALIGN_MSKEN0_Pos)
#define | PWM_MSKALIGN_MSKEN1_Pos (9)
#define | PWM_MSKALIGN_MSKEN1_Msk (0x1ul << PWM_MSKALIGN_MSKEN1_Pos)
#define | PWM_MSKALIGN_MSKEN2_Pos (10)
#define | PWM_MSKALIGN_MSKEN2_Msk (0x1ul << PWM_MSKALIGN_MSKEN2_Pos)
#define | PWM_MSKALIGN_MSKEN3_Pos (11)
#define | PWM_MSKALIGN_MSKEN3_Msk (0x1ul << PWM_MSKALIGN_MSKEN3_Pos)
#define | PWM_MSKALIGN_MSKEN4_Pos (12)
#define | PWM_MSKALIGN_MSKEN4_Msk (0x1ul << PWM_MSKALIGN_MSKEN4_Pos)
#define | PWM_MSKALIGN_MSKEN5_Pos (13)
#define | PWM_MSKALIGN_MSKEN5_Msk (0x1ul << PWM_MSKALIGN_MSKEN5_Pos)
#define | PWM_MSKALIGN_ALIGN0_Pos (16)
#define | PWM_MSKALIGN_ALIGN0_Msk (0x1ul << PWM_MSKALIGN_ALIGN0_Pos)
#define | PWM_MSKALIGN_ALIGN1_Pos (17)
#define | PWM_MSKALIGN_ALIGN1_Msk (0x1ul << PWM_MSKALIGN_ALIGN1_Pos)
#define | PWM_MSKALIGN_ALIGN2_Pos (18)
#define | PWM_MSKALIGN_ALIGN2_Msk (0x1ul << PWM_MSKALIGN_ALIGN2_Pos)
#define | PWM_MSKALIGN_ALIGN3_Pos (19)
#define | PWM_MSKALIGN_ALIGN3_Msk (0x1ul << PWM_MSKALIGN_ALIGN3_Pos)
#define | PWM_MSKALIGN_ALIGN4_Pos (20)
#define | PWM_MSKALIGN_ALIGN4_Msk (0x1ul << PWM_MSKALIGN_ALIGN4_Pos)
#define | PWM_MSKALIGN_ALIGN5_Pos (21)
#define | PWM_MSKALIGN_ALIGN5_Msk (0x1ul << PWM_MSKALIGN_ALIGN5_Pos)
#define | SPI_CTL_SPIEN_Pos (0)
#define | SPI_CTL_SPIEN_Msk (0x1ul << SPI_CTL_SPIEN_Pos)
#define | SPI_CTL_RXNEG_Pos (1)
#define | SPI_CTL_RXNEG_Msk (0x1ul << SPI_CTL_RXNEG_Pos)
#define | SPI_CTL_TXNEG_Pos (2)
#define | SPI_CTL_TXNEG_Msk (0x1ul << SPI_CTL_TXNEG_Pos)
#define | SPI_CTL_DWIDTH_Pos (3)
#define | SPI_CTL_DWIDTH_Msk (0x1ful << SPI_CTL_DWIDTH_Pos)
#define | SPI_CTL_LSB_Pos (10)
#define | SPI_CTL_LSB_Msk (0x1ul << SPI_CTL_LSB_Pos)
#define | SPI_CTL_CLKPOL_Pos (11)
#define | SPI_CTL_CLKPOL_Msk (0x1ul << SPI_CTL_CLKPOL_Pos)
#define | SPI_CTL_SUSPITV_Pos (12)
#define | SPI_CTL_SUSPITV_Msk (0xful << SPI_CTL_SUSPITV_Pos)
#define | SPI_CTL_UNITIF_Pos (16)
#define | SPI_CTL_UNITIF_Msk (0x1ul << SPI_CTL_UNITIF_Pos)
#define | SPI_CTL_UNITIEN_Pos (17)
#define | SPI_CTL_UNITIEN_Msk (0x1ul << SPI_CTL_UNITIEN_Pos)
#define | SPI_CTL_SLAVE_Pos (18)
#define | SPI_CTL_SLAVE_Msk (0x1ul << SPI_CTL_SLAVE_Pos)
#define | SPI_CTL_REORDER_Pos (19)
#define | SPI_CTL_REORDER_Msk (0x1ul << SPI_CTL_REORDER_Pos)
#define | SPI_CTL_FIFOEN_Pos (21)
#define | SPI_CTL_FIFOEN_Msk (0x1ul << SPI_CTL_FIFOEN_Pos)
#define | SPI_CTL_RXEMPTY_Pos (24)
#define | SPI_CTL_RXEMPTY_Msk (0x1ul << SPI_CTL_RXEMPTY_Pos)
#define | SPI_CTL_RXFULL_Pos (25)
#define | SPI_CTL_RXFULL_Msk (0x1ul << SPI_CTL_RXFULL_Pos)
#define | SPI_CTL_TXEMPTY_Pos (26)
#define | SPI_CTL_TXEMPTY_Msk (0x1ul << SPI_CTL_TXEMPTY_Pos)
#define | SPI_CTL_TXFULL_Pos (27)
#define | SPI_CTL_TXFULL_Msk (0x1ul << SPI_CTL_TXFULL_Pos)
#define | SPI_CLKDIV_DIVIDER_Pos (0)
#define | SPI_CLKDIV_DIVIDER_Msk (0xfful << SPI_CLKDIV_DIVIDER_Pos)
#define | SPI_SSCTL_SS_Pos (0)
#define | SPI_SSCTL_SS_Msk (0x1ul << SPI_SSCTL_SS_Pos)
#define | SPI_SSCTL_SSACTPOL_Pos (2)
#define | SPI_SSCTL_SSACTPOL_Msk (0x1ul << SPI_SSCTL_SSACTPOL_Pos)
#define | SPI_SSCTL_AUTOSS_Pos (3)
#define | SPI_SSCTL_AUTOSS_Msk (0x1ul << SPI_SSCTL_AUTOSS_Pos)
#define | SPI_SSCTL_SSLTEN_Pos (4)
#define | SPI_SSCTL_SSLTEN_Msk (0x1ul << SPI_SSCTL_SSLTEN_Pos)
#define | SPI_SSCTL_LTF_Pos (5)
#define | SPI_SSCTL_LTF_Msk (0x1ul << SPI_SSCTL_LTF_Pos)
#define | SPI_RX_RX_Pos (0)
#define | SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)
#define | SPI_TX_TX_Pos (0)
#define | SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)
#define | SPI_SLVCTL_SLV3WIRE_Pos (8)
#define | SPI_SLVCTL_SLV3WIRE_Msk (0x1ul << SPI_SLVCTL_SLV3WIRE_Pos)
#define | SPI_SLVCTL_SLVABT_Pos (9)
#define | SPI_SLVCTL_SLVABT_Msk (0x1ul << SPI_SLVCTL_SLVABT_Pos)
#define | SPI_SLVCTL_SLVSTIEN_Pos (10)
#define | SPI_SLVCTL_SLVSTIEN_Msk (0x1ul << SPI_SLVCTL_SLVSTIEN_Pos)
#define | SPI_SLVCTL_SLVSTIF_Pos (11)
#define | SPI_SLVCTL_SLVSTIF_Msk (0x1ul << SPI_SLVCTL_SLVSTIF_Pos)
#define | SPI_SLVCTL_SSINAIEN_Pos (16)
#define | SPI_SLVCTL_SSINAIEN_Msk (0x1ul << SPI_SLVCTL_SSINAIEN_Pos)
#define | SPI_SLVCTL_DIVMOD_Pos (31)
#define | SPI_SLVCTL_DIVMOD_Msk (0x1ul << SPI_SLVCTL_DIVMOD_Pos)
#define | SPI_FIFOCTL_RXRST_Pos (0)
#define | SPI_FIFOCTL_RXRST_Msk (0x1ul << SPI_FIFOCTL_RXRST_Pos)
#define | SPI_FIFOCTL_TXRST_Pos (1)
#define | SPI_FIFOCTL_TXRST_Msk (0x1ul << SPI_FIFOCTL_TXRST_Pos)
#define | SPI_FIFOCTL_RXTHIEN_Pos (2)
#define | SPI_FIFOCTL_RXTHIEN_Msk (0x1ul << SPI_FIFOCTL_RXTHIEN_Pos)
#define | SPI_FIFOCTL_TXTHIEN_Pos (3)
#define | SPI_FIFOCTL_TXTHIEN_Msk (0x1ul << SPI_FIFOCTL_TXTHIEN_Pos)
#define | SPI_FIFOCTL_RXOVIEN_Pos (6)
#define | SPI_FIFOCTL_RXOVIEN_Msk (0x1ul << SPI_FIFOCTL_RXOVIEN_Pos)
#define | SPI_FIFOCTL_RXTOIEN_Pos (21)
#define | SPI_FIFOCTL_RXTOIEN_Msk (0x1ul << SPI_FIFOCTL_RXTOIEN_Pos)
#define | SPI_FIFOCTL_RXTH_Pos (24)
#define | SPI_FIFOCTL_RXTH_Msk (0x3ul << SPI_FIFOCTL_RXTH_Pos)
#define | SPI_FIFOCTL_TXTH_Pos (28)
#define | SPI_FIFOCTL_TXTH_Msk (0x3ul << SPI_FIFOCTL_TXTH_Pos)
#define | SPI_STATUS_RXTHIF_Pos (0)
#define | SPI_STATUS_RXTHIF_Msk (0x1ul << SPI_STATUS_RXTHIF_Pos)
#define | SPI_STATUS_RXOVIF_Pos (2)
#define | SPI_STATUS_RXOVIF_Msk (0x1ul << SPI_STATUS_RXOVIF_Pos)
#define | SPI_STATUS_TXTHIF_Pos (4)
#define | SPI_STATUS_TXTHIF_Msk (0x1ul << SPI_STATUS_TXTHIF_Pos)
#define | SPI_STATUS_SLVSTIF_Pos (11)
#define | SPI_STATUS_SLVSTIF_Msk (0x1ul << SPI_STATUS_SLVSTIF_Pos)
#define | SPI_STATUS_RXCNT_Pos (12)
#define | SPI_STATUS_RXCNT_Msk (0xful << SPI_STATUS_RXCNT_Pos)
#define | SPI_STATUS_UNITIF_Pos (16)
#define | SPI_STATUS_UNITIF_Msk (0x1ul << SPI_STATUS_UNITIF_Pos)
#define | SPI_STATUS_SLVTOIF_Pos (20)
#define | SPI_STATUS_SLVTOIF_Msk (0x1ul << SPI_STATUS_SLVTOIF_Pos)
#define | SPI_STATUS_RXEMPTY_Pos (24)
#define | SPI_STATUS_RXEMPTY_Msk (0x1ul << SPI_STATUS_RXEMPTY_Pos)
#define | SPI_STATUS_RXFULL_Pos (25)
#define | SPI_STATUS_RXFULL_Msk (0x1ul << SPI_STATUS_RXFULL_Pos)
#define | SPI_STATUS_TXEMPTY_Pos (26)
#define | SPI_STATUS_TXEMPTY_Msk (0x1ul << SPI_STATUS_TXEMPTY_Pos)
#define | SPI_STATUS_TXFULL_Pos (27)
#define | SPI_STATUS_TXFULL_Msk (0x1ul << SPI_STATUS_TXFULL_Pos)
#define | SPI_STATUS_TXCNT_Pos (28)
#define | SPI_STATUS_TXCNT_Msk (0xful << SPI_STATUS_TXCNT_Pos)
#define | SYS_PDID_PDID_Pos (0)
#define | SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)
#define | SYS_RSTSTS_PORF_Pos (0)
#define | SYS_RSTSTS_PORF_Msk (0x1ul << SYS_RSTSTS_PORF_Pos)
#define | SYS_RSTSTS_PINRF_Pos (1)
#define | SYS_RSTSTS_PINRF_Msk (0x1ul << SYS_RSTSTS_PINRF_Pos)
#define | SYS_RSTSTS_WDTRF_Pos (2)
#define | SYS_RSTSTS_WDTRF_Msk (0x1ul << SYS_RSTSTS_WDTRF_Pos)
#define | SYS_RSTSTS_BODRF_Pos (4)
#define | SYS_RSTSTS_BODRF_Msk (0x1ul << SYS_RSTSTS_BODRF_Pos)
#define | SYS_RSTSTS_SYSRF_Pos (5)
#define | SYS_RSTSTS_SYSRF_Msk (0x1ul << SYS_RSTSTS_SYSRF_Pos)
#define | SYS_RSTSTS_CPURF_Pos (7)
#define | SYS_RSTSTS_CPURF_Msk (0x1ul << SYS_RSTSTS_CPURF_Pos)
#define | SYS_RSTSTS_CPULKRF_Pos (8)
#define | SYS_RSTSTS_CPULKRF_Msk (0x1ul << SYS_RSTSTS_CPULKRF_Pos)
#define | SYS_IPRST0_CHIPRST_Pos (0)
#define | SYS_IPRST0_CHIPRST_Msk (0x1ul << SYS_IPRST0_CHIPRST_Pos)
#define | SYS_IPRST0_CPURST_Pos (1)
#define | SYS_IPRST0_CPURST_Msk (0x1ul << SYS_IPRST0_CPURST_Pos)
#define | SYS_IPRST1_GPIORST_Pos (1)
#define | SYS_IPRST1_GPIORST_Msk (0x1ul << SYS_IPRST1_GPIORST_Pos)
#define | SYS_IPRST1_TMR0RST_Pos (2)
#define | SYS_IPRST1_TMR0RST_Msk (0x1ul << SYS_IPRST1_TMR0RST_Pos)
#define | SYS_IPRST1_TMR1RST_Pos (3)
#define | SYS_IPRST1_TMR1RST_Msk (0x1ul << SYS_IPRST1_TMR1RST_Pos)
#define | SYS_IPRST1_I2C0RST_Pos (8)
#define | SYS_IPRST1_I2C0RST_Msk (0x1ul << SYS_IPRST1_I2C0RST_Pos)
#define | SYS_IPRST1_I2C1RST_Pos (9)
#define | SYS_IPRST1_I2C1RST_Msk (0x1ul << SYS_IPRST1_I2C1RST_Pos)
#define | SYS_IPRST1_SPI0RST_Pos (12)
#define | SYS_IPRST1_SPI0RST_Msk (0x1ul << SYS_IPRST1_SPI0RST_Pos)
#define | SYS_IPRST1_UART0RST_Pos (16)
#define | SYS_IPRST1_UART0RST_Msk (0x1ul << SYS_IPRST1_UART0RST_Pos)
#define | SYS_IPRST1_UART1RST_Pos (17)
#define | SYS_IPRST1_UART1RST_Msk (0x1ul << SYS_IPRST1_UART1RST_Pos)
#define | SYS_IPRST1_PWM0RST_Pos (20)
#define | SYS_IPRST1_PWM0RST_Msk (0x1ul << SYS_IPRST1_PWM0RST_Pos)
#define | SYS_IPRST1_ACMPRST_Pos (22)
#define | SYS_IPRST1_ACMPRST_Msk (0x1ul << SYS_IPRST1_ACMPRST_Pos)
#define | SYS_IPRST1_ADCRST_Pos (28)
#define | SYS_IPRST1_ADCRST_Msk (0x1ul << SYS_IPRST1_ADCRST_Pos)
#define | SYS_BODCTL_BODEN_Pos (0)
#define | SYS_BODCTL_BODEN_Msk (0x1ul << SYS_BODCTL_BODEN_Pos)
#define | SYS_BODCTL_BODVL_Pos (1)
#define | SYS_BODCTL_BODVL_Msk (0x3ul << SYS_BODCTL_BODVL_Pos)
#define | SYS_BODCTL_BODRSTEN_Pos (3)
#define | SYS_BODCTL_BODRSTEN_Msk (0x1ul << SYS_BODCTL_BODRSTEN_Pos)
#define | SYS_BODCTL_BODIF_Pos (4)
#define | SYS_BODCTL_BODIF_Msk (0x1ul << SYS_BODCTL_BODIF_Pos)
#define | SYS_BODCTL_BODLPM_Pos (5)
#define | SYS_BODCTL_BODLPM_Msk (0x1ul << SYS_BODCTL_BODLPM_Pos)
#define | SYS_BODCTL_BODOUT_Pos (6)
#define | SYS_BODCTL_BODOUT_Msk (0x1ul << SYS_BODCTL_BODOUT_Pos)
#define | SYS_P0_MFP_MFP_Pos (0)
#define | SYS_P0_MFP_MFP_Msk (0xfful << SYS_P0_MFP_MFP_Pos)
#define | SYS_P0_MFP_ALT0_Pos (8)
#define | SYS_P0_MFP_ALT0_Msk (0x1ul << SYS_P0_MFP_ALT0_Pos)
#define | SYS_P0_MFP_ALT1_Pos (9)
#define | SYS_P0_MFP_ALT1_Msk (0x1ul << SYS_P0_MFP_ALT1_Pos)
#define | SYS_P0_MFP_ALT4_Pos (12)
#define | SYS_P0_MFP_ALT4_Msk (0x1ul << SYS_P0_MFP_ALT4_Pos)
#define | SYS_P0_MFP_ALT5_Pos (13)
#define | SYS_P0_MFP_ALT5_Msk (0x1ul << SYS_P0_MFP_ALT5_Pos)
#define | SYS_P0_MFP_ALT6_Pos (14)
#define | SYS_P0_MFP_ALT6_Msk (0x1ul << SYS_P0_MFP_ALT6_Pos)
#define | SYS_P0_MFP_ALT7_Pos (15)
#define | SYS_P0_MFP_ALT7_Msk (0x1ul << SYS_P0_MFP_ALT7_Pos)
#define | SYS_P0_MFP_TYPE_Pos (16)
#define | SYS_P0_MFP_TYPE_Msk (0xfful << SYS_P0_MFP_TYPE_Pos)
#define | SYS_P1_MFP_MFP_Pos (0)
#define | SYS_P1_MFP_MFP_Msk (0xfful << SYS_P1_MFP_MFP_Pos)
#define | SYS_P1_MFP_ALT0_Pos (8)
#define | SYS_P1_MFP_ALT0_Msk (0x1ul << SYS_P1_MFP_ALT0_Pos)
#define | SYS_P1_MFP_ALT2_Pos (10)
#define | SYS_P1_MFP_ALT2_Msk (0x1ul << SYS_P1_MFP_ALT2_Pos)
#define | SYS_P1_MFP_ALT3_Pos (11)
#define | SYS_P1_MFP_ALT3_Msk (0x1ul << SYS_P1_MFP_ALT3_Pos)
#define | SYS_P1_MFP_ALT4_Pos (12)
#define | SYS_P1_MFP_ALT4_Msk (0x1ul << SYS_P1_MFP_ALT4_Pos)
#define | SYS_P1_MFP_ALT5_Pos (13)
#define | SYS_P1_MFP_ALT5_Msk (0x1ul << SYS_P1_MFP_ALT5_Pos)
#define | SYS_P1_MFP_TYPE_Pos (16)
#define | SYS_P1_MFP_TYPE_Msk (0xfful << SYS_P1_MFP_TYPE_Pos)
#define | SYS_P1_MFP_P12EXT_Pos (26)
#define | SYS_P1_MFP_P12EXT_Msk (0x1ul << SYS_P1_MFP_P12EXT_Pos)
#define | SYS_P1_MFP_P13EXT_Pos (27)
#define | SYS_P1_MFP_P13EXT_Msk (0x1ul << SYS_P1_MFP_P13EXT_Pos)
#define | SYS_P1_MFP_P14EXT_Pos (28)
#define | SYS_P1_MFP_P14EXT_Msk (0x1ul << SYS_P1_MFP_P14EXT_Pos)
#define | SYS_P2_MFP_MFP_Pos (0)
#define | SYS_P2_MFP_MFP_Msk (0xfful << SYS_P2_MFP_MFP_Pos)
#define | SYS_P2_MFP_ALT2_Pos (10)
#define | SYS_P2_MFP_ALT2_Msk (0x1ul << SYS_P2_MFP_ALT2_Pos)
#define | SYS_P2_MFP_ALT3_Pos (11)
#define | SYS_P2_MFP_ALT3_Msk (0x1ul << SYS_P2_MFP_ALT3_Pos)
#define | SYS_P2_MFP_ALT4_Pos (12)
#define | SYS_P2_MFP_ALT4_Msk (0x1ul << SYS_P2_MFP_ALT4_Pos)
#define | SYS_P2_MFP_ALT5_Pos (13)
#define | SYS_P2_MFP_ALT5_Msk (0x1ul << SYS_P2_MFP_ALT5_Pos)
#define | SYS_P2_MFP_ALT6_Pos (14)
#define | SYS_P2_MFP_ALT6_Msk (0x1ul << SYS_P2_MFP_ALT6_Pos)
#define | SYS_P2_MFP_TYPE_Pos (16)
#define | SYS_P2_MFP_TYPE_Msk (0xfful << SYS_P2_MFP_TYPE_Pos)
#define | SYS_P3_MFP_MFP_Pos (0)
#define | SYS_P3_MFP_MFP_Msk (0xfful << SYS_P3_MFP_MFP_Pos)
#define | SYS_P3_MFP_ALT0_Pos (8)
#define | SYS_P3_MFP_ALT0_Msk (0x1ul << SYS_P3_MFP_ALT0_Pos)
#define | SYS_P3_MFP_ALT1_Pos (9)
#define | SYS_P3_MFP_ALT1_Msk (0x1ul << SYS_P3_MFP_ALT1_Pos)
#define | SYS_P3_MFP_ALT2_Pos (10)
#define | SYS_P3_MFP_ALT2_Msk (0x1ul << SYS_P3_MFP_ALT2_Pos)
#define | SYS_P3_MFP_ALT4_Pos (12)
#define | SYS_P3_MFP_ALT4_Msk (0x1ul << SYS_P3_MFP_ALT4_Pos)
#define | SYS_P3_MFP_ALT5_Pos (13)
#define | SYS_P3_MFP_ALT5_Msk (0x1ul << SYS_P3_MFP_ALT5_Pos)
#define | SYS_P3_MFP_ALT6_Pos (14)
#define | SYS_P3_MFP_ALT6_Msk (0x1ul << SYS_P3_MFP_ALT6_Pos)
#define | SYS_P3_MFP_TYPE_Pos (16)
#define | SYS_P3_MFP_TYPE_Msk (0xfful << SYS_P3_MFP_TYPE_Pos)
#define | SYS_P3_MFP_P32EXT_Pos (26)
#define | SYS_P3_MFP_P32EXT_Msk (0x1ul << SYS_P3_MFP_P32EXT_Pos)
#define | SYS_P4_MFP_MFP_Pos (0)
#define | SYS_P4_MFP_MFP_Msk (0xfful << SYS_P4_MFP_MFP_Pos)
#define | SYS_P4_MFP_ALT6_Pos (14)
#define | SYS_P4_MFP_ALT6_Msk (0x1ul << SYS_P4_MFP_ALT6_Pos)
#define | SYS_P4_MFP_ALT7_Pos (15)
#define | SYS_P4_MFP_ALT7_Msk (0x1ul << SYS_P4_MFP_ALT7_Pos)
#define | SYS_P4_MFP_TYPE_Pos (16)
#define | SYS_P4_MFP_TYPE_Msk (0xfful << SYS_P4_MFP_TYPE_Pos)
#define | SYS_P5_MFP_MFP_Pos (0)
#define | SYS_P5_MFP_MFP_Msk (0xfful << SYS_P5_MFP_MFP_Pos)
#define | SYS_P5_MFP_ALT0_Pos (8)
#define | SYS_P5_MFP_ALT0_Msk (0x1ul << SYS_P5_MFP_ALT0_Pos)
#define | SYS_P5_MFP_ALT1_Pos (9)
#define | SYS_P5_MFP_ALT1_Msk (0x1ul << SYS_P5_MFP_ALT1_Pos)
#define | SYS_P5_MFP_ALT2_Pos (10)
#define | SYS_P5_MFP_ALT2_Msk (0x1ul << SYS_P5_MFP_ALT2_Pos)
#define | SYS_P5_MFP_ALT3_Pos (11)
#define | SYS_P5_MFP_ALT3_Msk (0x1ul << SYS_P5_MFP_ALT3_Pos)
#define | SYS_P5_MFP_ALT4_Pos (12)
#define | SYS_P5_MFP_ALT4_Msk (0x1ul << SYS_P5_MFP_ALT4_Pos)
#define | SYS_P5_MFP_ALT5_Pos (13)
#define | SYS_P5_MFP_ALT5_Msk (0x1ul << SYS_P5_MFP_ALT5_Pos)
#define | SYS_P5_MFP_TYPE_Pos (16)
#define | SYS_P5_MFP_TYPE_Msk (0xfful << SYS_P5_MFP_TYPE_Pos)
#define | SYS_IRCTCTL_FREQSEL_Pos (0)
#define | SYS_IRCTCTL_FREQSEL_Msk (0x1ul << SYS_IRCTCTL_FREQSEL_Pos)
#define | SYS_IRCTCTL_LOOPSEL_Pos (4)
#define | SYS_IRCTCTL_LOOPSEL_Msk (0x3ul << SYS_IRCTCTL_LOOPSEL_Pos)
#define | SYS_IRCTIEN_TFAILIEN_Pos (1)
#define | SYS_IRCTIEN_TFAILIEN_Msk (0x1ul << SYS_IRCTIEN_TFAILIEN_Pos)
#define | SYS_IRCTIEN_CLKEIEN_Pos (2)
#define | SYS_IRCTIEN_CLKEIEN_Msk (0x1ul << SYS_IRCTIEN_CLKEIEN_Pos)
#define | SYS_IRCTISTS_FREQLOCK_Pos (0)
#define | SYS_IRCTISTS_FREQLOCK_Msk (0x1ul << SYS_IRCTISTS_FREQLOCK_Pos)
#define | SYS_IRCTISTS_TFAILIF_Pos (1)
#define | SYS_IRCTISTS_TFAILIF_Msk (0x1ul << SYS_IRCTISTS_TFAILIF_Pos)
#define | SYS_IRCTISTS_CLKERRIF_Pos (2)
#define | SYS_IRCTISTS_CLKERRIF_Msk (0x1ul << SYS_IRCTISTS_CLKERRIF_Pos)
#define | SYS_REGLCTL_REGLCTL_Pos (0)
#define | SYS_REGLCTL_REGLCTL_Msk (0xfful << SYS_REGLCTL_REGLCTL_Pos)
#define | TIMER_CTL_PSC_Pos (0)
#define | TIMER_CTL_PSC_Msk (0xfful << TIMER_CTL_PSC_Pos)
#define | TIMER_CTL_CMPCTL_Pos (17)
#define | TIMER_CTL_CMPCTL_Msk (0x1ul << TIMER_CTL_CMPCTL_Pos)
#define | TIMER_CTL_TGLPINSEL_Pos (18)
#define | TIMER_CTL_TGLPINSEL_Msk (0x1ul << TIMER_CTL_TGLPINSEL_Pos)
#define | TIMER_CTL_CAPSRC_Pos (19)
#define | TIMER_CTL_CAPSRC_Msk (0x1ul << TIMER_CTL_CAPSRC_Pos)
#define | TIMER_CTL_WKEN_Pos (23)
#define | TIMER_CTL_WKEN_Msk (0x1ul << TIMER_CTL_WKEN_Pos)
#define | TIMER_CTL_EXTCNTEN_Pos (24)
#define | TIMER_CTL_EXTCNTEN_Msk (0x1ul << TIMER_CTL_EXTCNTEN_Pos)
#define | TIMER_CTL_ACTSTS_Pos (25)
#define | TIMER_CTL_ACTSTS_Msk (0x1ul << TIMER_CTL_ACTSTS_Pos)
#define | TIMER_CTL_RSTCNT_Pos (26)
#define | TIMER_CTL_RSTCNT_Msk (0x1ul << TIMER_CTL_RSTCNT_Pos)
#define | TIMER_CTL_OPMODE_Pos (27)
#define | TIMER_CTL_OPMODE_Msk (0x3ul << TIMER_CTL_OPMODE_Pos)
#define | TIMER_CTL_INTEN_Pos (29)
#define | TIMER_CTL_INTEN_Msk (0x1ul << TIMER_CTL_INTEN_Pos)
#define | TIMER_CTL_CNTEN_Pos (30)
#define | TIMER_CTL_CNTEN_Msk (0x1ul << TIMER_CTL_CNTEN_Pos)
#define | TIMER_CTL_ICEDEBUG_Pos (31)
#define | TIMER_CTL_ICEDEBUG_Msk (0x1ul << TIMER_CTL_ICEDEBUG_Pos)
#define | TIMER_CMP_CMPDAT_Pos (0)
#define | TIMER_CMP_CMPDAT_Msk (0xfffffful << TIMER_CMP_CMPDAT_Pos)
#define | TIMER_INTSTS_TIF_Pos (0)
#define | TIMER_INTSTS_TIF_Msk (0x1ul << TIMER_INTSTS_TIF_Pos)
#define | TIMER_INTSTS_TWKF_Pos (1)
#define | TIMER_INTSTS_TWKF_Msk (0x1ul << TIMER_INTSTS_TWKF_Pos)
#define | TIMER_CNT_CNT_Pos (0)
#define | TIMER_CNT_CNT_Msk (0xfffffful << TIMER_CNT_CNT_Pos)
#define | TIMER_CAP_CAPDAT_Pos (0)
#define | TIMER_CAP_CAPDAT_Msk (0xfffffful << TIMER_CAP_CAPDAT_Pos)
#define | TIMER_EXTCTL_CNTPHASE_Pos (0)
#define | TIMER_EXTCTL_CNTPHASE_Msk (0x1ul << TIMER_EXTCTL_CNTPHASE_Pos)
#define | TIMER_EXTCTL_CAPEDGE_Pos (1)
#define | TIMER_EXTCTL_CAPEDGE_Msk (0x3ul << TIMER_EXTCTL_CAPEDGE_Pos)
#define | TIMER_EXTCTL_CAPEN_Pos (3)
#define | TIMER_EXTCTL_CAPEN_Msk (0x1ul << TIMER_EXTCTL_CAPEN_Pos)
#define | TIMER_EXTCTL_CAPFUNCS_Pos (4)
#define | TIMER_EXTCTL_CAPFUNCS_Msk (0x1ul << TIMER_EXTCTL_CAPFUNCS_Pos)
#define | TIMER_EXTCTL_CAPIEN_Pos (5)
#define | TIMER_EXTCTL_CAPIEN_Msk (0x1ul << TIMER_EXTCTL_CAPIEN_Pos)
#define | TIMER_EXTCTL_CAPDBEN_Pos (6)
#define | TIMER_EXTCTL_CAPDBEN_Msk (0x1ul << TIMER_EXTCTL_CAPDBEN_Pos)
#define | TIMER_EXTCTL_CNTDBEN_Pos (7)
#define | TIMER_EXTCTL_CNTDBEN_Msk (0x1ul << TIMER_EXTCTL_CNTDBEN_Pos)
#define | TIMER_EXTCTL_CAPSEL_Pos (8)
#define | TIMER_EXTCTL_CAPSEL_Msk (0x1ul << TIMER_EXTCTL_CAPSEL_Pos)
#define | TIMER_EXTCTL_ACMPSSEL_Pos (9)
#define | TIMER_EXTCTL_ACMPSSEL_Msk (0x1ul << TIMER_EXTCTL_ACMPSSEL_Pos)
#define | TIMER_EINTSTS_CAPIF_Pos (0)
#define | TIMER_EINTSTS_CAPIF_Msk (0x1ul << TIMER_EINTSTS_CAPIF_Pos)
#define | TIMER_CTL_PSC_Pos (0)
#define | TIMER_CTL_PSC_Msk (0xfful << TIMER_CTL_PSC_Pos)
#define | TIMER_CTL_CMPCTL_Pos (17)
#define | TIMER_CTL_CMPCTL_Msk (0x1ul << TIMER_CTL_CMPCTL_Pos)
#define | TIMER_CTL_TGLPINSEL_Pos (18)
#define | TIMER_CTL_TGLPINSEL_Msk (0x1ul << TIMER_CTL_TGLPINSEL_Pos)
#define | TIMER_CTL_CAPSRC_Pos (19)
#define | TIMER_CTL_CAPSRC_Msk (0x1ul << TIMER_CTL_CAPSRC_Pos)
#define | TIMER_CTL_WKEN_Pos (23)
#define | TIMER_CTL_WKEN_Msk (0x1ul << TIMER_CTL_WKEN_Pos)
#define | TIMER_CTL_EXTCNTEN_Pos (24)
#define | TIMER_CTL_EXTCNTEN_Msk (0x1ul << TIMER_CTL_EXTCNTEN_Pos)
#define | TIMER_CTL_ACTSTS_Pos (25)
#define | TIMER_CTL_ACTSTS_Msk (0x1ul << TIMER_CTL_ACTSTS_Pos)
#define | TIMER_CTL_RSTCNT_Pos (26)
#define | TIMER_CTL_RSTCNT_Msk (0x1ul << TIMER_CTL_RSTCNT_Pos)
#define | TIMER_CTL_OPMODE_Pos (27)
#define | TIMER_CTL_OPMODE_Msk (0x3ul << TIMER_CTL_OPMODE_Pos)
#define | TIMER_CTL_INTEN_Pos (29)
#define | TIMER_CTL_INTEN_Msk (0x1ul << TIMER_CTL_INTEN_Pos)
#define | TIMER_CTL_CNTEN_Pos (30)
#define | TIMER_CTL_CNTEN_Msk (0x1ul << TIMER_CTL_CNTEN_Pos)
#define | TIMER_CTL_ICEDEBUG_Pos (31)
#define | TIMER_CTL_ICEDEBUG_Msk (0x1ul << TIMER_CTL_ICEDEBUG_Pos)
#define | TIMER_CMP_CMPDAT_Pos (0)
#define | TIMER_CMP_CMPDAT_Msk (0xfffffful << TIMER_CMP_CMPDAT_Pos)
#define | TIMER_INTSTS_TIF_Pos (0)
#define | TIMER_INTSTS_TIF_Msk (0x1ul << TIMER_INTSTS_TIF_Pos)
#define | TIMER_INTSTS_TWKF_Pos (1)
#define | TIMER_INTSTS_TWKF_Msk (0x1ul << TIMER_INTSTS_TWKF_Pos)
#define | TIMER_CNT_CNT_Pos (0)
#define | TIMER_CNT_CNT_Msk (0xfffffful << TIMER_CNT_CNT_Pos)
#define | TIMER_CAP_CAPDAT_Pos (0)
#define | TIMER_CAP_CAPDAT_Msk (0xfffffful << TIMER_CAP_CAPDAT_Pos)
#define | TIMER_EXTCTL_CNTPHASE_Pos (0)
#define | TIMER_EXTCTL_CNTPHASE_Msk (0x1ul << TIMER_EXTCTL_CNTPHASE_Pos)
#define | TIMER_EXTCTL_CAPEDGE_Pos (1)
#define | TIMER_EXTCTL_CAPEDGE_Msk (0x3ul << TIMER_EXTCTL_CAPEDGE_Pos)
#define | TIMER_EXTCTL_CAPEN_Pos (3)
#define | TIMER_EXTCTL_CAPEN_Msk (0x1ul << TIMER_EXTCTL_CAPEN_Pos)
#define | TIMER_EXTCTL_CAPFUNCS_Pos (4)
#define | TIMER_EXTCTL_CAPFUNCS_Msk (0x1ul << TIMER_EXTCTL_CAPFUNCS_Pos)
#define | TIMER_EXTCTL_CAPIEN_Pos (5)
#define | TIMER_EXTCTL_CAPIEN_Msk (0x1ul << TIMER_EXTCTL_CAPIEN_Pos)
#define | TIMER_EXTCTL_CAPDBEN_Pos (6)
#define | TIMER_EXTCTL_CAPDBEN_Msk (0x1ul << TIMER_EXTCTL_CAPDBEN_Pos)
#define | TIMER_EXTCTL_CNTDBEN_Pos (7)
#define | TIMER_EXTCTL_CNTDBEN_Msk (0x1ul << TIMER_EXTCTL_CNTDBEN_Pos)
#define | TIMER_EXTCTL_CAPSEL_Pos (8)
#define | TIMER_EXTCTL_CAPSEL_Msk (0x1ul << TIMER_EXTCTL_CAPSEL_Pos)
#define | TIMER_EXTCTL_ACMPSSEL_Pos (9)
#define | TIMER_EXTCTL_ACMPSSEL_Msk (0x1ul << TIMER_EXTCTL_ACMPSSEL_Pos)
#define | TIMER_EINTSTS_CAPIF_Pos (0)
#define | TIMER_EINTSTS_CAPIF_Msk (0x1ul << TIMER_EINTSTS_CAPIF_Pos)
#define | UART_DAT_DAT_Pos (0)
#define | UART_DAT_DAT_Msk (0xfful << UART_DAT_DAT_Pos)
#define | UART_INTEN_RDAIEN_Pos (0)
#define | UART_INTEN_RDAIEN_Msk (0x1ul << UART_INTEN_RDAIEN_Pos)
#define | UART_INTEN_THREIEN_Pos (1)
#define | UART_INTEN_THREIEN_Msk (0x1ul << UART_INTEN_THREIEN_Pos)
#define | UART_INTEN_RLSIEN_Pos (2)
#define | UART_INTEN_RLSIEN_Msk (0x1ul << UART_INTEN_RLSIEN_Pos)
#define | UART_INTEN_MODEMIEN_Pos (3)
#define | UART_INTEN_MODEMIEN_Msk (0x1ul << UART_INTEN_MODEMIEN_Pos)
#define | UART_INTEN_RXTOIEN_Pos (4)
#define | UART_INTEN_RXTOIEN_Msk (0x1ul << UART_INTEN_RXTOIEN_Pos)
#define | UART_INTEN_BUFERRIEN_Pos (5)
#define | UART_INTEN_BUFERRIEN_Msk (0x1ul << UART_INTEN_BUFERRIEN_Pos)
#define | UART_INTEN_WKCTSIEN_Pos (9)
#define | UART_INTEN_WKCTSIEN_Msk (0x1ul << UART_INTEN_WKCTSIEN_Pos)
#define | UART_INTEN_TOCNTEN_Pos (11)
#define | UART_INTEN_TOCNTEN_Msk (0x1ul << UART_INTEN_TOCNTEN_Pos)
#define | UART_INTEN_ATORTSEN_Pos (12)
#define | UART_INTEN_ATORTSEN_Msk (0x1ul << UART_INTEN_ATORTSEN_Pos)
#define | UART_INTEN_ATOCTSEN_Pos (13)
#define | UART_INTEN_ATOCTSEN_Msk (0x1ul << UART_INTEN_ATOCTSEN_Pos)
#define | UART_FIFO_RXRST_Pos (1)
#define | UART_FIFO_RXRST_Msk (0x1ul << UART_FIFO_RXRST_Pos)
#define | UART_FIFO_TXRST_Pos (2)
#define | UART_FIFO_TXRST_Msk (0x1ul << UART_FIFO_TXRST_Pos)
#define | UART_FIFO_RFITL_Pos (4)
#define | UART_FIFO_RFITL_Msk (0xful << UART_FIFO_RFITL_Pos)
#define | UART_FIFO_RXOFF_Pos (8)
#define | UART_FIFO_RXOFF_Msk (0x1ul << UART_FIFO_RXOFF_Pos)
#define | UART_FIFO_RTSTRGLV_Pos (16)
#define | UART_FIFO_RTSTRGLV_Msk (0xful << UART_FIFO_RTSTRGLV_Pos)
#define | UART_LINE_WLS_Pos (0)
#define | UART_LINE_WLS_Msk (0x3ul << UART_LINE_WLS_Pos)
#define | UART_LINE_NSB_Pos (2)
#define | UART_LINE_NSB_Msk (0x1ul << UART_LINE_NSB_Pos)
#define | UART_LINE_PBE_Pos (3)
#define | UART_LINE_PBE_Msk (0x1ul << UART_LINE_PBE_Pos)
#define | UART_LINE_EPE_Pos (4)
#define | UART_LINE_EPE_Msk (0x1ul << UART_LINE_EPE_Pos)
#define | UART_LINE_SPE_Pos (5)
#define | UART_LINE_SPE_Msk (0x1ul << UART_LINE_SPE_Pos)
#define | UART_LINE_BCB_Pos (6)
#define | UART_LINE_BCB_Msk (0x1ul << UART_LINE_BCB_Pos)
#define | UART_MODEM_RTS_Pos (1)
#define | UART_MODEM_RTS_Msk (0x1ul << UART_MODEM_RTS_Pos)
#define | UART_MODEM_RTSACTLV_Pos (9)
#define | UART_MODEM_RTSACTLV_Msk (0x1ul << UART_MODEM_RTSACTLV_Pos)
#define | UART_MODEM_RTSSTS_Pos (13)
#define | UART_MODEM_RTSSTS_Msk (0x1ul << UART_MODEM_RTSSTS_Pos)
#define | UART_MODEMSTS_CTSDETF_Pos (0)
#define | UART_MODEMSTS_CTSDETF_Msk (0x1ul << UART_MODEMSTS_CTSDETF_Pos)
#define | UART_MODEMSTS_CTSSTS_Pos (4)
#define | UART_MODEMSTS_CTSSTS_Msk (0x1ul << UART_MODEMSTS_CTSSTS_Pos)
#define | UART_MODEMSTS_CTSACTLV_Pos (8)
#define | UART_MODEMSTS_CTSACTLV_Msk (0x1ul << UART_MODEMSTS_CTSACTLV_Pos)
#define | UART_FIFOSTS_RXOVIF_Pos (0)
#define | UART_FIFOSTS_RXOVIF_Msk (0x1ul << UART_FIFOSTS_RXOVIF_Pos)
#define | UART_FIFOSTS_ADDRDETF_Pos (3)
#define | UART_FIFOSTS_ADDRDETF_Msk (0x1ul << UART_FIFOSTS_ADDRDETF_Pos)
#define | UART_FIFOSTS_PEF_Pos (4)
#define | UART_FIFOSTS_PEF_Msk (0x1ul << UART_FIFOSTS_PEF_Pos)
#define | UART_FIFOSTS_FEF_Pos (5)
#define | UART_FIFOSTS_FEF_Msk (0x1ul << UART_FIFOSTS_FEF_Pos)
#define | UART_FIFOSTS_BIF_Pos (6)
#define | UART_FIFOSTS_BIF_Msk (0x1ul << UART_FIFOSTS_BIF_Pos)
#define | UART_FIFOSTS_RXPTR_Pos (8)
#define | UART_FIFOSTS_RXPTR_Msk (0x3ful << UART_FIFOSTS_RXPTR_Pos)
#define | UART_FIFOSTS_RXEMPTY_Pos (14)
#define | UART_FIFOSTS_RXEMPTY_Msk (0x1ul << UART_FIFOSTS_RXEMPTY_Pos)
#define | UART_FIFOSTS_RXFULL_Pos (15)
#define | UART_FIFOSTS_RXFULL_Msk (0x1ul << UART_FIFOSTS_RXFULL_Pos)
#define | UART_FIFOSTS_TXPTR_Pos (16)
#define | UART_FIFOSTS_TXPTR_Msk (0x3ful << UART_FIFOSTS_TXPTR_Pos)
#define | UART_FIFOSTS_TXEMPTY_Pos (22)
#define | UART_FIFOSTS_TXEMPTY_Msk (0x1ul << UART_FIFOSTS_TXEMPTY_Pos)
#define | UART_FIFOSTS_TXFULL_Pos (23)
#define | UART_FIFOSTS_TXFULL_Msk (0x1ul << UART_FIFOSTS_TXFULL_Pos)
#define | UART_FIFOSTS_TXOVIF_Pos (24)
#define | UART_FIFOSTS_TXOVIF_Msk (0x1ul << UART_FIFOSTS_TXOVIF_Pos)
#define | UART_FIFOSTS_TXEMPTYF_Pos (28)
#define | UART_FIFOSTS_TXEMPTYF_Msk (0x1ul << UART_FIFOSTS_TXEMPTYF_Pos)
#define | UART_INTSTS_RDAIF_Pos (0)
#define | UART_INTSTS_RDAIF_Msk (0x1ul << UART_INTSTS_RDAIF_Pos)
#define | UART_INTSTS_THREIF_Pos (1)
#define | UART_INTSTS_THREIF_Msk (0x1ul << UART_INTSTS_THREIF_Pos)
#define | UART_INTSTS_RLSIF_Pos (2)
#define | UART_INTSTS_RLSIF_Msk (0x1ul << UART_INTSTS_RLSIF_Pos)
#define | UART_INTSTS_MODEMIF_Pos (3)
#define | UART_INTSTS_MODEMIF_Msk (0x1ul << UART_INTSTS_MODEMIF_Pos)
#define | UART_INTSTS_RXTOIF_Pos (4)
#define | UART_INTSTS_RXTOIF_Msk (0x1ul << UART_INTSTS_RXTOIF_Pos)
#define | UART_INTSTS_BUFERRIF_Pos (5)
#define | UART_INTSTS_BUFERRIF_Msk (0x1ul << UART_INTSTS_BUFERRIF_Pos)
#define | UART_INTSTS_RDAINT_Pos (8)
#define | UART_INTSTS_RDAINT_Msk (0x1ul << UART_INTSTS_RDAINT_Pos)
#define | UART_INTSTS_THREINT_Pos (9)
#define | UART_INTSTS_THREINT_Msk (0x1ul << UART_INTSTS_THREINT_Pos)
#define | UART_INTSTS_RLSINT_Pos (10)
#define | UART_INTSTS_RLSINT_Msk (0x1ul << UART_INTSTS_RLSINT_Pos)
#define | UART_INTSTS_MODEMINT_Pos (11)
#define | UART_INTSTS_MODEMINT_Msk (0x1ul << UART_INTSTS_MODEMINT_Pos)
#define | UART_INTSTS_RXTOINT_Pos (12)
#define | UART_INTSTS_RXTOINT_Msk (0x1ul << UART_INTSTS_RXTOINT_Pos)
#define | UART_INTSTS_BUFERRINT_Pos (13)
#define | UART_INTSTS_BUFERRINT_Msk (0x1ul << UART_INTSTS_BUFERRINT_Pos)
#define | UART_INTSTS_CTSWKIF_Pos (16)
#define | UART_INTSTS_CTSWKIF_Msk (0x1ul << UART_INTSTS_CTSWKIF_Pos)
#define | UART_TOUT_TOIC_Pos (0)
#define | UART_TOUT_TOIC_Msk (0xfful << UART_TOUT_TOIC_Pos)
#define | UART_TOUT_DLY_Pos (8)
#define | UART_TOUT_DLY_Msk (0xfful << UART_TOUT_DLY_Pos)
#define | UART_BAUD_BRD_Pos (0)
#define | UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)
#define | UART_BAUD_EDIVM1_Pos (24)
#define | UART_BAUD_EDIVM1_Msk (0xful << UART_BAUD_EDIVM1_Pos)
#define | UART_BAUD_BAUDM0_Pos (28)
#define | UART_BAUD_BAUDM0_Msk (0x1ul << UART_BAUD_BAUDM0_Pos)
#define | UART_BAUD_BAUDM1_Pos (29)
#define | UART_BAUD_BAUDM1_Msk (0x1ul << UART_BAUD_BAUDM1_Pos)
#define | UART_IRDA_TXEN_Pos (1)
#define | UART_IRDA_TXEN_Msk (0x1ul << UART_IRDA_TXEN_Pos)
#define | UART_IRDA_TXINV_Pos (5)
#define | UART_IRDA_TXINV_Msk (0x1ul << UART_IRDA_TXINV_Pos)
#define | UART_IRDA_RXINV_Pos (6)
#define | UART_IRDA_RXINV_Msk (0x1ul << UART_IRDA_RXINV_Pos)
#define | UART_ALTCTL_RS485_NMM_Pos (8)
#define | UART_ALTCTL_RS485_NMM_Msk (0x1ul << UART_ALTCTL_RS485_NMM_Pos)
#define | UART_ALTCTL_RS485_AAD_Pos (9)
#define | UART_ALTCTL_RS485_AAD_Msk (0x1ul << UART_ALTCTL_RS485_AAD_Pos)
#define | UART_ALTCTL_RS485_AUD_Pos (10)
#define | UART_ALTCTL_RS485_AUD_Msk (0x1ul << UART_ALTCTL_RS485_AUD_Pos)
#define | UART_ALTCTL_ADDRDEN_Pos (15)
#define | UART_ALTCTL_ADDRDEN_Msk (0x1ul << UART_ALTCTL_ADDRDEN_Pos)
#define | UART_ALTCTL_ADDRMV_Pos (24)
#define | UART_ALTCTL_ADDRMV_Msk (0xfful << UART_ALTCTL_ADDRMV_Pos)
#define | UART_FUNSEL_FUN_SEL_Pos (0)
#define | UART_FUNSEL_FUN_SEL_Msk (0x3ul << UART_FUNSEL_FUN_SEL_Pos)
#define | WDT_CTL_RSTCNT_Pos (0)
#define | WDT_CTL_RSTCNT_Msk (0x1ul << WDT_CTL_RSTCNT_Pos)
#define | WDT_CTL_RSTEN_Pos (1)
#define | WDT_CTL_RSTEN_Msk (0x1ul << WDT_CTL_RSTEN_Pos)
#define | WDT_CTL_RSTF_Pos (2)
#define | WDT_CTL_RSTF_Msk (0x1ul << WDT_CTL_RSTF_Pos)
#define | WDT_CTL_IF_Pos (3)
#define | WDT_CTL_IF_Msk (0x1ul << WDT_CTL_IF_Pos)
#define | WDT_CTL_WKEN_Pos (4)
#define | WDT_CTL_WKEN_Msk (0x1ul << WDT_CTL_WKEN_Pos)
#define | WDT_CTL_WKF_Pos (5)
#define | WDT_CTL_WKF_Msk (0x1ul << WDT_CTL_WKF_Pos)
#define | WDT_CTL_INTEN_Pos (6)
#define | WDT_CTL_INTEN_Msk (0x1ul << WDT_CTL_INTEN_Pos)
#define | WDT_CTL_WDTEN_Pos (7)
#define | WDT_CTL_WDTEN_Msk (0x1ul << WDT_CTL_WDTEN_Pos)
#define | WDT_CTL_TOUTSEL_Pos (8)
#define | WDT_CTL_TOUTSEL_Msk (0x7ul << WDT_CTL_TOUTSEL_Pos)
#define | WDT_CTL_ICEDEBUG_Pos (31)
#define | WDT_CTL_ICEDEBUG_Msk (0x1ul << WDT_CTL_ICEDEBUG_Pos)
#define | WDT_ALTCTL_RSTDSEL_Pos (0)
#define | WDT_ALTCTL_RSTDSEL_Msk (0x3ul << WDT_ALTCTL_RSTDSEL_Pos)
#define | WWDT_RLDCNT_RLDCNT_Pos (0)
#define | WWDT_RLDCNT_RLDCNT_Msk (0xfffffffful << WWDT_RLDCNT_RLDCNT_Pos)
#define | WWDT_CTL_WWDTEN_Pos (0)
#define | WWDT_CTL_WWDTEN_Msk (0x1ul << WWDT_CTL_WWDTEN_Pos)
#define | WWDT_CTL_INTEN_Pos (1)
#define | WWDT_CTL_INTEN_Msk (0x1ul << WWDT_CTL_INTEN_Pos)
#define | WWDT_CTL_PSCSEL_Pos (8)
#define | WWDT_CTL_PSCSEL_Msk (0xful << WWDT_CTL_PSCSEL_Pos)
#define | WWDT_CTL_CMPDAT_Pos (16)
#define | WWDT_CTL_CMPDAT_Msk (0x3ful << WWDT_CTL_CMPDAT_Pos)
#define | WWDT_CTL_ICEDEBUG_Pos (31)
#define | WWDT_CTL_ICEDEBUG_Msk (0x1ul << WWDT_CTL_ICEDEBUG_Pos)
#define | WWDT_STATUS_WWDTIF_Pos (0)
#define | WWDT_STATUS_WWDTIF_Msk (0x1ul << WWDT_STATUS_WWDTIF_Pos)
#define | WWDT_STATUS_WWDTRF_Pos (1)
#define | WWDT_STATUS_WWDTRF_Msk (0x1ul << WWDT_STATUS_WWDTRF_Pos)
#define | WWDT_CNT_CNTDAT_Pos (0)
#define | WWDT_CNT_CNTDAT_Msk (0x3ful << WWDT_CNT_CNTDAT_Pos)

## Typedefs
typedef enum IRQn | IRQn_Type
typedef volatile unsigned char | vu8
| Define 8-bit unsigned volatile data type. More...
typedef volatile unsigned short | vu16
| Define 16-bit unsigned volatile data type. More...
typedef volatile unsigned long | vu32
| Define 32-bit unsigned volatile data type. More...

## Enumerations
enum | IRQn { NonMaskableInt_IRQn = -14 , HardFault_IRQn = -13 , SVCall_IRQn = -5 , PendSV_IRQn = -2 , SysTick_IRQn = -1 , BOD_IRQn = 0 , WDT_IRQn = 1 , EINT0_IRQn = 2 , EINT1_IRQn = 3 , GPIO01_IRQn = 4 , GPIO234_IRQn = 5 , PWM_IRQn = 6 , FB_IRQn = 7 , TMR0_IRQn = 8 , TMR1_IRQn = 9 , UART0_IRQn = 12 , UART1_IRQn = 13 , SPI_IRQn = 14 , GPIO5_IRQn = 16 , HIRC_IRQn = 17 , I2C0_IRQn = 18 , I2C1_IRQn = 19 , ACMP_IRQn = 25 , PDWU_IRQn = 28 , ADC_IRQn = 29 }

## Detailed Description

Mini58 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini58 series MCU.

Version
  V1.00

Revision
  36

Date
  16/06/08 1:31p

Note
  Copyright (C) 2022 Nuvoton Technology Corp. All rights reserved.

Definition in file Mini58Series.h.

## Macro Definition Documentation

## ◆ FMC_DFBA_DFBA_Msk

#define FMC_DFBA_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)

FMC_T::DFBA: DFBA Mask

Definition at line 1573 of file Mini58Series.h.

## ◆ FMC_DFBA_DFBA_Pos

#define FMC_DFBA_DFBA_Pos (0)

FMC_T::DFBA: DFBA Position

Definition at line 1572 of file Mini58Series.h.

## ◆ FMC_FATCTL_FOM_Msk

#define FMC_FATCTL_FOM_Msk (0x7ul << FMC_FATCTL_FOM_Pos)

FMC_T::FATCTL: FOM Mask

Definition at line 1576 of file Mini58Series.h.

## ◆ FMC_FATCTL_FOM_Pos

#define FMC_FATCTL_FOM_Pos (4)

FMC_T::FATCTL: FOM Position

Definition at line 1575 of file Mini58Series.h.

## ◆ FMC_ISPADDR_ISPADDR_Msk

#define FMC_ISPADDR_ISPADDR_Msk (0xfffffffful << FMC_ISPADDR_ISPADDR_Pos)

FMC_T::ISPADDR: ISPADDR Mask

Definition at line 1561 of file Mini58Series.h.

## ◆ FMC_ISPADDR_ISPADDR_Pos

#define FMC_ISPADDR_ISPADDR_Pos (0)

FMC_T::ISPADDR: ISPADDR Position

Definition at line 1560 of file Mini58Series.h.

## ◆ FMC_ISPCMD_CMD_Msk

#define FMC_ISPCMD_CMD_Msk (0x7ful << FMC_ISPCMD_CMD_Pos)

FMC_T::ISPCMD: CMD Mask

Definition at line 1567 of file Mini58Series.h.

## ◆ FMC_ISPCMD_CMD_Pos

#define FMC_ISPCMD_CMD_Pos (0)

FMC_T::ISPCMD: CMD Position

Definition at line 1566 of file Mini58Series.h.

## ◆ FMC_ISPCTL_APUEN_Msk

#define FMC_ISPCTL_APUEN_Msk (0x1ul << FMC_ISPCTL_APUEN_Pos)

FMC_T::ISPCTL: APUEN Mask

Definition at line 1549 of file Mini58Series.h.

## ◆ FMC_ISPCTL_APUEN_Pos

#define FMC_ISPCTL_APUEN_Pos (3)

FMC_T::ISPCTL: APUEN Position

Definition at line 1548 of file Mini58Series.h.

## ◆ FMC_ISPCTL_BS_Msk

#define FMC_ISPCTL_BS_Msk (0x1ul << FMC_ISPCTL_BS_Pos)

FMC_T::ISPCTL: BS Mask

Definition at line 1543 of file Mini58Series.h.

## ◆ FMC_ISPCTL_BS_Pos

#define FMC_ISPCTL_BS_Pos (1)

FMC_T::ISPCTL: BS Position

Definition at line 1542 of file Mini58Series.h.

## ◆ FMC_ISPCTL_CFGUEN_Msk

#define FMC_ISPCTL_CFGUEN_Msk (0x1ul << FMC_ISPCTL_CFGUEN_Pos)

FMC_T::ISPCTL: CFGUEN Mask

Definition at line 1552 of file Mini58Series.h.

## ◆ FMC_ISPCTL_CFGUEN_Pos

#define FMC_ISPCTL_CFGUEN_Pos (4)

FMC_T::ISPCTL: CFGUEN Position

Definition at line 1551 of file Mini58Series.h.

## ◆ FMC_ISPCTL_ISPEN_Msk

#define FMC_ISPCTL_ISPEN_Msk (0x1ul << FMC_ISPCTL_ISPEN_Pos)

FMC_T::ISPCTL: ISPEN Mask

Definition at line 1540 of file Mini58Series.h.

## ◆ FMC_ISPCTL_ISPEN_Pos

#define FMC_ISPCTL_ISPEN_Pos (0)

    @addtogroup FMC_CONST FMC Bit Field Definition
    Constant Definitions for FMC Controller

FMC_T::ISPCTL: ISPEN Position

Definition at line 1539 of file Mini58Series.h.

## ◆ FMC_ISPCTL_ISPFF_Msk

#define FMC_ISPCTL_ISPFF_Msk (0x1ul << FMC_ISPCTL_ISPFF_Pos)

FMC_T::ISPCTL: ISPFF Mask

Definition at line 1558 of file Mini58Series.h.

## ◆ FMC_ISPCTL_ISPFF_Pos

#define FMC_ISPCTL_ISPFF_Pos (6)

FMC_T::ISPCTL: ISPFF Position

Definition at line 1557 of file Mini58Series.h.

## ◆ FMC_ISPCTL_LDUEN_Msk

#define FMC_ISPCTL_LDUEN_Msk (0x1ul << FMC_ISPCTL_LDUEN_Pos)

FMC_T::ISPCTL: LDUEN Mask

Definition at line 1555 of file Mini58Series.h.

## ◆ FMC_ISPCTL_LDUEN_Pos

#define FMC_ISPCTL_LDUEN_Pos (5)

FMC_T::ISPCTL: LDUEN Position

Definition at line 1554 of file Mini58Series.h.

## ◆ FMC_ISPCTL_SPUEN_Msk

#define FMC_ISPCTL_SPUEN_Msk (0x1ul << FMC_ISPCTL_SPUEN_Pos)

FMC_T::ISPCTL: SPUEN Mask

Definition at line 1546 of file Mini58Series.h.

## ◆ FMC_ISPCTL_SPUEN_Pos

#define FMC_ISPCTL_SPUEN_Pos (2)

FMC_T::ISPCTL: SPUEN Position

Definition at line 1545 of file Mini58Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Msk

#define FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)

FMC_T::ISPDAT: ISPDAT Mask

Definition at line 1564 of file Mini58Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Pos

#define FMC_ISPDAT_ISPDAT_Pos (0)

FMC_T::ISPDAT: ISPDAT Position

Definition at line 1563 of file Mini58Series.h.

## ◆ FMC_ISPSTS_CBS_Msk

#define FMC_ISPSTS_CBS_Msk (0x3ul << FMC_ISPSTS_CBS_Pos)

FMC_T::ISPSTS: CBS Mask

Definition at line 1582 of file Mini58Series.h.

## ◆ FMC_ISPSTS_CBS_Pos

#define FMC_ISPSTS_CBS_Pos (1)

FMC_T::ISPSTS: CBS Position

Definition at line 1581 of file Mini58Series.h.

## ◆ FMC_ISPSTS_ISPBUSY_Msk

#define FMC_ISPSTS_ISPBUSY_Msk (0x1ul << FMC_ISPSTS_ISPBUSY_Pos)

FMC_T::ISPSTS: ISPBUSY Mask

Definition at line 1579 of file Mini58Series.h.

## ◆ FMC_ISPSTS_ISPBUSY_Pos

#define FMC_ISPSTS_ISPBUSY_Pos (0)

FMC_T::ISPSTS: ISPBUSY Position

Definition at line 1578 of file Mini58Series.h.

## ◆ FMC_ISPSTS_ISPFF_Msk

#define FMC_ISPSTS_ISPFF_Msk (0x1ul << FMC_ISPSTS_ISPFF_Pos)

FMC_T::ISPSTS: ISPFF Mask

Definition at line 1585 of file Mini58Series.h.

## ◆ FMC_ISPSTS_ISPFF_Pos

#define FMC_ISPSTS_ISPFF_Pos (6)

FMC_T::ISPSTS: ISPFF Position

Definition at line 1584 of file Mini58Series.h.

## ◆ FMC_ISPSTS_SCODE_Msk

#define FMC_ISPSTS_SCODE_Msk (0x1ul << FMC_ISPSTS_SCODE_Pos)

FMC_T::ISPSTS: SCODE Mask

Definition at line 1591 of file Mini58Series.h.

## ◆ FMC_ISPSTS_SCODE_Pos

#define FMC_ISPSTS_SCODE_Pos (31)

FMC_T::ISPSTS: SCODE Position

Definition at line 1590 of file Mini58Series.h.

## ◆ FMC_ISPSTS_VECMAP_Msk

#define FMC_ISPSTS_VECMAP_Msk (0xffful << FMC_ISPSTS_VECMAP_Pos)

FMC_T::ISPSTS: VECMAP Mask

Definition at line 1588 of file Mini58Series.h.

## ◆ FMC_ISPSTS_VECMAP_Pos

#define FMC_ISPSTS_VECMAP_Pos (9)

FMC_T::ISPSTS: VECMAP Position

Definition at line 1587 of file Mini58Series.h.

## ◆ FMC_ISPTRG_ISPGO_Msk

#define FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)

FMC_T::ISPTRG: ISPGO Mask

Definition at line 1570 of file Mini58Series.h.

## ◆ FMC_ISPTRG_ISPGO_Pos

#define FMC_ISPTRG_ISPGO_Pos (0)

FMC_T::ISPTRG: ISPGO Position

Definition at line 1569 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk [1/6]

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GP_T::DATMSK: DATMSK0 Mask

Definition at line 4341 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk [2/6]

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GP_T::DATMSK: DATMSK0 Mask

Definition at line 4341 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk [3/6]

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GP_T::DATMSK: DATMSK0 Mask

Definition at line 4341 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk [4/6]

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GP_T::DATMSK: DATMSK0 Mask

Definition at line 4341 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk [5/6]

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GP_T::DATMSK: DATMSK0 Mask

Definition at line 4341 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk [6/6]

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GP_T::DATMSK: DATMSK0 Mask

Definition at line 4341 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos [1/6]

#define GP_DATMSK_DATMSK0_Pos (0)

GP_T::DATMSK: DATMSK0 Position

Definition at line 4340 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos [2/6]

#define GP_DATMSK_DATMSK0_Pos (0)

GP_T::DATMSK: DATMSK0 Position

Definition at line 4340 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos [3/6]

#define GP_DATMSK_DATMSK0_Pos (0)

GP_T::DATMSK: DATMSK0 Position

Definition at line 4340 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos [4/6]

#define GP_DATMSK_DATMSK0_Pos (0)

GP_T::DATMSK: DATMSK0 Position

Definition at line 4340 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos [5/6]

#define GP_DATMSK_DATMSK0_Pos (0)

GP_T::DATMSK: DATMSK0 Position

Definition at line 4340 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos [6/6]

#define GP_DATMSK_DATMSK0_Pos (0)

GP_T::DATMSK: DATMSK0 Position

Definition at line 4340 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk [1/6]

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GP_T::DATMSK: DATMSK1 Mask

Definition at line 4344 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk [2/6]

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GP_T::DATMSK: DATMSK1 Mask

Definition at line 4344 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk [3/6]

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GP_T::DATMSK: DATMSK1 Mask

Definition at line 4344 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk [4/6]

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GP_T::DATMSK: DATMSK1 Mask

Definition at line 4344 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk [5/6]

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GP_T::DATMSK: DATMSK1 Mask

Definition at line 4344 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk [6/6]

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GP_T::DATMSK: DATMSK1 Mask

Definition at line 4344 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos [1/6]

#define GP_DATMSK_DATMSK1_Pos (1)

GP_T::DATMSK: DATMSK1 Position

Definition at line 4343 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos [2/6]

#define GP_DATMSK_DATMSK1_Pos (1)

GP_T::DATMSK: DATMSK1 Position

Definition at line 4343 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos [3/6]

#define GP_DATMSK_DATMSK1_Pos (1)

GP_T::DATMSK: DATMSK1 Position

Definition at line 4343 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos [4/6]

#define GP_DATMSK_DATMSK1_Pos (1)

GP_T::DATMSK: DATMSK1 Position

Definition at line 4343 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos [5/6]

#define GP_DATMSK_DATMSK1_Pos (1)

GP_T::DATMSK: DATMSK1 Position

Definition at line 4343 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos [6/6]

#define GP_DATMSK_DATMSK1_Pos (1)

GP_T::DATMSK: DATMSK1 Position

Definition at line 4343 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk [1/6]

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GP_T::DATMSK: DATMSK2 Mask

Definition at line 4347 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk [2/6]

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GP_T::DATMSK: DATMSK2 Mask

Definition at line 4347 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk [3/6]

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GP_T::DATMSK: DATMSK2 Mask

Definition at line 4347 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk [4/6]

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GP_T::DATMSK: DATMSK2 Mask

Definition at line 4347 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk [5/6]

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GP_T::DATMSK: DATMSK2 Mask

Definition at line 4347 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk [6/6]

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GP_T::DATMSK: DATMSK2 Mask

Definition at line 4347 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos [1/6]

#define GP_DATMSK_DATMSK2_Pos (2)

GP_T::DATMSK: DATMSK2 Position

Definition at line 4346 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos [2/6]

#define GP_DATMSK_DATMSK2_Pos (2)

GP_T::DATMSK: DATMSK2 Position

Definition at line 4346 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos [3/6]

#define GP_DATMSK_DATMSK2_Pos (2)

GP_T::DATMSK: DATMSK2 Position

Definition at line 4346 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos [4/6]

#define GP_DATMSK_DATMSK2_Pos (2)

GP_T::DATMSK: DATMSK2 Position

Definition at line 4346 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos [5/6]

#define GP_DATMSK_DATMSK2_Pos (2)

GP_T::DATMSK: DATMSK2 Position

Definition at line 4346 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos [6/6]

#define GP_DATMSK_DATMSK2_Pos (2)

GP_T::DATMSK: DATMSK2 Position

Definition at line 4346 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk [1/6]

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GP_T::DATMSK: DATMSK3 Mask

Definition at line 4350 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk [2/6]

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GP_T::DATMSK: DATMSK3 Mask

Definition at line 4350 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk [3/6]

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GP_T::DATMSK: DATMSK3 Mask

Definition at line 4350 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk [4/6]

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GP_T::DATMSK: DATMSK3 Mask

Definition at line 4350 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk [5/6]

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GP_T::DATMSK: DATMSK3 Mask

Definition at line 4350 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk [6/6]

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GP_T::DATMSK: DATMSK3 Mask

Definition at line 4350 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos [1/6]

#define GP_DATMSK_DATMSK3_Pos (3)

GP_T::DATMSK: DATMSK3 Position

Definition at line 4349 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos [2/6]

#define GP_DATMSK_DATMSK3_Pos (3)

GP_T::DATMSK: DATMSK3 Position

Definition at line 4349 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos [3/6]

#define GP_DATMSK_DATMSK3_Pos (3)

GP_T::DATMSK: DATMSK3 Position

Definition at line 4349 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos [4/6]

#define GP_DATMSK_DATMSK3_Pos (3)

GP_T::DATMSK: DATMSK3 Position

Definition at line 4349 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos [5/6]

#define GP_DATMSK_DATMSK3_Pos (3)

GP_T::DATMSK: DATMSK3 Position

Definition at line 4349 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos [6/6]

#define GP_DATMSK_DATMSK3_Pos (3)

GP_T::DATMSK: DATMSK3 Position

Definition at line 4349 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk [1/6]

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GP_T::DATMSK: DATMSK4 Mask

Definition at line 4353 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk [2/6]

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GP_T::DATMSK: DATMSK4 Mask

Definition at line 4353 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk [3/6]

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GP_T::DATMSK: DATMSK4 Mask

Definition at line 4353 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk [4/6]

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GP_T::DATMSK: DATMSK4 Mask

Definition at line 4353 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk [5/6]

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GP_T::DATMSK: DATMSK4 Mask

Definition at line 4353 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk [6/6]

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GP_T::DATMSK: DATMSK4 Mask

Definition at line 4353 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos [1/6]

#define GP_DATMSK_DATMSK4_Pos (4)

GP_T::DATMSK: DATMSK4 Position

Definition at line 4352 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos [2/6]

#define GP_DATMSK_DATMSK4_Pos (4)

GP_T::DATMSK: DATMSK4 Position

Definition at line 4352 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos [3/6]

#define GP_DATMSK_DATMSK4_Pos (4)

GP_T::DATMSK: DATMSK4 Position

Definition at line 4352 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos [4/6]

#define GP_DATMSK_DATMSK4_Pos (4)

GP_T::DATMSK: DATMSK4 Position

Definition at line 4352 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos [5/6]

#define GP_DATMSK_DATMSK4_Pos (4)

GP_T::DATMSK: DATMSK4 Position

Definition at line 4352 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos [6/6]

#define GP_DATMSK_DATMSK4_Pos (4)

GP_T::DATMSK: DATMSK4 Position

Definition at line 4352 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk [1/6]

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GP_T::DATMSK: DATMSK5 Mask

Definition at line 4356 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk [2/6]

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GP_T::DATMSK: DATMSK5 Mask

Definition at line 4356 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk [3/6]

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GP_T::DATMSK: DATMSK5 Mask

Definition at line 4356 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk [4/6]

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GP_T::DATMSK: DATMSK5 Mask

Definition at line 4356 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk [5/6]

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GP_T::DATMSK: DATMSK5 Mask

Definition at line 4356 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk [6/6]

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GP_T::DATMSK: DATMSK5 Mask

Definition at line 4356 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos [1/6]

#define GP_DATMSK_DATMSK5_Pos (5)

GP_T::DATMSK: DATMSK5 Position

Definition at line 4355 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos [2/6]

#define GP_DATMSK_DATMSK5_Pos (5)

GP_T::DATMSK: DATMSK5 Position

Definition at line 4355 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos [3/6]

#define GP_DATMSK_DATMSK5_Pos (5)

GP_T::DATMSK: DATMSK5 Position

Definition at line 4355 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos [4/6]

#define GP_DATMSK_DATMSK5_Pos (5)

GP_T::DATMSK: DATMSK5 Position

Definition at line 4355 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos [5/6]

#define GP_DATMSK_DATMSK5_Pos (5)

GP_T::DATMSK: DATMSK5 Position

Definition at line 4355 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos [6/6]

#define GP_DATMSK_DATMSK5_Pos (5)

GP_T::DATMSK: DATMSK5 Position

Definition at line 4355 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk [1/6]

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GP_T::DATMSK: DATMSK6 Mask

Definition at line 4359 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk [2/6]

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GP_T::DATMSK: DATMSK6 Mask

Definition at line 4359 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk [3/6]

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GP_T::DATMSK: DATMSK6 Mask

Definition at line 4359 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk [4/6]

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GP_T::DATMSK: DATMSK6 Mask

Definition at line 4359 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk [5/6]

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GP_T::DATMSK: DATMSK6 Mask

Definition at line 4359 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk [6/6]

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GP_T::DATMSK: DATMSK6 Mask

Definition at line 4359 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos [1/6]

#define GP_DATMSK_DATMSK6_Pos (6)

GP_T::DATMSK: DATMSK6 Position

Definition at line 4358 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos [2/6]

#define GP_DATMSK_DATMSK6_Pos (6)

GP_T::DATMSK: DATMSK6 Position

Definition at line 4358 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos [3/6]

#define GP_DATMSK_DATMSK6_Pos (6)

GP_T::DATMSK: DATMSK6 Position

Definition at line 4358 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos [4/6]

#define GP_DATMSK_DATMSK6_Pos (6)

GP_T::DATMSK: DATMSK6 Position

Definition at line 4358 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos [5/6]

#define GP_DATMSK_DATMSK6_Pos (6)

GP_T::DATMSK: DATMSK6 Position

Definition at line 4358 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos [6/6]

#define GP_DATMSK_DATMSK6_Pos (6)

GP_T::DATMSK: DATMSK6 Position

Definition at line 4358 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk [1/6]

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GP_T::DATMSK: DATMSK7 Mask

Definition at line 4362 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk [2/6]

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GP_T::DATMSK: DATMSK7 Mask

Definition at line 4362 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk [3/6]

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GP_T::DATMSK: DATMSK7 Mask

Definition at line 4362 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk [4/6]

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GP_T::DATMSK: DATMSK7 Mask

Definition at line 4362 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk [5/6]

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GP_T::DATMSK: DATMSK7 Mask

Definition at line 4362 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk [6/6]

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GP_T::DATMSK: DATMSK7 Mask

Definition at line 4362 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos [1/6]

#define GP_DATMSK_DATMSK7_Pos (7)

GP_T::DATMSK: DATMSK7 Position

Definition at line 4361 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos [2/6]

#define GP_DATMSK_DATMSK7_Pos (7)

GP_T::DATMSK: DATMSK7 Position

Definition at line 4361 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos [3/6]

#define GP_DATMSK_DATMSK7_Pos (7)

GP_T::DATMSK: DATMSK7 Position

Definition at line 4361 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos [4/6]

#define GP_DATMSK_DATMSK7_Pos (7)

GP_T::DATMSK: DATMSK7 Position

Definition at line 4361 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos [5/6]

#define GP_DATMSK_DATMSK7_Pos (7)

GP_T::DATMSK: DATMSK7 Position

Definition at line 4361 of file Mini58Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos [6/6]

#define GP_DATMSK_DATMSK7_Pos (7)

GP_T::DATMSK: DATMSK7 Position

Definition at line 4361 of file Mini58Series.h.

## ◆ GP_DBCTL_DBCLKSEL_Msk

#define GP_DBCTL_DBCLKSEL_Msk (0xful << GP_DBCTL_DBCLKSEL_Pos)

GP_T::DBCTL: DBCLKSEL Mask

Definition at line 4533 of file Mini58Series.h.

## ◆ GP_DBCTL_DBCLKSEL_Pos

#define GP_DBCTL_DBCLKSEL_Pos (0)

GP_T::DBCTL: DBCLKSEL Position

Definition at line 4532 of file Mini58Series.h.

## ◆ GP_DBCTL_DBCLKSRC_Msk

#define GP_DBCTL_DBCLKSRC_Msk (0x1ul << GP_DBCTL_DBCLKSRC_Pos)

GP_T::DBCTL: DBCLKSRC Mask

Definition at line 4536 of file Mini58Series.h.

## ◆ GP_DBCTL_DBCLKSRC_Pos

#define GP_DBCTL_DBCLKSRC_Pos (4)

GP_T::DBCTL: DBCLKSRC Position

Definition at line 4535 of file Mini58Series.h.

## ◆ GP_DBCTL_ICLKON_Msk

#define GP_DBCTL_ICLKON_Msk (0x1ul << GP_DBCTL_ICLKON_Pos)

GP_T::DBCTL: ICLKON Mask

Definition at line 4539 of file Mini58Series.h.

## ◆ GP_DBCTL_ICLKON_Pos

#define GP_DBCTL_ICLKON_Pos (5)

GP_T::DBCTL: ICLKON Position

Definition at line 4538 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Msk [1/6]

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GP_T::DBEN: DBEN0 Mask

Definition at line 4389 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Msk [2/6]

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GP_T::DBEN: DBEN0 Mask

Definition at line 4389 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Msk [3/6]

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GP_T::DBEN: DBEN0 Mask

Definition at line 4389 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Msk [4/6]

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GP_T::DBEN: DBEN0 Mask

Definition at line 4389 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Msk [5/6]

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GP_T::DBEN: DBEN0 Mask

Definition at line 4389 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Msk [6/6]

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GP_T::DBEN: DBEN0 Mask

Definition at line 4389 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Pos [1/6]

#define GP_DBEN_DBEN0_Pos (0)

GP_T::DBEN: DBEN0 Position

Definition at line 4388 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Pos [2/6]

#define GP_DBEN_DBEN0_Pos (0)

GP_T::DBEN: DBEN0 Position

Definition at line 4388 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Pos [3/6]

#define GP_DBEN_DBEN0_Pos (0)

GP_T::DBEN: DBEN0 Position

Definition at line 4388 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Pos [4/6]

#define GP_DBEN_DBEN0_Pos (0)

GP_T::DBEN: DBEN0 Position

Definition at line 4388 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Pos [5/6]

#define GP_DBEN_DBEN0_Pos (0)

GP_T::DBEN: DBEN0 Position

Definition at line 4388 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN0_Pos [6/6]

#define GP_DBEN_DBEN0_Pos (0)

GP_T::DBEN: DBEN0 Position

Definition at line 4388 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Msk [1/6]

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GP_T::DBEN: DBEN1 Mask

Definition at line 4392 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Msk [2/6]

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GP_T::DBEN: DBEN1 Mask

Definition at line 4392 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Msk [3/6]

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GP_T::DBEN: DBEN1 Mask

Definition at line 4392 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Msk [4/6]

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GP_T::DBEN: DBEN1 Mask

Definition at line 4392 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Msk [5/6]

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GP_T::DBEN: DBEN1 Mask

Definition at line 4392 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Msk [6/6]

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GP_T::DBEN: DBEN1 Mask

Definition at line 4392 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Pos [1/6]

#define GP_DBEN_DBEN1_Pos (1)

GP_T::DBEN: DBEN1 Position

Definition at line 4391 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Pos [2/6]

#define GP_DBEN_DBEN1_Pos (1)

GP_T::DBEN: DBEN1 Position

Definition at line 4391 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Pos [3/6]

#define GP_DBEN_DBEN1_Pos (1)

GP_T::DBEN: DBEN1 Position

Definition at line 4391 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Pos [4/6]

#define GP_DBEN_DBEN1_Pos (1)

GP_T::DBEN: DBEN1 Position

Definition at line 4391 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Pos [5/6]

#define GP_DBEN_DBEN1_Pos (1)

GP_T::DBEN: DBEN1 Position

Definition at line 4391 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN1_Pos [6/6]

#define GP_DBEN_DBEN1_Pos (1)

GP_T::DBEN: DBEN1 Position

Definition at line 4391 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Msk [1/6]

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GP_T::DBEN: DBEN2 Mask

Definition at line 4395 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Msk [2/6]

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GP_T::DBEN: DBEN2 Mask

Definition at line 4395 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Msk [3/6]

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GP_T::DBEN: DBEN2 Mask

Definition at line 4395 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Msk [4/6]

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GP_T::DBEN: DBEN2 Mask

Definition at line 4395 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Msk [5/6]

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GP_T::DBEN: DBEN2 Mask

Definition at line 4395 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Msk [6/6]

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GP_T::DBEN: DBEN2 Mask

Definition at line 4395 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Pos [1/6]

#define GP_DBEN_DBEN2_Pos (2)

GP_T::DBEN: DBEN2 Position

Definition at line 4394 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Pos [2/6]

#define GP_DBEN_DBEN2_Pos (2)

GP_T::DBEN: DBEN2 Position

Definition at line 4394 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Pos [3/6]

#define GP_DBEN_DBEN2_Pos (2)

GP_T::DBEN: DBEN2 Position

Definition at line 4394 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Pos [4/6]

#define GP_DBEN_DBEN2_Pos (2)

GP_T::DBEN: DBEN2 Position

Definition at line 4394 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Pos [5/6]

#define GP_DBEN_DBEN2_Pos (2)

GP_T::DBEN: DBEN2 Position

Definition at line 4394 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN2_Pos [6/6]

#define GP_DBEN_DBEN2_Pos (2)

GP_T::DBEN: DBEN2 Position

Definition at line 4394 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Msk [1/6]

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GP_T::DBEN: DBEN3 Mask

Definition at line 4398 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Msk [2/6]

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GP_T::DBEN: DBEN3 Mask

Definition at line 4398 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Msk [3/6]

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GP_T::DBEN: DBEN3 Mask

Definition at line 4398 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Msk [4/6]

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GP_T::DBEN: DBEN3 Mask

Definition at line 4398 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Msk [5/6]

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GP_T::DBEN: DBEN3 Mask

Definition at line 4398 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Msk [6/6]

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GP_T::DBEN: DBEN3 Mask

Definition at line 4398 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Pos [1/6]

#define GP_DBEN_DBEN3_Pos (3)

GP_T::DBEN: DBEN3 Position

Definition at line 4397 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Pos [2/6]

#define GP_DBEN_DBEN3_Pos (3)

GP_T::DBEN: DBEN3 Position

Definition at line 4397 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Pos [3/6]

#define GP_DBEN_DBEN3_Pos (3)

GP_T::DBEN: DBEN3 Position

Definition at line 4397 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Pos [4/6]

#define GP_DBEN_DBEN3_Pos (3)

GP_T::DBEN: DBEN3 Position

Definition at line 4397 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Pos [5/6]

#define GP_DBEN_DBEN3_Pos (3)

GP_T::DBEN: DBEN3 Position

Definition at line 4397 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN3_Pos [6/6]

#define GP_DBEN_DBEN3_Pos (3)

GP_T::DBEN: DBEN3 Position

Definition at line 4397 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Msk [1/6]

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GP_T::DBEN: DBEN4 Mask

Definition at line 4401 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Msk [2/6]

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GP_T::DBEN: DBEN4 Mask

Definition at line 4401 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Msk [3/6]

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GP_T::DBEN: DBEN4 Mask

Definition at line 4401 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Msk [4/6]

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GP_T::DBEN: DBEN4 Mask

Definition at line 4401 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Msk [5/6]

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GP_T::DBEN: DBEN4 Mask

Definition at line 4401 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Msk [6/6]

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GP_T::DBEN: DBEN4 Mask

Definition at line 4401 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Pos [1/6]

#define GP_DBEN_DBEN4_Pos (4)

GP_T::DBEN: DBEN4 Position

Definition at line 4400 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Pos [2/6]

#define GP_DBEN_DBEN4_Pos (4)

GP_T::DBEN: DBEN4 Position

Definition at line 4400 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Pos [3/6]

#define GP_DBEN_DBEN4_Pos (4)

GP_T::DBEN: DBEN4 Position

Definition at line 4400 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Pos [4/6]

#define GP_DBEN_DBEN4_Pos (4)

GP_T::DBEN: DBEN4 Position

Definition at line 4400 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Pos [5/6]

#define GP_DBEN_DBEN4_Pos (4)

GP_T::DBEN: DBEN4 Position

Definition at line 4400 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN4_Pos [6/6]

#define GP_DBEN_DBEN4_Pos (4)

GP_T::DBEN: DBEN4 Position

Definition at line 4400 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Msk [1/6]

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GP_T::DBEN: DBEN5 Mask

Definition at line 4404 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Msk [2/6]

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GP_T::DBEN: DBEN5 Mask

Definition at line 4404 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Msk [3/6]

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GP_T::DBEN: DBEN5 Mask

Definition at line 4404 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Msk [4/6]

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GP_T::DBEN: DBEN5 Mask

Definition at line 4404 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Msk [5/6]

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GP_T::DBEN: DBEN5 Mask

Definition at line 4404 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Msk [6/6]

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GP_T::DBEN: DBEN5 Mask

Definition at line 4404 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Pos [1/6]

#define GP_DBEN_DBEN5_Pos (5)

GP_T::DBEN: DBEN5 Position

Definition at line 4403 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Pos [2/6]

#define GP_DBEN_DBEN5_Pos (5)

GP_T::DBEN: DBEN5 Position

Definition at line 4403 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Pos [3/6]

#define GP_DBEN_DBEN5_Pos (5)

GP_T::DBEN: DBEN5 Position

Definition at line 4403 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Pos [4/6]

#define GP_DBEN_DBEN5_Pos (5)

GP_T::DBEN: DBEN5 Position

Definition at line 4403 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Pos [5/6]

#define GP_DBEN_DBEN5_Pos (5)

GP_T::DBEN: DBEN5 Position

Definition at line 4403 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN5_Pos [6/6]

#define GP_DBEN_DBEN5_Pos (5)

GP_T::DBEN: DBEN5 Position

Definition at line 4403 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Msk [1/6]

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GP_T::DBEN: DBEN6 Mask

Definition at line 4407 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Msk [2/6]

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GP_T::DBEN: DBEN6 Mask

Definition at line 4407 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Msk [3/6]

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GP_T::DBEN: DBEN6 Mask

Definition at line 4407 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Msk [4/6]

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GP_T::DBEN: DBEN6 Mask

Definition at line 4407 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Msk [5/6]

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GP_T::DBEN: DBEN6 Mask

Definition at line 4407 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Msk [6/6]

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GP_T::DBEN: DBEN6 Mask

Definition at line 4407 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Pos [1/6]

#define GP_DBEN_DBEN6_Pos (6)

GP_T::DBEN: DBEN6 Position

Definition at line 4406 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Pos [2/6]

#define GP_DBEN_DBEN6_Pos (6)

GP_T::DBEN: DBEN6 Position

Definition at line 4406 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Pos [3/6]

#define GP_DBEN_DBEN6_Pos (6)

GP_T::DBEN: DBEN6 Position

Definition at line 4406 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Pos [4/6]

#define GP_DBEN_DBEN6_Pos (6)

GP_T::DBEN: DBEN6 Position

Definition at line 4406 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Pos [5/6]

#define GP_DBEN_DBEN6_Pos (6)

GP_T::DBEN: DBEN6 Position

Definition at line 4406 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN6_Pos [6/6]

#define GP_DBEN_DBEN6_Pos (6)

GP_T::DBEN: DBEN6 Position

Definition at line 4406 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Msk [1/6]

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GP_T::DBEN: DBEN7 Mask

Definition at line 4410 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Msk [2/6]

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GP_T::DBEN: DBEN7 Mask

Definition at line 4410 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Msk [3/6]

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GP_T::DBEN: DBEN7 Mask

Definition at line 4410 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Msk [4/6]

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GP_T::DBEN: DBEN7 Mask

Definition at line 4410 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Msk [5/6]

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GP_T::DBEN: DBEN7 Mask

Definition at line 4410 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Msk [6/6]

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GP_T::DBEN: DBEN7 Mask

Definition at line 4410 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Pos [1/6]

#define GP_DBEN_DBEN7_Pos (7)

GP_T::DBEN: DBEN7 Position

Definition at line 4409 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Pos [2/6]

#define GP_DBEN_DBEN7_Pos (7)

GP_T::DBEN: DBEN7 Position

Definition at line 4409 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Pos [3/6]

#define GP_DBEN_DBEN7_Pos (7)

GP_T::DBEN: DBEN7 Position

Definition at line 4409 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Pos [4/6]

#define GP_DBEN_DBEN7_Pos (7)

GP_T::DBEN: DBEN7 Position

Definition at line 4409 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Pos [5/6]

#define GP_DBEN_DBEN7_Pos (7)

GP_T::DBEN: DBEN7 Position

Definition at line 4409 of file Mini58Series.h.

## ◆ GP_DBEN_DBEN7_Pos [6/6]

#define GP_DBEN_DBEN7_Pos (7)

GP_T::DBEN: DBEN7 Position

Definition at line 4409 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk [1/6]

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GP_T::DINOFF: DINOFF0 Mask

Definition at line 4293 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk [2/6]

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GP_T::DINOFF: DINOFF0 Mask

Definition at line 4293 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk [3/6]

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GP_T::DINOFF: DINOFF0 Mask

Definition at line 4293 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk [4/6]

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GP_T::DINOFF: DINOFF0 Mask

Definition at line 4293 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk [5/6]

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GP_T::DINOFF: DINOFF0 Mask

Definition at line 4293 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk [6/6]

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GP_T::DINOFF: DINOFF0 Mask

Definition at line 4293 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos [1/6]

#define GP_DINOFF_DINOFF0_Pos (16)

GP_T::DINOFF: DINOFF0 Position

Definition at line 4292 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos [2/6]

#define GP_DINOFF_DINOFF0_Pos (16)

GP_T::DINOFF: DINOFF0 Position

Definition at line 4292 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos [3/6]

#define GP_DINOFF_DINOFF0_Pos (16)

GP_T::DINOFF: DINOFF0 Position

Definition at line 4292 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos [4/6]

#define GP_DINOFF_DINOFF0_Pos (16)

GP_T::DINOFF: DINOFF0 Position

Definition at line 4292 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos [5/6]

#define GP_DINOFF_DINOFF0_Pos (16)

GP_T::DINOFF: DINOFF0 Position

Definition at line 4292 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos [6/6]

#define GP_DINOFF_DINOFF0_Pos (16)

GP_T::DINOFF: DINOFF0 Position

Definition at line 4292 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk [1/6]

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GP_T::DINOFF: DINOFF1 Mask

Definition at line 4296 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk [2/6]

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GP_T::DINOFF: DINOFF1 Mask

Definition at line 4296 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk [3/6]

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GP_T::DINOFF: DINOFF1 Mask

Definition at line 4296 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk [4/6]

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GP_T::DINOFF: DINOFF1 Mask

Definition at line 4296 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk [5/6]

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GP_T::DINOFF: DINOFF1 Mask

Definition at line 4296 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk [6/6]

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GP_T::DINOFF: DINOFF1 Mask

Definition at line 4296 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos [1/6]

#define GP_DINOFF_DINOFF1_Pos (17)

GP_T::DINOFF: DINOFF1 Position

Definition at line 4295 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos [2/6]

#define GP_DINOFF_DINOFF1_Pos (17)

GP_T::DINOFF: DINOFF1 Position

Definition at line 4295 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos [3/6]

#define GP_DINOFF_DINOFF1_Pos (17)

GP_T::DINOFF: DINOFF1 Position

Definition at line 4295 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos [4/6]

#define GP_DINOFF_DINOFF1_Pos (17)

GP_T::DINOFF: DINOFF1 Position

Definition at line 4295 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos [5/6]

#define GP_DINOFF_DINOFF1_Pos (17)

GP_T::DINOFF: DINOFF1 Position

Definition at line 4295 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos [6/6]

#define GP_DINOFF_DINOFF1_Pos (17)

GP_T::DINOFF: DINOFF1 Position

Definition at line 4295 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk [1/6]

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GP_T::DINOFF: DINOFF2 Mask

Definition at line 4299 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk [2/6]

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GP_T::DINOFF: DINOFF2 Mask

Definition at line 4299 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk [3/6]

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GP_T::DINOFF: DINOFF2 Mask

Definition at line 4299 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk [4/6]

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GP_T::DINOFF: DINOFF2 Mask

Definition at line 4299 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk [5/6]

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GP_T::DINOFF: DINOFF2 Mask

Definition at line 4299 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk [6/6]

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GP_T::DINOFF: DINOFF2 Mask

Definition at line 4299 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos [1/6]

#define GP_DINOFF_DINOFF2_Pos (18)

GP_T::DINOFF: DINOFF2 Position

Definition at line 4298 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos [2/6]

#define GP_DINOFF_DINOFF2_Pos (18)

GP_T::DINOFF: DINOFF2 Position

Definition at line 4298 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos [3/6]

#define GP_DINOFF_DINOFF2_Pos (18)

GP_T::DINOFF: DINOFF2 Position

Definition at line 4298 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos [4/6]

#define GP_DINOFF_DINOFF2_Pos (18)

GP_T::DINOFF: DINOFF2 Position

Definition at line 4298 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos [5/6]

#define GP_DINOFF_DINOFF2_Pos (18)

GP_T::DINOFF: DINOFF2 Position

Definition at line 4298 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos [6/6]

#define GP_DINOFF_DINOFF2_Pos (18)

GP_T::DINOFF: DINOFF2 Position

Definition at line 4298 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk [1/6]

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GP_T::DINOFF: DINOFF3 Mask

Definition at line 4302 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk [2/6]

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GP_T::DINOFF: DINOFF3 Mask

Definition at line 4302 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk [3/6]

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GP_T::DINOFF: DINOFF3 Mask

Definition at line 4302 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk [4/6]

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GP_T::DINOFF: DINOFF3 Mask

Definition at line 4302 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk [5/6]

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GP_T::DINOFF: DINOFF3 Mask

Definition at line 4302 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk [6/6]

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GP_T::DINOFF: DINOFF3 Mask

Definition at line 4302 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos [1/6]

#define GP_DINOFF_DINOFF3_Pos (19)

GP_T::DINOFF: DINOFF3 Position

Definition at line 4301 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos [2/6]

#define GP_DINOFF_DINOFF3_Pos (19)

GP_T::DINOFF: DINOFF3 Position

Definition at line 4301 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos [3/6]

#define GP_DINOFF_DINOFF3_Pos (19)

GP_T::DINOFF: DINOFF3 Position

Definition at line 4301 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos [4/6]

#define GP_DINOFF_DINOFF3_Pos (19)

GP_T::DINOFF: DINOFF3 Position

Definition at line 4301 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos [5/6]

#define GP_DINOFF_DINOFF3_Pos (19)

GP_T::DINOFF: DINOFF3 Position

Definition at line 4301 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos [6/6]

#define GP_DINOFF_DINOFF3_Pos (19)

GP_T::DINOFF: DINOFF3 Position

Definition at line 4301 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk [1/6]

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GP_T::DINOFF: DINOFF4 Mask

Definition at line 4305 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk [2/6]

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GP_T::DINOFF: DINOFF4 Mask

Definition at line 4305 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk [3/6]

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GP_T::DINOFF: DINOFF4 Mask

Definition at line 4305 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk [4/6]

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GP_T::DINOFF: DINOFF4 Mask

Definition at line 4305 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk [5/6]

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GP_T::DINOFF: DINOFF4 Mask

Definition at line 4305 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk [6/6]

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GP_T::DINOFF: DINOFF4 Mask

Definition at line 4305 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos [1/6]

#define GP_DINOFF_DINOFF4_Pos (20)

GP_T::DINOFF: DINOFF4 Position

Definition at line 4304 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos [2/6]

#define GP_DINOFF_DINOFF4_Pos (20)

GP_T::DINOFF: DINOFF4 Position

Definition at line 4304 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos [3/6]

#define GP_DINOFF_DINOFF4_Pos (20)

GP_T::DINOFF: DINOFF4 Position

Definition at line 4304 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos [4/6]

#define GP_DINOFF_DINOFF4_Pos (20)

GP_T::DINOFF: DINOFF4 Position

Definition at line 4304 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos [5/6]

#define GP_DINOFF_DINOFF4_Pos (20)

GP_T::DINOFF: DINOFF4 Position

Definition at line 4304 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos [6/6]

#define GP_DINOFF_DINOFF4_Pos (20)

GP_T::DINOFF: DINOFF4 Position

Definition at line 4304 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk [1/6]

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GP_T::DINOFF: DINOFF5 Mask

Definition at line 4308 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk [2/6]

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GP_T::DINOFF: DINOFF5 Mask

Definition at line 4308 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk [3/6]

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GP_T::DINOFF: DINOFF5 Mask

Definition at line 4308 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk [4/6]

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GP_T::DINOFF: DINOFF5 Mask

Definition at line 4308 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk [5/6]

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GP_T::DINOFF: DINOFF5 Mask

Definition at line 4308 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk [6/6]

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GP_T::DINOFF: DINOFF5 Mask

Definition at line 4308 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos [1/6]

#define GP_DINOFF_DINOFF5_Pos (21)

GP_T::DINOFF: DINOFF5 Position

Definition at line 4307 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos [2/6]

#define GP_DINOFF_DINOFF5_Pos (21)

GP_T::DINOFF: DINOFF5 Position

Definition at line 4307 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos [3/6]

#define GP_DINOFF_DINOFF5_Pos (21)

GP_T::DINOFF: DINOFF5 Position

Definition at line 4307 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos [4/6]

#define GP_DINOFF_DINOFF5_Pos (21)

GP_T::DINOFF: DINOFF5 Position

Definition at line 4307 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos [5/6]

#define GP_DINOFF_DINOFF5_Pos (21)

GP_T::DINOFF: DINOFF5 Position

Definition at line 4307 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos [6/6]

#define GP_DINOFF_DINOFF5_Pos (21)

GP_T::DINOFF: DINOFF5 Position

Definition at line 4307 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk [1/6]

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GP_T::DINOFF: DINOFF6 Mask

Definition at line 4311 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk [2/6]

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GP_T::DINOFF: DINOFF6 Mask

Definition at line 4311 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk [3/6]

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GP_T::DINOFF: DINOFF6 Mask

Definition at line 4311 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk [4/6]

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GP_T::DINOFF: DINOFF6 Mask

Definition at line 4311 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk [5/6]

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GP_T::DINOFF: DINOFF6 Mask

Definition at line 4311 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk [6/6]

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GP_T::DINOFF: DINOFF6 Mask

Definition at line 4311 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos [1/6]

#define GP_DINOFF_DINOFF6_Pos (22)

GP_T::DINOFF: DINOFF6 Position

Definition at line 4310 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos [2/6]

#define GP_DINOFF_DINOFF6_Pos (22)

GP_T::DINOFF: DINOFF6 Position

Definition at line 4310 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos [3/6]

#define GP_DINOFF_DINOFF6_Pos (22)

GP_T::DINOFF: DINOFF6 Position

Definition at line 4310 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos [4/6]

#define GP_DINOFF_DINOFF6_Pos (22)

GP_T::DINOFF: DINOFF6 Position

Definition at line 4310 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos [5/6]

#define GP_DINOFF_DINOFF6_Pos (22)

GP_T::DINOFF: DINOFF6 Position

Definition at line 4310 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos [6/6]

#define GP_DINOFF_DINOFF6_Pos (22)

GP_T::DINOFF: DINOFF6 Position

Definition at line 4310 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk [1/6]

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GP_T::DINOFF: DINOFF7 Mask

Definition at line 4314 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk [2/6]

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GP_T::DINOFF: DINOFF7 Mask

Definition at line 4314 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk [3/6]

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GP_T::DINOFF: DINOFF7 Mask

Definition at line 4314 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk [4/6]

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GP_T::DINOFF: DINOFF7 Mask

Definition at line 4314 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk [5/6]

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GP_T::DINOFF: DINOFF7 Mask

Definition at line 4314 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk [6/6]

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GP_T::DINOFF: DINOFF7 Mask

Definition at line 4314 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos [1/6]

#define GP_DINOFF_DINOFF7_Pos (23)

GP_T::DINOFF: DINOFF7 Position

Definition at line 4313 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos [2/6]

#define GP_DINOFF_DINOFF7_Pos (23)

GP_T::DINOFF: DINOFF7 Position

Definition at line 4313 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos [3/6]

#define GP_DINOFF_DINOFF7_Pos (23)

GP_T::DINOFF: DINOFF7 Position

Definition at line 4313 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos [4/6]

#define GP_DINOFF_DINOFF7_Pos (23)

GP_T::DINOFF: DINOFF7 Position

Definition at line 4313 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos [5/6]

#define GP_DINOFF_DINOFF7_Pos (23)

GP_T::DINOFF: DINOFF7 Position

Definition at line 4313 of file Mini58Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos [6/6]

#define GP_DINOFF_DINOFF7_Pos (23)

GP_T::DINOFF: DINOFF7 Position

Definition at line 4313 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Msk [1/6]

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GP_T::DOUT: DOUT0 Mask

Definition at line 4317 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Msk [2/6]

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GP_T::DOUT: DOUT0 Mask

Definition at line 4317 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Msk [3/6]

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GP_T::DOUT: DOUT0 Mask

Definition at line 4317 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Msk [4/6]

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GP_T::DOUT: DOUT0 Mask

Definition at line 4317 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Msk [5/6]

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GP_T::DOUT: DOUT0 Mask

Definition at line 4317 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Msk [6/6]

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GP_T::DOUT: DOUT0 Mask

Definition at line 4317 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Pos [1/6]

#define GP_DOUT_DOUT0_Pos (0)

GP_T::DOUT: DOUT0 Position

Definition at line 4316 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Pos [2/6]

#define GP_DOUT_DOUT0_Pos (0)

GP_T::DOUT: DOUT0 Position

Definition at line 4316 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Pos [3/6]

#define GP_DOUT_DOUT0_Pos (0)

GP_T::DOUT: DOUT0 Position

Definition at line 4316 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Pos [4/6]

#define GP_DOUT_DOUT0_Pos (0)

GP_T::DOUT: DOUT0 Position

Definition at line 4316 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Pos [5/6]

#define GP_DOUT_DOUT0_Pos (0)

GP_T::DOUT: DOUT0 Position

Definition at line 4316 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT0_Pos [6/6]

#define GP_DOUT_DOUT0_Pos (0)

GP_T::DOUT: DOUT0 Position

Definition at line 4316 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Msk [1/6]

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GP_T::DOUT: DOUT1 Mask

Definition at line 4320 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Msk [2/6]

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GP_T::DOUT: DOUT1 Mask

Definition at line 4320 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Msk [3/6]

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GP_T::DOUT: DOUT1 Mask

Definition at line 4320 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Msk [4/6]

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GP_T::DOUT: DOUT1 Mask

Definition at line 4320 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Msk [5/6]

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GP_T::DOUT: DOUT1 Mask

Definition at line 4320 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Msk [6/6]

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GP_T::DOUT: DOUT1 Mask

Definition at line 4320 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Pos [1/6]

#define GP_DOUT_DOUT1_Pos (1)

GP_T::DOUT: DOUT1 Position

Definition at line 4319 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Pos [2/6]

#define GP_DOUT_DOUT1_Pos (1)

GP_T::DOUT: DOUT1 Position

Definition at line 4319 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Pos [3/6]

#define GP_DOUT_DOUT1_Pos (1)

GP_T::DOUT: DOUT1 Position

Definition at line 4319 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Pos [4/6]

#define GP_DOUT_DOUT1_Pos (1)

GP_T::DOUT: DOUT1 Position

Definition at line 4319 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Pos [5/6]

#define GP_DOUT_DOUT1_Pos (1)

GP_T::DOUT: DOUT1 Position

Definition at line 4319 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT1_Pos [6/6]

#define GP_DOUT_DOUT1_Pos (1)

GP_T::DOUT: DOUT1 Position

Definition at line 4319 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Msk [1/6]

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GP_T::DOUT: DOUT2 Mask

Definition at line 4323 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Msk [2/6]

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GP_T::DOUT: DOUT2 Mask

Definition at line 4323 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Msk [3/6]

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GP_T::DOUT: DOUT2 Mask

Definition at line 4323 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Msk [4/6]

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GP_T::DOUT: DOUT2 Mask

Definition at line 4323 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Msk [5/6]

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GP_T::DOUT: DOUT2 Mask

Definition at line 4323 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Msk [6/6]

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GP_T::DOUT: DOUT2 Mask

Definition at line 4323 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Pos [1/6]

#define GP_DOUT_DOUT2_Pos (2)

GP_T::DOUT: DOUT2 Position

Definition at line 4322 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Pos [2/6]

#define GP_DOUT_DOUT2_Pos (2)

GP_T::DOUT: DOUT2 Position

Definition at line 4322 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Pos [3/6]

#define GP_DOUT_DOUT2_Pos (2)

GP_T::DOUT: DOUT2 Position

Definition at line 4322 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Pos [4/6]

#define GP_DOUT_DOUT2_Pos (2)

GP_T::DOUT: DOUT2 Position

Definition at line 4322 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Pos [5/6]

#define GP_DOUT_DOUT2_Pos (2)

GP_T::DOUT: DOUT2 Position

Definition at line 4322 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT2_Pos [6/6]

#define GP_DOUT_DOUT2_Pos (2)

GP_T::DOUT: DOUT2 Position

Definition at line 4322 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Msk [1/6]

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GP_T::DOUT: DOUT3 Mask

Definition at line 4326 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Msk [2/6]

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GP_T::DOUT: DOUT3 Mask

Definition at line 4326 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Msk [3/6]

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GP_T::DOUT: DOUT3 Mask

Definition at line 4326 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Msk [4/6]

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GP_T::DOUT: DOUT3 Mask

Definition at line 4326 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Msk [5/6]

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GP_T::DOUT: DOUT3 Mask

Definition at line 4326 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Msk [6/6]

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GP_T::DOUT: DOUT3 Mask

Definition at line 4326 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Pos [1/6]

#define GP_DOUT_DOUT3_Pos (3)

GP_T::DOUT: DOUT3 Position

Definition at line 4325 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Pos [2/6]

#define GP_DOUT_DOUT3_Pos (3)

GP_T::DOUT: DOUT3 Position

Definition at line 4325 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Pos [3/6]

#define GP_DOUT_DOUT3_Pos (3)

GP_T::DOUT: DOUT3 Position

Definition at line 4325 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Pos [4/6]

#define GP_DOUT_DOUT3_Pos (3)

GP_T::DOUT: DOUT3 Position

Definition at line 4325 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Pos [5/6]

#define GP_DOUT_DOUT3_Pos (3)

GP_T::DOUT: DOUT3 Position

Definition at line 4325 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT3_Pos [6/6]

#define GP_DOUT_DOUT3_Pos (3)

GP_T::DOUT: DOUT3 Position

Definition at line 4325 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Msk [1/6]

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GP_T::DOUT: DOUT4 Mask

Definition at line 4329 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Msk [2/6]

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GP_T::DOUT: DOUT4 Mask

Definition at line 4329 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Msk [3/6]

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GP_T::DOUT: DOUT4 Mask

Definition at line 4329 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Msk [4/6]

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GP_T::DOUT: DOUT4 Mask

Definition at line 4329 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Msk [5/6]

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GP_T::DOUT: DOUT4 Mask

Definition at line 4329 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Msk [6/6]

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GP_T::DOUT: DOUT4 Mask

Definition at line 4329 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Pos [1/6]

#define GP_DOUT_DOUT4_Pos (4)

GP_T::DOUT: DOUT4 Position

Definition at line 4328 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Pos [2/6]

#define GP_DOUT_DOUT4_Pos (4)

GP_T::DOUT: DOUT4 Position

Definition at line 4328 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Pos [3/6]

#define GP_DOUT_DOUT4_Pos (4)

GP_T::DOUT: DOUT4 Position

Definition at line 4328 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Pos [4/6]

#define GP_DOUT_DOUT4_Pos (4)

GP_T::DOUT: DOUT4 Position

Definition at line 4328 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Pos [5/6]

#define GP_DOUT_DOUT4_Pos (4)

GP_T::DOUT: DOUT4 Position

Definition at line 4328 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT4_Pos [6/6]

#define GP_DOUT_DOUT4_Pos (4)

GP_T::DOUT: DOUT4 Position

Definition at line 4328 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Msk [1/6]

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GP_T::DOUT: DOUT5 Mask

Definition at line 4332 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Msk [2/6]

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GP_T::DOUT: DOUT5 Mask

Definition at line 4332 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Msk [3/6]

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GP_T::DOUT: DOUT5 Mask

Definition at line 4332 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Msk [4/6]

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GP_T::DOUT: DOUT5 Mask

Definition at line 4332 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Msk [5/6]

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GP_T::DOUT: DOUT5 Mask

Definition at line 4332 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Msk [6/6]

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GP_T::DOUT: DOUT5 Mask

Definition at line 4332 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Pos [1/6]

#define GP_DOUT_DOUT5_Pos (5)

GP_T::DOUT: DOUT5 Position

Definition at line 4331 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Pos [2/6]

#define GP_DOUT_DOUT5_Pos (5)

GP_T::DOUT: DOUT5 Position

Definition at line 4331 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Pos [3/6]

#define GP_DOUT_DOUT5_Pos (5)

GP_T::DOUT: DOUT5 Position

Definition at line 4331 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Pos [4/6]

#define GP_DOUT_DOUT5_Pos (5)

GP_T::DOUT: DOUT5 Position

Definition at line 4331 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Pos [5/6]

#define GP_DOUT_DOUT5_Pos (5)

GP_T::DOUT: DOUT5 Position

Definition at line 4331 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT5_Pos [6/6]

#define GP_DOUT_DOUT5_Pos (5)

GP_T::DOUT: DOUT5 Position

Definition at line 4331 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Msk [1/6]

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GP_T::DOUT: DOUT6 Mask

Definition at line 4335 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Msk [2/6]

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GP_T::DOUT: DOUT6 Mask

Definition at line 4335 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Msk [3/6]

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GP_T::DOUT: DOUT6 Mask

Definition at line 4335 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Msk [4/6]

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GP_T::DOUT: DOUT6 Mask

Definition at line 4335 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Msk [5/6]

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GP_T::DOUT: DOUT6 Mask

Definition at line 4335 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Msk [6/6]

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GP_T::DOUT: DOUT6 Mask

Definition at line 4335 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Pos [1/6]

#define GP_DOUT_DOUT6_Pos (6)

GP_T::DOUT: DOUT6 Position

Definition at line 4334 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Pos [2/6]

#define GP_DOUT_DOUT6_Pos (6)

GP_T::DOUT: DOUT6 Position

Definition at line 4334 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Pos [3/6]

#define GP_DOUT_DOUT6_Pos (6)

GP_T::DOUT: DOUT6 Position

Definition at line 4334 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Pos [4/6]

#define GP_DOUT_DOUT6_Pos (6)

GP_T::DOUT: DOUT6 Position

Definition at line 4334 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Pos [5/6]

#define GP_DOUT_DOUT6_Pos (6)

GP_T::DOUT: DOUT6 Position

Definition at line 4334 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT6_Pos [6/6]

#define GP_DOUT_DOUT6_Pos (6)

GP_T::DOUT: DOUT6 Position

Definition at line 4334 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Msk [1/6]

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GP_T::DOUT: DOUT7 Mask

Definition at line 4338 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Msk [2/6]

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GP_T::DOUT: DOUT7 Mask

Definition at line 4338 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Msk [3/6]

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GP_T::DOUT: DOUT7 Mask

Definition at line 4338 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Msk [4/6]

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GP_T::DOUT: DOUT7 Mask

Definition at line 4338 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Msk [5/6]

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GP_T::DOUT: DOUT7 Mask

Definition at line 4338 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Msk [6/6]

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GP_T::DOUT: DOUT7 Mask

Definition at line 4338 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Pos [1/6]

#define GP_DOUT_DOUT7_Pos (7)

GP_T::DOUT: DOUT7 Position

Definition at line 4337 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Pos [2/6]

#define GP_DOUT_DOUT7_Pos (7)

GP_T::DOUT: DOUT7 Position

Definition at line 4337 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Pos [3/6]

#define GP_DOUT_DOUT7_Pos (7)

GP_T::DOUT: DOUT7 Position

Definition at line 4337 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Pos [4/6]

#define GP_DOUT_DOUT7_Pos (7)

GP_T::DOUT: DOUT7 Position

Definition at line 4337 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Pos [5/6]

#define GP_DOUT_DOUT7_Pos (7)

GP_T::DOUT: DOUT7 Position

Definition at line 4337 of file Mini58Series.h.

## ◆ GP_DOUT_DOUT7_Pos [6/6]

#define GP_DOUT_DOUT7_Pos (7)

GP_T::DOUT: DOUT7 Position

Definition at line 4337 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Msk [1/6]

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GP_T::INTEN: FLIEN0 Mask

Definition at line 4437 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Msk [2/6]

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GP_T::INTEN: FLIEN0 Mask

Definition at line 4437 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Msk [3/6]

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GP_T::INTEN: FLIEN0 Mask

Definition at line 4437 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Msk [4/6]

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GP_T::INTEN: FLIEN0 Mask

Definition at line 4437 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Msk [5/6]

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GP_T::INTEN: FLIEN0 Mask

Definition at line 4437 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Msk [6/6]

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GP_T::INTEN: FLIEN0 Mask

Definition at line 4437 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Pos [1/6]

#define GP_INTEN_FLIEN0_Pos (0)

GP_T::INTEN: FLIEN0 Position

Definition at line 4436 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Pos [2/6]

#define GP_INTEN_FLIEN0_Pos (0)

GP_T::INTEN: FLIEN0 Position

Definition at line 4436 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Pos [3/6]

#define GP_INTEN_FLIEN0_Pos (0)

GP_T::INTEN: FLIEN0 Position

Definition at line 4436 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Pos [4/6]

#define GP_INTEN_FLIEN0_Pos (0)

GP_T::INTEN: FLIEN0 Position

Definition at line 4436 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Pos [5/6]

#define GP_INTEN_FLIEN0_Pos (0)

GP_T::INTEN: FLIEN0 Position

Definition at line 4436 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN0_Pos [6/6]

#define GP_INTEN_FLIEN0_Pos (0)

GP_T::INTEN: FLIEN0 Position

Definition at line 4436 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Msk [1/6]

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GP_T::INTEN: FLIEN1 Mask

Definition at line 4440 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Msk [2/6]

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GP_T::INTEN: FLIEN1 Mask

Definition at line 4440 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Msk [3/6]

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GP_T::INTEN: FLIEN1 Mask

Definition at line 4440 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Msk [4/6]

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GP_T::INTEN: FLIEN1 Mask

Definition at line 4440 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Msk [5/6]

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GP_T::INTEN: FLIEN1 Mask

Definition at line 4440 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Msk [6/6]

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GP_T::INTEN: FLIEN1 Mask

Definition at line 4440 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Pos [1/6]

#define GP_INTEN_FLIEN1_Pos (1)

GP_T::INTEN: FLIEN1 Position

Definition at line 4439 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Pos [2/6]

#define GP_INTEN_FLIEN1_Pos (1)

GP_T::INTEN: FLIEN1 Position

Definition at line 4439 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Pos [3/6]

#define GP_INTEN_FLIEN1_Pos (1)

GP_T::INTEN: FLIEN1 Position

Definition at line 4439 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Pos [4/6]

#define GP_INTEN_FLIEN1_Pos (1)

GP_T::INTEN: FLIEN1 Position

Definition at line 4439 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Pos [5/6]

#define GP_INTEN_FLIEN1_Pos (1)

GP_T::INTEN: FLIEN1 Position

Definition at line 4439 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN1_Pos [6/6]

#define GP_INTEN_FLIEN1_Pos (1)

GP_T::INTEN: FLIEN1 Position

Definition at line 4439 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Msk [1/6]

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GP_T::INTEN: FLIEN2 Mask

Definition at line 4443 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Msk [2/6]

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GP_T::INTEN: FLIEN2 Mask

Definition at line 4443 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Msk [3/6]

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GP_T::INTEN: FLIEN2 Mask

Definition at line 4443 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Msk [4/6]

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GP_T::INTEN: FLIEN2 Mask

Definition at line 4443 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Msk [5/6]

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GP_T::INTEN: FLIEN2 Mask

Definition at line 4443 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Msk [6/6]

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GP_T::INTEN: FLIEN2 Mask

Definition at line 4443 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Pos [1/6]

#define GP_INTEN_FLIEN2_Pos (2)

GP_T::INTEN: FLIEN2 Position

Definition at line 4442 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Pos [2/6]

#define GP_INTEN_FLIEN2_Pos (2)

GP_T::INTEN: FLIEN2 Position

Definition at line 4442 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Pos [3/6]

#define GP_INTEN_FLIEN2_Pos (2)

GP_T::INTEN: FLIEN2 Position

Definition at line 4442 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Pos [4/6]

#define GP_INTEN_FLIEN2_Pos (2)

GP_T::INTEN: FLIEN2 Position

Definition at line 4442 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Pos [5/6]

#define GP_INTEN_FLIEN2_Pos (2)

GP_T::INTEN: FLIEN2 Position

Definition at line 4442 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN2_Pos [6/6]

#define GP_INTEN_FLIEN2_Pos (2)

GP_T::INTEN: FLIEN2 Position

Definition at line 4442 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Msk [1/6]

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GP_T::INTEN: FLIEN3 Mask

Definition at line 4446 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Msk [2/6]

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GP_T::INTEN: FLIEN3 Mask

Definition at line 4446 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Msk [3/6]

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GP_T::INTEN: FLIEN3 Mask

Definition at line 4446 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Msk [4/6]

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GP_T::INTEN: FLIEN3 Mask

Definition at line 4446 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Msk [5/6]

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GP_T::INTEN: FLIEN3 Mask

Definition at line 4446 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Msk [6/6]

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GP_T::INTEN: FLIEN3 Mask

Definition at line 4446 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Pos [1/6]

#define GP_INTEN_FLIEN3_Pos (3)

GP_T::INTEN: FLIEN3 Position

Definition at line 4445 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Pos [2/6]

#define GP_INTEN_FLIEN3_Pos (3)

GP_T::INTEN: FLIEN3 Position

Definition at line 4445 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Pos [3/6]

#define GP_INTEN_FLIEN3_Pos (3)

GP_T::INTEN: FLIEN3 Position

Definition at line 4445 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Pos [4/6]

#define GP_INTEN_FLIEN3_Pos (3)

GP_T::INTEN: FLIEN3 Position

Definition at line 4445 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Pos [5/6]

#define GP_INTEN_FLIEN3_Pos (3)

GP_T::INTEN: FLIEN3 Position

Definition at line 4445 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN3_Pos [6/6]

#define GP_INTEN_FLIEN3_Pos (3)

GP_T::INTEN: FLIEN3 Position

Definition at line 4445 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Msk [1/6]

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GP_T::INTEN: FLIEN4 Mask

Definition at line 4449 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Msk [2/6]

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GP_T::INTEN: FLIEN4 Mask

Definition at line 4449 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Msk [3/6]

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GP_T::INTEN: FLIEN4 Mask

Definition at line 4449 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Msk [4/6]

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GP_T::INTEN: FLIEN4 Mask

Definition at line 4449 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Msk [5/6]

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GP_T::INTEN: FLIEN4 Mask

Definition at line 4449 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Msk [6/6]

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GP_T::INTEN: FLIEN4 Mask

Definition at line 4449 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Pos [1/6]

#define GP_INTEN_FLIEN4_Pos (4)

GP_T::INTEN: FLIEN4 Position

Definition at line 4448 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Pos [2/6]

#define GP_INTEN_FLIEN4_Pos (4)

GP_T::INTEN: FLIEN4 Position

Definition at line 4448 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Pos [3/6]

#define GP_INTEN_FLIEN4_Pos (4)

GP_T::INTEN: FLIEN4 Position

Definition at line 4448 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Pos [4/6]

#define GP_INTEN_FLIEN4_Pos (4)

GP_T::INTEN: FLIEN4 Position

Definition at line 4448 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Pos [5/6]

#define GP_INTEN_FLIEN4_Pos (4)

GP_T::INTEN: FLIEN4 Position

Definition at line 4448 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN4_Pos [6/6]

#define GP_INTEN_FLIEN4_Pos (4)

GP_T::INTEN: FLIEN4 Position

Definition at line 4448 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Msk [1/6]

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GP_T::INTEN: FLIEN5 Mask

Definition at line 4452 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Msk [2/6]

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GP_T::INTEN: FLIEN5 Mask

Definition at line 4452 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Msk [3/6]

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GP_T::INTEN: FLIEN5 Mask

Definition at line 4452 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Msk [4/6]

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GP_T::INTEN: FLIEN5 Mask

Definition at line 4452 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Msk [5/6]

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GP_T::INTEN: FLIEN5 Mask

Definition at line 4452 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Msk [6/6]

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GP_T::INTEN: FLIEN5 Mask

Definition at line 4452 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Pos [1/6]

#define GP_INTEN_FLIEN5_Pos (5)

GP_T::INTEN: FLIEN5 Position

Definition at line 4451 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Pos [2/6]

#define GP_INTEN_FLIEN5_Pos (5)

GP_T::INTEN: FLIEN5 Position

Definition at line 4451 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Pos [3/6]

#define GP_INTEN_FLIEN5_Pos (5)

GP_T::INTEN: FLIEN5 Position

Definition at line 4451 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Pos [4/6]

#define GP_INTEN_FLIEN5_Pos (5)

GP_T::INTEN: FLIEN5 Position

Definition at line 4451 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Pos [5/6]

#define GP_INTEN_FLIEN5_Pos (5)

GP_T::INTEN: FLIEN5 Position

Definition at line 4451 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN5_Pos [6/6]

#define GP_INTEN_FLIEN5_Pos (5)

GP_T::INTEN: FLIEN5 Position

Definition at line 4451 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Msk [1/6]

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GP_T::INTEN: FLIEN6 Mask

Definition at line 4455 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Msk [2/6]

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GP_T::INTEN: FLIEN6 Mask

Definition at line 4455 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Msk [3/6]

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GP_T::INTEN: FLIEN6 Mask

Definition at line 4455 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Msk [4/6]

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GP_T::INTEN: FLIEN6 Mask

Definition at line 4455 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Msk [5/6]

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GP_T::INTEN: FLIEN6 Mask

Definition at line 4455 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Msk [6/6]

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GP_T::INTEN: FLIEN6 Mask

Definition at line 4455 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Pos [1/6]

#define GP_INTEN_FLIEN6_Pos (6)

GP_T::INTEN: FLIEN6 Position

Definition at line 4454 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Pos [2/6]

#define GP_INTEN_FLIEN6_Pos (6)

GP_T::INTEN: FLIEN6 Position

Definition at line 4454 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Pos [3/6]

#define GP_INTEN_FLIEN6_Pos (6)

GP_T::INTEN: FLIEN6 Position

Definition at line 4454 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Pos [4/6]

#define GP_INTEN_FLIEN6_Pos (6)

GP_T::INTEN: FLIEN6 Position

Definition at line 4454 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Pos [5/6]

#define GP_INTEN_FLIEN6_Pos (6)

GP_T::INTEN: FLIEN6 Position

Definition at line 4454 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN6_Pos [6/6]

#define GP_INTEN_FLIEN6_Pos (6)

GP_T::INTEN: FLIEN6 Position

Definition at line 4454 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Msk [1/6]

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GP_T::INTEN: FLIEN7 Mask

Definition at line 4458 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Msk [2/6]

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GP_T::INTEN: FLIEN7 Mask

Definition at line 4458 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Msk [3/6]

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GP_T::INTEN: FLIEN7 Mask

Definition at line 4458 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Msk [4/6]

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GP_T::INTEN: FLIEN7 Mask

Definition at line 4458 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Msk [5/6]

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GP_T::INTEN: FLIEN7 Mask

Definition at line 4458 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Msk [6/6]

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GP_T::INTEN: FLIEN7 Mask

Definition at line 4458 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Pos [1/6]

#define GP_INTEN_FLIEN7_Pos (7)

GP_T::INTEN: FLIEN7 Position

Definition at line 4457 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Pos [2/6]

#define GP_INTEN_FLIEN7_Pos (7)

GP_T::INTEN: FLIEN7 Position

Definition at line 4457 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Pos [3/6]

#define GP_INTEN_FLIEN7_Pos (7)

GP_T::INTEN: FLIEN7 Position

Definition at line 4457 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Pos [4/6]

#define GP_INTEN_FLIEN7_Pos (7)

GP_T::INTEN: FLIEN7 Position

Definition at line 4457 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Pos [5/6]

#define GP_INTEN_FLIEN7_Pos (7)

GP_T::INTEN: FLIEN7 Position

Definition at line 4457 of file Mini58Series.h.

## ◆ GP_INTEN_FLIEN7_Pos [6/6]

#define GP_INTEN_FLIEN7_Pos (7)

GP_T::INTEN: FLIEN7 Position

Definition at line 4457 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Msk [1/6]

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GP_T::INTEN: RHIEN0 Mask

Definition at line 4461 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Msk [2/6]

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GP_T::INTEN: RHIEN0 Mask

Definition at line 4461 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Msk [3/6]

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GP_T::INTEN: RHIEN0 Mask

Definition at line 4461 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Msk [4/6]

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GP_T::INTEN: RHIEN0 Mask

Definition at line 4461 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Msk [5/6]

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GP_T::INTEN: RHIEN0 Mask

Definition at line 4461 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Msk [6/6]

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GP_T::INTEN: RHIEN0 Mask

Definition at line 4461 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Pos [1/6]

#define GP_INTEN_RHIEN0_Pos (16)

GP_T::INTEN: RHIEN0 Position

Definition at line 4460 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Pos [2/6]

#define GP_INTEN_RHIEN0_Pos (16)

GP_T::INTEN: RHIEN0 Position

Definition at line 4460 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Pos [3/6]

#define GP_INTEN_RHIEN0_Pos (16)

GP_T::INTEN: RHIEN0 Position

Definition at line 4460 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Pos [4/6]

#define GP_INTEN_RHIEN0_Pos (16)

GP_T::INTEN: RHIEN0 Position

Definition at line 4460 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Pos [5/6]

#define GP_INTEN_RHIEN0_Pos (16)

GP_T::INTEN: RHIEN0 Position

Definition at line 4460 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN0_Pos [6/6]

#define GP_INTEN_RHIEN0_Pos (16)

GP_T::INTEN: RHIEN0 Position

Definition at line 4460 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Msk [1/6]

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GP_T::INTEN: RHIEN1 Mask

Definition at line 4464 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Msk [2/6]

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GP_T::INTEN: RHIEN1 Mask

Definition at line 4464 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Msk [3/6]

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GP_T::INTEN: RHIEN1 Mask

Definition at line 4464 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Msk [4/6]

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GP_T::INTEN: RHIEN1 Mask

Definition at line 4464 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Msk [5/6]

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GP_T::INTEN: RHIEN1 Mask

Definition at line 4464 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Msk [6/6]

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GP_T::INTEN: RHIEN1 Mask

Definition at line 4464 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Pos [1/6]

#define GP_INTEN_RHIEN1_Pos (17)

GP_T::INTEN: RHIEN1 Position

Definition at line 4463 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Pos [2/6]

#define GP_INTEN_RHIEN1_Pos (17)

GP_T::INTEN: RHIEN1 Position

Definition at line 4463 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Pos [3/6]

#define GP_INTEN_RHIEN1_Pos (17)

GP_T::INTEN: RHIEN1 Position

Definition at line 4463 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Pos [4/6]

#define GP_INTEN_RHIEN1_Pos (17)

GP_T::INTEN: RHIEN1 Position

Definition at line 4463 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Pos [5/6]

#define GP_INTEN_RHIEN1_Pos (17)

GP_T::INTEN: RHIEN1 Position

Definition at line 4463 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN1_Pos [6/6]

#define GP_INTEN_RHIEN1_Pos (17)

GP_T::INTEN: RHIEN1 Position

Definition at line 4463 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Msk [1/6]

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GP_T::INTEN: RHIEN2 Mask

Definition at line 4467 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Msk [2/6]

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GP_T::INTEN: RHIEN2 Mask

Definition at line 4467 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Msk [3/6]

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GP_T::INTEN: RHIEN2 Mask

Definition at line 4467 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Msk [4/6]

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GP_T::INTEN: RHIEN2 Mask

Definition at line 4467 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Msk [5/6]

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GP_T::INTEN: RHIEN2 Mask

Definition at line 4467 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Msk [6/6]

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GP_T::INTEN: RHIEN2 Mask

Definition at line 4467 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Pos [1/6]

#define GP_INTEN_RHIEN2_Pos (18)

GP_T::INTEN: RHIEN2 Position

Definition at line 4466 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Pos [2/6]

#define GP_INTEN_RHIEN2_Pos (18)

GP_T::INTEN: RHIEN2 Position

Definition at line 4466 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Pos [3/6]

#define GP_INTEN_RHIEN2_Pos (18)

GP_T::INTEN: RHIEN2 Position

Definition at line 4466 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Pos [4/6]

#define GP_INTEN_RHIEN2_Pos (18)

GP_T::INTEN: RHIEN2 Position

Definition at line 4466 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Pos [5/6]

#define GP_INTEN_RHIEN2_Pos (18)

GP_T::INTEN: RHIEN2 Position

Definition at line 4466 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN2_Pos [6/6]

#define GP_INTEN_RHIEN2_Pos (18)

GP_T::INTEN: RHIEN2 Position

Definition at line 4466 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Msk [1/6]

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GP_T::INTEN: RHIEN3 Mask

Definition at line 4470 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Msk [2/6]

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GP_T::INTEN: RHIEN3 Mask

Definition at line 4470 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Msk [3/6]

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GP_T::INTEN: RHIEN3 Mask

Definition at line 4470 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Msk [4/6]

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GP_T::INTEN: RHIEN3 Mask

Definition at line 4470 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Msk [5/6]

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GP_T::INTEN: RHIEN3 Mask

Definition at line 4470 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Msk [6/6]

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GP_T::INTEN: RHIEN3 Mask

Definition at line 4470 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Pos [1/6]

#define GP_INTEN_RHIEN3_Pos (19)

GP_T::INTEN: RHIEN3 Position

Definition at line 4469 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Pos [2/6]

#define GP_INTEN_RHIEN3_Pos (19)

GP_T::INTEN: RHIEN3 Position

Definition at line 4469 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Pos [3/6]

#define GP_INTEN_RHIEN3_Pos (19)

GP_T::INTEN: RHIEN3 Position

Definition at line 4469 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Pos [4/6]

#define GP_INTEN_RHIEN3_Pos (19)

GP_T::INTEN: RHIEN3 Position

Definition at line 4469 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Pos [5/6]

#define GP_INTEN_RHIEN3_Pos (19)

GP_T::INTEN: RHIEN3 Position

Definition at line 4469 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN3_Pos [6/6]

#define GP_INTEN_RHIEN3_Pos (19)

GP_T::INTEN: RHIEN3 Position

Definition at line 4469 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Msk [1/6]

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GP_T::INTEN: RHIEN4 Mask

Definition at line 4473 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Msk [2/6]

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GP_T::INTEN: RHIEN4 Mask

Definition at line 4473 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Msk [3/6]

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GP_T::INTEN: RHIEN4 Mask

Definition at line 4473 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Msk [4/6]

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GP_T::INTEN: RHIEN4 Mask

Definition at line 4473 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Msk [5/6]

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GP_T::INTEN: RHIEN4 Mask

Definition at line 4473 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Msk [6/6]

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GP_T::INTEN: RHIEN4 Mask

Definition at line 4473 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Pos [1/6]

#define GP_INTEN_RHIEN4_Pos (20)

GP_T::INTEN: RHIEN4 Position

Definition at line 4472 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Pos [2/6]

#define GP_INTEN_RHIEN4_Pos (20)

GP_T::INTEN: RHIEN4 Position

Definition at line 4472 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Pos [3/6]

#define GP_INTEN_RHIEN4_Pos (20)

GP_T::INTEN: RHIEN4 Position

Definition at line 4472 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Pos [4/6]

#define GP_INTEN_RHIEN4_Pos (20)

GP_T::INTEN: RHIEN4 Position

Definition at line 4472 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Pos [5/6]

#define GP_INTEN_RHIEN4_Pos (20)

GP_T::INTEN: RHIEN4 Position

Definition at line 4472 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN4_Pos [6/6]

#define GP_INTEN_RHIEN4_Pos (20)

GP_T::INTEN: RHIEN4 Position

Definition at line 4472 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Msk [1/6]

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GP_T::INTEN: RHIEN5 Mask

Definition at line 4476 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Msk [2/6]

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GP_T::INTEN: RHIEN5 Mask

Definition at line 4476 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Msk [3/6]

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GP_T::INTEN: RHIEN5 Mask

Definition at line 4476 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Msk [4/6]

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GP_T::INTEN: RHIEN5 Mask

Definition at line 4476 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Msk [5/6]

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GP_T::INTEN: RHIEN5 Mask

Definition at line 4476 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Msk [6/6]

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GP_T::INTEN: RHIEN5 Mask

Definition at line 4476 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Pos [1/6]

#define GP_INTEN_RHIEN5_Pos (21)

GP_T::INTEN: RHIEN5 Position

Definition at line 4475 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Pos [2/6]

#define GP_INTEN_RHIEN5_Pos (21)

GP_T::INTEN: RHIEN5 Position

Definition at line 4475 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Pos [3/6]

#define GP_INTEN_RHIEN5_Pos (21)

GP_T::INTEN: RHIEN5 Position

Definition at line 4475 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Pos [4/6]

#define GP_INTEN_RHIEN5_Pos (21)

GP_T::INTEN: RHIEN5 Position

Definition at line 4475 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Pos [5/6]

#define GP_INTEN_RHIEN5_Pos (21)

GP_T::INTEN: RHIEN5 Position

Definition at line 4475 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN5_Pos [6/6]

#define GP_INTEN_RHIEN5_Pos (21)

GP_T::INTEN: RHIEN5 Position

Definition at line 4475 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Msk [1/6]

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GP_T::INTEN: RHIEN6 Mask

Definition at line 4479 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Msk [2/6]

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GP_T::INTEN: RHIEN6 Mask

Definition at line 4479 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Msk [3/6]

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GP_T::INTEN: RHIEN6 Mask

Definition at line 4479 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Msk [4/6]

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GP_T::INTEN: RHIEN6 Mask

Definition at line 4479 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Msk [5/6]

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GP_T::INTEN: RHIEN6 Mask

Definition at line 4479 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Msk [6/6]

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GP_T::INTEN: RHIEN6 Mask

Definition at line 4479 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Pos [1/6]

#define GP_INTEN_RHIEN6_Pos (22)

GP_T::INTEN: RHIEN6 Position

Definition at line 4478 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Pos [2/6]

#define GP_INTEN_RHIEN6_Pos (22)

GP_T::INTEN: RHIEN6 Position

Definition at line 4478 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Pos [3/6]

#define GP_INTEN_RHIEN6_Pos (22)

GP_T::INTEN: RHIEN6 Position

Definition at line 4478 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Pos [4/6]

#define GP_INTEN_RHIEN6_Pos (22)

GP_T::INTEN: RHIEN6 Position

Definition at line 4478 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Pos [5/6]

#define GP_INTEN_RHIEN6_Pos (22)

GP_T::INTEN: RHIEN6 Position

Definition at line 4478 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN6_Pos [6/6]

#define GP_INTEN_RHIEN6_Pos (22)

GP_T::INTEN: RHIEN6 Position

Definition at line 4478 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Msk [1/6]

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GP_T::INTEN: RHIEN7 Mask

Definition at line 4482 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Msk [2/6]

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GP_T::INTEN: RHIEN7 Mask

Definition at line 4482 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Msk [3/6]

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GP_T::INTEN: RHIEN7 Mask

Definition at line 4482 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Msk [4/6]

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GP_T::INTEN: RHIEN7 Mask

Definition at line 4482 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Msk [5/6]

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GP_T::INTEN: RHIEN7 Mask

Definition at line 4482 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Msk [6/6]

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GP_T::INTEN: RHIEN7 Mask

Definition at line 4482 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Pos [1/6]

#define GP_INTEN_RHIEN7_Pos (23)

GP_T::INTEN: RHIEN7 Position

Definition at line 4481 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Pos [2/6]

#define GP_INTEN_RHIEN7_Pos (23)

GP_T::INTEN: RHIEN7 Position

Definition at line 4481 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Pos [3/6]

#define GP_INTEN_RHIEN7_Pos (23)

GP_T::INTEN: RHIEN7 Position

Definition at line 4481 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Pos [4/6]

#define GP_INTEN_RHIEN7_Pos (23)

GP_T::INTEN: RHIEN7 Position

Definition at line 4481 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Pos [5/6]

#define GP_INTEN_RHIEN7_Pos (23)

GP_T::INTEN: RHIEN7 Position

Definition at line 4481 of file Mini58Series.h.

## ◆ GP_INTEN_RHIEN7_Pos [6/6]

#define GP_INTEN_RHIEN7_Pos (23)

GP_T::INTEN: RHIEN7 Position

Definition at line 4481 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk [1/6]

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GP_T::INTSRC: INTSRC0 Mask

Definition at line 4485 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk [2/6]

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GP_T::INTSRC: INTSRC0 Mask

Definition at line 4485 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk [3/6]

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GP_T::INTSRC: INTSRC0 Mask

Definition at line 4485 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk [4/6]

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GP_T::INTSRC: INTSRC0 Mask

Definition at line 4485 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk [5/6]

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GP_T::INTSRC: INTSRC0 Mask

Definition at line 4485 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk [6/6]

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GP_T::INTSRC: INTSRC0 Mask

Definition at line 4485 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos [1/6]

#define GP_INTSRC_INTSRC0_Pos (0)

GP_T::INTSRC: INTSRC0 Position

Definition at line 4484 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos [2/6]

#define GP_INTSRC_INTSRC0_Pos (0)

GP_T::INTSRC: INTSRC0 Position

Definition at line 4484 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos [3/6]

#define GP_INTSRC_INTSRC0_Pos (0)

GP_T::INTSRC: INTSRC0 Position

Definition at line 4484 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos [4/6]

#define GP_INTSRC_INTSRC0_Pos (0)

GP_T::INTSRC: INTSRC0 Position

Definition at line 4484 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos [5/6]

#define GP_INTSRC_INTSRC0_Pos (0)

GP_T::INTSRC: INTSRC0 Position

Definition at line 4484 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos [6/6]

#define GP_INTSRC_INTSRC0_Pos (0)

GP_T::INTSRC: INTSRC0 Position

Definition at line 4484 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Msk [1/6]

#define GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)

GP_T::INTSRC: INTSRC10 Mask

Definition at line 4515 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Msk [2/6]

#define GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)

GP_T::INTSRC: INTSRC10 Mask

Definition at line 4515 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Msk [3/6]

#define GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)

GP_T::INTSRC: INTSRC10 Mask

Definition at line 4515 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Msk [4/6]

#define GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)

GP_T::INTSRC: INTSRC10 Mask

Definition at line 4515 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Msk [5/6]

#define GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)

GP_T::INTSRC: INTSRC10 Mask

Definition at line 4515 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Msk [6/6]

#define GP_INTSRC_INTSRC10_Msk (0x1ul << GP_INTSRC_INTSRC10_Pos)

GP_T::INTSRC: INTSRC10 Mask

Definition at line 4515 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Pos [1/6]

#define GP_INTSRC_INTSRC10_Pos (10)

GP_T::INTSRC: INTSRC10 Position

Definition at line 4514 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Pos [2/6]

#define GP_INTSRC_INTSRC10_Pos (10)

GP_T::INTSRC: INTSRC10 Position

Definition at line 4514 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Pos [3/6]

#define GP_INTSRC_INTSRC10_Pos (10)

GP_T::INTSRC: INTSRC10 Position

Definition at line 4514 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Pos [4/6]

#define GP_INTSRC_INTSRC10_Pos (10)

GP_T::INTSRC: INTSRC10 Position

Definition at line 4514 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Pos [5/6]

#define GP_INTSRC_INTSRC10_Pos (10)

GP_T::INTSRC: INTSRC10 Position

Definition at line 4514 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC10_Pos [6/6]

#define GP_INTSRC_INTSRC10_Pos (10)

GP_T::INTSRC: INTSRC10 Position

Definition at line 4514 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Msk [1/6]

#define GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)

GP_T::INTSRC: INTSRC11 Mask

Definition at line 4518 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Msk [2/6]

#define GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)

GP_T::INTSRC: INTSRC11 Mask

Definition at line 4518 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Msk [3/6]

#define GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)

GP_T::INTSRC: INTSRC11 Mask

Definition at line 4518 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Msk [4/6]

#define GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)

GP_T::INTSRC: INTSRC11 Mask

Definition at line 4518 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Msk [5/6]

#define GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)

GP_T::INTSRC: INTSRC11 Mask

Definition at line 4518 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Msk [6/6]

#define GP_INTSRC_INTSRC11_Msk (0x1ul << GP_INTSRC_INTSRC11_Pos)

GP_T::INTSRC: INTSRC11 Mask

Definition at line 4518 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Pos [1/6]

#define GP_INTSRC_INTSRC11_Pos (11)

GP_T::INTSRC: INTSRC11 Position

Definition at line 4517 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Pos [2/6]

#define GP_INTSRC_INTSRC11_Pos (11)

GP_T::INTSRC: INTSRC11 Position

Definition at line 4517 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Pos [3/6]

#define GP_INTSRC_INTSRC11_Pos (11)

GP_T::INTSRC: INTSRC11 Position

Definition at line 4517 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Pos [4/6]

#define GP_INTSRC_INTSRC11_Pos (11)

GP_T::INTSRC: INTSRC11 Position

Definition at line 4517 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Pos [5/6]

#define GP_INTSRC_INTSRC11_Pos (11)

GP_T::INTSRC: INTSRC11 Position

Definition at line 4517 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC11_Pos [6/6]

#define GP_INTSRC_INTSRC11_Pos (11)

GP_T::INTSRC: INTSRC11 Position

Definition at line 4517 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Msk [1/6]

#define GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)

GP_T::INTSRC: INTSRC12 Mask

Definition at line 4521 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Msk [2/6]

#define GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)

GP_T::INTSRC: INTSRC12 Mask

Definition at line 4521 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Msk [3/6]

#define GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)

GP_T::INTSRC: INTSRC12 Mask

Definition at line 4521 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Msk [4/6]

#define GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)

GP_T::INTSRC: INTSRC12 Mask

Definition at line 4521 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Msk [5/6]

#define GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)

GP_T::INTSRC: INTSRC12 Mask

Definition at line 4521 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Msk [6/6]

#define GP_INTSRC_INTSRC12_Msk (0x1ul << GP_INTSRC_INTSRC12_Pos)

GP_T::INTSRC: INTSRC12 Mask

Definition at line 4521 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Pos [1/6]

#define GP_INTSRC_INTSRC12_Pos (12)

GP_T::INTSRC: INTSRC12 Position

Definition at line 4520 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Pos [2/6]

#define GP_INTSRC_INTSRC12_Pos (12)

GP_T::INTSRC: INTSRC12 Position

Definition at line 4520 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Pos [3/6]

#define GP_INTSRC_INTSRC12_Pos (12)

GP_T::INTSRC: INTSRC12 Position

Definition at line 4520 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Pos [4/6]

#define GP_INTSRC_INTSRC12_Pos (12)

GP_T::INTSRC: INTSRC12 Position

Definition at line 4520 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Pos [5/6]

#define GP_INTSRC_INTSRC12_Pos (12)

GP_T::INTSRC: INTSRC12 Position

Definition at line 4520 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC12_Pos [6/6]

#define GP_INTSRC_INTSRC12_Pos (12)

GP_T::INTSRC: INTSRC12 Position

Definition at line 4520 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Msk [1/6]

#define GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)

GP_T::INTSRC: INTSRC13 Mask

Definition at line 4524 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Msk [2/6]

#define GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)

GP_T::INTSRC: INTSRC13 Mask

Definition at line 4524 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Msk [3/6]

#define GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)

GP_T::INTSRC: INTSRC13 Mask

Definition at line 4524 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Msk [4/6]

#define GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)

GP_T::INTSRC: INTSRC13 Mask

Definition at line 4524 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Msk [5/6]

#define GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)

GP_T::INTSRC: INTSRC13 Mask

Definition at line 4524 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Msk [6/6]

#define GP_INTSRC_INTSRC13_Msk (0x1ul << GP_INTSRC_INTSRC13_Pos)

GP_T::INTSRC: INTSRC13 Mask

Definition at line 4524 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Pos [1/6]

#define GP_INTSRC_INTSRC13_Pos (13)

GP_T::INTSRC: INTSRC13 Position

Definition at line 4523 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Pos [2/6]

#define GP_INTSRC_INTSRC13_Pos (13)

GP_T::INTSRC: INTSRC13 Position

Definition at line 4523 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Pos [3/6]

#define GP_INTSRC_INTSRC13_Pos (13)

GP_T::INTSRC: INTSRC13 Position

Definition at line 4523 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Pos [4/6]

#define GP_INTSRC_INTSRC13_Pos (13)

GP_T::INTSRC: INTSRC13 Position

Definition at line 4523 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Pos [5/6]

#define GP_INTSRC_INTSRC13_Pos (13)

GP_T::INTSRC: INTSRC13 Position

Definition at line 4523 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC13_Pos [6/6]

#define GP_INTSRC_INTSRC13_Pos (13)

GP_T::INTSRC: INTSRC13 Position

Definition at line 4523 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Msk [1/6]

#define GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)

GP_T::INTSRC: INTSRC14 Mask

Definition at line 4527 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Msk [2/6]

#define GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)

GP_T::INTSRC: INTSRC14 Mask

Definition at line 4527 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Msk [3/6]

#define GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)

GP_T::INTSRC: INTSRC14 Mask

Definition at line 4527 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Msk [4/6]

#define GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)

GP_T::INTSRC: INTSRC14 Mask

Definition at line 4527 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Msk [5/6]

#define GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)

GP_T::INTSRC: INTSRC14 Mask

Definition at line 4527 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Msk [6/6]

#define GP_INTSRC_INTSRC14_Msk (0x1ul << GP_INTSRC_INTSRC14_Pos)

GP_T::INTSRC: INTSRC14 Mask

Definition at line 4527 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Pos [1/6]

#define GP_INTSRC_INTSRC14_Pos (14)

GP_T::INTSRC: INTSRC14 Position

Definition at line 4526 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Pos [2/6]

#define GP_INTSRC_INTSRC14_Pos (14)

GP_T::INTSRC: INTSRC14 Position

Definition at line 4526 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Pos [3/6]

#define GP_INTSRC_INTSRC14_Pos (14)

GP_T::INTSRC: INTSRC14 Position

Definition at line 4526 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Pos [4/6]

#define GP_INTSRC_INTSRC14_Pos (14)

GP_T::INTSRC: INTSRC14 Position

Definition at line 4526 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Pos [5/6]

#define GP_INTSRC_INTSRC14_Pos (14)

GP_T::INTSRC: INTSRC14 Position

Definition at line 4526 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC14_Pos [6/6]

#define GP_INTSRC_INTSRC14_Pos (14)

GP_T::INTSRC: INTSRC14 Position

Definition at line 4526 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Msk [1/6]

#define GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)

GP_T::INTSRC: INTSRC15 Mask

Definition at line 4530 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Msk [2/6]

#define GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)

GP_T::INTSRC: INTSRC15 Mask

Definition at line 4530 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Msk [3/6]

#define GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)

GP_T::INTSRC: INTSRC15 Mask

Definition at line 4530 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Msk [4/6]

#define GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)

GP_T::INTSRC: INTSRC15 Mask

Definition at line 4530 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Msk [5/6]

#define GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)

GP_T::INTSRC: INTSRC15 Mask

Definition at line 4530 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Msk [6/6]

#define GP_INTSRC_INTSRC15_Msk (0x1ul << GP_INTSRC_INTSRC15_Pos)

GP_T::INTSRC: INTSRC15 Mask

Definition at line 4530 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Pos [1/6]

#define GP_INTSRC_INTSRC15_Pos (15)

GP_T::INTSRC: INTSRC15 Position

Definition at line 4529 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Pos [2/6]

#define GP_INTSRC_INTSRC15_Pos (15)

GP_T::INTSRC: INTSRC15 Position

Definition at line 4529 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Pos [3/6]

#define GP_INTSRC_INTSRC15_Pos (15)

GP_T::INTSRC: INTSRC15 Position

Definition at line 4529 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Pos [4/6]

#define GP_INTSRC_INTSRC15_Pos (15)

GP_T::INTSRC: INTSRC15 Position

Definition at line 4529 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Pos [5/6]

#define GP_INTSRC_INTSRC15_Pos (15)

GP_T::INTSRC: INTSRC15 Position

Definition at line 4529 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC15_Pos [6/6]

#define GP_INTSRC_INTSRC15_Pos (15)

GP_T::INTSRC: INTSRC15 Position

Definition at line 4529 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk [1/6]

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GP_T::INTSRC: INTSRC1 Mask

Definition at line 4488 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk [2/6]

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GP_T::INTSRC: INTSRC1 Mask

Definition at line 4488 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk [3/6]

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GP_T::INTSRC: INTSRC1 Mask

Definition at line 4488 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk [4/6]

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GP_T::INTSRC: INTSRC1 Mask

Definition at line 4488 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk [5/6]

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GP_T::INTSRC: INTSRC1 Mask

Definition at line 4488 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk [6/6]

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GP_T::INTSRC: INTSRC1 Mask

Definition at line 4488 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos [1/6]

#define GP_INTSRC_INTSRC1_Pos (1)

GP_T::INTSRC: INTSRC1 Position

Definition at line 4487 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos [2/6]

#define GP_INTSRC_INTSRC1_Pos (1)

GP_T::INTSRC: INTSRC1 Position

Definition at line 4487 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos [3/6]

#define GP_INTSRC_INTSRC1_Pos (1)

GP_T::INTSRC: INTSRC1 Position

Definition at line 4487 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos [4/6]

#define GP_INTSRC_INTSRC1_Pos (1)

GP_T::INTSRC: INTSRC1 Position

Definition at line 4487 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos [5/6]

#define GP_INTSRC_INTSRC1_Pos (1)

GP_T::INTSRC: INTSRC1 Position

Definition at line 4487 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos [6/6]

#define GP_INTSRC_INTSRC1_Pos (1)

GP_T::INTSRC: INTSRC1 Position

Definition at line 4487 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk [1/6]

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GP_T::INTSRC: INTSRC2 Mask

Definition at line 4491 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk [2/6]

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GP_T::INTSRC: INTSRC2 Mask

Definition at line 4491 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk [3/6]

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GP_T::INTSRC: INTSRC2 Mask

Definition at line 4491 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk [4/6]

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GP_T::INTSRC: INTSRC2 Mask

Definition at line 4491 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk [5/6]

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GP_T::INTSRC: INTSRC2 Mask

Definition at line 4491 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk [6/6]

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GP_T::INTSRC: INTSRC2 Mask

Definition at line 4491 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos [1/6]

#define GP_INTSRC_INTSRC2_Pos (2)

GP_T::INTSRC: INTSRC2 Position

Definition at line 4490 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos [2/6]

#define GP_INTSRC_INTSRC2_Pos (2)

GP_T::INTSRC: INTSRC2 Position

Definition at line 4490 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos [3/6]

#define GP_INTSRC_INTSRC2_Pos (2)

GP_T::INTSRC: INTSRC2 Position

Definition at line 4490 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos [4/6]

#define GP_INTSRC_INTSRC2_Pos (2)

GP_T::INTSRC: INTSRC2 Position

Definition at line 4490 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos [5/6]

#define GP_INTSRC_INTSRC2_Pos (2)

GP_T::INTSRC: INTSRC2 Position

Definition at line 4490 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos [6/6]

#define GP_INTSRC_INTSRC2_Pos (2)

GP_T::INTSRC: INTSRC2 Position

Definition at line 4490 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk [1/6]

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GP_T::INTSRC: INTSRC3 Mask

Definition at line 4494 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk [2/6]

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GP_T::INTSRC: INTSRC3 Mask

Definition at line 4494 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk [3/6]

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GP_T::INTSRC: INTSRC3 Mask

Definition at line 4494 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk [4/6]

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GP_T::INTSRC: INTSRC3 Mask

Definition at line 4494 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk [5/6]

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GP_T::INTSRC: INTSRC3 Mask

Definition at line 4494 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk [6/6]

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GP_T::INTSRC: INTSRC3 Mask

Definition at line 4494 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos [1/6]

#define GP_INTSRC_INTSRC3_Pos (3)

GP_T::INTSRC: INTSRC3 Position

Definition at line 4493 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos [2/6]

#define GP_INTSRC_INTSRC3_Pos (3)

GP_T::INTSRC: INTSRC3 Position

Definition at line 4493 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos [3/6]

#define GP_INTSRC_INTSRC3_Pos (3)

GP_T::INTSRC: INTSRC3 Position

Definition at line 4493 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos [4/6]

#define GP_INTSRC_INTSRC3_Pos (3)

GP_T::INTSRC: INTSRC3 Position

Definition at line 4493 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos [5/6]

#define GP_INTSRC_INTSRC3_Pos (3)

GP_T::INTSRC: INTSRC3 Position

Definition at line 4493 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos [6/6]

#define GP_INTSRC_INTSRC3_Pos (3)

GP_T::INTSRC: INTSRC3 Position

Definition at line 4493 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk [1/6]

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GP_T::INTSRC: INTSRC4 Mask

Definition at line 4497 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk [2/6]

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GP_T::INTSRC: INTSRC4 Mask

Definition at line 4497 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk [3/6]

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GP_T::INTSRC: INTSRC4 Mask

Definition at line 4497 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk [4/6]

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GP_T::INTSRC: INTSRC4 Mask

Definition at line 4497 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk [5/6]

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GP_T::INTSRC: INTSRC4 Mask

Definition at line 4497 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk [6/6]

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GP_T::INTSRC: INTSRC4 Mask

Definition at line 4497 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos [1/6]

#define GP_INTSRC_INTSRC4_Pos (4)

GP_T::INTSRC: INTSRC4 Position

Definition at line 4496 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos [2/6]

#define GP_INTSRC_INTSRC4_Pos (4)

GP_T::INTSRC: INTSRC4 Position

Definition at line 4496 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos [3/6]

#define GP_INTSRC_INTSRC4_Pos (4)

GP_T::INTSRC: INTSRC4 Position

Definition at line 4496 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos [4/6]

#define GP_INTSRC_INTSRC4_Pos (4)

GP_T::INTSRC: INTSRC4 Position

Definition at line 4496 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos [5/6]

#define GP_INTSRC_INTSRC4_Pos (4)

GP_T::INTSRC: INTSRC4 Position

Definition at line 4496 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos [6/6]

#define GP_INTSRC_INTSRC4_Pos (4)

GP_T::INTSRC: INTSRC4 Position

Definition at line 4496 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk [1/6]

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GP_T::INTSRC: INTSRC5 Mask

Definition at line 4500 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk [2/6]

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GP_T::INTSRC: INTSRC5 Mask

Definition at line 4500 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk [3/6]

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GP_T::INTSRC: INTSRC5 Mask

Definition at line 4500 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk [4/6]

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GP_T::INTSRC: INTSRC5 Mask

Definition at line 4500 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk [5/6]

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GP_T::INTSRC: INTSRC5 Mask

Definition at line 4500 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk [6/6]

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GP_T::INTSRC: INTSRC5 Mask

Definition at line 4500 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos [1/6]

#define GP_INTSRC_INTSRC5_Pos (5)

GP_T::INTSRC: INTSRC5 Position

Definition at line 4499 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos [2/6]

#define GP_INTSRC_INTSRC5_Pos (5)

GP_T::INTSRC: INTSRC5 Position

Definition at line 4499 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos [3/6]

#define GP_INTSRC_INTSRC5_Pos (5)

GP_T::INTSRC: INTSRC5 Position

Definition at line 4499 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos [4/6]

#define GP_INTSRC_INTSRC5_Pos (5)

GP_T::INTSRC: INTSRC5 Position

Definition at line 4499 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos [5/6]

#define GP_INTSRC_INTSRC5_Pos (5)

GP_T::INTSRC: INTSRC5 Position

Definition at line 4499 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos [6/6]

#define GP_INTSRC_INTSRC5_Pos (5)

GP_T::INTSRC: INTSRC5 Position

Definition at line 4499 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk [1/6]

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GP_T::INTSRC: INTSRC6 Mask

Definition at line 4503 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk [2/6]

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GP_T::INTSRC: INTSRC6 Mask

Definition at line 4503 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk [3/6]

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GP_T::INTSRC: INTSRC6 Mask

Definition at line 4503 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk [4/6]

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GP_T::INTSRC: INTSRC6 Mask

Definition at line 4503 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk [5/6]

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GP_T::INTSRC: INTSRC6 Mask

Definition at line 4503 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk [6/6]

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GP_T::INTSRC: INTSRC6 Mask

Definition at line 4503 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos [1/6]

#define GP_INTSRC_INTSRC6_Pos (6)

GP_T::INTSRC: INTSRC6 Position

Definition at line 4502 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos [2/6]

#define GP_INTSRC_INTSRC6_Pos (6)

GP_T::INTSRC: INTSRC6 Position

Definition at line 4502 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos [3/6]

#define GP_INTSRC_INTSRC6_Pos (6)

GP_T::INTSRC: INTSRC6 Position

Definition at line 4502 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos [4/6]

#define GP_INTSRC_INTSRC6_Pos (6)

GP_T::INTSRC: INTSRC6 Position

Definition at line 4502 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos [5/6]

#define GP_INTSRC_INTSRC6_Pos (6)

GP_T::INTSRC: INTSRC6 Position

Definition at line 4502 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos [6/6]

#define GP_INTSRC_INTSRC6_Pos (6)

GP_T::INTSRC: INTSRC6 Position

Definition at line 4502 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk [1/6]

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GP_T::INTSRC: INTSRC7 Mask

Definition at line 4506 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk [2/6]

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GP_T::INTSRC: INTSRC7 Mask

Definition at line 4506 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk [3/6]

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GP_T::INTSRC: INTSRC7 Mask

Definition at line 4506 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk [4/6]

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GP_T::INTSRC: INTSRC7 Mask

Definition at line 4506 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk [5/6]

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GP_T::INTSRC: INTSRC7 Mask

Definition at line 4506 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk [6/6]

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GP_T::INTSRC: INTSRC7 Mask

Definition at line 4506 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos [1/6]

#define GP_INTSRC_INTSRC7_Pos (7)

GP_T::INTSRC: INTSRC7 Position

Definition at line 4505 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos [2/6]

#define GP_INTSRC_INTSRC7_Pos (7)

GP_T::INTSRC: INTSRC7 Position

Definition at line 4505 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos [3/6]

#define GP_INTSRC_INTSRC7_Pos (7)

GP_T::INTSRC: INTSRC7 Position

Definition at line 4505 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos [4/6]

#define GP_INTSRC_INTSRC7_Pos (7)

GP_T::INTSRC: INTSRC7 Position

Definition at line 4505 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos [5/6]

#define GP_INTSRC_INTSRC7_Pos (7)

GP_T::INTSRC: INTSRC7 Position

Definition at line 4505 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos [6/6]

#define GP_INTSRC_INTSRC7_Pos (7)

GP_T::INTSRC: INTSRC7 Position

Definition at line 4505 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Msk [1/6]

#define GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)

GP_T::INTSRC: INTSRC8 Mask

Definition at line 4509 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Msk [2/6]

#define GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)

GP_T::INTSRC: INTSRC8 Mask

Definition at line 4509 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Msk [3/6]

#define GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)

GP_T::INTSRC: INTSRC8 Mask

Definition at line 4509 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Msk [4/6]

#define GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)

GP_T::INTSRC: INTSRC8 Mask

Definition at line 4509 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Msk [5/6]

#define GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)

GP_T::INTSRC: INTSRC8 Mask

Definition at line 4509 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Msk [6/6]

#define GP_INTSRC_INTSRC8_Msk (0x1ul << GP_INTSRC_INTSRC8_Pos)

GP_T::INTSRC: INTSRC8 Mask

Definition at line 4509 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Pos [1/6]

#define GP_INTSRC_INTSRC8_Pos (8)

GP_T::INTSRC: INTSRC8 Position

Definition at line 4508 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Pos [2/6]

#define GP_INTSRC_INTSRC8_Pos (8)

GP_T::INTSRC: INTSRC8 Position

Definition at line 4508 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Pos [3/6]

#define GP_INTSRC_INTSRC8_Pos (8)

GP_T::INTSRC: INTSRC8 Position

Definition at line 4508 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Pos [4/6]

#define GP_INTSRC_INTSRC8_Pos (8)

GP_T::INTSRC: INTSRC8 Position

Definition at line 4508 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Pos [5/6]

#define GP_INTSRC_INTSRC8_Pos (8)

GP_T::INTSRC: INTSRC8 Position

Definition at line 4508 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC8_Pos [6/6]

#define GP_INTSRC_INTSRC8_Pos (8)

GP_T::INTSRC: INTSRC8 Position

Definition at line 4508 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Msk [1/6]

#define GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)

GP_T::INTSRC: INTSRC9 Mask

Definition at line 4512 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Msk [2/6]

#define GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)

GP_T::INTSRC: INTSRC9 Mask

Definition at line 4512 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Msk [3/6]

#define GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)

GP_T::INTSRC: INTSRC9 Mask

Definition at line 4512 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Msk [4/6]

#define GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)

GP_T::INTSRC: INTSRC9 Mask

Definition at line 4512 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Msk [5/6]

#define GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)

GP_T::INTSRC: INTSRC9 Mask

Definition at line 4512 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Msk [6/6]

#define GP_INTSRC_INTSRC9_Msk (0x1ul << GP_INTSRC_INTSRC9_Pos)

GP_T::INTSRC: INTSRC9 Mask

Definition at line 4512 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Pos [1/6]

#define GP_INTSRC_INTSRC9_Pos (9)

GP_T::INTSRC: INTSRC9 Position

Definition at line 4511 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Pos [2/6]

#define GP_INTSRC_INTSRC9_Pos (9)

GP_T::INTSRC: INTSRC9 Position

Definition at line 4511 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Pos [3/6]

#define GP_INTSRC_INTSRC9_Pos (9)

GP_T::INTSRC: INTSRC9 Position

Definition at line 4511 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Pos [4/6]

#define GP_INTSRC_INTSRC9_Pos (9)

GP_T::INTSRC: INTSRC9 Position

Definition at line 4511 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Pos [5/6]

#define GP_INTSRC_INTSRC9_Pos (9)

GP_T::INTSRC: INTSRC9 Position

Definition at line 4511 of file Mini58Series.h.

## ◆ GP_INTSRC_INTSRC9_Pos [6/6]

#define GP_INTSRC_INTSRC9_Pos (9)

GP_T::INTSRC: INTSRC9 Position

Definition at line 4511 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk [1/6]

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GP_T::INTTYPE: TYPE0 Mask

Definition at line 4413 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk [2/6]

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GP_T::INTTYPE: TYPE0 Mask

Definition at line 4413 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk [3/6]

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GP_T::INTTYPE: TYPE0 Mask

Definition at line 4413 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk [4/6]

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GP_T::INTTYPE: TYPE0 Mask

Definition at line 4413 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk [5/6]

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GP_T::INTTYPE: TYPE0 Mask

Definition at line 4413 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk [6/6]

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GP_T::INTTYPE: TYPE0 Mask

Definition at line 4413 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos [1/6]

#define GP_INTTYPE_TYPE0_Pos (0)

GP_T::INTTYPE: TYPE0 Position

Definition at line 4412 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos [2/6]

#define GP_INTTYPE_TYPE0_Pos (0)

GP_T::INTTYPE: TYPE0 Position

Definition at line 4412 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos [3/6]

#define GP_INTTYPE_TYPE0_Pos (0)

GP_T::INTTYPE: TYPE0 Position

Definition at line 4412 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos [4/6]

#define GP_INTTYPE_TYPE0_Pos (0)

GP_T::INTTYPE: TYPE0 Position

Definition at line 4412 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos [5/6]

#define GP_INTTYPE_TYPE0_Pos (0)

GP_T::INTTYPE: TYPE0 Position

Definition at line 4412 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos [6/6]

#define GP_INTTYPE_TYPE0_Pos (0)

GP_T::INTTYPE: TYPE0 Position

Definition at line 4412 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk [1/6]

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GP_T::INTTYPE: TYPE1 Mask

Definition at line 4416 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk [2/6]

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GP_T::INTTYPE: TYPE1 Mask

Definition at line 4416 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk [3/6]

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GP_T::INTTYPE: TYPE1 Mask

Definition at line 4416 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk [4/6]

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GP_T::INTTYPE: TYPE1 Mask

Definition at line 4416 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk [5/6]

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GP_T::INTTYPE: TYPE1 Mask

Definition at line 4416 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk [6/6]

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GP_T::INTTYPE: TYPE1 Mask

Definition at line 4416 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos [1/6]

#define GP_INTTYPE_TYPE1_Pos (1)

GP_T::INTTYPE: TYPE1 Position

Definition at line 4415 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos [2/6]

#define GP_INTTYPE_TYPE1_Pos (1)

GP_T::INTTYPE: TYPE1 Position

Definition at line 4415 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos [3/6]

#define GP_INTTYPE_TYPE1_Pos (1)

GP_T::INTTYPE: TYPE1 Position

Definition at line 4415 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos [4/6]

#define GP_INTTYPE_TYPE1_Pos (1)

GP_T::INTTYPE: TYPE1 Position

Definition at line 4415 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos [5/6]

#define GP_INTTYPE_TYPE1_Pos (1)

GP_T::INTTYPE: TYPE1 Position

Definition at line 4415 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos [6/6]

#define GP_INTTYPE_TYPE1_Pos (1)

GP_T::INTTYPE: TYPE1 Position

Definition at line 4415 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk [1/6]

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GP_T::INTTYPE: TYPE2 Mask

Definition at line 4419 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk [2/6]

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GP_T::INTTYPE: TYPE2 Mask

Definition at line 4419 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk [3/6]

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GP_T::INTTYPE: TYPE2 Mask

Definition at line 4419 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk [4/6]

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GP_T::INTTYPE: TYPE2 Mask

Definition at line 4419 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk [5/6]

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GP_T::INTTYPE: TYPE2 Mask

Definition at line 4419 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk [6/6]

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GP_T::INTTYPE: TYPE2 Mask

Definition at line 4419 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos [1/6]

#define GP_INTTYPE_TYPE2_Pos (2)

GP_T::INTTYPE: TYPE2 Position

Definition at line 4418 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos [2/6]

#define GP_INTTYPE_TYPE2_Pos (2)

GP_T::INTTYPE: TYPE2 Position

Definition at line 4418 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos [3/6]

#define GP_INTTYPE_TYPE2_Pos (2)

GP_T::INTTYPE: TYPE2 Position

Definition at line 4418 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos [4/6]

#define GP_INTTYPE_TYPE2_Pos (2)

GP_T::INTTYPE: TYPE2 Position

Definition at line 4418 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos [5/6]

#define GP_INTTYPE_TYPE2_Pos (2)

GP_T::INTTYPE: TYPE2 Position

Definition at line 4418 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos [6/6]

#define GP_INTTYPE_TYPE2_Pos (2)

GP_T::INTTYPE: TYPE2 Position

Definition at line 4418 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk [1/6]

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GP_T::INTTYPE: TYPE3 Mask

Definition at line 4422 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk [2/6]

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GP_T::INTTYPE: TYPE3 Mask

Definition at line 4422 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk [3/6]

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GP_T::INTTYPE: TYPE3 Mask

Definition at line 4422 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk [4/6]

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GP_T::INTTYPE: TYPE3 Mask

Definition at line 4422 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk [5/6]

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GP_T::INTTYPE: TYPE3 Mask

Definition at line 4422 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk [6/6]

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GP_T::INTTYPE: TYPE3 Mask

Definition at line 4422 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos [1/6]

#define GP_INTTYPE_TYPE3_Pos (3)

GP_T::INTTYPE: TYPE3 Position

Definition at line 4421 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos [2/6]

#define GP_INTTYPE_TYPE3_Pos (3)

GP_T::INTTYPE: TYPE3 Position

Definition at line 4421 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos [3/6]

#define GP_INTTYPE_TYPE3_Pos (3)

GP_T::INTTYPE: TYPE3 Position

Definition at line 4421 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos [4/6]

#define GP_INTTYPE_TYPE3_Pos (3)

GP_T::INTTYPE: TYPE3 Position

Definition at line 4421 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos [5/6]

#define GP_INTTYPE_TYPE3_Pos (3)

GP_T::INTTYPE: TYPE3 Position

Definition at line 4421 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos [6/6]

#define GP_INTTYPE_TYPE3_Pos (3)

GP_T::INTTYPE: TYPE3 Position

Definition at line 4421 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk [1/6]

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GP_T::INTTYPE: TYPE4 Mask

Definition at line 4425 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk [2/6]

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GP_T::INTTYPE: TYPE4 Mask

Definition at line 4425 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk [3/6]

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GP_T::INTTYPE: TYPE4 Mask

Definition at line 4425 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk [4/6]

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GP_T::INTTYPE: TYPE4 Mask

Definition at line 4425 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk [5/6]

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GP_T::INTTYPE: TYPE4 Mask

Definition at line 4425 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk [6/6]

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GP_T::INTTYPE: TYPE4 Mask

Definition at line 4425 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos [1/6]

#define GP_INTTYPE_TYPE4_Pos (4)

GP_T::INTTYPE: TYPE4 Position

Definition at line 4424 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos [2/6]

#define GP_INTTYPE_TYPE4_Pos (4)

GP_T::INTTYPE: TYPE4 Position

Definition at line 4424 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos [3/6]

#define GP_INTTYPE_TYPE4_Pos (4)

GP_T::INTTYPE: TYPE4 Position

Definition at line 4424 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos [4/6]

#define GP_INTTYPE_TYPE4_Pos (4)

GP_T::INTTYPE: TYPE4 Position

Definition at line 4424 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos [5/6]

#define GP_INTTYPE_TYPE4_Pos (4)

GP_T::INTTYPE: TYPE4 Position

Definition at line 4424 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos [6/6]

#define GP_INTTYPE_TYPE4_Pos (4)

GP_T::INTTYPE: TYPE4 Position

Definition at line 4424 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk [1/6]

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GP_T::INTTYPE: TYPE5 Mask

Definition at line 4428 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk [2/6]

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GP_T::INTTYPE: TYPE5 Mask

Definition at line 4428 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk [3/6]

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GP_T::INTTYPE: TYPE5 Mask

Definition at line 4428 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk [4/6]

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GP_T::INTTYPE: TYPE5 Mask

Definition at line 4428 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk [5/6]

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GP_T::INTTYPE: TYPE5 Mask

Definition at line 4428 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk [6/6]

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GP_T::INTTYPE: TYPE5 Mask

Definition at line 4428 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos [1/6]

#define GP_INTTYPE_TYPE5_Pos (5)

GP_T::INTTYPE: TYPE5 Position

Definition at line 4427 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos [2/6]

#define GP_INTTYPE_TYPE5_Pos (5)

GP_T::INTTYPE: TYPE5 Position

Definition at line 4427 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos [3/6]

#define GP_INTTYPE_TYPE5_Pos (5)

GP_T::INTTYPE: TYPE5 Position

Definition at line 4427 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos [4/6]

#define GP_INTTYPE_TYPE5_Pos (5)

GP_T::INTTYPE: TYPE5 Position

Definition at line 4427 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos [5/6]

#define GP_INTTYPE_TYPE5_Pos (5)

GP_T::INTTYPE: TYPE5 Position

Definition at line 4427 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos [6/6]

#define GP_INTTYPE_TYPE5_Pos (5)

GP_T::INTTYPE: TYPE5 Position

Definition at line 4427 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk [1/6]

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GP_T::INTTYPE: TYPE6 Mask

Definition at line 4431 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk [2/6]

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GP_T::INTTYPE: TYPE6 Mask

Definition at line 4431 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk [3/6]

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GP_T::INTTYPE: TYPE6 Mask

Definition at line 4431 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk [4/6]

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GP_T::INTTYPE: TYPE6 Mask

Definition at line 4431 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk [5/6]

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GP_T::INTTYPE: TYPE6 Mask

Definition at line 4431 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk [6/6]

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GP_T::INTTYPE: TYPE6 Mask

Definition at line 4431 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos [1/6]

#define GP_INTTYPE_TYPE6_Pos (6)

GP_T::INTTYPE: TYPE6 Position

Definition at line 4430 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos [2/6]

#define GP_INTTYPE_TYPE6_Pos (6)

GP_T::INTTYPE: TYPE6 Position

Definition at line 4430 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos [3/6]

#define GP_INTTYPE_TYPE6_Pos (6)

GP_T::INTTYPE: TYPE6 Position

Definition at line 4430 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos [4/6]

#define GP_INTTYPE_TYPE6_Pos (6)

GP_T::INTTYPE: TYPE6 Position

Definition at line 4430 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos [5/6]

#define GP_INTTYPE_TYPE6_Pos (6)

GP_T::INTTYPE: TYPE6 Position

Definition at line 4430 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos [6/6]

#define GP_INTTYPE_TYPE6_Pos (6)

GP_T::INTTYPE: TYPE6 Position

Definition at line 4430 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk [1/6]

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GP_T::INTTYPE: TYPE7 Mask

Definition at line 4434 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk [2/6]

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GP_T::INTTYPE: TYPE7 Mask

Definition at line 4434 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk [3/6]

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GP_T::INTTYPE: TYPE7 Mask

Definition at line 4434 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk [4/6]

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GP_T::INTTYPE: TYPE7 Mask

Definition at line 4434 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk [5/6]

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GP_T::INTTYPE: TYPE7 Mask

Definition at line 4434 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk [6/6]

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GP_T::INTTYPE: TYPE7 Mask

Definition at line 4434 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos [1/6]

#define GP_INTTYPE_TYPE7_Pos (7)

GP_T::INTTYPE: TYPE7 Position

Definition at line 4433 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos [2/6]

#define GP_INTTYPE_TYPE7_Pos (7)

GP_T::INTTYPE: TYPE7 Position

Definition at line 4433 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos [3/6]

#define GP_INTTYPE_TYPE7_Pos (7)

GP_T::INTTYPE: TYPE7 Position

Definition at line 4433 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos [4/6]

#define GP_INTTYPE_TYPE7_Pos (7)

GP_T::INTTYPE: TYPE7 Position

Definition at line 4433 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos [5/6]

#define GP_INTTYPE_TYPE7_Pos (7)

GP_T::INTTYPE: TYPE7 Position

Definition at line 4433 of file Mini58Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos [6/6]

#define GP_INTTYPE_TYPE7_Pos (7)

GP_T::INTTYPE: TYPE7 Position

Definition at line 4433 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Msk [1/6]

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GP_T::MODE: MODE0 Mask

Definition at line 4275 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Msk [2/6]

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GP_T::MODE: MODE0 Mask

Definition at line 4275 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Msk [3/6]

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GP_T::MODE: MODE0 Mask

Definition at line 4275 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Msk [4/6]

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GP_T::MODE: MODE0 Mask

Definition at line 4275 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Msk [5/6]

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GP_T::MODE: MODE0 Mask

Definition at line 4275 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Msk [6/6]

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GP_T::MODE: MODE0 Mask

Definition at line 4275 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Pos [1/6]

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GP_T::MODE: MODE0 Position

GP_T::MODE: MODE0 Position

Definition at line 4274 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Pos [2/6]

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GP_T::MODE: MODE0 Position

GP_T::MODE: MODE0 Position

Definition at line 4274 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Pos [3/6]

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GP_T::MODE: MODE0 Position

GP_T::MODE: MODE0 Position

Definition at line 4274 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Pos [4/6]

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GP_T::MODE: MODE0 Position

GP_T::MODE: MODE0 Position

Definition at line 4274 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Pos [5/6]

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GP_T::MODE: MODE0 Position

GP_T::MODE: MODE0 Position

Definition at line 4274 of file Mini58Series.h.

## ◆ GP_MODE_MODE0_Pos [6/6]

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GP_T::MODE: MODE0 Position

GP_T::MODE: MODE0 Position

Definition at line 4274 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Msk [1/6]

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GP_T::MODE: MODE1 Mask

Definition at line 4278 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Msk [2/6]

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GP_T::MODE: MODE1 Mask

Definition at line 4278 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Msk [3/6]

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GP_T::MODE: MODE1 Mask

Definition at line 4278 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Msk [4/6]

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GP_T::MODE: MODE1 Mask

Definition at line 4278 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Msk [5/6]

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GP_T::MODE: MODE1 Mask

Definition at line 4278 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Msk [6/6]

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GP_T::MODE: MODE1 Mask

Definition at line 4278 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Pos [1/6]

#define GP_MODE_MODE1_Pos (2)

GP_T::MODE: MODE1 Position

Definition at line 4277 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Pos [2/6]

#define GP_MODE_MODE1_Pos (2)

GP_T::MODE: MODE1 Position

Definition at line 4277 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Pos [3/6]

#define GP_MODE_MODE1_Pos (2)

GP_T::MODE: MODE1 Position

Definition at line 4277 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Pos [4/6]

#define GP_MODE_MODE1_Pos (2)

GP_T::MODE: MODE1 Position

Definition at line 4277 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Pos [5/6]

#define GP_MODE_MODE1_Pos (2)

GP_T::MODE: MODE1 Position

Definition at line 4277 of file Mini58Series.h.

## ◆ GP_MODE_MODE1_Pos [6/6]

#define GP_MODE_MODE1_Pos (2)

GP_T::MODE: MODE1 Position

Definition at line 4277 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Msk [1/6]

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GP_T::MODE: MODE2 Mask

Definition at line 4281 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Msk [2/6]

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GP_T::MODE: MODE2 Mask

Definition at line 4281 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Msk [3/6]

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GP_T::MODE: MODE2 Mask

Definition at line 4281 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Msk [4/6]

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GP_T::MODE: MODE2 Mask

Definition at line 4281 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Msk [5/6]

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GP_T::MODE: MODE2 Mask

Definition at line 4281 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Msk [6/6]

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GP_T::MODE: MODE2 Mask

Definition at line 4281 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Pos [1/6]

#define GP_MODE_MODE2_Pos (4)

GP_T::MODE: MODE2 Position

Definition at line 4280 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Pos [2/6]

#define GP_MODE_MODE2_Pos (4)

GP_T::MODE: MODE2 Position

Definition at line 4280 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Pos [3/6]

#define GP_MODE_MODE2_Pos (4)

GP_T::MODE: MODE2 Position

Definition at line 4280 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Pos [4/6]

#define GP_MODE_MODE2_Pos (4)

GP_T::MODE: MODE2 Position

Definition at line 4280 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Pos [5/6]

#define GP_MODE_MODE2_Pos (4)

GP_T::MODE: MODE2 Position

Definition at line 4280 of file Mini58Series.h.

## ◆ GP_MODE_MODE2_Pos [6/6]

#define GP_MODE_MODE2_Pos (4)

GP_T::MODE: MODE2 Position

Definition at line 4280 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Msk [1/6]

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GP_T::MODE: MODE3 Mask

Definition at line 4284 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Msk [2/6]

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GP_T::MODE: MODE3 Mask

Definition at line 4284 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Msk [3/6]

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GP_T::MODE: MODE3 Mask

Definition at line 4284 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Msk [4/6]

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GP_T::MODE: MODE3 Mask

Definition at line 4284 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Msk [5/6]

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GP_T::MODE: MODE3 Mask

Definition at line 4284 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Msk [6/6]

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GP_T::MODE: MODE3 Mask

Definition at line 4284 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Pos [1/6]

#define GP_MODE_MODE3_Pos (6)

GP_T::MODE: MODE3 Position

Definition at line 4283 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Pos [2/6]

#define GP_MODE_MODE3_Pos (6)

GP_T::MODE: MODE3 Position

Definition at line 4283 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Pos [3/6]

#define GP_MODE_MODE3_Pos (6)

GP_T::MODE: MODE3 Position

Definition at line 4283 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Pos [4/6]

#define GP_MODE_MODE3_Pos (6)

GP_T::MODE: MODE3 Position

Definition at line 4283 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Pos [5/6]

#define GP_MODE_MODE3_Pos (6)

GP_T::MODE: MODE3 Position

Definition at line 4283 of file Mini58Series.h.

## ◆ GP_MODE_MODE3_Pos [6/6]

#define GP_MODE_MODE3_Pos (6)

GP_T::MODE: MODE3 Position

Definition at line 4283 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Msk [1/6]

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GP_T::MODE: MODE4 Mask

Definition at line 4287 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Msk [2/6]

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GP_T::MODE: MODE4 Mask

Definition at line 4287 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Msk [3/6]

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GP_T::MODE: MODE4 Mask

Definition at line 4287 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Msk [4/6]

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GP_T::MODE: MODE4 Mask

Definition at line 4287 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Msk [5/6]

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GP_T::MODE: MODE4 Mask

Definition at line 4287 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Msk [6/6]

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GP_T::MODE: MODE4 Mask

Definition at line 4287 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Pos [1/6]

#define GP_MODE_MODE4_Pos (8)

GP_T::MODE: MODE4 Position

Definition at line 4286 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Pos [2/6]

#define GP_MODE_MODE4_Pos (8)

GP_T::MODE: MODE4 Position

Definition at line 4286 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Pos [3/6]

#define GP_MODE_MODE4_Pos (8)

GP_T::MODE: MODE4 Position

Definition at line 4286 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Pos [4/6]

#define GP_MODE_MODE4_Pos (8)

GP_T::MODE: MODE4 Position

Definition at line 4286 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Pos [5/6]

#define GP_MODE_MODE4_Pos (8)

GP_T::MODE: MODE4 Position

Definition at line 4286 of file Mini58Series.h.

## ◆ GP_MODE_MODE4_Pos [6/6]

#define GP_MODE_MODE4_Pos (8)

GP_T::MODE: MODE4 Position

Definition at line 4286 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Msk [1/6]

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GP_T::MODE: MODE5 Mask

Definition at line 4290 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Msk [2/6]

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GP_T::MODE: MODE5 Mask

Definition at line 4290 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Msk [3/6]

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GP_T::MODE: MODE5 Mask

Definition at line 4290 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Msk [4/6]

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GP_T::MODE: MODE5 Mask

Definition at line 4290 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Msk [5/6]

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GP_T::MODE: MODE5 Mask

Definition at line 4290 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Msk [6/6]

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GP_T::MODE: MODE5 Mask

Definition at line 4290 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Pos [1/6]

#define GP_MODE_MODE5_Pos (10)

GP_T::MODE: MODE5 Position

Definition at line 4289 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Pos [2/6]

#define GP_MODE_MODE5_Pos (10)

GP_T::MODE: MODE5 Position

Definition at line 4289 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Pos [3/6]

#define GP_MODE_MODE5_Pos (10)

GP_T::MODE: MODE5 Position

Definition at line 4289 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Pos [4/6]

#define GP_MODE_MODE5_Pos (10)

GP_T::MODE: MODE5 Position

Definition at line 4289 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Pos [5/6]

#define GP_MODE_MODE5_Pos (10)

GP_T::MODE: MODE5 Position

Definition at line 4289 of file Mini58Series.h.

## ◆ GP_MODE_MODE5_Pos [6/6]

#define GP_MODE_MODE5_Pos (10)

GP_T::MODE: MODE5 Position

Definition at line 4289 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Msk [1/6]

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GP_T::PIN: PIN0 Mask

Definition at line 4365 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Msk [2/6]

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GP_T::PIN: PIN0 Mask

Definition at line 4365 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Msk [3/6]

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GP_T::PIN: PIN0 Mask

Definition at line 4365 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Msk [4/6]

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GP_T::PIN: PIN0 Mask

Definition at line 4365 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Msk [5/6]

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GP_T::PIN: PIN0 Mask

Definition at line 4365 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Msk [6/6]

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GP_T::PIN: PIN0 Mask

Definition at line 4365 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Pos [1/6]

#define GP_PIN_PIN0_Pos (0)

GP_T::PIN: PIN0 Position

Definition at line 4364 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Pos [2/6]

#define GP_PIN_PIN0_Pos (0)

GP_T::PIN: PIN0 Position

Definition at line 4364 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Pos [3/6]

#define GP_PIN_PIN0_Pos (0)

GP_T::PIN: PIN0 Position

Definition at line 4364 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Pos [4/6]

#define GP_PIN_PIN0_Pos (0)

GP_T::PIN: PIN0 Position

Definition at line 4364 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Pos [5/6]

#define GP_PIN_PIN0_Pos (0)

GP_T::PIN: PIN0 Position

Definition at line 4364 of file Mini58Series.h.

## ◆ GP_PIN_PIN0_Pos [6/6]

#define GP_PIN_PIN0_Pos (0)

GP_T::PIN: PIN0 Position

Definition at line 4364 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Msk [1/6]

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GP_T::PIN: PIN1 Mask

Definition at line 4368 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Msk [2/6]

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GP_T::PIN: PIN1 Mask

Definition at line 4368 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Msk [3/6]

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GP_T::PIN: PIN1 Mask

Definition at line 4368 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Msk [4/6]

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GP_T::PIN: PIN1 Mask

Definition at line 4368 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Msk [5/6]

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GP_T::PIN: PIN1 Mask

Definition at line 4368 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Msk [6/6]

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GP_T::PIN: PIN1 Mask

Definition at line 4368 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Pos [1/6]

#define GP_PIN_PIN1_Pos (1)

GP_T::PIN: PIN1 Position

Definition at line 4367 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Pos [2/6]

#define GP_PIN_PIN1_Pos (1)

GP_T::PIN: PIN1 Position

Definition at line 4367 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Pos [3/6]

#define GP_PIN_PIN1_Pos (1)

GP_T::PIN: PIN1 Position

Definition at line 4367 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Pos [4/6]

#define GP_PIN_PIN1_Pos (1)

GP_T::PIN: PIN1 Position

Definition at line 4367 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Pos [5/6]

#define GP_PIN_PIN1_Pos (1)

GP_T::PIN: PIN1 Position

Definition at line 4367 of file Mini58Series.h.

## ◆ GP_PIN_PIN1_Pos [6/6]

#define GP_PIN_PIN1_Pos (1)

GP_T::PIN: PIN1 Position

Definition at line 4367 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Msk [1/6]

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GP_T::PIN: PIN2 Mask

Definition at line 4371 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Msk [2/6]

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GP_T::PIN: PIN2 Mask

Definition at line 4371 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Msk [3/6]

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GP_T::PIN: PIN2 Mask

Definition at line 4371 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Msk [4/6]

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GP_T::PIN: PIN2 Mask

Definition at line 4371 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Msk [5/6]

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GP_T::PIN: PIN2 Mask

Definition at line 4371 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Msk [6/6]

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GP_T::PIN: PIN2 Mask

Definition at line 4371 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Pos [1/6]

#define GP_PIN_PIN2_Pos (2)

GP_T::PIN: PIN2 Position

Definition at line 4370 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Pos [2/6]

#define GP_PIN_PIN2_Pos (2)

GP_T::PIN: PIN2 Position

Definition at line 4370 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Pos [3/6]

#define GP_PIN_PIN2_Pos (2)

GP_T::PIN: PIN2 Position

Definition at line 4370 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Pos [4/6]

#define GP_PIN_PIN2_Pos (2)

GP_T::PIN: PIN2 Position

Definition at line 4370 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Pos [5/6]

#define GP_PIN_PIN2_Pos (2)

GP_T::PIN: PIN2 Position

Definition at line 4370 of file Mini58Series.h.

## ◆ GP_PIN_PIN2_Pos [6/6]

#define GP_PIN_PIN2_Pos (2)

GP_T::PIN: PIN2 Position

Definition at line 4370 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Msk [1/6]

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GP_T::PIN: PIN3 Mask

Definition at line 4374 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Msk [2/6]

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GP_T::PIN: PIN3 Mask

Definition at line 4374 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Msk [3/6]

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GP_T::PIN: PIN3 Mask

Definition at line 4374 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Msk [4/6]

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GP_T::PIN: PIN3 Mask

Definition at line 4374 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Msk [5/6]

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GP_T::PIN: PIN3 Mask

Definition at line 4374 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Msk [6/6]

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GP_T::PIN: PIN3 Mask

Definition at line 4374 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Pos [1/6]

#define GP_PIN_PIN3_Pos (3)

GP_T::PIN: PIN3 Position

Definition at line 4373 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Pos [2/6]

#define GP_PIN_PIN3_Pos (3)

GP_T::PIN: PIN3 Position

Definition at line 4373 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Pos [3/6]

#define GP_PIN_PIN3_Pos (3)

GP_T::PIN: PIN3 Position

Definition at line 4373 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Pos [4/6]

#define GP_PIN_PIN3_Pos (3)

GP_T::PIN: PIN3 Position

Definition at line 4373 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Pos [5/6]

#define GP_PIN_PIN3_Pos (3)

GP_T::PIN: PIN3 Position

Definition at line 4373 of file Mini58Series.h.

## ◆ GP_PIN_PIN3_Pos [6/6]

#define GP_PIN_PIN3_Pos (3)

GP_T::PIN: PIN3 Position

Definition at line 4373 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Msk [1/6]

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GP_T::PIN: PIN4 Mask

Definition at line 4377 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Msk [2/6]

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GP_T::PIN: PIN4 Mask

Definition at line 4377 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Msk [3/6]

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GP_T::PIN: PIN4 Mask

Definition at line 4377 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Msk [4/6]

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GP_T::PIN: PIN4 Mask

Definition at line 4377 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Msk [5/6]

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GP_T::PIN: PIN4 Mask

Definition at line 4377 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Msk [6/6]

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GP_T::PIN: PIN4 Mask

Definition at line 4377 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Pos [1/6]

#define GP_PIN_PIN4_Pos (4)

GP_T::PIN: PIN4 Position

Definition at line 4376 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Pos [2/6]

#define GP_PIN_PIN4_Pos (4)

GP_T::PIN: PIN4 Position

Definition at line 4376 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Pos [3/6]

#define GP_PIN_PIN4_Pos (4)

GP_T::PIN: PIN4 Position

Definition at line 4376 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Pos [4/6]

#define GP_PIN_PIN4_Pos (4)

GP_T::PIN: PIN4 Position

Definition at line 4376 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Pos [5/6]

#define GP_PIN_PIN4_Pos (4)

GP_T::PIN: PIN4 Position

Definition at line 4376 of file Mini58Series.h.

## ◆ GP_PIN_PIN4_Pos [6/6]

#define GP_PIN_PIN4_Pos (4)

GP_T::PIN: PIN4 Position

Definition at line 4376 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Msk [1/6]

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GP_T::PIN: PIN5 Mask

Definition at line 4380 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Msk [2/6]

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GP_T::PIN: PIN5 Mask

Definition at line 4380 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Msk [3/6]

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GP_T::PIN: PIN5 Mask

Definition at line 4380 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Msk [4/6]

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GP_T::PIN: PIN5 Mask

Definition at line 4380 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Msk [5/6]

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GP_T::PIN: PIN5 Mask

Definition at line 4380 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Msk [6/6]

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GP_T::PIN: PIN5 Mask

Definition at line 4380 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Pos [1/6]

#define GP_PIN_PIN5_Pos (5)

GP_T::PIN: PIN5 Position

Definition at line 4379 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Pos [2/6]

#define GP_PIN_PIN5_Pos (5)

GP_T::PIN: PIN5 Position

Definition at line 4379 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Pos [3/6]

#define GP_PIN_PIN5_Pos (5)

GP_T::PIN: PIN5 Position

Definition at line 4379 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Pos [4/6]

#define GP_PIN_PIN5_Pos (5)

GP_T::PIN: PIN5 Position

Definition at line 4379 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Pos [5/6]

#define GP_PIN_PIN5_Pos (5)

GP_T::PIN: PIN5 Position

Definition at line 4379 of file Mini58Series.h.

## ◆ GP_PIN_PIN5_Pos [6/6]

#define GP_PIN_PIN5_Pos (5)

GP_T::PIN: PIN5 Position

Definition at line 4379 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Msk [1/6]

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GP_T::PIN: PIN6 Mask

Definition at line 4383 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Msk [2/6]

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GP_T::PIN: PIN6 Mask

Definition at line 4383 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Msk [3/6]

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GP_T::PIN: PIN6 Mask

Definition at line 4383 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Msk [4/6]

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GP_T::PIN: PIN6 Mask

Definition at line 4383 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Msk [5/6]

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GP_T::PIN: PIN6 Mask

Definition at line 4383 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Msk [6/6]

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GP_T::PIN: PIN6 Mask

Definition at line 4383 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Pos [1/6]

#define GP_PIN_PIN6_Pos (6)

GP_T::PIN: PIN6 Position

Definition at line 4382 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Pos [2/6]

#define GP_PIN_PIN6_Pos (6)

GP_T::PIN: PIN6 Position

Definition at line 4382 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Pos [3/6]

#define GP_PIN_PIN6_Pos (6)

GP_T::PIN: PIN6 Position

Definition at line 4382 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Pos [4/6]

#define GP_PIN_PIN6_Pos (6)

GP_T::PIN: PIN6 Position

Definition at line 4382 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Pos [5/6]

#define GP_PIN_PIN6_Pos (6)

GP_T::PIN: PIN6 Position

Definition at line 4382 of file Mini58Series.h.

## ◆ GP_PIN_PIN6_Pos [6/6]

#define GP_PIN_PIN6_Pos (6)

GP_T::PIN: PIN6 Position

Definition at line 4382 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Msk [1/6]

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GP_T::PIN: PIN7 Mask

Definition at line 4386 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Msk [2/6]

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GP_T::PIN: PIN7 Mask

Definition at line 4386 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Msk [3/6]

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GP_T::PIN: PIN7 Mask

Definition at line 4386 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Msk [4/6]

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GP_T::PIN: PIN7 Mask

Definition at line 4386 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Msk [5/6]

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GP_T::PIN: PIN7 Mask

Definition at line 4386 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Msk [6/6]

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GP_T::PIN: PIN7 Mask

Definition at line 4386 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Pos [1/6]

#define GP_PIN_PIN7_Pos (7)

GP_T::PIN: PIN7 Position

Definition at line 4385 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Pos [2/6]

#define GP_PIN_PIN7_Pos (7)

GP_T::PIN: PIN7 Position

Definition at line 4385 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Pos [3/6]

#define GP_PIN_PIN7_Pos (7)

GP_T::PIN: PIN7 Position

Definition at line 4385 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Pos [4/6]

#define GP_PIN_PIN7_Pos (7)

GP_T::PIN: PIN7 Position

Definition at line 4385 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Pos [5/6]

#define GP_PIN_PIN7_Pos (7)

GP_T::PIN: PIN7 Position

Definition at line 4385 of file Mini58Series.h.

## ◆ GP_PIN_PIN7_Pos [6/6]

#define GP_PIN_PIN7_Pos (7)

GP_T::PIN: PIN7 Position

Definition at line 4385 of file Mini58Series.h.

## ◆ I2C_ADDR0_ADDR_Msk

#define I2C_ADDR0_ADDR_Msk (0x7ful << I2C_ADDR0_ADDR_Pos)

I2C_T::ADDR0: ADDR Mask

Definition at line 4865 of file Mini58Series.h.

## ◆ I2C_ADDR0_ADDR_Pos

#define I2C_ADDR0_ADDR_Pos (1)

I2C_T::ADDR0: ADDR Position

Definition at line 4864 of file Mini58Series.h.

## ◆ I2C_ADDR0_GC_Msk

#define I2C_ADDR0_GC_Msk (0x1ul << I2C_ADDR0_GC_Pos)

I2C_T::ADDR0: GC Mask

Definition at line 4862 of file Mini58Series.h.

## ◆ I2C_ADDR0_GC_Pos

#define I2C_ADDR0_GC_Pos (0)

I2C_T::ADDR0: GC Position

Definition at line 4861 of file Mini58Series.h.

## ◆ I2C_ADDR1_ADDR_Msk

#define I2C_ADDR1_ADDR_Msk (0x7ful << I2C_ADDR1_ADDR_Pos)

I2C_T::ADDR1: ADDR Mask

Definition at line 4889 of file Mini58Series.h.

## ◆ I2C_ADDR1_ADDR_Pos

#define I2C_ADDR1_ADDR_Pos (1)

I2C_T::ADDR1: ADDR Position

Definition at line 4888 of file Mini58Series.h.

## ◆ I2C_ADDR1_GC_Msk

#define I2C_ADDR1_GC_Msk (0x1ul << I2C_ADDR1_GC_Pos)

I2C_T::ADDR1: GC Mask

Definition at line 4886 of file Mini58Series.h.

## ◆ I2C_ADDR1_GC_Pos

#define I2C_ADDR1_GC_Pos (0)

I2C_T::ADDR1: GC Position

Definition at line 4885 of file Mini58Series.h.

## ◆ I2C_ADDR2_ADDR_Msk

#define I2C_ADDR2_ADDR_Msk (0x7ful << I2C_ADDR2_ADDR_Pos)

I2C_T::ADDR2: ADDR Mask

Definition at line 4895 of file Mini58Series.h.

## ◆ I2C_ADDR2_ADDR_Pos

#define I2C_ADDR2_ADDR_Pos (1)

I2C_T::ADDR2: ADDR Position

Definition at line 4894 of file Mini58Series.h.

## ◆ I2C_ADDR2_GC_Msk

#define I2C_ADDR2_GC_Msk (0x1ul << I2C_ADDR2_GC_Pos)

I2C_T::ADDR2: GC Mask

Definition at line 4892 of file Mini58Series.h.

## ◆ I2C_ADDR2_GC_Pos

#define I2C_ADDR2_GC_Pos (0)

I2C_T::ADDR2: GC Position

Definition at line 4891 of file Mini58Series.h.

## ◆ I2C_ADDR3_ADDR_Msk

#define I2C_ADDR3_ADDR_Msk (0x7ful << I2C_ADDR3_ADDR_Pos)

I2C_T::ADDR3: ADDR Mask

Definition at line 4901 of file Mini58Series.h.

## ◆ I2C_ADDR3_ADDR_Pos

#define I2C_ADDR3_ADDR_Pos (1)

I2C_T::ADDR3: ADDR Position

Definition at line 4900 of file Mini58Series.h.

## ◆ I2C_ADDR3_GC_Msk

#define I2C_ADDR3_GC_Msk (0x1ul << I2C_ADDR3_GC_Pos)

I2C_T::ADDR3: GC Mask

Definition at line 4898 of file Mini58Series.h.

## ◆ I2C_ADDR3_GC_Pos

#define I2C_ADDR3_GC_Pos (0)

I2C_T::ADDR3: GC Position

Definition at line 4897 of file Mini58Series.h.

## ◆ I2C_ADDRMSK0_ADDRMSK_Msk

#define I2C_ADDRMSK0_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK0_ADDRMSK_Pos)

I2C_T::ADDRMSK0: ADDRMSK Mask

Definition at line 4904 of file Mini58Series.h.

## ◆ I2C_ADDRMSK0_ADDRMSK_Pos

#define I2C_ADDRMSK0_ADDRMSK_Pos (1)

I2C_T::ADDRMSK0: ADDRMSK Position

Definition at line 4903 of file Mini58Series.h.

## ◆ I2C_ADDRMSK1_ADDRMSK_Msk

#define I2C_ADDRMSK1_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK1_ADDRMSK_Pos)

I2C_T::ADDRMSK1: ADDRMSK Mask

Definition at line 4907 of file Mini58Series.h.

## ◆ I2C_ADDRMSK1_ADDRMSK_Pos

#define I2C_ADDRMSK1_ADDRMSK_Pos (1)

I2C_T::ADDRMSK1: ADDRMSK Position

Definition at line 4906 of file Mini58Series.h.

## ◆ I2C_ADDRMSK2_ADDRMSK_Msk

#define I2C_ADDRMSK2_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK2_ADDRMSK_Pos)

I2C_T::ADDRMSK2: ADDRMSK Mask

Definition at line 4910 of file Mini58Series.h.

## ◆ I2C_ADDRMSK2_ADDRMSK_Pos

#define I2C_ADDRMSK2_ADDRMSK_Pos (1)

I2C_T::ADDRMSK2: ADDRMSK Position

Definition at line 4909 of file Mini58Series.h.

## ◆ I2C_ADDRMSK3_ADDRMSK_Msk

#define I2C_ADDRMSK3_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK3_ADDRMSK_Pos)

I2C_T::ADDRMSK3: ADDRMSK Mask

Definition at line 4913 of file Mini58Series.h.

## ◆ I2C_ADDRMSK3_ADDRMSK_Pos

#define I2C_ADDRMSK3_ADDRMSK_Pos (1)

I2C_T::ADDRMSK3: ADDRMSK Position

Definition at line 4912 of file Mini58Series.h.

## ◆ I2C_CLKDIV_DIVIDER_Msk

#define I2C_CLKDIV_DIVIDER_Msk (0xfful << I2C_CLKDIV_DIVIDER_Pos)

I2C_T::CLKDIV: DIVIDER Mask

Definition at line 4874 of file Mini58Series.h.

## ◆ I2C_CLKDIV_DIVIDER_Pos

#define I2C_CLKDIV_DIVIDER_Pos (0)

I2C_T::CLKDIV: DIVIDER Position

Definition at line 4873 of file Mini58Series.h.

## ◆ I2C_CTL1_NSTRETCH_Msk

#define I2C_CTL1_NSTRETCH_Msk (0x1ul << I2C_CTL1_NSTRETCH_Pos)

I2C_T::CTL1: NSTRETCH Mask

Definition at line 4922 of file Mini58Series.h.

## ◆ I2C_CTL1_NSTRETCH_Pos

#define I2C_CTL1_NSTRETCH_Pos (2)

I2C_T::CTL1: NSTRETCH Position

Definition at line 4921 of file Mini58Series.h.

## ◆ I2C_CTL1_OVIEN_Msk

#define I2C_CTL1_OVIEN_Msk (0x1ul << I2C_CTL1_OVIEN_Pos)

I2C_T::CTL1: OVIEN Mask

Definition at line 4925 of file Mini58Series.h.

## ◆ I2C_CTL1_OVIEN_Pos

#define I2C_CTL1_OVIEN_Pos (3)

I2C_T::CTL1: OVIEN Position

Definition at line 4924 of file Mini58Series.h.

## ◆ I2C_CTL1_TWOLVFIFO_Msk

#define I2C_CTL1_TWOLVFIFO_Msk (0x1ul << I2C_CTL1_TWOLVFIFO_Pos)

I2C_T::CTL1: TWOLVFIFO Mask

Definition at line 4919 of file Mini58Series.h.

## ◆ I2C_CTL1_TWOLVFIFO_Pos

#define I2C_CTL1_TWOLVFIFO_Pos (1)

I2C_T::CTL1: TWOLVFIFO Position

Definition at line 4918 of file Mini58Series.h.

## ◆ I2C_CTL1_URIEN_Msk

#define I2C_CTL1_URIEN_Msk (0x1ul << I2C_CTL1_URIEN_Pos)

I2C_T::CTL1: URIEN Mask

Definition at line 4928 of file Mini58Series.h.

## ◆ I2C_CTL1_URIEN_Pos

#define I2C_CTL1_URIEN_Pos (4)

I2C_T::CTL1: URIEN Position

Definition at line 4927 of file Mini58Series.h.

## ◆ I2C_CTL1_WKEN_Msk

#define I2C_CTL1_WKEN_Msk (0x1ul << I2C_CTL1_WKEN_Pos)

I2C_T::CTL1: WKEN Mask

Definition at line 4916 of file Mini58Series.h.

## ◆ I2C_CTL1_WKEN_Pos

#define I2C_CTL1_WKEN_Pos (0)

I2C_T::CTL1: WKEN Position

Definition at line 4915 of file Mini58Series.h.

## ◆ I2C_CTL_AA_Msk

#define I2C_CTL_AA_Msk (0x1ul << I2C_CTL_AA_Pos)

I2C_T::CTL: AA Mask

Definition at line 4844 of file Mini58Series.h.

## ◆ I2C_CTL_AA_Pos

#define I2C_CTL_AA_Pos (2)

    @addtogroup I2C_CONST I2C Bit Field Definition
    Constant Definitions for I2C Controller

I2C_T::CTL: AA Position

Definition at line 4843 of file Mini58Series.h.

## ◆ I2C_CTL_I2CEN_Msk

#define I2C_CTL_I2CEN_Msk (0x1ul << I2C_CTL_I2CEN_Pos)

I2C_T::CTL: I2CEN Mask

Definition at line 4856 of file Mini58Series.h.

## ◆ I2C_CTL_I2CEN_Pos

#define I2C_CTL_I2CEN_Pos (6)

I2C_T::CTL: I2CEN Position

Definition at line 4855 of file Mini58Series.h.

## ◆ I2C_CTL_INTEN_Msk

#define I2C_CTL_INTEN_Msk (0x1ul << I2C_CTL_INTEN_Pos)

I2C_T::CTL: INTEN Mask

Definition at line 4859 of file Mini58Series.h.

## ◆ I2C_CTL_INTEN_Pos

#define I2C_CTL_INTEN_Pos (7)

I2C_T::CTL: INTEN Position

Definition at line 4858 of file Mini58Series.h.

## ◆ I2C_CTL_SI_Msk

#define I2C_CTL_SI_Msk (0x1ul << I2C_CTL_SI_Pos)

I2C_T::CTL: SI Mask

Definition at line 4847 of file Mini58Series.h.

## ◆ I2C_CTL_SI_Pos

#define I2C_CTL_SI_Pos (3)

I2C_T::CTL: SI Position

Definition at line 4846 of file Mini58Series.h.

## ◆ I2C_CTL_STA_Msk

#define I2C_CTL_STA_Msk (0x1ul << I2C_CTL_STA_Pos)

I2C_T::CTL: STA Mask

Definition at line 4853 of file Mini58Series.h.

## ◆ I2C_CTL_STA_Pos

#define I2C_CTL_STA_Pos (5)

I2C_T::CTL: STA Position

Definition at line 4852 of file Mini58Series.h.

## ◆ I2C_CTL_STO_Msk

#define I2C_CTL_STO_Msk (0x1ul << I2C_CTL_STO_Pos)

I2C_T::CTL: STO Mask

Definition at line 4850 of file Mini58Series.h.

## ◆ I2C_CTL_STO_Pos

#define I2C_CTL_STO_Pos (4)

I2C_T::CTL: STO Position

Definition at line 4849 of file Mini58Series.h.

## ◆ I2C_DAT_DAT_Msk

#define I2C_DAT_DAT_Msk (0xfful << I2C_DAT_DAT_Pos)

I2C_T::DAT: DAT Mask

Definition at line 4868 of file Mini58Series.h.

## ◆ I2C_DAT_DAT_Pos

#define I2C_DAT_DAT_Pos (0)

I2C_T::DAT: DAT Position

Definition at line 4867 of file Mini58Series.h.

## ◆ I2C_STATUS1_EMPTY_Msk

#define I2C_STATUS1_EMPTY_Msk (0x1ul << I2C_STATUS1_EMPTY_Pos)

I2C_T::STATUS1: EMPTY Mask

Definition at line 4937 of file Mini58Series.h.

## ◆ I2C_STATUS1_EMPTY_Pos

#define I2C_STATUS1_EMPTY_Pos (2)

I2C_T::STATUS1: EMPTY Position

Definition at line 4936 of file Mini58Series.h.

## ◆ I2C_STATUS1_FULL_Msk

#define I2C_STATUS1_FULL_Msk (0x1ul << I2C_STATUS1_FULL_Pos)

I2C_T::STATUS1: FULL Mask

Definition at line 4934 of file Mini58Series.h.

## ◆ I2C_STATUS1_FULL_Pos

#define I2C_STATUS1_FULL_Pos (1)

I2C_T::STATUS1: FULL Position

Definition at line 4933 of file Mini58Series.h.

## ◆ I2C_STATUS1_OVIF_Msk

#define I2C_STATUS1_OVIF_Msk (0x1ul << I2C_STATUS1_OVIF_Pos)

I2C_T::STATUS1: OVIF Mask

Definition at line 4940 of file Mini58Series.h.

## ◆ I2C_STATUS1_OVIF_Pos

#define I2C_STATUS1_OVIF_Pos (3)

I2C_T::STATUS1: OVIF Position

Definition at line 4939 of file Mini58Series.h.

## ◆ I2C_STATUS1_URIF_Msk

#define I2C_STATUS1_URIF_Msk (0x1ul << I2C_STATUS1_URIF_Pos)

I2C_T::STATUS1: URIF Mask

Definition at line 4943 of file Mini58Series.h.

## ◆ I2C_STATUS1_URIF_Pos

#define I2C_STATUS1_URIF_Pos (4)

I2C_T::STATUS1: URIF Position

Definition at line 4942 of file Mini58Series.h.

## ◆ I2C_STATUS1_WKIF_Msk

#define I2C_STATUS1_WKIF_Msk (0x1ul << I2C_STATUS1_WKIF_Pos)

I2C_T::STATUS1: WKIF Mask

Definition at line 4931 of file Mini58Series.h.

## ◆ I2C_STATUS1_WKIF_Pos

#define I2C_STATUS1_WKIF_Pos (0)

I2C_T::STATUS1: WKIF Position

Definition at line 4930 of file Mini58Series.h.

## ◆ I2C_STATUS_STATUS_Msk

#define I2C_STATUS_STATUS_Msk (0xfful << I2C_STATUS_STATUS_Pos)

I2C_T::STATUS: STATUS Mask

Definition at line 4871 of file Mini58Series.h.

## ◆ I2C_STATUS_STATUS_Pos

#define I2C_STATUS_STATUS_Pos (0)

I2C_T::STATUS: STATUS Position

Definition at line 4870 of file Mini58Series.h.

## ◆ I2C_TOCTL_TOCEN_Msk

#define I2C_TOCTL_TOCEN_Msk (0x1ul << I2C_TOCTL_TOCEN_Pos)

I2C_T::TOCTL: TOCEN Mask

Definition at line 4883 of file Mini58Series.h.

## ◆ I2C_TOCTL_TOCEN_Pos

#define I2C_TOCTL_TOCEN_Pos (2)

I2C_T::TOCTL: TOCEN Position

Definition at line 4882 of file Mini58Series.h.

## ◆ I2C_TOCTL_TOCURIEN_Msk

#define I2C_TOCTL_TOCURIEN_Msk (0x1ul << I2C_TOCTL_TOCURIEN_Pos)

I2C_T::TOCTL: TOCURIEN Mask

Definition at line 4880 of file Mini58Series.h.

## ◆ I2C_TOCTL_TOCURIEN_Pos

#define I2C_TOCTL_TOCURIEN_Pos (1)

I2C_T::TOCTL: TOCURIEN Position

Definition at line 4879 of file Mini58Series.h.

## ◆ I2C_TOCTL_TOIF_Msk

#define I2C_TOCTL_TOIF_Msk (0x1ul << I2C_TOCTL_TOIF_Pos)

I2C_T::TOCTL: TOIF Mask

Definition at line 4877 of file Mini58Series.h.

## ◆ I2C_TOCTL_TOIF_Pos

#define I2C_TOCTL_TOIF_Pos (0)

I2C_T::TOCTL: TOIF Position

Definition at line 4876 of file Mini58Series.h.

## ◆ INT_CON_NMI_SEL_EN_Msk

#define INT_CON_NMI_SEL_EN_Msk (0x1ul << INT_CON_NMI_SEL_EN_Pos)

INT_T::CON: NMI_SEL_EN Mask

Definition at line 5363 of file Mini58Series.h.

## ◆ INT_CON_NMI_SEL_EN_Pos

#define INT_CON_NMI_SEL_EN_Pos (8)

INT_T::CON: NMI_SEL_EN Position

Definition at line 5362 of file Mini58Series.h.

## ◆ INT_CON_NMI_SEL_Msk

#define INT_CON_NMI_SEL_Msk (0x1ful << INT_CON_NMI_SEL_Pos)

INT_T::CON: NMI_SEL Mask

Definition at line 5360 of file Mini58Series.h.

## ◆ INT_CON_NMI_SEL_Pos

#define INT_CON_NMI_SEL_Pos (0)

INT_T::CON: NMI_SEL Position

Definition at line 5359 of file Mini58Series.h.

## ◆ INT_IRQ0_SRC_BOD_INT_Msk

#define INT_IRQ0_SRC_BOD_INT_Msk (0x1ul << INT_IRQ0_SRC_BOD_INT_Pos)

INT_T::IRQ0_SRC: BOD_INT Mask

Definition at line 5288 of file Mini58Series.h.

## ◆ INT_IRQ0_SRC_BOD_INT_Pos

#define INT_IRQ0_SRC_BOD_INT_Pos (0)

    @addtogroup INT_CONST INT Bit Field Definition
    Constant Definitions for INT Controller

INT_T::IRQ0_SRC: BOD_INT Position

Definition at line 5287 of file Mini58Series.h.

## ◆ INT_IRQ12_SRC_UART0_INT_Msk

#define INT_IRQ12_SRC_UART0_INT_Msk (0x1ul << INT_IRQ12_SRC_UART0_INT_Pos)

INT_T::IRQ12_SRC: UART0_INT Mask

Definition at line 5330 of file Mini58Series.h.

## ◆ INT_IRQ12_SRC_UART0_INT_Pos

#define INT_IRQ12_SRC_UART0_INT_Pos (0)

INT_T::IRQ12_SRC: UART0_INT Position

Definition at line 5329 of file Mini58Series.h.

## ◆ INT_IRQ13_SRC_UART1_INT_Msk

#define INT_IRQ13_SRC_UART1_INT_Msk (0x1ul << INT_IRQ13_SRC_UART1_INT_Pos)

INT_T::IRQ13_SRC: UART1_INT Mask

Definition at line 5333 of file Mini58Series.h.

## ◆ INT_IRQ13_SRC_UART1_INT_Pos

#define INT_IRQ13_SRC_UART1_INT_Pos (0)

INT_T::IRQ13_SRC: UART1_INT Position

Definition at line 5332 of file Mini58Series.h.

## ◆ INT_IRQ14_SRC_SPI_INT_Msk

#define INT_IRQ14_SRC_SPI_INT_Msk (0x1ul << INT_IRQ14_SRC_SPI_INT_Pos)

INT_T::IRQ14_SRC: SPI_INT Mask

Definition at line 5336 of file Mini58Series.h.

## ◆ INT_IRQ14_SRC_SPI_INT_Pos

#define INT_IRQ14_SRC_SPI_INT_Pos (0)

INT_T::IRQ14_SRC: SPI_INT Position

Definition at line 5335 of file Mini58Series.h.

## ◆ INT_IRQ16_SRC_GP5_INT_Msk

#define INT_IRQ16_SRC_GP5_INT_Msk (0x1ul << INT_IRQ16_SRC_GP5_INT_Pos)

INT_T::IRQ16_SRC: GP5_INT Mask

Definition at line 5339 of file Mini58Series.h.

## ◆ INT_IRQ16_SRC_GP5_INT_Pos

#define INT_IRQ16_SRC_GP5_INT_Pos (0)

INT_T::IRQ16_SRC: GP5_INT Position

Definition at line 5338 of file Mini58Series.h.

## ◆ INT_IRQ17_SRC_HIRC_TRIM_INT_Msk

#define INT_IRQ17_SRC_HIRC_TRIM_INT_Msk (0x1ul << INT_IRQ17_SRC_HIRC_TRIM_INT_Pos)

INT_T::IRQ17_SRC: HIRC_TRIM_INT Mask

Definition at line 5342 of file Mini58Series.h.

## ◆ INT_IRQ17_SRC_HIRC_TRIM_INT_Pos

#define INT_IRQ17_SRC_HIRC_TRIM_INT_Pos (0)

INT_T::IRQ17_SRC: HIRC_TRIM_INT Position

Definition at line 5341 of file Mini58Series.h.

## ◆ INT_IRQ18_SRC_I2C0_INT_Msk

#define INT_IRQ18_SRC_I2C0_INT_Msk (0x1ul << INT_IRQ18_SRC_I2C0_INT_Pos)

INT_T::IRQ18_SRC: I2C0_INT Mask

Definition at line 5345 of file Mini58Series.h.

## ◆ INT_IRQ18_SRC_I2C0_INT_Pos

#define INT_IRQ18_SRC_I2C0_INT_Pos (0)

INT_T::IRQ18_SRC: I2C0_INT Position

Definition at line 5344 of file Mini58Series.h.

## ◆ INT_IRQ19_SRC_I2C1_INT_Msk

#define INT_IRQ19_SRC_I2C1_INT_Msk (0x1ul << INT_IRQ19_SRC_I2C1_INT_Pos)

INT_T::IRQ19_SRC: I2C1_INT Mask

Definition at line 5348 of file Mini58Series.h.

## ◆ INT_IRQ19_SRC_I2C1_INT_Pos

#define INT_IRQ19_SRC_I2C1_INT_Pos (0)

INT_T::IRQ19_SRC: I2C1_INT Position

Definition at line 5347 of file Mini58Series.h.

## ◆ INT_IRQ1_SRC_WDT_INT_Msk

#define INT_IRQ1_SRC_WDT_INT_Msk (0x1ul << INT_IRQ1_SRC_WDT_INT_Pos)

INT_T::IRQ1_SRC: WDT_INT Mask

Definition at line 5291 of file Mini58Series.h.

## ◆ INT_IRQ1_SRC_WDT_INT_Pos

#define INT_IRQ1_SRC_WDT_INT_Pos (0)

INT_T::IRQ1_SRC: WDT_INT Position

Definition at line 5290 of file Mini58Series.h.

## ◆ INT_IRQ1_SRC_WWDT_INT_Msk

#define INT_IRQ1_SRC_WWDT_INT_Msk (0x1ul << INT_IRQ1_SRC_WWDT_INT_Pos)

INT_T::IRQ1_SRC: WWDT_INT Mask

Definition at line 5294 of file Mini58Series.h.

## ◆ INT_IRQ1_SRC_WWDT_INT_Pos

#define INT_IRQ1_SRC_WWDT_INT_Pos (1)

INT_T::IRQ1_SRC: WWDT_INT Position

Definition at line 5293 of file Mini58Series.h.

## ◆ INT_IRQ25_SRC_ACMP_INT_Msk

#define INT_IRQ25_SRC_ACMP_INT_Msk (0x1ul << INT_IRQ25_SRC_ACMP_INT_Pos)

INT_T::IRQ25_SRC: ACMP_INT Mask

Definition at line 5351 of file Mini58Series.h.

## ◆ INT_IRQ25_SRC_ACMP_INT_Pos

#define INT_IRQ25_SRC_ACMP_INT_Pos (0)

INT_T::IRQ25_SRC: ACMP_INT Position

Definition at line 5350 of file Mini58Series.h.

## ◆ INT_IRQ28_SRC_PWRWU_INT_Msk

#define INT_IRQ28_SRC_PWRWU_INT_Msk (0x1ul << INT_IRQ28_SRC_PWRWU_INT_Pos)

INT_T::IRQ28_SRC: PWRWU_INT Mask

Definition at line 5354 of file Mini58Series.h.

## ◆ INT_IRQ28_SRC_PWRWU_INT_Pos

#define INT_IRQ28_SRC_PWRWU_INT_Pos (0)

INT_T::IRQ28_SRC: PWRWU_INT Position

Definition at line 5353 of file Mini58Series.h.

## ◆ INT_IRQ29_SRC_ADC_INT_Msk

#define INT_IRQ29_SRC_ADC_INT_Msk (0x1ul << INT_IRQ29_SRC_ADC_INT_Pos)

INT_T::IRQ29_SRC: ADC_INT Mask

Definition at line 5357 of file Mini58Series.h.

## ◆ INT_IRQ29_SRC_ADC_INT_Pos

#define INT_IRQ29_SRC_ADC_INT_Pos (0)

INT_T::IRQ29_SRC: ADC_INT Position

Definition at line 5356 of file Mini58Series.h.

## ◆ INT_IRQ2_SRC_EINT0_Msk

#define INT_IRQ2_SRC_EINT0_Msk (0x1ul << INT_IRQ2_SRC_EINT0_Pos)

INT_T::IRQ2_SRC: EINT0 Mask

Definition at line 5297 of file Mini58Series.h.

## ◆ INT_IRQ2_SRC_EINT0_Pos

#define INT_IRQ2_SRC_EINT0_Pos (0)

INT_T::IRQ2_SRC: EINT0 Position

Definition at line 5296 of file Mini58Series.h.

## ◆ INT_IRQ3_SRC_EINT1_Msk

#define INT_IRQ3_SRC_EINT1_Msk (0x1ul << INT_IRQ_SRC3_EINT1_Pos)

INT_T::IRQ3_SRC: EINT1 Mask

Definition at line 5300 of file Mini58Series.h.

## ◆ INT_IRQ3_SRC_EINT1_Pos

#define INT_IRQ3_SRC_EINT1_Pos (0)

INT_T::IRQ3_SRC: EINT1 Position

Definition at line 5299 of file Mini58Series.h.

## ◆ INT_IRQ4_SRC_GP0_INT_Msk

#define INT_IRQ4_SRC_GP0_INT_Msk (0x1ul << INT_IRQ4_SRC_GP0_INT_Pos)

INT_T::IRQ4_SRC: GP0_INT Mask

Definition at line 5303 of file Mini58Series.h.

## ◆ INT_IRQ4_SRC_GP0_INT_Pos

#define INT_IRQ4_SRC_GP0_INT_Pos (0)

INT_T::IRQ4_SRC: GP0_INT Position

Definition at line 5302 of file Mini58Series.h.

## ◆ INT_IRQ4_SRC_GP1_INT_Msk

#define INT_IRQ4_SRC_GP1_INT_Msk (0x1ul << INT_IRQ4_SRC_GP1_INT_Pos)

INT_T::IRQ4_SRC: GP1_INT Mask

Definition at line 5306 of file Mini58Series.h.

## ◆ INT_IRQ4_SRC_GP1_INT_Pos

#define INT_IRQ4_SRC_GP1_INT_Pos (1)

INT_T::IRQ4_SRC: GP1_INT Position

Definition at line 5305 of file Mini58Series.h.

## ◆ INT_IRQ5_SRC_GP2_INT_Msk

#define INT_IRQ5_SRC_GP2_INT_Msk (0x1ul << INT_IRQ5_SRC_GP2_INT_Pos)

INT_T::IRQ5_SRC: GP2_INT Mask

Definition at line 5309 of file Mini58Series.h.

## ◆ INT_IRQ5_SRC_GP2_INT_Pos

#define INT_IRQ5_SRC_GP2_INT_Pos (0)

INT_T::IRQ5_SRC: GP2_INT Position

Definition at line 5308 of file Mini58Series.h.

## ◆ INT_IRQ5_SRC_GP3_INT_Msk

#define INT_IRQ5_SRC_GP3_INT_Msk (0x1ul << INT_IRQ5_SRC_GP3_INT_Pos)

INT_T::IRQ5_SRC: GP3_INT Mask

Definition at line 5312 of file Mini58Series.h.

## ◆ INT_IRQ5_SRC_GP3_INT_Pos

#define INT_IRQ5_SRC_GP3_INT_Pos (1)

INT_T::IRQ5_SRC: GP3_INT Position

Definition at line 5311 of file Mini58Series.h.

## ◆ INT_IRQ5_SRC_GP4_INT_Msk

#define INT_IRQ5_SRC_GP4_INT_Msk (0x1ul << INT_IRQ5_SRC_GP4_INT_Pos)

INT_T::IRQ5_SRC: GP4_INT Mask

Definition at line 5315 of file Mini58Series.h.

## ◆ INT_IRQ5_SRC_GP4_INT_Pos

#define INT_IRQ5_SRC_GP4_INT_Pos (2)

INT_T::IRQ5_SRC: GP4_INT Position

Definition at line 5314 of file Mini58Series.h.

## ◆ INT_IRQ6_SRC_PWM_INT_Msk

#define INT_IRQ6_SRC_PWM_INT_Msk (0x1ul << INT_IRQ6_SRC_PWM_INT_Pos)

INT_T::IRQ6_SRC: PWM_INT Mask

Definition at line 5318 of file Mini58Series.h.

## ◆ INT_IRQ6_SRC_PWM_INT_Pos

#define INT_IRQ6_SRC_PWM_INT_Pos (0)

INT_T::IRQ6_SRC: PWM_INT Position

Definition at line 5317 of file Mini58Series.h.

## ◆ INT_IRQ7_SRC_BRAKE_INT_Msk

#define INT_IRQ7_SRC_BRAKE_INT_Msk (0x1ul << INT_IRQ_SRC_BRAKE_INT_Pos)

INT_T::IRQ7_SRC: BRAKE_INT Mask

Definition at line 5321 of file Mini58Series.h.

## ◆ INT_IRQ7_SRC_BRAKE_INT_Pos

#define INT_IRQ7_SRC_BRAKE_INT_Pos (0)

INT_T::IRQ7_SRC: BRAKE_INT Position

Definition at line 5320 of file Mini58Series.h.

## ◆ INT_IRQ8_SRC_TMR0_INT_Msk

#define INT_IRQ8_SRC_TMR0_INT_Msk (0x1ul << INT_IRQ8_SRC_TMR0_INT_Pos)

INT_T::IRQ8_SRC: TMR0_INT Mask

Definition at line 5324 of file Mini58Series.h.

## ◆ INT_IRQ8_SRC_TMR0_INT_Pos

#define INT_IRQ8_SRC_TMR0_INT_Pos (0)

INT_T::IRQ8_SRC: TMR0_INT Position

Definition at line 5323 of file Mini58Series.h.

## ◆ INT_IRQ9_SRC_TMR1_INT_Msk

#define INT_IRQ9_SRC_TMR1_INT_Msk (0x1ul << INT_IRQ9_SRC_TMR1_INT_Pos)

INT_T::IRQ9_SRC: TMR1_INT Mask

Definition at line 5327 of file Mini58Series.h.

## ◆ INT_IRQ9_SRC_TMR1_INT_Pos

#define INT_IRQ9_SRC_TMR1_INT_Pos (0)

INT_T::IRQ9_SRC: TMR1_INT Position

Definition at line 5326 of file Mini58Series.h.

## ◆ INT_IRQ_MCU_IRQ_Msk

#define INT_IRQ_MCU_IRQ_Msk (0xfffffffful << INT_IRQ_MCU_IRQ_Pos)

INT_T::IRQ: MCU_IRQ Mask

Definition at line 5366 of file Mini58Series.h.

## ◆ INT_IRQ_MCU_IRQ_Pos

#define INT_IRQ_MCU_IRQ_Pos (0)

INT_T::IRQ: MCU_IRQ Position

Definition at line 5365 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN0_Msk

#define PWM_ADCTCTL0_CDTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN0_Pos)

PWM_T::ADCTCTL0: CDTRGEN0 Mask

Definition at line 8569 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN0_Pos

#define PWM_ADCTCTL0_CDTRGEN0_Pos (2)

PWM_T::ADCTCTL0: CDTRGEN0 Position

Definition at line 8568 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN1_Msk

#define PWM_ADCTCTL0_CDTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN1_Pos)

PWM_T::ADCTCTL0: CDTRGEN1 Mask

Definition at line 8581 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN1_Pos

#define PWM_ADCTCTL0_CDTRGEN1_Pos (10)

PWM_T::ADCTCTL0: CDTRGEN1 Position

Definition at line 8580 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN2_Msk

#define PWM_ADCTCTL0_CDTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN2_Pos)

PWM_T::ADCTCTL0: CDTRGEN2 Mask

Definition at line 8593 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN2_Pos

#define PWM_ADCTCTL0_CDTRGEN2_Pos (18)

PWM_T::ADCTCTL0: CDTRGEN2 Position

Definition at line 8592 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN3_Msk

#define PWM_ADCTCTL0_CDTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN3_Pos)

PWM_T::ADCTCTL0: CDTRGEN3 Mask

Definition at line 8605 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN3_Pos

#define PWM_ADCTCTL0_CDTRGEN3_Pos (26)

PWM_T::ADCTCTL0: CDTRGEN3 Position

Definition at line 8604 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN0_Msk

#define PWM_ADCTCTL0_CPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN0_Pos)

PWM_T::ADCTCTL0: CPTRGEN0 Mask

Definition at line 8566 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN0_Pos

#define PWM_ADCTCTL0_CPTRGEN0_Pos (1)

PWM_T::ADCTCTL0: CPTRGEN0 Position

Definition at line 8565 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN1_Msk

#define PWM_ADCTCTL0_CPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN1_Pos)

PWM_T::ADCTCTL0: CPTRGEN1 Mask

Definition at line 8578 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN1_Pos

#define PWM_ADCTCTL0_CPTRGEN1_Pos (9)

PWM_T::ADCTCTL0: CPTRGEN1 Position

Definition at line 8577 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN2_Msk

#define PWM_ADCTCTL0_CPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN2_Pos)

PWM_T::ADCTCTL0: CPTRGEN2 Mask

Definition at line 8590 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN2_Pos

#define PWM_ADCTCTL0_CPTRGEN2_Pos (17)

PWM_T::ADCTCTL0: CPTRGEN2 Position

Definition at line 8589 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN3_Msk

#define PWM_ADCTCTL0_CPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN3_Pos)

PWM_T::ADCTCTL0: CPTRGEN3 Mask

Definition at line 8602 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN3_Pos

#define PWM_ADCTCTL0_CPTRGEN3_Pos (25)

PWM_T::ADCTCTL0: CPTRGEN3 Position

Definition at line 8601 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN0_Msk

#define PWM_ADCTCTL0_CUTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN0_Pos)

PWM_T::ADCTCTL0: CUTRGEN0 Mask

Definition at line 8563 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN0_Pos

#define PWM_ADCTCTL0_CUTRGEN0_Pos (0)

PWM_T::ADCTCTL0: CUTRGEN0 Position

Definition at line 8562 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN1_Msk

#define PWM_ADCTCTL0_CUTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN1_Pos)

PWM_T::ADCTCTL0: CUTRGEN1 Mask

Definition at line 8575 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN1_Pos

#define PWM_ADCTCTL0_CUTRGEN1_Pos (8)

PWM_T::ADCTCTL0: CUTRGEN1 Position

Definition at line 8574 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN2_Msk

#define PWM_ADCTCTL0_CUTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN2_Pos)

PWM_T::ADCTCTL0: CUTRGEN2 Mask

Definition at line 8587 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN2_Pos

#define PWM_ADCTCTL0_CUTRGEN2_Pos (16)

PWM_T::ADCTCTL0: CUTRGEN2 Position

Definition at line 8586 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN3_Msk

#define PWM_ADCTCTL0_CUTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN3_Pos)

PWM_T::ADCTCTL0: CUTRGEN3 Mask

Definition at line 8599 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN3_Pos

#define PWM_ADCTCTL0_CUTRGEN3_Pos (24)

PWM_T::ADCTCTL0: CUTRGEN3 Position

Definition at line 8598 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN0_Msk

#define PWM_ADCTCTL0_ZPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN0_Pos)

PWM_T::ADCTCTL0: ZPTRGEN0 Mask

Definition at line 8572 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN0_Pos

#define PWM_ADCTCTL0_ZPTRGEN0_Pos (3)

PWM_T::ADCTCTL0: ZPTRGEN0 Position

Definition at line 8571 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN1_Msk

#define PWM_ADCTCTL0_ZPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN1_Pos)

PWM_T::ADCTCTL0: ZPTRGEN1 Mask

Definition at line 8584 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN1_Pos

#define PWM_ADCTCTL0_ZPTRGEN1_Pos (11)

PWM_T::ADCTCTL0: ZPTRGEN1 Position

Definition at line 8583 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN2_Msk

#define PWM_ADCTCTL0_ZPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN2_Pos)

PWM_T::ADCTCTL0: ZPTRGEN2 Mask

Definition at line 8596 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN2_Pos

#define PWM_ADCTCTL0_ZPTRGEN2_Pos (19)

PWM_T::ADCTCTL0: ZPTRGEN2 Position

Definition at line 8595 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN3_Msk

#define PWM_ADCTCTL0_ZPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN3_Pos)

PWM_T::ADCTCTL0: ZPTRGEN3 Mask

Definition at line 8608 of file Mini58Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN3_Pos

#define PWM_ADCTCTL0_ZPTRGEN3_Pos (27)

PWM_T::ADCTCTL0: ZPTRGEN3 Position

Definition at line 8607 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN4_Msk

#define PWM_ADCTCTL1_CDTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN4_Pos)

PWM_T::ADCTCTL1: CDTRGEN4 Mask

Definition at line 8617 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN4_Pos

#define PWM_ADCTCTL1_CDTRGEN4_Pos (2)

PWM_T::ADCTCTL1: CDTRGEN4 Position

Definition at line 8616 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN5_Msk

#define PWM_ADCTCTL1_CDTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN5_Pos)

PWM_T::ADCTCTL1: CDTRGEN5 Mask

Definition at line 8629 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN5_Pos

#define PWM_ADCTCTL1_CDTRGEN5_Pos (10)

PWM_T::ADCTCTL1: CDTRGEN5 Position

Definition at line 8628 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN4_Msk

#define PWM_ADCTCTL1_CPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN4_Pos)

PWM_T::ADCTCTL1: CPTRGEN4 Mask

Definition at line 8614 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN4_Pos

#define PWM_ADCTCTL1_CPTRGEN4_Pos (1)

PWM_T::ADCTCTL1: CPTRGEN4 Position

Definition at line 8613 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN5_Msk

#define PWM_ADCTCTL1_CPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN5_Pos)

PWM_T::ADCTCTL1: CPTRGEN5 Mask

Definition at line 8626 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN5_Pos

#define PWM_ADCTCTL1_CPTRGEN5_Pos (9)

PWM_T::ADCTCTL1: CPTRGEN5 Position

Definition at line 8625 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN4_Msk

#define PWM_ADCTCTL1_CUTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN4_Pos)

PWM_T::ADCTCTL1: CUTRGEN4 Mask

Definition at line 8611 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN4_Pos

#define PWM_ADCTCTL1_CUTRGEN4_Pos (0)

PWM_T::ADCTCTL1: CUTRGEN4 Position

Definition at line 8610 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN5_Msk

#define PWM_ADCTCTL1_CUTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN5_Pos)

PWM_T::ADCTCTL1: CUTRGEN5 Mask

Definition at line 8623 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN5_Pos

#define PWM_ADCTCTL1_CUTRGEN5_Pos (8)

PWM_T::ADCTCTL1: CUTRGEN5 Position

Definition at line 8622 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN4_Msk

#define PWM_ADCTCTL1_ZPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN4_Pos)

PWM_T::ADCTCTL1: ZPTRGEN4 Mask

Definition at line 8620 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN4_Pos

#define PWM_ADCTCTL1_ZPTRGEN4_Pos (3)

PWM_T::ADCTCTL1: ZPTRGEN4 Position

Definition at line 8619 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN5_Msk

#define PWM_ADCTCTL1_ZPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN5_Pos)

PWM_T::ADCTCTL1: ZPTRGEN5 Mask

Definition at line 8632 of file Mini58Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN5_Pos

#define PWM_ADCTCTL1_ZPTRGEN5_Pos (11)

PWM_T::ADCTCTL1: ZPTRGEN5 Position

Definition at line 8631 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF0_Msk

#define PWM_ADCTSTS0_CDTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF0_Pos)

PWM_T::ADCTSTS0: CDTRGF0 Mask

Definition at line 8641 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF0_Pos

#define PWM_ADCTSTS0_CDTRGF0_Pos (2)

PWM_T::ADCTSTS0: CDTRGF0 Position

Definition at line 8640 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF1_Msk

#define PWM_ADCTSTS0_CDTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF1_Pos)

PWM_T::ADCTSTS0: CDTRGF1 Mask

Definition at line 8653 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF1_Pos

#define PWM_ADCTSTS0_CDTRGF1_Pos (10)

PWM_T::ADCTSTS0: CDTRGF1 Position

Definition at line 8652 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF2_Msk

#define PWM_ADCTSTS0_CDTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF2_Pos)

PWM_T::ADCTSTS0: CDTRGF2 Mask

Definition at line 8665 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF2_Pos

#define PWM_ADCTSTS0_CDTRGF2_Pos (18)

PWM_T::ADCTSTS0: CDTRGF2 Position

Definition at line 8664 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF3_Msk

#define PWM_ADCTSTS0_CDTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF3_Pos)

PWM_T::ADCTSTS0: CDTRGF3 Mask

Definition at line 8677 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF3_Pos

#define PWM_ADCTSTS0_CDTRGF3_Pos (26)

PWM_T::ADCTSTS0: CDTRGF3 Position

Definition at line 8676 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF0_Msk

#define PWM_ADCTSTS0_CPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF0_Pos)

PWM_T::ADCTSTS0: CPTRGF0 Mask

Definition at line 8638 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF0_Pos

#define PWM_ADCTSTS0_CPTRGF0_Pos (1)

PWM_T::ADCTSTS0: CPTRGF0 Position

Definition at line 8637 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF1_Msk

#define PWM_ADCTSTS0_CPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF1_Pos)

PWM_T::ADCTSTS0: CPTRGF1 Mask

Definition at line 8650 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF1_Pos

#define PWM_ADCTSTS0_CPTRGF1_Pos (9)

PWM_T::ADCTSTS0: CPTRGF1 Position

Definition at line 8649 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF2_Msk

#define PWM_ADCTSTS0_CPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF2_Pos)

PWM_T::ADCTSTS0: CPTRGF2 Mask

Definition at line 8662 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF2_Pos

#define PWM_ADCTSTS0_CPTRGF2_Pos (17)

PWM_T::ADCTSTS0: CPTRGF2 Position

Definition at line 8661 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF3_Msk

#define PWM_ADCTSTS0_CPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF3_Pos)

PWM_T::ADCTSTS0: CPTRGF3 Mask

Definition at line 8674 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF3_Pos

#define PWM_ADCTSTS0_CPTRGF3_Pos (25)

PWM_T::ADCTSTS0: CPTRGF3 Position

Definition at line 8673 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF0_Msk

#define PWM_ADCTSTS0_CUTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF0_Pos)

PWM_T::ADCTSTS0: CUTRGF0 Mask

Definition at line 8635 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF0_Pos

#define PWM_ADCTSTS0_CUTRGF0_Pos (0)

PWM_T::ADCTSTS0: CUTRGF0 Position

Definition at line 8634 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF1_Msk

#define PWM_ADCTSTS0_CUTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF1_Pos)

PWM_T::ADCTSTS0: CUTRGF1 Mask

Definition at line 8647 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF1_Pos

#define PWM_ADCTSTS0_CUTRGF1_Pos (8)

PWM_T::ADCTSTS0: CUTRGF1 Position

Definition at line 8646 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF2_Msk

#define PWM_ADCTSTS0_CUTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF2_Pos)

PWM_T::ADCTSTS0: CUTRGF2 Mask

Definition at line 8659 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF2_Pos

#define PWM_ADCTSTS0_CUTRGF2_Pos (16)

PWM_T::ADCTSTS0: CUTRGF2 Position

Definition at line 8658 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF3_Msk

#define PWM_ADCTSTS0_CUTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF3_Pos)

PWM_T::ADCTSTS0: CUTRGF3 Mask

Definition at line 8671 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF3_Pos

#define PWM_ADCTSTS0_CUTRGF3_Pos (24)

PWM_T::ADCTSTS0: CUTRGF3 Position

Definition at line 8670 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF0_Msk

#define PWM_ADCTSTS0_ZPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF0_Pos)

PWM_T::ADCTSTS0: ZPTRGF0 Mask

Definition at line 8644 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF0_Pos

#define PWM_ADCTSTS0_ZPTRGF0_Pos (3)

PWM_T::ADCTSTS0: ZPTRGF0 Position

Definition at line 8643 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF1_Msk

#define PWM_ADCTSTS0_ZPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF1_Pos)

PWM_T::ADCTSTS0: ZPTRGF1 Mask

Definition at line 8656 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF1_Pos

#define PWM_ADCTSTS0_ZPTRGF1_Pos (11)

PWM_T::ADCTSTS0: ZPTRGF1 Position

Definition at line 8655 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF2_Msk

#define PWM_ADCTSTS0_ZPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF2_Pos)

PWM_T::ADCTSTS0: ZPTRGF2 Mask

Definition at line 8668 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF2_Pos

#define PWM_ADCTSTS0_ZPTRGF2_Pos (19)

PWM_T::ADCTSTS0: ZPTRGF2 Position

Definition at line 8667 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF3_Msk

#define PWM_ADCTSTS0_ZPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF3_Pos)

PWM_T::ADCTSTS0: ZPTRGF3 Mask

Definition at line 8680 of file Mini58Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF3_Pos

#define PWM_ADCTSTS0_ZPTRGF3_Pos (27)

PWM_T::ADCTSTS0: ZPTRGF3 Position

Definition at line 8679 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF4_Msk

#define PWM_ADCTSTS1_CDTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF4_Pos)

PWM_T::ADCTSTS1: CDTRGF4 Mask

Definition at line 8689 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF4_Pos

#define PWM_ADCTSTS1_CDTRGF4_Pos (2)

PWM_T::ADCTSTS1: CDTRGF4 Position

Definition at line 8688 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF5_Msk

#define PWM_ADCTSTS1_CDTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF5_Pos)

PWM_T::ADCTSTS1: CDTRGF5 Mask

Definition at line 8701 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF5_Pos

#define PWM_ADCTSTS1_CDTRGF5_Pos (10)

PWM_T::ADCTSTS1: CDTRGF5 Position

Definition at line 8700 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF4_Msk

#define PWM_ADCTSTS1_CPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF4_Pos)

PWM_T::ADCTSTS1: CPTRGF4 Mask

Definition at line 8686 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF4_Pos

#define PWM_ADCTSTS1_CPTRGF4_Pos (1)

PWM_T::ADCTSTS1: CPTRGF4 Position

Definition at line 8685 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF5_Msk

#define PWM_ADCTSTS1_CPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF5_Pos)

PWM_T::ADCTSTS1: CPTRGF5 Mask

Definition at line 8698 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF5_Pos

#define PWM_ADCTSTS1_CPTRGF5_Pos (9)

PWM_T::ADCTSTS1: CPTRGF5 Position

Definition at line 8697 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF4_Msk

#define PWM_ADCTSTS1_CUTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF4_Pos)

PWM_T::ADCTSTS1: CUTRGF4 Mask

Definition at line 8683 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF4_Pos

#define PWM_ADCTSTS1_CUTRGF4_Pos (0)

PWM_T::ADCTSTS1: CUTRGF4 Position

Definition at line 8682 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF5_Msk

#define PWM_ADCTSTS1_CUTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF5_Pos)

PWM_T::ADCTSTS1: CUTRGF5 Mask

Definition at line 8695 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF5_Pos

#define PWM_ADCTSTS1_CUTRGF5_Pos (8)

PWM_T::ADCTSTS1: CUTRGF5 Position

Definition at line 8694 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF4_Msk

#define PWM_ADCTSTS1_ZPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF4_Pos)

PWM_T::ADCTSTS1: ZPTRGF4 Mask

Definition at line 8692 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF4_Pos

#define PWM_ADCTSTS1_ZPTRGF4_Pos (3)

PWM_T::ADCTSTS1: ZPTRGF4 Position

Definition at line 8691 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF5_Msk

#define PWM_ADCTSTS1_ZPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF5_Pos)

PWM_T::ADCTSTS1: ZPTRGF5 Mask

Definition at line 8704 of file Mini58Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF5_Pos

#define PWM_ADCTSTS1_ZPTRGF5_Pos (11)

PWM_T::ADCTSTS1: ZPTRGF5 Position

Definition at line 8703 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD0_Msk

#define PWM_BRKCTL_BKOD0_Msk (0x1ul << PWM_BRKCTL_BKOD0_Pos)

PWM_T::BRKCTL: BKOD0 Mask

Definition at line 8530 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD0_Pos

#define PWM_BRKCTL_BKOD0_Pos (24)

PWM_T::BRKCTL: BKOD0 Position

Definition at line 8529 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD1_Msk

#define PWM_BRKCTL_BKOD1_Msk (0x1ul << PWM_BRKCTL_BKOD1_Pos)

PWM_T::BRKCTL: BKOD1 Mask

Definition at line 8533 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD1_Pos

#define PWM_BRKCTL_BKOD1_Pos (25)

PWM_T::BRKCTL: BKOD1 Position

Definition at line 8532 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD2_Msk

#define PWM_BRKCTL_BKOD2_Msk (0x1ul << PWM_BRKCTL_BKOD2_Pos)

PWM_T::BRKCTL: BKOD2 Mask

Definition at line 8536 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD2_Pos

#define PWM_BRKCTL_BKOD2_Pos (26)

PWM_T::BRKCTL: BKOD2 Position

Definition at line 8535 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD3_Msk

#define PWM_BRKCTL_BKOD3_Msk (0x1ul << PWM_BRKCTL_BKOD3_Pos)

PWM_T::BRKCTL: BKOD3 Mask

Definition at line 8539 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD3_Pos

#define PWM_BRKCTL_BKOD3_Pos (27)

PWM_T::BRKCTL: BKOD3 Position

Definition at line 8538 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD4_Msk

#define PWM_BRKCTL_BKOD4_Msk (0x1ul << PWM_BRKCTL_BKOD4_Pos)

PWM_T::BRKCTL: BKOD4 Mask

Definition at line 8542 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD4_Pos

#define PWM_BRKCTL_BKOD4_Pos (28)

PWM_T::BRKCTL: BKOD4 Position

Definition at line 8541 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD5_Msk

#define PWM_BRKCTL_BKOD5_Msk (0x1ul << PWM_BRKCTL_BKOD5_Pos)

PWM_T::BRKCTL: BKOD5 Mask

Definition at line 8545 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BKOD5_Pos

#define PWM_BRKCTL_BKOD5_Pos (29)

PWM_T::BRKCTL: BKOD5 Position

Definition at line 8544 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK0EN_Msk

#define PWM_BRKCTL_BRK0EN_Msk (0x1ul << PWM_BRKCTL_BRK0EN_Pos)

PWM_T::BRKCTL: BRK0EN Mask

Definition at line 8509 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK0EN_Pos

#define PWM_BRKCTL_BRK0EN_Pos (0)

PWM_T::BRKCTL: BRK0EN Position

Definition at line 8508 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK0SEL_Msk

#define PWM_BRKCTL_BRK0SEL_Msk (0x1ul << PWM_BRKCTL_BRK0SEL_Pos)

PWM_T::BRKCTL: BRK0SEL Mask

Definition at line 8515 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK0SEL_Pos

#define PWM_BRKCTL_BRK0SEL_Pos (2)

PWM_T::BRKCTL: BRK0SEL Position

Definition at line 8514 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK1EN_Msk

#define PWM_BRKCTL_BRK1EN_Msk (0x1ul << PWM_BRKCTL_BRK1EN_Pos)

PWM_T::BRKCTL: BRK1EN Mask

Definition at line 8512 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK1EN_Pos

#define PWM_BRKCTL_BRK1EN_Pos (1)

PWM_T::BRKCTL: BRK1EN Position

Definition at line 8511 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK1SEL_Msk

#define PWM_BRKCTL_BRK1SEL_Msk (0x1ul << PWM_BRKCTL_BRK1SEL_Pos)

PWM_T::BRKCTL: BRK1SEL Mask

Definition at line 8518 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRK1SEL_Pos

#define PWM_BRKCTL_BRK1SEL_Pos (3)

PWM_T::BRKCTL: BRK1SEL Position

Definition at line 8517 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRKACT_Msk

#define PWM_BRKCTL_BRKACT_Msk (0x1ul << PWM_BRKCTL_BRKACT_Pos)

PWM_T::BRKCTL: BRKACT Mask

Definition at line 8524 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRKACT_Pos

#define PWM_BRKCTL_BRKACT_Pos (8)

PWM_T::BRKCTL: BRKACT Position

Definition at line 8523 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRKSTS_Msk

#define PWM_BRKCTL_BRKSTS_Msk (0x1ul << PWM_BRKCTL_BRKSTS_Pos)

PWM_T::BRKCTL: BRKSTS Mask

Definition at line 8521 of file Mini58Series.h.

## ◆ PWM_BRKCTL_BRKSTS_Pos

#define PWM_BRKCTL_BRKSTS_Pos (7)

PWM_T::BRKCTL: BRKSTS Position

Definition at line 8520 of file Mini58Series.h.

## ◆ PWM_BRKCTL_D6BKOD_Msk

#define PWM_BRKCTL_D6BKOD_Msk (0x1ul << PWM_BRKCTL_D6BKOD_Pos)

PWM_T::BRKCTL: D6BKOD Mask

Definition at line 8548 of file Mini58Series.h.

## ◆ PWM_BRKCTL_D6BKOD_Pos

#define PWM_BRKCTL_D6BKOD_Pos (30)

PWM_T::BRKCTL: D6BKOD Position

Definition at line 8547 of file Mini58Series.h.

## ◆ PWM_BRKCTL_D7BKOD_Msk

#define PWM_BRKCTL_D7BKOD_Msk (0x1ul << PWM_BRKCTL_D7BKOD_Pos)

PWM_T::BRKCTL: D7BKOD Mask

Definition at line 8551 of file Mini58Series.h.

## ◆ PWM_BRKCTL_D7BKOD_Pos

#define PWM_BRKCTL_D7BKOD_Pos (31)

PWM_T::BRKCTL: D7BKOD Position

Definition at line 8550 of file Mini58Series.h.

## ◆ PWM_BRKCTL_SWBRK_Msk

#define PWM_BRKCTL_SWBRK_Msk (0x1ul << PWM_BRKCTL_SWBRK_Pos)

PWM_T::BRKCTL: SWBRK Mask

Definition at line 8527 of file Mini58Series.h.

## ◆ PWM_BRKCTL_SWBRK_Pos

#define PWM_BRKCTL_SWBRK_Pos (9)

PWM_T::BRKCTL: SWBRK Position

Definition at line 8526 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV0_Msk

#define PWM_CLKDIV_CLKDIV0_Msk (0x7ul << PWM_CLKDIV_CLKDIV0_Pos)

PWM_T::CLKDIV: CLKDIV0 Mask

Definition at line 7909 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV0_Pos

#define PWM_CLKDIV_CLKDIV0_Pos (0)

PWM_T::CLKDIV: CLKDIV0 Position

Definition at line 7908 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV1_Msk

#define PWM_CLKDIV_CLKDIV1_Msk (0x7ul << PWM_CLKDIV_CLKDIV1_Pos)

PWM_T::CLKDIV: CLKDIV1 Mask

Definition at line 7912 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV1_Pos

#define PWM_CLKDIV_CLKDIV1_Pos (4)

PWM_T::CLKDIV: CLKDIV1 Position

Definition at line 7911 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV2_Msk

#define PWM_CLKDIV_CLKDIV2_Msk (0x7ul << PWM_CLKDIV_CLKDIV2_Pos)

PWM_T::CLKDIV: CLKDIV2 Mask

Definition at line 7915 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV2_Pos

#define PWM_CLKDIV_CLKDIV2_Pos (8)

PWM_T::CLKDIV: CLKDIV2 Position

Definition at line 7914 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV3_Msk

#define PWM_CLKDIV_CLKDIV3_Msk (0x7ul << PWM_CLKDIV_CLKDIV3_Pos)

PWM_T::CLKDIV: CLKDIV3 Mask

Definition at line 7918 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV3_Pos

#define PWM_CLKDIV_CLKDIV3_Pos (12)

PWM_T::CLKDIV: CLKDIV3 Position

Definition at line 7917 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV4_Msk

#define PWM_CLKDIV_CLKDIV4_Msk (0x7ul << PWM_CLKDIV_CLKDIV4_Pos)

PWM_T::CLKDIV: CLKDIV4 Mask

Definition at line 7921 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV4_Pos

#define PWM_CLKDIV_CLKDIV4_Pos (16)

PWM_T::CLKDIV: CLKDIV4 Position

Definition at line 7920 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV5_Msk

#define PWM_CLKDIV_CLKDIV5_Msk (0x7ul << PWM_CLKDIV_CLKDIV5_Pos)

PWM_T::CLKDIV: CLKDIV5 Mask

Definition at line 7924 of file Mini58Series.h.

## ◆ PWM_CLKDIV_CLKDIV5_Pos

#define PWM_CLKDIV_CLKDIV5_Pos (20)

PWM_T::CLKDIV: CLKDIV5 Position

Definition at line 7923 of file Mini58Series.h.

## ◆ PWM_CLKPSC_CLKPSC01_Msk

#define PWM_CLKPSC_CLKPSC01_Msk (0xfful << PWM_CLKPSC_CLKPSC01_Pos)

PWM_T::CLKPSC: CLKPSC01 Mask

Definition at line 7900 of file Mini58Series.h.

## ◆ PWM_CLKPSC_CLKPSC01_Pos

#define PWM_CLKPSC_CLKPSC01_Pos (0)

    @addtogroup PWM_CONST PWM Bit Field Definition
    Constant Definitions for PWM Controller

PWM_T::CLKPSC: CLKPSC01 Position

Definition at line 7899 of file Mini58Series.h.

## ◆ PWM_CLKPSC_CLKPSC23_Msk

#define PWM_CLKPSC_CLKPSC23_Msk (0xfful << PWM_CLKPSC_CLKPSC23_Pos)

PWM_T::CLKPSC: CLKPSC23 Mask

Definition at line 7903 of file Mini58Series.h.

## ◆ PWM_CLKPSC_CLKPSC23_Pos

#define PWM_CLKPSC_CLKPSC23_Pos (8)

PWM_T::CLKPSC: CLKPSC23 Position

Definition at line 7902 of file Mini58Series.h.

## ◆ PWM_CLKPSC_CLKPSC45_Msk

#define PWM_CLKPSC_CLKPSC45_Msk (0xfful << PWM_CLKPSC_CLKPSC45_Pos)

PWM_T::CLKPSC: CLKPSC45 Mask

Definition at line 7906 of file Mini58Series.h.

## ◆ PWM_CLKPSC_CLKPSC45_Pos

#define PWM_CLKPSC_CLKPSC45_Pos (16)

PWM_T::CLKPSC: CLKPSC45 Position

Definition at line 7905 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP0_Msk

#define PWM_CMPDAT0_CMP0_Msk (0xfffful << PWM_CMPDAT0_CMP0_Pos)

PWM_T::CMPDAT0: CMP0 Mask

Definition at line 8119 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP0_Pos

#define PWM_CMPDAT0_CMP0_Pos (0)

PWM_T::CMPDAT0: CMP0 Position

Definition at line 8118 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP1_Msk

#define PWM_CMPDAT0_CMP1_Msk (0xfffful << PWM_CMPDAT0_CMP1_Pos)

PWM_T::CMPDAT0: CMP1 Mask

Definition at line 8122 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP1_Pos

#define PWM_CMPDAT0_CMP1_Pos (0)

PWM_T::CMPDAT0: CMP1 Position

Definition at line 8121 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP2_Msk

#define PWM_CMPDAT0_CMP2_Msk (0xfffful << PWM_CMPDAT0_CMP2_Pos)

PWM_T::CMPDAT0: CMP2 Mask

Definition at line 8125 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP2_Pos

#define PWM_CMPDAT0_CMP2_Pos (0)

PWM_T::CMPDAT0: CMP2 Position

Definition at line 8124 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP3_Msk

#define PWM_CMPDAT0_CMP3_Msk (0xfffful << PWM_CMPDAT0_CMP3_Pos)

PWM_T::CMPDAT0: CMP3 Mask

Definition at line 8128 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP3_Pos

#define PWM_CMPDAT0_CMP3_Pos (0)

PWM_T::CMPDAT0: CMP3 Position

Definition at line 8127 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP4_Msk

#define PWM_CMPDAT0_CMP4_Msk (0xfffful << PWM_CMPDAT0_CMP4_Pos)

PWM_T::CMPDAT0: CMP4 Mask

Definition at line 8131 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP4_Pos

#define PWM_CMPDAT0_CMP4_Pos (0)

PWM_T::CMPDAT0: CMP4 Position

Definition at line 8130 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP5_Msk

#define PWM_CMPDAT0_CMP5_Msk (0xfffful << PWM_CMPDAT0_CMP5_Pos)

PWM_T::CMPDAT0: CMP5 Mask

Definition at line 8134 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMP5_Pos

#define PWM_CMPDAT0_CMP5_Pos (0)

PWM_T::CMPDAT0: CMP5 Position

Definition at line 8133 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD0_Msk

#define PWM_CMPDAT0_CMPD0_Msk (0xfffful << PWM_CMPDAT0_CMPD0_Pos)

PWM_T::CMPDAT0: CMPD0 Mask

Definition at line 8137 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD0_Pos

#define PWM_CMPDAT0_CMPD0_Pos (16)

PWM_T::CMPDAT0: CMPD0 Position

Definition at line 8136 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD1_Msk

#define PWM_CMPDAT0_CMPD1_Msk (0xfffful << PWM_CMPDAT0_CMPD1_Pos)

PWM_T::CMPDAT0: CMPD1 Mask

Definition at line 8140 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD1_Pos

#define PWM_CMPDAT0_CMPD1_Pos (16)

PWM_T::CMPDAT0: CMPD1 Position

Definition at line 8139 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD2_Msk

#define PWM_CMPDAT0_CMPD2_Msk (0xfffful << PWM_CMPDAT0_CMPD2_Pos)

PWM_T::CMPDAT0: CMPD2 Mask

Definition at line 8143 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD2_Pos

#define PWM_CMPDAT0_CMPD2_Pos (16)

PWM_T::CMPDAT0: CMPD2 Position

Definition at line 8142 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD3_Msk

#define PWM_CMPDAT0_CMPD3_Msk (0xfffful << PWM_CMPDAT0_CMPD3_Pos)

PWM_T::CMPDAT0: CMPD3 Mask

Definition at line 8146 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD3_Pos

#define PWM_CMPDAT0_CMPD3_Pos (16)

PWM_T::CMPDAT0: CMPD3 Position

Definition at line 8145 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD4_Msk

#define PWM_CMPDAT0_CMPD4_Msk (0xfffful << PWM_CMPDAT0_CMPD4_Pos)

PWM_T::CMPDAT0: CMPD4 Mask

Definition at line 8149 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD4_Pos

#define PWM_CMPDAT0_CMPD4_Pos (16)

PWM_T::CMPDAT0: CMPD4 Position

Definition at line 8148 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD5_Msk

#define PWM_CMPDAT0_CMPD5_Msk (0xfffful << PWM_CMPDAT0_CMPD5_Pos)

PWM_T::CMPDAT0: CMPD5 Mask

Definition at line 8152 of file Mini58Series.h.

## ◆ PWM_CMPDAT0_CMPD5_Pos

#define PWM_CMPDAT0_CMPD5_Pos (16)

PWM_T::CMPDAT0: CMPD5 Position

Definition at line 8151 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP0_Msk

#define PWM_CMPDAT1_CMP0_Msk (0xfffful << PWM_CMPDAT1_CMP0_Pos)

PWM_T::CMPDAT1: CMP0 Mask

Definition at line 8155 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP0_Pos

#define PWM_CMPDAT1_CMP0_Pos (0)

PWM_T::CMPDAT1: CMP0 Position

Definition at line 8154 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP1_Msk

#define PWM_CMPDAT1_CMP1_Msk (0xfffful << PWM_CMPDAT1_CMP1_Pos)

PWM_T::CMPDAT1: CMP1 Mask

Definition at line 8158 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP1_Pos

#define PWM_CMPDAT1_CMP1_Pos (0)

PWM_T::CMPDAT1: CMP1 Position

Definition at line 8157 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP2_Msk

#define PWM_CMPDAT1_CMP2_Msk (0xfffful << PWM_CMPDAT1_CMP2_Pos)

PWM_T::CMPDAT1: CMP2 Mask

Definition at line 8161 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP2_Pos

#define PWM_CMPDAT1_CMP2_Pos (0)

PWM_T::CMPDAT1: CMP2 Position

Definition at line 8160 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP3_Msk

#define PWM_CMPDAT1_CMP3_Msk (0xfffful << PWM_CMPDAT1_CMP3_Pos)

PWM_T::CMPDAT1: CMP3 Mask

Definition at line 8164 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP3_Pos

#define PWM_CMPDAT1_CMP3_Pos (0)

PWM_T::CMPDAT1: CMP3 Position

Definition at line 8163 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP4_Msk

#define PWM_CMPDAT1_CMP4_Msk (0xfffful << PWM_CMPDAT1_CMP4_Pos)

PWM_T::CMPDAT1: CMP4 Mask

Definition at line 8167 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP4_Pos

#define PWM_CMPDAT1_CMP4_Pos (0)

PWM_T::CMPDAT1: CMP4 Position

Definition at line 8166 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP5_Msk

#define PWM_CMPDAT1_CMP5_Msk (0xfffful << PWM_CMPDAT1_CMP5_Pos)

PWM_T::CMPDAT1: CMP5 Mask

Definition at line 8170 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMP5_Pos

#define PWM_CMPDAT1_CMP5_Pos (0)

PWM_T::CMPDAT1: CMP5 Position

Definition at line 8169 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD0_Msk

#define PWM_CMPDAT1_CMPD0_Msk (0xfffful << PWM_CMPDAT1_CMPD0_Pos)

PWM_T::CMPDAT1: CMPD0 Mask

Definition at line 8173 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD0_Pos

#define PWM_CMPDAT1_CMPD0_Pos (16)

PWM_T::CMPDAT1: CMPD0 Position

Definition at line 8172 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD1_Msk

#define PWM_CMPDAT1_CMPD1_Msk (0xfffful << PWM_CMPDAT1_CMPD1_Pos)

PWM_T::CMPDAT1: CMPD1 Mask

Definition at line 8176 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD1_Pos

#define PWM_CMPDAT1_CMPD1_Pos (16)

PWM_T::CMPDAT1: CMPD1 Position

Definition at line 8175 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD2_Msk

#define PWM_CMPDAT1_CMPD2_Msk (0xfffful << PWM_CMPDAT1_CMPD2_Pos)

PWM_T::CMPDAT1: CMPD2 Mask

Definition at line 8179 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD2_Pos

#define PWM_CMPDAT1_CMPD2_Pos (16)

PWM_T::CMPDAT1: CMPD2 Position

Definition at line 8178 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD3_Msk

#define PWM_CMPDAT1_CMPD3_Msk (0xfffful << PWM_CMPDAT1_CMPD3_Pos)

PWM_T::CMPDAT1: CMPD3 Mask

Definition at line 8182 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD3_Pos

#define PWM_CMPDAT1_CMPD3_Pos (16)

PWM_T::CMPDAT1: CMPD3 Position

Definition at line 8181 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD4_Msk

#define PWM_CMPDAT1_CMPD4_Msk (0xfffful << PWM_CMPDAT1_CMPD4_Pos)

PWM_T::CMPDAT1: CMPD4 Mask

Definition at line 8185 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD4_Pos

#define PWM_CMPDAT1_CMPD4_Pos (16)

PWM_T::CMPDAT1: CMPD4 Position

Definition at line 8184 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD5_Msk

#define PWM_CMPDAT1_CMPD5_Msk (0xfffful << PWM_CMPDAT1_CMPD5_Pos)

PWM_T::CMPDAT1: CMPD5 Mask

Definition at line 8188 of file Mini58Series.h.

## ◆ PWM_CMPDAT1_CMPD5_Pos

#define PWM_CMPDAT1_CMPD5_Pos (16)

PWM_T::CMPDAT1: CMPD5 Position

Definition at line 8187 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP0_Msk

#define PWM_CMPDAT2_CMP0_Msk (0xfffful << PWM_CMPDAT2_CMP0_Pos)

PWM_T::CMPDAT2: CMP0 Mask

Definition at line 8191 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP0_Pos

#define PWM_CMPDAT2_CMP0_Pos (0)

PWM_T::CMPDAT2: CMP0 Position

Definition at line 8190 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP1_Msk

#define PWM_CMPDAT2_CMP1_Msk (0xfffful << PWM_CMPDAT2_CMP1_Pos)

PWM_T::CMPDAT2: CMP1 Mask

Definition at line 8194 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP1_Pos

#define PWM_CMPDAT2_CMP1_Pos (0)

PWM_T::CMPDAT2: CMP1 Position

Definition at line 8193 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP2_Msk

#define PWM_CMPDAT2_CMP2_Msk (0xfffful << PWM_CMPDAT2_CMP2_Pos)

PWM_T::CMPDAT2: CMP2 Mask

Definition at line 8197 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP2_Pos

#define PWM_CMPDAT2_CMP2_Pos (0)

PWM_T::CMPDAT2: CMP2 Position

Definition at line 8196 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP3_Msk

#define PWM_CMPDAT2_CMP3_Msk (0xfffful << PWM_CMPDAT2_CMP3_Pos)

PWM_T::CMPDAT2: CMP3 Mask

Definition at line 8200 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP3_Pos

#define PWM_CMPDAT2_CMP3_Pos (0)

PWM_T::CMPDAT2: CMP3 Position

Definition at line 8199 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP4_Msk

#define PWM_CMPDAT2_CMP4_Msk (0xfffful << PWM_CMPDAT2_CMP4_Pos)

PWM_T::CMPDAT2: CMP4 Mask

Definition at line 8203 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP4_Pos

#define PWM_CMPDAT2_CMP4_Pos (0)

PWM_T::CMPDAT2: CMP4 Position

Definition at line 8202 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP5_Msk

#define PWM_CMPDAT2_CMP5_Msk (0xfffful << PWM_CMPDAT2_CMP5_Pos)

PWM_T::CMPDAT2: CMP5 Mask

Definition at line 8206 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMP5_Pos

#define PWM_CMPDAT2_CMP5_Pos (0)

PWM_T::CMPDAT2: CMP5 Position

Definition at line 8205 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD0_Msk

#define PWM_CMPDAT2_CMPD0_Msk (0xfffful << PWM_CMPDAT2_CMPD0_Pos)

PWM_T::CMPDAT2: CMPD0 Mask

Definition at line 8209 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD0_Pos

#define PWM_CMPDAT2_CMPD0_Pos (16)

PWM_T::CMPDAT2: CMPD0 Position

Definition at line 8208 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD1_Msk

#define PWM_CMPDAT2_CMPD1_Msk (0xfffful << PWM_CMPDAT2_CMPD1_Pos)

PWM_T::CMPDAT2: CMPD1 Mask

Definition at line 8212 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD1_Pos

#define PWM_CMPDAT2_CMPD1_Pos (16)

PWM_T::CMPDAT2: CMPD1 Position

Definition at line 8211 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD2_Msk

#define PWM_CMPDAT2_CMPD2_Msk (0xfffful << PWM_CMPDAT2_CMPD2_Pos)

PWM_T::CMPDAT2: CMPD2 Mask

Definition at line 8215 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD2_Pos

#define PWM_CMPDAT2_CMPD2_Pos (16)

PWM_T::CMPDAT2: CMPD2 Position

Definition at line 8214 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD3_Msk

#define PWM_CMPDAT2_CMPD3_Msk (0xfffful << PWM_CMPDAT2_CMPD3_Pos)

PWM_T::CMPDAT2: CMPD3 Mask

Definition at line 8218 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD3_Pos

#define PWM_CMPDAT2_CMPD3_Pos (16)

PWM_T::CMPDAT2: CMPD3 Position

Definition at line 8217 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD4_Msk

#define PWM_CMPDAT2_CMPD4_Msk (0xfffful << PWM_CMPDAT2_CMPD4_Pos)

PWM_T::CMPDAT2: CMPD4 Mask

Definition at line 8221 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD4_Pos

#define PWM_CMPDAT2_CMPD4_Pos (16)

PWM_T::CMPDAT2: CMPD4 Position

Definition at line 8220 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD5_Msk

#define PWM_CMPDAT2_CMPD5_Msk (0xfffful << PWM_CMPDAT2_CMPD5_Pos)

PWM_T::CMPDAT2: CMPD5 Mask

Definition at line 8224 of file Mini58Series.h.

## ◆ PWM_CMPDAT2_CMPD5_Pos

#define PWM_CMPDAT2_CMPD5_Pos (16)

PWM_T::CMPDAT2: CMPD5 Position

Definition at line 8223 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP0_Msk

#define PWM_CMPDAT3_CMP0_Msk (0xfffful << PWM_CMPDAT3_CMP0_Pos)

PWM_T::CMPDAT3: CMP0 Mask

Definition at line 8227 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP0_Pos

#define PWM_CMPDAT3_CMP0_Pos (0)

PWM_T::CMPDAT3: CMP0 Position

Definition at line 8226 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP1_Msk

#define PWM_CMPDAT3_CMP1_Msk (0xfffful << PWM_CMPDAT3_CMP1_Pos)

PWM_T::CMPDAT3: CMP1 Mask

Definition at line 8230 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP1_Pos

#define PWM_CMPDAT3_CMP1_Pos (0)

PWM_T::CMPDAT3: CMP1 Position

Definition at line 8229 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP2_Msk

#define PWM_CMPDAT3_CMP2_Msk (0xfffful << PWM_CMPDAT3_CMP2_Pos)

PWM_T::CMPDAT3: CMP2 Mask

Definition at line 8233 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP2_Pos

#define PWM_CMPDAT3_CMP2_Pos (0)

PWM_T::CMPDAT3: CMP2 Position

Definition at line 8232 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP3_Msk

#define PWM_CMPDAT3_CMP3_Msk (0xfffful << PWM_CMPDAT3_CMP3_Pos)

PWM_T::CMPDAT3: CMP3 Mask

Definition at line 8236 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP3_Pos

#define PWM_CMPDAT3_CMP3_Pos (0)

PWM_T::CMPDAT3: CMP3 Position

Definition at line 8235 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP4_Msk

#define PWM_CMPDAT3_CMP4_Msk (0xfffful << PWM_CMPDAT3_CMP4_Pos)

PWM_T::CMPDAT3: CMP4 Mask

Definition at line 8239 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP4_Pos

#define PWM_CMPDAT3_CMP4_Pos (0)

PWM_T::CMPDAT3: CMP4 Position

Definition at line 8238 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP5_Msk

#define PWM_CMPDAT3_CMP5_Msk (0xfffful << PWM_CMPDAT3_CMP5_Pos)

PWM_T::CMPDAT3: CMP5 Mask

Definition at line 8242 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMP5_Pos

#define PWM_CMPDAT3_CMP5_Pos (0)

PWM_T::CMPDAT3: CMP5 Position

Definition at line 8241 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD0_Msk

#define PWM_CMPDAT3_CMPD0_Msk (0xfffful << PWM_CMPDAT3_CMPD0_Pos)

PWM_T::CMPDAT3: CMPD0 Mask

Definition at line 8245 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD0_Pos

#define PWM_CMPDAT3_CMPD0_Pos (16)

PWM_T::CMPDAT3: CMPD0 Position

Definition at line 8244 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD1_Msk

#define PWM_CMPDAT3_CMPD1_Msk (0xfffful << PWM_CMPDAT3_CMPD1_Pos)

PWM_T::CMPDAT3: CMPD1 Mask

Definition at line 8248 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD1_Pos

#define PWM_CMPDAT3_CMPD1_Pos (16)

PWM_T::CMPDAT3: CMPD1 Position

Definition at line 8247 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD2_Msk

#define PWM_CMPDAT3_CMPD2_Msk (0xfffful << PWM_CMPDAT3_CMPD2_Pos)

PWM_T::CMPDAT3: CMPD2 Mask

Definition at line 8251 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD2_Pos

#define PWM_CMPDAT3_CMPD2_Pos (16)

PWM_T::CMPDAT3: CMPD2 Position

Definition at line 8250 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD3_Msk

#define PWM_CMPDAT3_CMPD3_Msk (0xfffful << PWM_CMPDAT3_CMPD3_Pos)

PWM_T::CMPDAT3: CMPD3 Mask

Definition at line 8254 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD3_Pos

#define PWM_CMPDAT3_CMPD3_Pos (16)

PWM_T::CMPDAT3: CMPD3 Position

Definition at line 8253 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD4_Msk

#define PWM_CMPDAT3_CMPD4_Msk (0xfffful << PWM_CMPDAT3_CMPD4_Pos)

PWM_T::CMPDAT3: CMPD4 Mask

Definition at line 8257 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD4_Pos

#define PWM_CMPDAT3_CMPD4_Pos (16)

PWM_T::CMPDAT3: CMPD4 Position

Definition at line 8256 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD5_Msk

#define PWM_CMPDAT3_CMPD5_Msk (0xfffful << PWM_CMPDAT3_CMPD5_Pos)

PWM_T::CMPDAT3: CMPD5 Mask

Definition at line 8260 of file Mini58Series.h.

## ◆ PWM_CMPDAT3_CMPD5_Pos

#define PWM_CMPDAT3_CMPD5_Pos (16)

PWM_T::CMPDAT3: CMPD5 Position

Definition at line 8259 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP0_Msk

#define PWM_CMPDAT4_CMP0_Msk (0xfffful << PWM_CMPDAT4_CMP0_Pos)

PWM_T::CMPDAT4: CMP0 Mask

Definition at line 8263 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP0_Pos

#define PWM_CMPDAT4_CMP0_Pos (0)

PWM_T::CMPDAT4: CMP0 Position

Definition at line 8262 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP1_Msk

#define PWM_CMPDAT4_CMP1_Msk (0xfffful << PWM_CMPDAT4_CMP1_Pos)

PWM_T::CMPDAT4: CMP1 Mask

Definition at line 8266 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP1_Pos

#define PWM_CMPDAT4_CMP1_Pos (0)

PWM_T::CMPDAT4: CMP1 Position

Definition at line 8265 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP2_Msk

#define PWM_CMPDAT4_CMP2_Msk (0xfffful << PWM_CMPDAT4_CMP2_Pos)

PWM_T::CMPDAT4: CMP2 Mask

Definition at line 8269 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP2_Pos

#define PWM_CMPDAT4_CMP2_Pos (0)

PWM_T::CMPDAT4: CMP2 Position

Definition at line 8268 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP3_Msk

#define PWM_CMPDAT4_CMP3_Msk (0xfffful << PWM_CMPDAT4_CMP3_Pos)

PWM_T::CMPDAT4: CMP3 Mask

Definition at line 8272 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP3_Pos

#define PWM_CMPDAT4_CMP3_Pos (0)

PWM_T::CMPDAT4: CMP3 Position

Definition at line 8271 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP4_Msk

#define PWM_CMPDAT4_CMP4_Msk (0xfffful << PWM_CMPDAT4_CMP4_Pos)

PWM_T::CMPDAT4: CMP4 Mask

Definition at line 8275 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP4_Pos

#define PWM_CMPDAT4_CMP4_Pos (0)

PWM_T::CMPDAT4: CMP4 Position

Definition at line 8274 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP5_Msk

#define PWM_CMPDAT4_CMP5_Msk (0xfffful << PWM_CMPDAT4_CMP5_Pos)

PWM_T::CMPDAT4: CMP5 Mask

Definition at line 8278 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMP5_Pos

#define PWM_CMPDAT4_CMP5_Pos (0)

PWM_T::CMPDAT4: CMP5 Position

Definition at line 8277 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD0_Msk

#define PWM_CMPDAT4_CMPD0_Msk (0xfffful << PWM_CMPDAT4_CMPD0_Pos)

PWM_T::CMPDAT4: CMPD0 Mask

Definition at line 8281 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD0_Pos

#define PWM_CMPDAT4_CMPD0_Pos (16)

PWM_T::CMPDAT4: CMPD0 Position

Definition at line 8280 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD1_Msk

#define PWM_CMPDAT4_CMPD1_Msk (0xfffful << PWM_CMPDAT4_CMPD1_Pos)

PWM_T::CMPDAT4: CMPD1 Mask

Definition at line 8284 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD1_Pos

#define PWM_CMPDAT4_CMPD1_Pos (16)

PWM_T::CMPDAT4: CMPD1 Position

Definition at line 8283 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD2_Msk

#define PWM_CMPDAT4_CMPD2_Msk (0xfffful << PWM_CMPDAT4_CMPD2_Pos)

PWM_T::CMPDAT4: CMPD2 Mask

Definition at line 8287 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD2_Pos

#define PWM_CMPDAT4_CMPD2_Pos (16)

PWM_T::CMPDAT4: CMPD2 Position

Definition at line 8286 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD3_Msk

#define PWM_CMPDAT4_CMPD3_Msk (0xfffful << PWM_CMPDAT4_CMPD3_Pos)

PWM_T::CMPDAT4: CMPD3 Mask

Definition at line 8290 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD3_Pos

#define PWM_CMPDAT4_CMPD3_Pos (16)

PWM_T::CMPDAT4: CMPD3 Position

Definition at line 8289 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD4_Msk

#define PWM_CMPDAT4_CMPD4_Msk (0xfffful << PWM_CMPDAT4_CMPD4_Pos)

PWM_T::CMPDAT4: CMPD4 Mask

Definition at line 8293 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD4_Pos

#define PWM_CMPDAT4_CMPD4_Pos (16)

PWM_T::CMPDAT4: CMPD4 Position

Definition at line 8292 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD5_Msk

#define PWM_CMPDAT4_CMPD5_Msk (0xfffful << PWM_CMPDAT4_CMPD5_Pos)

PWM_T::CMPDAT4: CMPD5 Mask

Definition at line 8296 of file Mini58Series.h.

## ◆ PWM_CMPDAT4_CMPD5_Pos

#define PWM_CMPDAT4_CMPD5_Pos (16)

PWM_T::CMPDAT4: CMPD5 Position

Definition at line 8295 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP0_Msk

#define PWM_CMPDAT5_CMP0_Msk (0xfffful << PWM_CMPDAT5_CMP0_Pos)

PWM_T::CMPDAT5: CMP0 Mask

Definition at line 8299 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP0_Pos

#define PWM_CMPDAT5_CMP0_Pos (0)

PWM_T::CMPDAT5: CMP0 Position

Definition at line 8298 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP1_Msk

#define PWM_CMPDAT5_CMP1_Msk (0xfffful << PWM_CMPDAT5_CMP1_Pos)

PWM_T::CMPDAT5: CMP1 Mask

Definition at line 8302 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP1_Pos

#define PWM_CMPDAT5_CMP1_Pos (0)

PWM_T::CMPDAT5: CMP1 Position

Definition at line 8301 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP2_Msk

#define PWM_CMPDAT5_CMP2_Msk (0xfffful << PWM_CMPDAT5_CMP2_Pos)

PWM_T::CMPDAT5: CMP2 Mask

Definition at line 8305 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP2_Pos

#define PWM_CMPDAT5_CMP2_Pos (0)

PWM_T::CMPDAT5: CMP2 Position

Definition at line 8304 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP3_Msk

#define PWM_CMPDAT5_CMP3_Msk (0xfffful << PWM_CMPDAT5_CMP3_Pos)

PWM_T::CMPDAT5: CMP3 Mask

Definition at line 8308 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP3_Pos

#define PWM_CMPDAT5_CMP3_Pos (0)

PWM_T::CMPDAT5: CMP3 Position

Definition at line 8307 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP4_Msk

#define PWM_CMPDAT5_CMP4_Msk (0xfffful << PWM_CMPDAT5_CMP4_Pos)

PWM_T::CMPDAT5: CMP4 Mask

Definition at line 8311 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP4_Pos

#define PWM_CMPDAT5_CMP4_Pos (0)

PWM_T::CMPDAT5: CMP4 Position

Definition at line 8310 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP5_Msk

#define PWM_CMPDAT5_CMP5_Msk (0xfffful << PWM_CMPDAT5_CMP5_Pos)

PWM_T::CMPDAT5: CMP5 Mask

Definition at line 8314 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMP5_Pos

#define PWM_CMPDAT5_CMP5_Pos (0)

PWM_T::CMPDAT5: CMP5 Position

Definition at line 8313 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD0_Msk

#define PWM_CMPDAT5_CMPD0_Msk (0xfffful << PWM_CMPDAT5_CMPD0_Pos)

PWM_T::CMPDAT5: CMPD0 Mask

Definition at line 8317 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD0_Pos

#define PWM_CMPDAT5_CMPD0_Pos (16)

PWM_T::CMPDAT5: CMPD0 Position

Definition at line 8316 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD1_Msk

#define PWM_CMPDAT5_CMPD1_Msk (0xfffful << PWM_CMPDAT5_CMPD1_Pos)

PWM_T::CMPDAT5: CMPD1 Mask

Definition at line 8320 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD1_Pos

#define PWM_CMPDAT5_CMPD1_Pos (16)

PWM_T::CMPDAT5: CMPD1 Position

Definition at line 8319 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD2_Msk

#define PWM_CMPDAT5_CMPD2_Msk (0xfffful << PWM_CMPDAT5_CMPD2_Pos)

PWM_T::CMPDAT5: CMPD2 Mask

Definition at line 8323 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD2_Pos

#define PWM_CMPDAT5_CMPD2_Pos (16)

PWM_T::CMPDAT5: CMPD2 Position

Definition at line 8322 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD3_Msk

#define PWM_CMPDAT5_CMPD3_Msk (0xfffful << PWM_CMPDAT5_CMPD3_Pos)

PWM_T::CMPDAT5: CMPD3 Mask

Definition at line 8326 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD3_Pos

#define PWM_CMPDAT5_CMPD3_Pos (16)

PWM_T::CMPDAT5: CMPD3 Position

Definition at line 8325 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD4_Msk

#define PWM_CMPDAT5_CMPD4_Msk (0xfffful << PWM_CMPDAT5_CMPD4_Pos)

PWM_T::CMPDAT5: CMPD4 Mask

Definition at line 8329 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD4_Pos

#define PWM_CMPDAT5_CMPD4_Pos (16)

PWM_T::CMPDAT5: CMPD4 Position

Definition at line 8328 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD5_Msk

#define PWM_CMPDAT5_CMPD5_Msk (0xfffful << PWM_CMPDAT5_CMPD5_Pos)

PWM_T::CMPDAT5: CMPD5 Mask

Definition at line 8332 of file Mini58Series.h.

## ◆ PWM_CMPDAT5_CMPD5_Pos

#define PWM_CMPDAT5_CMPD5_Pos (16)

PWM_T::CMPDAT5: CMPD5 Position

Definition at line 8331 of file Mini58Series.h.

## ◆ PWM_CTL_ASYMEN_Msk

#define PWM_CTL_ASYMEN_Msk (0x1ul << PWM_CTL_ASYMEN_Pos)

PWM_T::CTL: ASYMEN Mask

Definition at line 7981 of file Mini58Series.h.

## ◆ PWM_CTL_ASYMEN_Pos

#define PWM_CTL_ASYMEN_Pos (21)

PWM_T::CTL: ASYMEN Position

Definition at line 7980 of file Mini58Series.h.

## ◆ PWM_CTL_CNTCLR_Msk

#define PWM_CTL_CNTCLR_Msk (0x1ul << PWM_CTL_CNTCLR_Pos)

PWM_T::CTL: CNTCLR Mask

Definition at line 7999 of file Mini58Series.h.

## ◆ PWM_CTL_CNTCLR_Pos

#define PWM_CTL_CNTCLR_Pos (27)

PWM_T::CTL: CNTCLR Position

Definition at line 7998 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN0_Msk

#define PWM_CTL_CNTEN0_Msk (0x1ul << PWM_CTL_CNTEN0_Pos)

PWM_T::CTL: CNTEN0 Mask

Definition at line 7927 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN0_Pos

#define PWM_CTL_CNTEN0_Pos (0)

PWM_T::CTL: CNTEN0 Position

Definition at line 7926 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN1_Msk

#define PWM_CTL_CNTEN1_Msk (0x1ul << PWM_CTL_CNTEN1_Pos)

PWM_T::CTL: CNTEN1 Mask

Definition at line 7939 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN1_Pos

#define PWM_CTL_CNTEN1_Pos (4)

PWM_T::CTL: CNTEN1 Position

Definition at line 7938 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN2_Msk

#define PWM_CTL_CNTEN2_Msk (0x1ul << PWM_CTL_CNTEN2_Pos)

PWM_T::CTL: CNTEN2 Mask

Definition at line 7951 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN2_Pos

#define PWM_CTL_CNTEN2_Pos (8)

PWM_T::CTL: CNTEN2 Position

Definition at line 7950 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN3_Msk

#define PWM_CTL_CNTEN3_Msk (0x1ul << PWM_CTL_CNTEN3_Pos)

PWM_T::CTL: CNTEN3 Mask

Definition at line 7960 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN3_Pos

#define PWM_CTL_CNTEN3_Pos (12)

PWM_T::CTL: CNTEN3 Position

Definition at line 7959 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN4_Msk

#define PWM_CTL_CNTEN4_Msk (0x1ul << PWM_CTL_CNTEN4_Pos)

PWM_T::CTL: CNTEN4 Mask

Definition at line 7969 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN4_Pos

#define PWM_CTL_CNTEN4_Pos (16)

PWM_T::CTL: CNTEN4 Position

Definition at line 7968 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN5_Msk

#define PWM_CTL_CNTEN5_Msk (0x1ul << PWM_CTL_CNTEN5_Pos)

PWM_T::CTL: CNTEN5 Mask

Definition at line 7978 of file Mini58Series.h.

## ◆ PWM_CTL_CNTEN5_Pos

#define PWM_CTL_CNTEN5_Pos (20)

PWM_T::CTL: CNTEN5 Position

Definition at line 7977 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE0_Msk

#define PWM_CTL_CNTMODE0_Msk (0x1ul << PWM_CTL_CNTMODE0_Pos)

PWM_T::CTL: CNTMODE0 Mask

Definition at line 7936 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE0_Pos

#define PWM_CTL_CNTMODE0_Pos (3)

PWM_T::CTL: CNTMODE0 Position

Definition at line 7935 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE1_Msk

#define PWM_CTL_CNTMODE1_Msk (0x1ul << PWM_CTL_CNTMODE1_Pos)

PWM_T::CTL: CNTMODE1 Mask

Definition at line 7948 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE1_Pos

#define PWM_CTL_CNTMODE1_Pos (7)

PWM_T::CTL: CNTMODE1 Position

Definition at line 7947 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE2_Msk

#define PWM_CTL_CNTMODE2_Msk (0x1ul << PWM_CTL_CNTMODE2_Pos)

PWM_T::CTL: CNTMODE2 Mask

Definition at line 7957 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE2_Pos

#define PWM_CTL_CNTMODE2_Pos (11)

PWM_T::CTL: CNTMODE2 Position

Definition at line 7956 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE3_Msk

#define PWM_CTL_CNTMODE3_Msk (0x1ul << PWM_CTL_CNTMODE3_Pos)

PWM_T::CTL: CNTMODE3 Mask

Definition at line 7966 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE3_Pos

#define PWM_CTL_CNTMODE3_Pos (15)

PWM_T::CTL: CNTMODE3 Position

Definition at line 7965 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE4_Msk

#define PWM_CTL_CNTMODE4_Msk (0x1ul << PWM_CTL_CNTMODE4_Pos)

PWM_T::CTL: CNTMODE4 Mask

Definition at line 7975 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE4_Pos

#define PWM_CTL_CNTMODE4_Pos (19)

PWM_T::CTL: CNTMODE4 Position

Definition at line 7974 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE5_Msk

#define PWM_CTL_CNTMODE5_Msk (0x1ul << PWM_CTL_CNTMODE5_Pos)

PWM_T::CTL: CNTMODE5 Mask

Definition at line 7987 of file Mini58Series.h.

## ◆ PWM_CTL_CNTMODE5_Pos

#define PWM_CTL_CNTMODE5_Pos (23)

PWM_T::CTL: CNTMODE5 Position

Definition at line 7986 of file Mini58Series.h.

## ◆ PWM_CTL_CNTTYPE_Msk

#define PWM_CTL_CNTTYPE_Msk (0x1ul << PWM_CTL_CNTTYPE_Pos)

PWM_T::CTL: CNTTYPE Mask

Definition at line 8008 of file Mini58Series.h.

## ◆ PWM_CTL_CNTTYPE_Pos

#define PWM_CTL_CNTTYPE_Pos (31)

PWM_T::CTL: CNTTYPE Position

Definition at line 8007 of file Mini58Series.h.

## ◆ PWM_CTL_DBGTRIOFF_Msk

#define PWM_CTL_DBGTRIOFF_Msk (0x1ul << PWM_CTL_DBGTRIOFF_Pos)

PWM_T::CTL: DBGTRIOFF Mask

Definition at line 7930 of file Mini58Series.h.

## ◆ PWM_CTL_DBGTRIOFF_Pos

#define PWM_CTL_DBGTRIOFF_Pos (1)

PWM_T::CTL: DBGTRIOFF Position

Definition at line 7929 of file Mini58Series.h.

## ◆ PWM_CTL_DTCNT01_Msk

#define PWM_CTL_DTCNT01_Msk (0x1ul << PWM_CTL_DTCNT01_Pos)

PWM_T::CTL: DTCNT01 Mask

Definition at line 7990 of file Mini58Series.h.

## ◆ PWM_CTL_DTCNT01_Pos

#define PWM_CTL_DTCNT01_Pos (24)

PWM_T::CTL: DTCNT01 Position

Definition at line 7989 of file Mini58Series.h.

## ◆ PWM_CTL_DTCNT23_Msk

#define PWM_CTL_DTCNT23_Msk (0x1ul << PWM_CTL_DTCNT23_Pos)

PWM_T::CTL: DTCNT23 Mask

Definition at line 7993 of file Mini58Series.h.

## ◆ PWM_CTL_DTCNT23_Pos

#define PWM_CTL_DTCNT23_Pos (25)

PWM_T::CTL: DTCNT23 Position

Definition at line 7992 of file Mini58Series.h.

## ◆ PWM_CTL_DTCNT45_Msk

#define PWM_CTL_DTCNT45_Msk (0x1ul << PWM_CTL_DTCNT45_Pos)

PWM_T::CTL: DTCNT45 Mask

Definition at line 7996 of file Mini58Series.h.

## ◆ PWM_CTL_DTCNT45_Pos

#define PWM_CTL_DTCNT45_Pos (26)

PWM_T::CTL: DTCNT45 Position

Definition at line 7995 of file Mini58Series.h.

## ◆ PWM_CTL_GROUPEN_Msk

#define PWM_CTL_GROUPEN_Msk (0x1ul << PWM_CTL_GROUPEN_Pos)

PWM_T::CTL: GROUPEN Mask

Definition at line 8005 of file Mini58Series.h.

## ◆ PWM_CTL_GROUPEN_Pos

#define PWM_CTL_GROUPEN_Pos (30)

PWM_T::CTL: GROUPEN Position

Definition at line 8004 of file Mini58Series.h.

## ◆ PWM_CTL_HCUPDT_Msk

#define PWM_CTL_HCUPDT_Msk (0x1ul << PWM_CTL_HCUPDT_Pos)

PWM_T::CTL: HCUPDT Mask

Definition at line 7942 of file Mini58Series.h.

## ◆ PWM_CTL_HCUPDT_Pos

#define PWM_CTL_HCUPDT_Pos (5)

PWM_T::CTL: HCUPDT Position

Definition at line 7941 of file Mini58Series.h.

## ◆ PWM_CTL_MODE_Msk

#define PWM_CTL_MODE_Msk (0x3ul << PWM_CTL_MODE_Pos)

PWM_T::CTL: MODE Mask

Definition at line 8002 of file Mini58Series.h.

## ◆ PWM_CTL_MODE_Pos

#define PWM_CTL_MODE_Pos (28)

PWM_T::CTL: MODE Position

Definition at line 8001 of file Mini58Series.h.

## ◆ PWM_CTL_PINV0_Msk

#define PWM_CTL_PINV0_Msk (0x1ul << PWM_CTL_PINV0_Pos)

PWM_T::CTL: PINV0 Mask

Definition at line 7933 of file Mini58Series.h.

## ◆ PWM_CTL_PINV0_Pos

#define PWM_CTL_PINV0_Pos (2)

PWM_T::CTL: PINV0 Position

Definition at line 7932 of file Mini58Series.h.

## ◆ PWM_CTL_PINV1_Msk

#define PWM_CTL_PINV1_Msk (0x1ul << PWM_CTL_PINV1_Pos)

PWM_T::CTL: PINV1 Mask

Definition at line 7945 of file Mini58Series.h.

## ◆ PWM_CTL_PINV1_Pos

#define PWM_CTL_PINV1_Pos (6)

PWM_T::CTL: PINV1 Position

Definition at line 7944 of file Mini58Series.h.

## ◆ PWM_CTL_PINV2_Msk

#define PWM_CTL_PINV2_Msk (0x1ul << PWM_CTL_PINV2_Pos)

PWM_T::CTL: PINV2 Mask

Definition at line 7954 of file Mini58Series.h.

## ◆ PWM_CTL_PINV2_Pos

#define PWM_CTL_PINV2_Pos (10)

PWM_T::CTL: PINV2 Position

Definition at line 7953 of file Mini58Series.h.

## ◆ PWM_CTL_PINV3_Msk

#define PWM_CTL_PINV3_Msk (0x1ul << PWM_CTL_PINV3_Pos)

PWM_T::CTL: PINV3 Mask

Definition at line 7963 of file Mini58Series.h.

## ◆ PWM_CTL_PINV3_Pos

#define PWM_CTL_PINV3_Pos (14)

PWM_T::CTL: PINV3 Position

Definition at line 7962 of file Mini58Series.h.

## ◆ PWM_CTL_PINV4_Msk

#define PWM_CTL_PINV4_Msk (0x1ul << PWM_CTL_PINV4_Pos)

PWM_T::CTL: PINV4 Mask

Definition at line 7972 of file Mini58Series.h.

## ◆ PWM_CTL_PINV4_Pos

#define PWM_CTL_PINV4_Pos (18)

PWM_T::CTL: PINV4 Position

Definition at line 7971 of file Mini58Series.h.

## ◆ PWM_CTL_PINV5_Msk

#define PWM_CTL_PINV5_Msk (0x1ul << PWM_CTL_PINV5_Pos)

PWM_T::CTL: PINV5 Mask

Definition at line 7984 of file Mini58Series.h.

## ◆ PWM_CTL_PINV5_Pos

#define PWM_CTL_PINV5_Pos (22)

PWM_T::CTL: PINV5 Position

Definition at line 7983 of file Mini58Series.h.

## ◆ PWM_DTCTL_DTI01_Msk

#define PWM_DTCTL_DTI01_Msk (0xfful << PWM_DTCTL_DTI01_Pos)

PWM_T::DTCTL: DTI01 Mask

Definition at line 8554 of file Mini58Series.h.

## ◆ PWM_DTCTL_DTI01_Pos

#define PWM_DTCTL_DTI01_Pos (0)

PWM_T::DTCTL: DTI01 Position

Definition at line 8553 of file Mini58Series.h.

## ◆ PWM_DTCTL_DTI23_Msk

#define PWM_DTCTL_DTI23_Msk (0xfful << PWM_DTCTL_DTI23_Pos)

PWM_T::DTCTL: DTI23 Mask

Definition at line 8557 of file Mini58Series.h.

## ◆ PWM_DTCTL_DTI23_Pos

#define PWM_DTCTL_DTI23_Pos (8)

PWM_T::DTCTL: DTI23 Position

Definition at line 8556 of file Mini58Series.h.

## ◆ PWM_DTCTL_DTI45_Msk

#define PWM_DTCTL_DTI45_Msk (0xfful << PWM_DTCTL_DTI45_Pos)

PWM_T::DTCTL: DTI45 Mask

Definition at line 8560 of file Mini58Series.h.

## ◆ PWM_DTCTL_DTI45_Pos

#define PWM_DTCTL_DTI45_Pos (16)

PWM_T::DTCTL: DTI45 Position

Definition at line 8559 of file Mini58Series.h.

## ◆ PWM_IFA_IFAEN_Msk

#define PWM_IFA_IFAEN_Msk (0x1ul << PWM_IFA_IFAEN_Pos)

PWM_T::IFA: IFAEN Mask

Definition at line 8899 of file Mini58Series.h.

## ◆ PWM_IFA_IFAEN_Pos

#define PWM_IFA_IFAEN_Pos (0)

PWM_T::IFA: IFAEN Position

Definition at line 8898 of file Mini58Series.h.

## ◆ PWM_IFA_IFCNT_Msk

#define PWM_IFA_IFCNT_Msk (0xful << PWM_IFA_IFCNT_Pos)

PWM_T::IFA: IFCNT Mask

Definition at line 8902 of file Mini58Series.h.

## ◆ PWM_IFA_IFCNT_Pos

#define PWM_IFA_IFCNT_Pos (4)

PWM_T::IFA: IFCNT Position

Definition at line 8901 of file Mini58Series.h.

## ◆ PWM_INTEN_BRKIEN_Msk

#define PWM_INTEN_BRKIEN_Msk (0x1ul << PWM_INTEN_BRKIEN_Pos)

PWM_T::INTEN: BRKIEN Mask

Definition at line 8371 of file Mini58Series.h.

## ◆ PWM_INTEN_BRKIEN_Pos

#define PWM_INTEN_BRKIEN_Pos (16)

PWM_T::INTEN: BRKIEN Position

Definition at line 8370 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN0_Msk

#define PWM_INTEN_CMPDIEN0_Msk (0x1ul << PWM_INTEN_CMPDIEN0_Pos)

PWM_T::INTEN: CMPDIEN0 Mask

Definition at line 8353 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN0_Pos

#define PWM_INTEN_CMPDIEN0_Pos (8)

PWM_T::INTEN: CMPDIEN0 Position

Definition at line 8352 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN1_Msk

#define PWM_INTEN_CMPDIEN1_Msk (0x1ul << PWM_INTEN_CMPDIEN1_Pos)

PWM_T::INTEN: CMPDIEN1 Mask

Definition at line 8356 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN1_Pos

#define PWM_INTEN_CMPDIEN1_Pos (9)

PWM_T::INTEN: CMPDIEN1 Position

Definition at line 8355 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN2_Msk

#define PWM_INTEN_CMPDIEN2_Msk (0x1ul << PWM_INTEN_CMPDIEN2_Pos)

PWM_T::INTEN: CMPDIEN2 Mask

Definition at line 8359 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN2_Pos

#define PWM_INTEN_CMPDIEN2_Pos (10)

PWM_T::INTEN: CMPDIEN2 Position

Definition at line 8358 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN3_Msk

#define PWM_INTEN_CMPDIEN3_Msk (0x1ul << PWM_INTEN_CMPDIEN3_Pos)

PWM_T::INTEN: CMPDIEN3 Mask

Definition at line 8362 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN3_Pos

#define PWM_INTEN_CMPDIEN3_Pos (11)

PWM_T::INTEN: CMPDIEN3 Position

Definition at line 8361 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN4_Msk

#define PWM_INTEN_CMPDIEN4_Msk (0x1ul << PWM_INTEN_CMPDIEN4_Pos)

PWM_T::INTEN: CMPDIEN4 Mask

Definition at line 8365 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN4_Pos

#define PWM_INTEN_CMPDIEN4_Pos (12)

PWM_T::INTEN: CMPDIEN4 Position

Definition at line 8364 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN5_Msk

#define PWM_INTEN_CMPDIEN5_Msk (0x1ul << PWM_INTEN_CMPDIEN5_Pos)

PWM_T::INTEN: CMPDIEN5 Mask

Definition at line 8368 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPDIEN5_Pos

#define PWM_INTEN_CMPDIEN5_Pos (13)

PWM_T::INTEN: CMPDIEN5 Position

Definition at line 8367 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN0_Msk

#define PWM_INTEN_CMPUIEN0_Msk (0x1ul << PWM_INTEN_CMPUIEN0_Pos)

PWM_T::INTEN: CMPUIEN0 Mask

Definition at line 8395 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN0_Pos

#define PWM_INTEN_CMPUIEN0_Pos (24)

PWM_T::INTEN: CMPUIEN0 Position

Definition at line 8394 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN1_Msk

#define PWM_INTEN_CMPUIEN1_Msk (0x1ul << PWM_INTEN_CMPUIEN1_Pos)

PWM_T::INTEN: CMPUIEN1 Mask

Definition at line 8398 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN1_Pos

#define PWM_INTEN_CMPUIEN1_Pos (25)

PWM_T::INTEN: CMPUIEN1 Position

Definition at line 8397 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN2_Msk

#define PWM_INTEN_CMPUIEN2_Msk (0x1ul << PWM_INTEN_CMPUIEN2_Pos)

PWM_T::INTEN: CMPUIEN2 Mask

Definition at line 8401 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN2_Pos

#define PWM_INTEN_CMPUIEN2_Pos (26)

PWM_T::INTEN: CMPUIEN2 Position

Definition at line 8400 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN3_Msk

#define PWM_INTEN_CMPUIEN3_Msk (0x1ul << PWM_INTEN_CMPUIEN3_Pos)

PWM_T::INTEN: CMPUIEN3 Mask

Definition at line 8404 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN3_Pos

#define PWM_INTEN_CMPUIEN3_Pos (27)

PWM_T::INTEN: CMPUIEN3 Position

Definition at line 8403 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN4_Msk

#define PWM_INTEN_CMPUIEN4_Msk (0x1ul << PWM_INTEN_CMPUIEN4_Pos)

PWM_T::INTEN: CMPUIEN4 Mask

Definition at line 8407 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN4_Pos

#define PWM_INTEN_CMPUIEN4_Pos (28)

PWM_T::INTEN: CMPUIEN4 Position

Definition at line 8406 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN5_Msk

#define PWM_INTEN_CMPUIEN5_Msk (0x1ul << PWM_INTEN_CMPUIEN5_Pos)

PWM_T::INTEN: CMPUIEN5 Mask

Definition at line 8410 of file Mini58Series.h.

## ◆ PWM_INTEN_CMPUIEN5_Pos

#define PWM_INTEN_CMPUIEN5_Pos (29)

PWM_T::INTEN: CMPUIEN5 Position

Definition at line 8409 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN0_Msk

#define PWM_INTEN_PIEN0_Msk (0x1ul << PWM_INTEN_PIEN0_Pos)

PWM_T::INTEN: PIEN0 Mask

Definition at line 8377 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN0_Pos

#define PWM_INTEN_PIEN0_Pos (18)

PWM_T::INTEN: PIEN0 Position

Definition at line 8376 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN1_Msk

#define PWM_INTEN_PIEN1_Msk (0x1ul << PWM_INTEN_PIEN1_Pos)

PWM_T::INTEN: PIEN1 Mask

Definition at line 8380 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN1_Pos

#define PWM_INTEN_PIEN1_Pos (19)

PWM_T::INTEN: PIEN1 Position

Definition at line 8379 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN2_Msk

#define PWM_INTEN_PIEN2_Msk (0x1ul << PWM_INTEN_PIEN2_Pos)

PWM_T::INTEN: PIEN2 Mask

Definition at line 8383 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN2_Pos

#define PWM_INTEN_PIEN2_Pos (20)

PWM_T::INTEN: PIEN2 Position

Definition at line 8382 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN3_Msk

#define PWM_INTEN_PIEN3_Msk (0x1ul << PWM_INTEN_PIEN3_Pos)

PWM_T::INTEN: PIEN3 Mask

Definition at line 8386 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN3_Pos

#define PWM_INTEN_PIEN3_Pos (21)

PWM_T::INTEN: PIEN3 Position

Definition at line 8385 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN4_Msk

#define PWM_INTEN_PIEN4_Msk (0x1ul << PWM_INTEN_PIEN4_Pos)

PWM_T::INTEN: PIEN4 Mask

Definition at line 8389 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN4_Pos

#define PWM_INTEN_PIEN4_Pos (22)

PWM_T::INTEN: PIEN4 Position

Definition at line 8388 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN5_Msk

#define PWM_INTEN_PIEN5_Msk (0x1ul << PWM_INTEN_PIEN5_Pos)

PWM_T::INTEN: PIEN5 Mask

Definition at line 8392 of file Mini58Series.h.

## ◆ PWM_INTEN_PIEN5_Pos

#define PWM_INTEN_PIEN5_Pos (23)

PWM_T::INTEN: PIEN5 Position

Definition at line 8391 of file Mini58Series.h.

## ◆ PWM_INTEN_PINTTYPE_Msk

#define PWM_INTEN_PINTTYPE_Msk (0x1ul << PWM_INTEN_PINTTYPE_Pos)

PWM_T::INTEN: PINTTYPE Mask

Definition at line 8374 of file Mini58Series.h.

## ◆ PWM_INTEN_PINTTYPE_Pos

#define PWM_INTEN_PINTTYPE_Pos (17)

PWM_T::INTEN: PINTTYPE Position

Definition at line 8373 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN0_Msk

#define PWM_INTEN_ZIEN0_Msk (0x1ul << PWM_INTEN_ZIEN0_Pos)

PWM_T::INTEN: ZIEN0 Mask

Definition at line 8335 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN0_Pos

#define PWM_INTEN_ZIEN0_Pos (0)

PWM_T::INTEN: ZIEN0 Position

Definition at line 8334 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN1_Msk

#define PWM_INTEN_ZIEN1_Msk (0x1ul << PWM_INTEN_ZIEN1_Pos)

PWM_T::INTEN: ZIEN1 Mask

Definition at line 8338 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN1_Pos

#define PWM_INTEN_ZIEN1_Pos (1)

PWM_T::INTEN: ZIEN1 Position

Definition at line 8337 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN2_Msk

#define PWM_INTEN_ZIEN2_Msk (0x1ul << PWM_INTEN_ZIEN2_Pos)

PWM_T::INTEN: ZIEN2 Mask

Definition at line 8341 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN2_Pos

#define PWM_INTEN_ZIEN2_Pos (2)

PWM_T::INTEN: ZIEN2 Position

Definition at line 8340 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN3_Msk

#define PWM_INTEN_ZIEN3_Msk (0x1ul << PWM_INTEN_ZIEN3_Pos)

PWM_T::INTEN: ZIEN3 Mask

Definition at line 8344 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN3_Pos

#define PWM_INTEN_ZIEN3_Pos (3)

PWM_T::INTEN: ZIEN3 Position

Definition at line 8343 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN4_Msk

#define PWM_INTEN_ZIEN4_Msk (0x1ul << PWM_INTEN_ZIEN4_Pos)

PWM_T::INTEN: ZIEN4 Mask

Definition at line 8347 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN4_Pos

#define PWM_INTEN_ZIEN4_Pos (4)

PWM_T::INTEN: ZIEN4 Position

Definition at line 8346 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN5_Msk

#define PWM_INTEN_ZIEN5_Msk (0x1ul << PWM_INTEN_ZIEN5_Pos)

PWM_T::INTEN: ZIEN5 Mask

Definition at line 8350 of file Mini58Series.h.

## ◆ PWM_INTEN_ZIEN5_Pos

#define PWM_INTEN_ZIEN5_Pos (5)

PWM_T::INTEN: ZIEN5 Position

Definition at line 8349 of file Mini58Series.h.

## ◆ PWM_INTSTS_BRKIF0_Msk

#define PWM_INTSTS_BRKIF0_Msk (0x1ul << PWM_INTSTS_BRKIF0_Pos)

PWM_T::INTSTS: BRKIF0 Mask

Definition at line 8449 of file Mini58Series.h.

## ◆ PWM_INTSTS_BRKIF0_Pos

#define PWM_INTSTS_BRKIF0_Pos (16)

PWM_T::INTSTS: BRKIF0 Position

Definition at line 8448 of file Mini58Series.h.

## ◆ PWM_INTSTS_BRKIF1_Msk

#define PWM_INTSTS_BRKIF1_Msk (0x1ul << PWM_INTSTS_BRKIF1_Pos)

PWM_T::INTSTS: BRKIF1 Mask

Definition at line 8452 of file Mini58Series.h.

## ◆ PWM_INTSTS_BRKIF1_Pos

#define PWM_INTSTS_BRKIF1_Pos (17)

PWM_T::INTSTS: BRKIF1 Position

Definition at line 8451 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF0_Msk

#define PWM_INTSTS_CMPDIF0_Msk (0x1ul << PWM_INTSTS_CMPDIF0_Pos)

PWM_T::INTSTS: CMPDIF0 Mask

Definition at line 8431 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF0_Pos

#define PWM_INTSTS_CMPDIF0_Pos (8)

PWM_T::INTSTS: CMPDIF0 Position

Definition at line 8430 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF1_Msk

#define PWM_INTSTS_CMPDIF1_Msk (0x1ul << PWM_INTSTS_CMPDIF1_Pos)

PWM_T::INTSTS: CMPDIF1 Mask

Definition at line 8434 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF1_Pos

#define PWM_INTSTS_CMPDIF1_Pos (9)

PWM_T::INTSTS: CMPDIF1 Position

Definition at line 8433 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF2_Msk

#define PWM_INTSTS_CMPDIF2_Msk (0x1ul << PWM_INTSTS_CMPDIF2_Pos)

PWM_T::INTSTS: CMPDIF2 Mask

Definition at line 8437 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF2_Pos

#define PWM_INTSTS_CMPDIF2_Pos (10)

PWM_T::INTSTS: CMPDIF2 Position

Definition at line 8436 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF3_Msk

#define PWM_INTSTS_CMPDIF3_Msk (0x1ul << PWM_INTSTS_CMPDIF3_Pos)

PWM_T::INTSTS: CMPDIF3 Mask

Definition at line 8440 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF3_Pos

#define PWM_INTSTS_CMPDIF3_Pos (11)

PWM_T::INTSTS: CMPDIF3 Position

Definition at line 8439 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF4_Msk

#define PWM_INTSTS_CMPDIF4_Msk (0x1ul << PWM_INTSTS_CMPDIF4_Pos)

PWM_T::INTSTS: CMPDIF4 Mask

Definition at line 8443 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF4_Pos

#define PWM_INTSTS_CMPDIF4_Pos (12)

PWM_T::INTSTS: CMPDIF4 Position

Definition at line 8442 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF5_Msk

#define PWM_INTSTS_CMPDIF5_Msk (0x1ul << PWM_INTSTS_CMPDIF5_Pos)

PWM_T::INTSTS: CMPDIF5 Mask

Definition at line 8446 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPDIF5_Pos

#define PWM_INTSTS_CMPDIF5_Pos (13)

PWM_T::INTSTS: CMPDIF5 Position

Definition at line 8445 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF0_Msk

#define PWM_INTSTS_CMPUIF0_Msk (0x1ul << PWM_INTSTS_CMPUIF0_Pos)

PWM_T::INTSTS: CMPUIF0 Mask

Definition at line 8473 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF0_Pos

#define PWM_INTSTS_CMPUIF0_Pos (24)

PWM_T::INTSTS: CMPUIF0 Position

Definition at line 8472 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF1_Msk

#define PWM_INTSTS_CMPUIF1_Msk (0x1ul << PWM_INTSTS_CMPUIF1_Pos)

PWM_T::INTSTS: CMPUIF1 Mask

Definition at line 8476 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF1_Pos

#define PWM_INTSTS_CMPUIF1_Pos (25)

PWM_T::INTSTS: CMPUIF1 Position

Definition at line 8475 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF2_Msk

#define PWM_INTSTS_CMPUIF2_Msk (0x1ul << PWM_INTSTS_CMPUIF2_Pos)

PWM_T::INTSTS: CMPUIF2 Mask

Definition at line 8479 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF2_Pos

#define PWM_INTSTS_CMPUIF2_Pos (26)

PWM_T::INTSTS: CMPUIF2 Position

Definition at line 8478 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF3_Msk

#define PWM_INTSTS_CMPUIF3_Msk (0x1ul << PWM_INTSTS_CMPUIF3_Pos)

PWM_T::INTSTS: CMPUIF3 Mask

Definition at line 8482 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF3_Pos

#define PWM_INTSTS_CMPUIF3_Pos (27)

PWM_T::INTSTS: CMPUIF3 Position

Definition at line 8481 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF4_Msk

#define PWM_INTSTS_CMPUIF4_Msk (0x1ul << PWM_INTSTS_CMPUIF4_Pos)

PWM_T::INTSTS: CMPUIF4 Mask

Definition at line 8485 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF4_Pos

#define PWM_INTSTS_CMPUIF4_Pos (28)

PWM_T::INTSTS: CMPUIF4 Position

Definition at line 8484 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF5_Msk

#define PWM_INTSTS_CMPUIF5_Msk (0x1ul << PWM_INTSTS_CMPUIF5_Pos)

PWM_T::INTSTS: CMPUIF5 Mask

Definition at line 8488 of file Mini58Series.h.

## ◆ PWM_INTSTS_CMPUIF5_Pos

#define PWM_INTSTS_CMPUIF5_Pos (29)

PWM_T::INTSTS: CMPUIF5 Position

Definition at line 8487 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF0_Msk

#define PWM_INTSTS_PIF0_Msk (0x1ul << PWM_INTSTS_PIF0_Pos)

PWM_T::INTSTS: PIF0 Mask

Definition at line 8455 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF0_Pos

#define PWM_INTSTS_PIF0_Pos (18)

PWM_T::INTSTS: PIF0 Position

Definition at line 8454 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF1_Msk

#define PWM_INTSTS_PIF1_Msk (0x1ul << PWM_INTSTS_PIF1_Pos)

PWM_T::INTSTS: PIF1 Mask

Definition at line 8458 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF1_Pos

#define PWM_INTSTS_PIF1_Pos (19)

PWM_T::INTSTS: PIF1 Position

Definition at line 8457 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF2_Msk

#define PWM_INTSTS_PIF2_Msk (0x1ul << PWM_INTSTS_PIF2_Pos)

PWM_T::INTSTS: PIF2 Mask

Definition at line 8461 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF2_Pos

#define PWM_INTSTS_PIF2_Pos (20)

PWM_T::INTSTS: PIF2 Position

Definition at line 8460 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF3_Msk

#define PWM_INTSTS_PIF3_Msk (0x1ul << PWM_INTSTS_PIF3_Pos)

PWM_T::INTSTS: PIF3 Mask

Definition at line 8464 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF3_Pos

#define PWM_INTSTS_PIF3_Pos (21)

PWM_T::INTSTS: PIF3 Position

Definition at line 8463 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF4_Msk

#define PWM_INTSTS_PIF4_Msk (0x1ul << PWM_INTSTS_PIF4_Pos)

PWM_T::INTSTS: PIF4 Mask

Definition at line 8467 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF4_Pos

#define PWM_INTSTS_PIF4_Pos (22)

PWM_T::INTSTS: PIF4 Position

Definition at line 8466 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF5_Msk

#define PWM_INTSTS_PIF5_Msk (0x1ul << PWM_INTSTS_PIF5_Pos)

PWM_T::INTSTS: PIF5 Mask

Definition at line 8470 of file Mini58Series.h.

## ◆ PWM_INTSTS_PIF5_Pos

#define PWM_INTSTS_PIF5_Pos (23)

PWM_T::INTSTS: PIF5 Position

Definition at line 8469 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF0_Msk

#define PWM_INTSTS_ZIF0_Msk (0x1ul << PWM_INTSTS_ZIF0_Pos)

PWM_T::INTSTS: ZIF0 Mask

Definition at line 8413 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF0_Pos

#define PWM_INTSTS_ZIF0_Pos (0)

PWM_T::INTSTS: ZIF0 Position

Definition at line 8412 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF1_Msk

#define PWM_INTSTS_ZIF1_Msk (0x1ul << PWM_INTSTS_ZIF1_Pos)

PWM_T::INTSTS: ZIF1 Mask

Definition at line 8416 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF1_Pos

#define PWM_INTSTS_ZIF1_Pos (1)

PWM_T::INTSTS: ZIF1 Position

Definition at line 8415 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF2_Msk

#define PWM_INTSTS_ZIF2_Msk (0x1ul << PWM_INTSTS_ZIF2_Pos)

PWM_T::INTSTS: ZIF2 Mask

Definition at line 8419 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF2_Pos

#define PWM_INTSTS_ZIF2_Pos (2)

PWM_T::INTSTS: ZIF2 Position

Definition at line 8418 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF3_Msk

#define PWM_INTSTS_ZIF3_Msk (0x1ul << PWM_INTSTS_ZIF3_Pos)

PWM_T::INTSTS: ZIF3 Mask

Definition at line 8422 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF3_Pos

#define PWM_INTSTS_ZIF3_Pos (3)

PWM_T::INTSTS: ZIF3 Position

Definition at line 8421 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF4_Msk

#define PWM_INTSTS_ZIF4_Msk (0x1ul << PWM_INTSTS_ZIF4_Pos)

PWM_T::INTSTS: ZIF4 Mask

Definition at line 8425 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF4_Pos

#define PWM_INTSTS_ZIF4_Pos (4)

PWM_T::INTSTS: ZIF4 Position

Definition at line 8424 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF5_Msk

#define PWM_INTSTS_ZIF5_Msk (0x1ul << PWM_INTSTS_ZIF5_Pos)

PWM_T::INTSTS: ZIF5 Mask

Definition at line 8428 of file Mini58Series.h.

## ◆ PWM_INTSTS_ZIF5_Pos

#define PWM_INTSTS_ZIF5_Pos (5)

PWM_T::INTSTS: ZIF5 Position

Definition at line 8427 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN0_Msk

#define PWM_MSKALIGN_ALIGN0_Msk (0x1ul << PWM_MSKALIGN_ALIGN0_Pos)

PWM_T::MSKALIGN: ALIGN0 Mask

Definition at line 8944 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN0_Pos

#define PWM_MSKALIGN_ALIGN0_Pos (16)

PWM_T::MSKALIGN: ALIGN0 Position

Definition at line 8943 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN1_Msk

#define PWM_MSKALIGN_ALIGN1_Msk (0x1ul << PWM_MSKALIGN_ALIGN1_Pos)

PWM_T::MSKALIGN: ALIGN1 Mask

Definition at line 8947 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN1_Pos

#define PWM_MSKALIGN_ALIGN1_Pos (17)

PWM_T::MSKALIGN: ALIGN1 Position

Definition at line 8946 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN2_Msk

#define PWM_MSKALIGN_ALIGN2_Msk (0x1ul << PWM_MSKALIGN_ALIGN2_Pos)

PWM_T::MSKALIGN: ALIGN2 Mask

Definition at line 8950 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN2_Pos

#define PWM_MSKALIGN_ALIGN2_Pos (18)

PWM_T::MSKALIGN: ALIGN2 Position

Definition at line 8949 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN3_Msk

#define PWM_MSKALIGN_ALIGN3_Msk (0x1ul << PWM_MSKALIGN_ALIGN3_Pos)

PWM_T::MSKALIGN: ALIGN3 Mask

Definition at line 8953 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN3_Pos

#define PWM_MSKALIGN_ALIGN3_Pos (19)

PWM_T::MSKALIGN: ALIGN3 Position

Definition at line 8952 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN4_Msk

#define PWM_MSKALIGN_ALIGN4_Msk (0x1ul << PWM_MSKALIGN_ALIGN4_Pos)

PWM_T::MSKALIGN: ALIGN4 Mask

Definition at line 8956 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN4_Pos

#define PWM_MSKALIGN_ALIGN4_Pos (20)

PWM_T::MSKALIGN: ALIGN4 Position

Definition at line 8955 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN5_Msk

#define PWM_MSKALIGN_ALIGN5_Msk (0x1ul << PWM_MSKALIGN_ALIGN5_Pos)

PWM_T::MSKALIGN: ALIGN5 Mask

Definition at line 8959 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_ALIGN5_Pos

#define PWM_MSKALIGN_ALIGN5_Pos (21)

PWM_T::MSKALIGN: ALIGN5 Position

Definition at line 8958 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT0_Msk

#define PWM_MSKALIGN_MSKDAT0_Msk (0x1ul << PWM_MSKALIGN_MSKDAT0_Pos)

PWM_T::MSKALIGN: MSKDAT0 Mask

Definition at line 8908 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT0_Pos

#define PWM_MSKALIGN_MSKDAT0_Pos (0)

PWM_T::MSKALIGN: MSKDAT0 Position

Definition at line 8907 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT1_Msk

#define PWM_MSKALIGN_MSKDAT1_Msk (0x1ul << PWM_MSKALIGN_MSKDAT1_Pos)

PWM_T::MSKALIGN: MSKDAT1 Mask

Definition at line 8911 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT1_Pos

#define PWM_MSKALIGN_MSKDAT1_Pos (1)

PWM_T::MSKALIGN: MSKDAT1 Position

Definition at line 8910 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT2_Msk

#define PWM_MSKALIGN_MSKDAT2_Msk (0x1ul << PWM_MSKALIGN_MSKDAT2_Pos)

PWM_T::MSKALIGN: MSKDAT2 Mask

Definition at line 8914 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT2_Pos

#define PWM_MSKALIGN_MSKDAT2_Pos (2)

PWM_T::MSKALIGN: MSKDAT2 Position

Definition at line 8913 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT3_Msk

#define PWM_MSKALIGN_MSKDAT3_Msk (0x1ul << PWM_MSKALIGN_MSKDAT3_Pos)

PWM_T::MSKALIGN: MSKDAT3 Mask

Definition at line 8917 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT3_Pos

#define PWM_MSKALIGN_MSKDAT3_Pos (3)

PWM_T::MSKALIGN: MSKDAT3 Position

Definition at line 8916 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT4_Msk

#define PWM_MSKALIGN_MSKDAT4_Msk (0x1ul << PWM_MSKALIGN_MSKDAT4_Pos)

PWM_T::MSKALIGN: MSKDAT4 Mask

Definition at line 8920 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT4_Pos

#define PWM_MSKALIGN_MSKDAT4_Pos (4)

PWM_T::MSKALIGN: MSKDAT4 Position

Definition at line 8919 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT5_Msk

#define PWM_MSKALIGN_MSKDAT5_Msk (0x1ul << PWM_MSKALIGN_MSKDAT5_Pos)

PWM_T::MSKALIGN: MSKDAT5 Mask

Definition at line 8923 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKDAT5_Pos

#define PWM_MSKALIGN_MSKDAT5_Pos (5)

PWM_T::MSKALIGN: MSKDAT5 Position

Definition at line 8922 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN0_Msk

#define PWM_MSKALIGN_MSKEN0_Msk (0x1ul << PWM_MSKALIGN_MSKEN0_Pos)

PWM_T::MSKALIGN: MSKEN0 Mask

Definition at line 8926 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN0_Pos

#define PWM_MSKALIGN_MSKEN0_Pos (8)

PWM_T::MSKALIGN: MSKEN0 Position

Definition at line 8925 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN1_Msk

#define PWM_MSKALIGN_MSKEN1_Msk (0x1ul << PWM_MSKALIGN_MSKEN1_Pos)

PWM_T::MSKALIGN: MSKEN1 Mask

Definition at line 8929 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN1_Pos

#define PWM_MSKALIGN_MSKEN1_Pos (9)

PWM_T::MSKALIGN: MSKEN1 Position

Definition at line 8928 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN2_Msk

#define PWM_MSKALIGN_MSKEN2_Msk (0x1ul << PWM_MSKALIGN_MSKEN2_Pos)

PWM_T::MSKALIGN: MSKEN2 Mask

Definition at line 8932 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN2_Pos

#define PWM_MSKALIGN_MSKEN2_Pos (10)

PWM_T::MSKALIGN: MSKEN2 Position

Definition at line 8931 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN3_Msk

#define PWM_MSKALIGN_MSKEN3_Msk (0x1ul << PWM_MSKALIGN_MSKEN3_Pos)

PWM_T::MSKALIGN: MSKEN3 Mask

Definition at line 8935 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN3_Pos

#define PWM_MSKALIGN_MSKEN3_Pos (11)

PWM_T::MSKALIGN: MSKEN3 Position

Definition at line 8934 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN4_Msk

#define PWM_MSKALIGN_MSKEN4_Msk (0x1ul << PWM_MSKALIGN_MSKEN4_Pos)

PWM_T::MSKALIGN: MSKEN4 Mask

Definition at line 8938 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN4_Pos

#define PWM_MSKALIGN_MSKEN4_Pos (12)

PWM_T::MSKALIGN: MSKEN4 Position

Definition at line 8937 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN5_Msk

#define PWM_MSKALIGN_MSKEN5_Msk (0x1ul << PWM_MSKALIGN_MSKEN5_Pos)

PWM_T::MSKALIGN: MSKEN5 Mask

Definition at line 8941 of file Mini58Series.h.

## ◆ PWM_MSKALIGN_MSKEN5_Pos

#define PWM_MSKALIGN_MSKEN5_Pos (13)

PWM_T::MSKALIGN: MSKEN5 Position

Definition at line 8940 of file Mini58Series.h.

## ◆ PWM_PCACTL_PCAEN_Msk

#define PWM_PCACTL_PCAEN_Msk (0x1ul << PWM_PCACTL_PCAEN_Pos)

PWM_T::PCACTL: PCAEN Mask

Definition at line 8905 of file Mini58Series.h.

## ◆ PWM_PCACTL_PCAEN_Pos

#define PWM_PCACTL_PCAEN_Pos (0)

PWM_T::PCACTL: PCAEN Position

Definition at line 8904 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD0_Msk

#define PWM_PERIOD0_PERIOD0_Msk (0xfffful << PWM_PERIOD0_PERIOD0_Pos)

PWM_T::PERIOD0: PERIOD0 Mask

Definition at line 8011 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD0_Pos

#define PWM_PERIOD0_PERIOD0_Pos (0)

PWM_T::PERIOD0: PERIOD0 Position

Definition at line 8010 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD1_Msk

#define PWM_PERIOD0_PERIOD1_Msk (0xfffful << PWM_PERIOD0_PERIOD1_Pos)

PWM_T::PERIOD0: PERIOD1 Mask

Definition at line 8014 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD1_Pos

#define PWM_PERIOD0_PERIOD1_Pos (0)

PWM_T::PERIOD0: PERIOD1 Position

Definition at line 8013 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD2_Msk

#define PWM_PERIOD0_PERIOD2_Msk (0xfffful << PWM_PERIOD0_PERIOD2_Pos)

PWM_T::PERIOD0: PERIOD2 Mask

Definition at line 8017 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD2_Pos

#define PWM_PERIOD0_PERIOD2_Pos (0)

PWM_T::PERIOD0: PERIOD2 Position

Definition at line 8016 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD3_Msk

#define PWM_PERIOD0_PERIOD3_Msk (0xfffful << PWM_PERIOD0_PERIOD3_Pos)

PWM_T::PERIOD0: PERIOD3 Mask

Definition at line 8020 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD3_Pos

#define PWM_PERIOD0_PERIOD3_Pos (0)

PWM_T::PERIOD0: PERIOD3 Position

Definition at line 8019 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD4_Msk

#define PWM_PERIOD0_PERIOD4_Msk (0xfffful << PWM_PERIOD0_PERIOD4_Pos)

PWM_T::PERIOD0: PERIOD4 Mask

Definition at line 8023 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD4_Pos

#define PWM_PERIOD0_PERIOD4_Pos (0)

PWM_T::PERIOD0: PERIOD4 Position

Definition at line 8022 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD5_Msk

#define PWM_PERIOD0_PERIOD5_Msk (0xfffful << PWM_PERIOD0_PERIOD5_Pos)

PWM_T::PERIOD0: PERIOD5 Mask

Definition at line 8026 of file Mini58Series.h.

## ◆ PWM_PERIOD0_PERIOD5_Pos

#define PWM_PERIOD0_PERIOD5_Pos (0)

PWM_T::PERIOD0: PERIOD5 Position

Definition at line 8025 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD0_Msk

#define PWM_PERIOD1_PERIOD0_Msk (0xfffful << PWM_PERIOD1_PERIOD0_Pos)

PWM_T::PERIOD1: PERIOD0 Mask

Definition at line 8029 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD0_Pos

#define PWM_PERIOD1_PERIOD0_Pos (0)

PWM_T::PERIOD1: PERIOD0 Position

Definition at line 8028 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD1_Msk

#define PWM_PERIOD1_PERIOD1_Msk (0xfffful << PWM_PERIOD1_PERIOD1_Pos)

PWM_T::PERIOD1: PERIOD1 Mask

Definition at line 8032 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD1_Pos

#define PWM_PERIOD1_PERIOD1_Pos (0)

PWM_T::PERIOD1: PERIOD1 Position

Definition at line 8031 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD2_Msk

#define PWM_PERIOD1_PERIOD2_Msk (0xfffful << PWM_PERIOD1_PERIOD2_Pos)

PWM_T::PERIOD1: PERIOD2 Mask

Definition at line 8035 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD2_Pos

#define PWM_PERIOD1_PERIOD2_Pos (0)

PWM_T::PERIOD1: PERIOD2 Position

Definition at line 8034 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD3_Msk

#define PWM_PERIOD1_PERIOD3_Msk (0xfffful << PWM_PERIOD1_PERIOD3_Pos)

PWM_T::PERIOD1: PERIOD3 Mask

Definition at line 8038 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD3_Pos

#define PWM_PERIOD1_PERIOD3_Pos (0)

PWM_T::PERIOD1: PERIOD3 Position

Definition at line 8037 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD4_Msk

#define PWM_PERIOD1_PERIOD4_Msk (0xfffful << PWM_PERIOD1_PERIOD4_Pos)

PWM_T::PERIOD1: PERIOD4 Mask

Definition at line 8041 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD4_Pos

#define PWM_PERIOD1_PERIOD4_Pos (0)

PWM_T::PERIOD1: PERIOD4 Position

Definition at line 8040 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD5_Msk

#define PWM_PERIOD1_PERIOD5_Msk (0xfffful << PWM_PERIOD1_PERIOD5_Pos)

PWM_T::PERIOD1: PERIOD5 Mask

Definition at line 8044 of file Mini58Series.h.

## ◆ PWM_PERIOD1_PERIOD5_Pos

#define PWM_PERIOD1_PERIOD5_Pos (0)

PWM_T::PERIOD1: PERIOD5 Position

Definition at line 8043 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD0_Msk

#define PWM_PERIOD2_PERIOD0_Msk (0xfffful << PWM_PERIOD2_PERIOD0_Pos)

PWM_T::PERIOD2: PERIOD0 Mask

Definition at line 8047 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD0_Pos

#define PWM_PERIOD2_PERIOD0_Pos (0)

PWM_T::PERIOD2: PERIOD0 Position

Definition at line 8046 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD1_Msk

#define PWM_PERIOD2_PERIOD1_Msk (0xfffful << PWM_PERIOD2_PERIOD1_Pos)

PWM_T::PERIOD2: PERIOD1 Mask

Definition at line 8050 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD1_Pos

#define PWM_PERIOD2_PERIOD1_Pos (0)

PWM_T::PERIOD2: PERIOD1 Position

Definition at line 8049 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD2_Msk

#define PWM_PERIOD2_PERIOD2_Msk (0xfffful << PWM_PERIOD2_PERIOD2_Pos)

PWM_T::PERIOD2: PERIOD2 Mask

Definition at line 8053 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD2_Pos

#define PWM_PERIOD2_PERIOD2_Pos (0)

PWM_T::PERIOD2: PERIOD2 Position

Definition at line 8052 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD3_Msk

#define PWM_PERIOD2_PERIOD3_Msk (0xfffful << PWM_PERIOD2_PERIOD3_Pos)

PWM_T::PERIOD2: PERIOD3 Mask

Definition at line 8056 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD3_Pos

#define PWM_PERIOD2_PERIOD3_Pos (0)

PWM_T::PERIOD2: PERIOD3 Position

Definition at line 8055 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD4_Msk

#define PWM_PERIOD2_PERIOD4_Msk (0xfffful << PWM_PERIOD2_PERIOD4_Pos)

PWM_T::PERIOD2: PERIOD4 Mask

Definition at line 8059 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD4_Pos

#define PWM_PERIOD2_PERIOD4_Pos (0)

PWM_T::PERIOD2: PERIOD4 Position

Definition at line 8058 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD5_Msk

#define PWM_PERIOD2_PERIOD5_Msk (0xfffful << PWM_PERIOD2_PERIOD5_Pos)

PWM_T::PERIOD2: PERIOD5 Mask

Definition at line 8062 of file Mini58Series.h.

## ◆ PWM_PERIOD2_PERIOD5_Pos

#define PWM_PERIOD2_PERIOD5_Pos (0)

PWM_T::PERIOD2: PERIOD5 Position

Definition at line 8061 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD0_Msk

#define PWM_PERIOD3_PERIOD0_Msk (0xfffful << PWM_PERIOD3_PERIOD0_Pos)

PWM_T::PERIOD3: PERIOD0 Mask

Definition at line 8065 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD0_Pos

#define PWM_PERIOD3_PERIOD0_Pos (0)

PWM_T::PERIOD3: PERIOD0 Position

Definition at line 8064 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD1_Msk

#define PWM_PERIOD3_PERIOD1_Msk (0xfffful << PWM_PERIOD3_PERIOD1_Pos)

PWM_T::PERIOD3: PERIOD1 Mask

Definition at line 8068 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD1_Pos

#define PWM_PERIOD3_PERIOD1_Pos (0)

PWM_T::PERIOD3: PERIOD1 Position

Definition at line 8067 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD2_Msk

#define PWM_PERIOD3_PERIOD2_Msk (0xfffful << PWM_PERIOD3_PERIOD2_Pos)

PWM_T::PERIOD3: PERIOD2 Mask

Definition at line 8071 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD2_Pos

#define PWM_PERIOD3_PERIOD2_Pos (0)

PWM_T::PERIOD3: PERIOD2 Position

Definition at line 8070 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD3_Msk

#define PWM_PERIOD3_PERIOD3_Msk (0xfffful << PWM_PERIOD3_PERIOD3_Pos)

PWM_T::PERIOD3: PERIOD3 Mask

Definition at line 8074 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD3_Pos

#define PWM_PERIOD3_PERIOD3_Pos (0)

PWM_T::PERIOD3: PERIOD3 Position

Definition at line 8073 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD4_Msk

#define PWM_PERIOD3_PERIOD4_Msk (0xfffful << PWM_PERIOD3_PERIOD4_Pos)

PWM_T::PERIOD3: PERIOD4 Mask

Definition at line 8077 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD4_Pos

#define PWM_PERIOD3_PERIOD4_Pos (0)

PWM_T::PERIOD3: PERIOD4 Position

Definition at line 8076 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD5_Msk

#define PWM_PERIOD3_PERIOD5_Msk (0xfffful << PWM_PERIOD3_PERIOD5_Pos)

PWM_T::PERIOD3: PERIOD5 Mask

Definition at line 8080 of file Mini58Series.h.

## ◆ PWM_PERIOD3_PERIOD5_Pos

#define PWM_PERIOD3_PERIOD5_Pos (0)

PWM_T::PERIOD3: PERIOD5 Position

Definition at line 8079 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD0_Msk

#define PWM_PERIOD4_PERIOD0_Msk (0xfffful << PWM_PERIOD4_PERIOD0_Pos)

PWM_T::PERIOD4: PERIOD0 Mask

Definition at line 8083 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD0_Pos

#define PWM_PERIOD4_PERIOD0_Pos (0)

PWM_T::PERIOD4: PERIOD0 Position

Definition at line 8082 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD1_Msk

#define PWM_PERIOD4_PERIOD1_Msk (0xfffful << PWM_PERIOD4_PERIOD1_Pos)

PWM_T::PERIOD4: PERIOD1 Mask

Definition at line 8086 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD1_Pos

#define PWM_PERIOD4_PERIOD1_Pos (0)

PWM_T::PERIOD4: PERIOD1 Position

Definition at line 8085 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD2_Msk

#define PWM_PERIOD4_PERIOD2_Msk (0xfffful << PWM_PERIOD4_PERIOD2_Pos)

PWM_T::PERIOD4: PERIOD2 Mask

Definition at line 8089 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD2_Pos

#define PWM_PERIOD4_PERIOD2_Pos (0)

PWM_T::PERIOD4: PERIOD2 Position

Definition at line 8088 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD3_Msk

#define PWM_PERIOD4_PERIOD3_Msk (0xfffful << PWM_PERIOD4_PERIOD3_Pos)

PWM_T::PERIOD4: PERIOD3 Mask

Definition at line 8092 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD3_Pos

#define PWM_PERIOD4_PERIOD3_Pos (0)

PWM_T::PERIOD4: PERIOD3 Position

Definition at line 8091 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD4_Msk

#define PWM_PERIOD4_PERIOD4_Msk (0xfffful << PWM_PERIOD4_PERIOD4_Pos)

PWM_T::PERIOD4: PERIOD4 Mask

Definition at line 8095 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD4_Pos

#define PWM_PERIOD4_PERIOD4_Pos (0)

PWM_T::PERIOD4: PERIOD4 Position

Definition at line 8094 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD5_Msk

#define PWM_PERIOD4_PERIOD5_Msk (0xfffful << PWM_PERIOD4_PERIOD5_Pos)

PWM_T::PERIOD4: PERIOD5 Mask

Definition at line 8098 of file Mini58Series.h.

## ◆ PWM_PERIOD4_PERIOD5_Pos

#define PWM_PERIOD4_PERIOD5_Pos (0)

PWM_T::PERIOD4: PERIOD5 Position

Definition at line 8097 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD0_Msk

#define PWM_PERIOD5_PERIOD0_Msk (0xfffful << PWM_PERIOD5_PERIOD0_Pos)

PWM_T::PERIOD5: PERIOD0 Mask

Definition at line 8101 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD0_Pos

#define PWM_PERIOD5_PERIOD0_Pos (0)

PWM_T::PERIOD5: PERIOD0 Position

Definition at line 8100 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD1_Msk

#define PWM_PERIOD5_PERIOD1_Msk (0xfffful << PWM_PERIOD5_PERIOD1_Pos)

PWM_T::PERIOD5: PERIOD1 Mask

Definition at line 8104 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD1_Pos

#define PWM_PERIOD5_PERIOD1_Pos (0)

PWM_T::PERIOD5: PERIOD1 Position

Definition at line 8103 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD2_Msk

#define PWM_PERIOD5_PERIOD2_Msk (0xfffful << PWM_PERIOD5_PERIOD2_Pos)

PWM_T::PERIOD5: PERIOD2 Mask

Definition at line 8107 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD2_Pos

#define PWM_PERIOD5_PERIOD2_Pos (0)

PWM_T::PERIOD5: PERIOD2 Position

Definition at line 8106 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD3_Msk

#define PWM_PERIOD5_PERIOD3_Msk (0xfffful << PWM_PERIOD5_PERIOD3_Pos)

PWM_T::PERIOD5: PERIOD3 Mask

Definition at line 8110 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD3_Pos

#define PWM_PERIOD5_PERIOD3_Pos (0)

PWM_T::PERIOD5: PERIOD3 Position

Definition at line 8109 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD4_Msk

#define PWM_PERIOD5_PERIOD4_Msk (0xfffful << PWM_PERIOD5_PERIOD4_Pos)

PWM_T::PERIOD5: PERIOD4 Mask

Definition at line 8113 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD4_Pos

#define PWM_PERIOD5_PERIOD4_Pos (0)

PWM_T::PERIOD5: PERIOD4 Position

Definition at line 8112 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD5_Msk

#define PWM_PERIOD5_PERIOD5_Msk (0xfffful << PWM_PERIOD5_PERIOD5_Pos)

PWM_T::PERIOD5: PERIOD5 Mask

Definition at line 8116 of file Mini58Series.h.

## ◆ PWM_PERIOD5_PERIOD5_Pos

#define PWM_PERIOD5_PERIOD5_Pos (0)

PWM_T::PERIOD5: PERIOD5 Position

Definition at line 8115 of file Mini58Series.h.

## ◆ PWM_PHCHG_A0POSSEL_Msk

#define PWM_PHCHG_A0POSSEL_Msk (0x3ul << PWM_PHCHG_A0POSSEL_Pos)

PWM_T::PHCHG: A0POSSEL Mask

Definition at line 8788 of file Mini58Series.h.

## ◆ PWM_PHCHG_A0POSSEL_Pos

#define PWM_PHCHG_A0POSSEL_Pos (28)

PWM_T::PHCHG: A0POSSEL Position

Definition at line 8787 of file Mini58Series.h.

## ◆ PWM_PHCHG_A1POSSEL_Msk

#define PWM_PHCHG_A1POSSEL_Msk (0x3ul << PWM_PHCHG_A1POSSEL_Pos)

PWM_T::PHCHG: A1POSSEL Mask

Definition at line 8767 of file Mini58Series.h.

## ◆ PWM_PHCHG_A1POSSEL_Pos

#define PWM_PHCHG_A1POSSEL_Pos (20)

PWM_T::PHCHG: A1POSSEL Position

Definition at line 8766 of file Mini58Series.h.

## ◆ PWM_PHCHG_ACMP0TEN_Msk

#define PWM_PHCHG_ACMP0TEN_Msk (0x1ul << PWM_PHCHG_ACMP0TEN_Pos)

PWM_T::PHCHG: ACMP0TEN Mask

Definition at line 8794 of file Mini58Series.h.

## ◆ PWM_PHCHG_ACMP0TEN_Pos

#define PWM_PHCHG_ACMP0TEN_Pos (31)

PWM_T::PHCHG: ACMP0TEN Position

Definition at line 8793 of file Mini58Series.h.

## ◆ PWM_PHCHG_ACMP1TEN_Msk

#define PWM_PHCHG_ACMP1TEN_Msk (0x1ul << PWM_PHCHG_ACMP1TEN_Pos)

PWM_T::PHCHG: ACMP1TEN Mask

Definition at line 8773 of file Mini58Series.h.

## ◆ PWM_PHCHG_ACMP1TEN_Pos

#define PWM_PHCHG_ACMP1TEN_Pos (23)

PWM_T::PHCHG: ACMP1TEN Position

Definition at line 8772 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN00_Msk

#define PWM_PHCHG_AOFFEN00_Msk (0x1ul << PWM_PHCHG_AOFFEN00_Pos)

PWM_T::PHCHG: AOFFEN00 Mask

Definition at line 8776 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN00_Pos

#define PWM_PHCHG_AOFFEN00_Pos (24)

PWM_T::PHCHG: AOFFEN00 Position

Definition at line 8775 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN01_Msk

#define PWM_PHCHG_AOFFEN01_Msk (0x1ul << PWM_PHCHG_AOFFEN01_Pos)

PWM_T::PHCHG: AOFFEN01 Mask

Definition at line 8755 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN01_Pos

#define PWM_PHCHG_AOFFEN01_Pos (16)

PWM_T::PHCHG: AOFFEN01 Position

Definition at line 8754 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN10_Msk

#define PWM_PHCHG_AOFFEN10_Msk (0x1ul << PWM_PHCHG_AOFFEN10_Pos)

PWM_T::PHCHG: AOFFEN10 Mask

Definition at line 8779 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN10_Pos

#define PWM_PHCHG_AOFFEN10_Pos (25)

PWM_T::PHCHG: AOFFEN10 Position

Definition at line 8778 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN11_Msk

#define PWM_PHCHG_AOFFEN11_Msk (0x1ul << PWM_PHCHG_AOFFEN11_Pos)

PWM_T::PHCHG: AOFFEN11 Mask

Definition at line 8758 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN11_Pos

#define PWM_PHCHG_AOFFEN11_Pos (17)

PWM_T::PHCHG: AOFFEN11 Position

Definition at line 8757 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN20_Msk

#define PWM_PHCHG_AOFFEN20_Msk (0x1ul << PWM_PHCHG_AOFFEN20_Pos)

PWM_T::PHCHG: AOFFEN20 Mask

Definition at line 8782 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN20_Pos

#define PWM_PHCHG_AOFFEN20_Pos (26)

PWM_T::PHCHG: AOFFEN20 Position

Definition at line 8781 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN21_Msk

#define PWM_PHCHG_AOFFEN21_Msk (0x1ul << PWM_PHCHG_AOFFEN21_Pos)

PWM_T::PHCHG: AOFFEN21 Mask

Definition at line 8761 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN21_Pos

#define PWM_PHCHG_AOFFEN21_Pos (18)

PWM_T::PHCHG: AOFFEN21 Position

Definition at line 8760 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN30_Msk

#define PWM_PHCHG_AOFFEN30_Msk (0x1ul << PWM_PHCHG_AOFFEN30_Pos)

PWM_T::PHCHG: AOFFEN30 Mask

Definition at line 8785 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN30_Pos

#define PWM_PHCHG_AOFFEN30_Pos (27)

PWM_T::PHCHG: AOFFEN30 Position

Definition at line 8784 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN31_Msk

#define PWM_PHCHG_AOFFEN31_Msk (0x1ul << PWM_PHCHG_AOFFEN31_Pos)

PWM_T::PHCHG: AOFFEN31 Mask

Definition at line 8764 of file Mini58Series.h.

## ◆ PWM_PHCHG_AOFFEN31_Pos

#define PWM_PHCHG_AOFFEN31_Pos (19)

PWM_T::PHCHG: AOFFEN31 Position

Definition at line 8763 of file Mini58Series.h.

## ◆ PWM_PHCHG_AUTOCLR0_Msk

#define PWM_PHCHG_AUTOCLR0_Msk (0x1ul << PWM_PHCHG_AUTOCLR0_Pos)

PWM_T::PHCHG: AUTOCLR0 Mask

Definition at line 8749 of file Mini58Series.h.

## ◆ PWM_PHCHG_AUTOCLR0_Pos

#define PWM_PHCHG_AUTOCLR0_Pos (14)

PWM_T::PHCHG: AUTOCLR0 Position

Definition at line 8748 of file Mini58Series.h.

## ◆ PWM_PHCHG_AUTOCLR1_Msk

#define PWM_PHCHG_AUTOCLR1_Msk (0x1ul << PWM_PHCHG_AUTOCLR1_Pos)

PWM_T::PHCHG: AUTOCLR1 Mask

Definition at line 8752 of file Mini58Series.h.

## ◆ PWM_PHCHG_AUTOCLR1_Pos

#define PWM_PHCHG_AUTOCLR1_Pos (15)

PWM_T::PHCHG: AUTOCLR1 Position

Definition at line 8751 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT0_Msk

#define PWM_PHCHG_MSKDAT0_Msk (0x1ul << PWM_PHCHG_MSKDAT0_Pos)

PWM_T::PHCHG: MSKDAT0 Mask

Definition at line 8707 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT0_Pos

#define PWM_PHCHG_MSKDAT0_Pos (0)

PWM_T::PHCHG: MSKDAT0 Position

Definition at line 8706 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT1_Msk

#define PWM_PHCHG_MSKDAT1_Msk (0x1ul << PWM_PHCHG_MSKDAT1_Pos)

PWM_T::PHCHG: MSKDAT1 Mask

Definition at line 8710 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT1_Pos

#define PWM_PHCHG_MSKDAT1_Pos (1)

PWM_T::PHCHG: MSKDAT1 Position

Definition at line 8709 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT2_Msk

#define PWM_PHCHG_MSKDAT2_Msk (0x1ul << PWM_PHCHG_MSKDAT2_Pos)

PWM_T::PHCHG: MSKDAT2 Mask

Definition at line 8713 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT2_Pos

#define PWM_PHCHG_MSKDAT2_Pos (2)

PWM_T::PHCHG: MSKDAT2 Position

Definition at line 8712 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT3_Msk

#define PWM_PHCHG_MSKDAT3_Msk (0x1ul << PWM_PHCHG_MSKDAT3_Pos)

PWM_T::PHCHG: MSKDAT3 Mask

Definition at line 8716 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT3_Pos

#define PWM_PHCHG_MSKDAT3_Pos (3)

PWM_T::PHCHG: MSKDAT3 Position

Definition at line 8715 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT4_Msk

#define PWM_PHCHG_MSKDAT4_Msk (0x1ul << PWM_PHCHG_MSKDAT4_Pos)

PWM_T::PHCHG: MSKDAT4 Mask

Definition at line 8719 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT4_Pos

#define PWM_PHCHG_MSKDAT4_Pos (4)

PWM_T::PHCHG: MSKDAT4 Position

Definition at line 8718 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT5_Msk

#define PWM_PHCHG_MSKDAT5_Msk (0x1ul << PWM_PHCHG_MSKDAT5_Pos)

PWM_T::PHCHG: MSKDAT5 Mask

Definition at line 8722 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT5_Pos

#define PWM_PHCHG_MSKDAT5_Pos (5)

PWM_T::PHCHG: MSKDAT5 Position

Definition at line 8721 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT6_Msk

#define PWM_PHCHG_MSKDAT6_Msk (0x1ul << PWM_PHCHG_MSKDAT6_Pos)

PWM_T::PHCHG: MSKDAT6 Mask

Definition at line 8725 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT6_Pos

#define PWM_PHCHG_MSKDAT6_Pos (6)

PWM_T::PHCHG: MSKDAT6 Position

Definition at line 8724 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT7_Msk

#define PWM_PHCHG_MSKDAT7_Msk (0x1ul << PWM_PHCHG_MSKDAT7_Pos)

PWM_T::PHCHG: MSKDAT7 Mask

Definition at line 8728 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKDAT7_Pos

#define PWM_PHCHG_MSKDAT7_Pos (7)

PWM_T::PHCHG: MSKDAT7 Position

Definition at line 8727 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN0_Msk

#define PWM_PHCHG_MSKEN0_Msk (0x1ul << PWM_PHCHG_MSKEN0_Pos)

PWM_T::PHCHG: MSKEN0 Mask

Definition at line 8731 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN0_Pos

#define PWM_PHCHG_MSKEN0_Pos (8)

PWM_T::PHCHG: MSKEN0 Position

Definition at line 8730 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN1_Msk

#define PWM_PHCHG_MSKEN1_Msk (0x1ul << PWM_PHCHG_MSKEN1_Pos)

PWM_T::PHCHG: MSKEN1 Mask

Definition at line 8734 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN1_Pos

#define PWM_PHCHG_MSKEN1_Pos (9)

PWM_T::PHCHG: MSKEN1 Position

Definition at line 8733 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN2_Msk

#define PWM_PHCHG_MSKEN2_Msk (0x1ul << PWM_PHCHG_MSKEN2_Pos)

PWM_T::PHCHG: MSKEN2 Mask

Definition at line 8737 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN2_Pos

#define PWM_PHCHG_MSKEN2_Pos (10)

PWM_T::PHCHG: MSKEN2 Position

Definition at line 8736 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN3_Msk

#define PWM_PHCHG_MSKEN3_Msk (0x1ul << PWM_PHCHG_MSKEN3_Pos)

PWM_T::PHCHG: MSKEN3 Mask

Definition at line 8740 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN3_Pos

#define PWM_PHCHG_MSKEN3_Pos (11)

PWM_T::PHCHG: MSKEN3 Position

Definition at line 8739 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN4_Msk

#define PWM_PHCHG_MSKEN4_Msk (0x1ul << PWM_PHCHG_MSKEN4_Pos)

PWM_T::PHCHG: MSKEN4 Mask

Definition at line 8743 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN4_Pos

#define PWM_PHCHG_MSKEN4_Pos (12)

PWM_T::PHCHG: MSKEN4 Position

Definition at line 8742 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN5_Msk

#define PWM_PHCHG_MSKEN5_Msk (0x1ul << PWM_PHCHG_MSKEN5_Pos)

PWM_T::PHCHG: MSKEN5 Mask

Definition at line 8746 of file Mini58Series.h.

## ◆ PWM_PHCHG_MSKEN5_Pos

#define PWM_PHCHG_MSKEN5_Pos (13)

PWM_T::PHCHG: MSKEN5 Position

Definition at line 8745 of file Mini58Series.h.

## ◆ PWM_PHCHG_TMR0TEN_Msk

#define PWM_PHCHG_TMR0TEN_Msk (0x1ul << PWM_PHCHG_TMR0TEN_Pos)

PWM_T::PHCHG: TMR0TEN Mask

Definition at line 8791 of file Mini58Series.h.

## ◆ PWM_PHCHG_TMR0TEN_Pos

#define PWM_PHCHG_TMR0TEN_Pos (30)

PWM_T::PHCHG: TMR0TEN Position

Definition at line 8790 of file Mini58Series.h.

## ◆ PWM_PHCHG_TMR1TEN_Msk

#define PWM_PHCHG_TMR1TEN_Msk (0x1ul << PWM_PHCHG_TMR1TEN_Pos)

PWM_T::PHCHG: TMR1TEN Mask

Definition at line 8770 of file Mini58Series.h.

## ◆ PWM_PHCHG_TMR1TEN_Pos

#define PWM_PHCHG_TMR1TEN_Pos (22)

PWM_T::PHCHG: TMR1TEN Position

Definition at line 8769 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_MASKEND6_Msk

#define PWM_PHCHGMSK_MASKEND6_Msk (0x1ul << PWM_PHCHGMSK_MASKEND6_Pos)

PWM_T::PHCHGMSK: MASKEND6 Mask

Definition at line 8887 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_MASKEND6_Pos

#define PWM_PHCHGMSK_MASKEND6_Pos (6)

PWM_T::PHCHGMSK: MASKEND6 Position

Definition at line 8886 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_MASKEND7_Msk

#define PWM_PHCHGMSK_MASKEND7_Msk (0x1ul << PWM_PHCHGMSK_MASKEND7_Pos)

PWM_T::PHCHGMSK: MASKEND7 Mask

Definition at line 8890 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_MASKEND7_Pos

#define PWM_PHCHGMSK_MASKEND7_Pos (7)

PWM_T::PHCHGMSK: MASKEND7 Position

Definition at line 8889 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_POSCTL0_Msk

#define PWM_PHCHGMSK_POSCTL0_Msk (0x1ul << PWM_PHCHGMSK_POSCTL0_Pos)

PWM_T::PHCHGMSK: POSCTL0 Mask

Definition at line 8893 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_POSCTL0_Pos

#define PWM_PHCHGMSK_POSCTL0_Pos (8)

PWM_T::PHCHGMSK: POSCTL0 Position

Definition at line 8892 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_POSCTL1_Msk

#define PWM_PHCHGMSK_POSCTL1_Msk (0x1ul << PWM_PHCHGMSK_POSCTL1_Pos)

PWM_T::PHCHGMSK: POSCTL1 Mask

Definition at line 8896 of file Mini58Series.h.

## ◆ PWM_PHCHGMSK_POSCTL1_Pos

#define PWM_PHCHGMSK_POSCTL1_Pos (9)

PWM_T::PHCHGMSK: POSCTL1 Position

Definition at line 8895 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_A0POSSEL_Msk

#define PWM_PHCHGNXT_A0POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A0POSSEL_Pos)

PWM_T::PHCHGNXT: A0POSSEL Mask

Definition at line 8878 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_A0POSSEL_Pos

#define PWM_PHCHGNXT_A0POSSEL_Pos (28)

PWM_T::PHCHGNXT: A0POSSEL Position

Definition at line 8877 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_A1POSSEL_Msk

#define PWM_PHCHGNXT_A1POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A1POSSEL_Pos)

PWM_T::PHCHGNXT: A1POSSEL Mask

Definition at line 8857 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_A1POSSEL_Pos

#define PWM_PHCHGNXT_A1POSSEL_Pos (20)

PWM_T::PHCHGNXT: A1POSSEL Position

Definition at line 8856 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_ACMP0TEN_Msk

#define PWM_PHCHGNXT_ACMP0TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP0TEN_Pos)

PWM_T::PHCHGNXT: ACMP0TEN Mask

Definition at line 8884 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_ACMP0TEN_Pos

#define PWM_PHCHGNXT_ACMP0TEN_Pos (31)

PWM_T::PHCHGNXT: ACMP0TEN Position

Definition at line 8883 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_ACMP1TEN_Msk

#define PWM_PHCHGNXT_ACMP1TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP1TEN_Pos)

PWM_T::PHCHGNXT: ACMP1TEN Mask

Definition at line 8863 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_ACMP1TEN_Pos

#define PWM_PHCHGNXT_ACMP1TEN_Pos (23)

PWM_T::PHCHGNXT: ACMP1TEN Position

Definition at line 8862 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN00_Msk

#define PWM_PHCHGNXT_AOFFEN00_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN00_Pos)

PWM_T::PHCHGNXT: AOFFEN00 Mask

Definition at line 8866 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN00_Pos

#define PWM_PHCHGNXT_AOFFEN00_Pos (24)

PWM_T::PHCHGNXT: AOFFEN00 Position

Definition at line 8865 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN01_Msk

#define PWM_PHCHGNXT_AOFFEN01_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN01_Pos)

PWM_T::PHCHGNXT: AOFFEN01 Mask

Definition at line 8845 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN01_Pos

#define PWM_PHCHGNXT_AOFFEN01_Pos (16)

PWM_T::PHCHGNXT: AOFFEN01 Position

Definition at line 8844 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN10_Msk

#define PWM_PHCHGNXT_AOFFEN10_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN10_Pos)

PWM_T::PHCHGNXT: AOFFEN10 Mask

Definition at line 8869 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN10_Pos

#define PWM_PHCHGNXT_AOFFEN10_Pos (25)

PWM_T::PHCHGNXT: AOFFEN10 Position

Definition at line 8868 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN11_Msk

#define PWM_PHCHGNXT_AOFFEN11_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN11_Pos)

PWM_T::PHCHGNXT: AOFFEN11 Mask

Definition at line 8848 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN11_Pos

#define PWM_PHCHGNXT_AOFFEN11_Pos (17)

PWM_T::PHCHGNXT: AOFFEN11 Position

Definition at line 8847 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN20_Msk

#define PWM_PHCHGNXT_AOFFEN20_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN20_Pos)

PWM_T::PHCHGNXT: AOFFEN20 Mask

Definition at line 8872 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN20_Pos

#define PWM_PHCHGNXT_AOFFEN20_Pos (26)

PWM_T::PHCHGNXT: AOFFEN20 Position

Definition at line 8871 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN21_Msk

#define PWM_PHCHGNXT_AOFFEN21_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN21_Pos)

PWM_T::PHCHGNXT: AOFFEN21 Mask

Definition at line 8851 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN21_Pos

#define PWM_PHCHGNXT_AOFFEN21_Pos (18)

PWM_T::PHCHGNXT: AOFFEN21 Position

Definition at line 8850 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN30_Msk

#define PWM_PHCHGNXT_AOFFEN30_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN30_Pos)

PWM_T::PHCHGNXT: AOFFEN30 Mask

Definition at line 8875 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN30_Pos

#define PWM_PHCHGNXT_AOFFEN30_Pos (27)

PWM_T::PHCHGNXT: AOFFEN30 Position

Definition at line 8874 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN31_Msk

#define PWM_PHCHGNXT_AOFFEN31_Msk (0x1ul << PWM_PHCHGNXT_AOFFEN31_Pos)

PWM_T::PHCHGNXT: AOFFEN31 Mask

Definition at line 8854 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AOFFEN31_Pos

#define PWM_PHCHGNXT_AOFFEN31_Pos (19)

PWM_T::PHCHGNXT: AOFFEN31 Position

Definition at line 8853 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR0_Msk

#define PWM_PHCHGNXT_AUTOCLR0_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR0_Pos)

PWM_T::PHCHGNXT: AUTOCLR0 Mask

Definition at line 8839 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR0_Pos

#define PWM_PHCHGNXT_AUTOCLR0_Pos (14)

PWM_T::PHCHGNXT: AUTOCLR0 Position

Definition at line 8838 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR1_Msk

#define PWM_PHCHGNXT_AUTOCLR1_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR1_Pos)

PWM_T::PHCHGNXT: AUTOCLR1 Mask

Definition at line 8842 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR1_Pos

#define PWM_PHCHGNXT_AUTOCLR1_Pos (15)

PWM_T::PHCHGNXT: AUTOCLR1 Position

Definition at line 8841 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT0_Msk

#define PWM_PHCHGNXT_MSKDAT0_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT0_Pos)

PWM_T::PHCHGNXT: MSKDAT0 Mask

Definition at line 8797 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT0_Pos

#define PWM_PHCHGNXT_MSKDAT0_Pos (0)

PWM_T::PHCHGNXT: MSKDAT0 Position

Definition at line 8796 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT1_Msk

#define PWM_PHCHGNXT_MSKDAT1_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT1_Pos)

PWM_T::PHCHGNXT: MSKDAT1 Mask

Definition at line 8800 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT1_Pos

#define PWM_PHCHGNXT_MSKDAT1_Pos (1)

PWM_T::PHCHGNXT: MSKDAT1 Position

Definition at line 8799 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT2_Msk

#define PWM_PHCHGNXT_MSKDAT2_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT2_Pos)

PWM_T::PHCHGNXT: MSKDAT2 Mask

Definition at line 8803 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT2_Pos

#define PWM_PHCHGNXT_MSKDAT2_Pos (2)

PWM_T::PHCHGNXT: MSKDAT2 Position

Definition at line 8802 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT3_Msk

#define PWM_PHCHGNXT_MSKDAT3_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT3_Pos)

PWM_T::PHCHGNXT: MSKDAT3 Mask

Definition at line 8806 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT3_Pos

#define PWM_PHCHGNXT_MSKDAT3_Pos (3)

PWM_T::PHCHGNXT: MSKDAT3 Position

Definition at line 8805 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT4_Msk

#define PWM_PHCHGNXT_MSKDAT4_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT4_Pos)

PWM_T::PHCHGNXT: MSKDAT4 Mask

Definition at line 8809 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT4_Pos

#define PWM_PHCHGNXT_MSKDAT4_Pos (4)

PWM_T::PHCHGNXT: MSKDAT4 Position

Definition at line 8808 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT5_Msk

#define PWM_PHCHGNXT_MSKDAT5_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT5_Pos)

PWM_T::PHCHGNXT: MSKDAT5 Mask

Definition at line 8812 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT5_Pos

#define PWM_PHCHGNXT_MSKDAT5_Pos (5)

PWM_T::PHCHGNXT: MSKDAT5 Position

Definition at line 8811 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT6_Msk

#define PWM_PHCHGNXT_MSKDAT6_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT6_Pos)

PWM_T::PHCHGNXT: MSKDAT6 Mask

Definition at line 8815 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT6_Pos

#define PWM_PHCHGNXT_MSKDAT6_Pos (6)

PWM_T::PHCHGNXT: MSKDAT6 Position

Definition at line 8814 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT7_Msk

#define PWM_PHCHGNXT_MSKDAT7_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT7_Pos)

PWM_T::PHCHGNXT: MSKDAT7 Mask

Definition at line 8818 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT7_Pos

#define PWM_PHCHGNXT_MSKDAT7_Pos (7)

PWM_T::PHCHGNXT: MSKDAT7 Position

Definition at line 8817 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN0_Msk

#define PWM_PHCHGNXT_MSKEN0_Msk (0x1ul << PWM_PHCHGNXT_MSKEN0_Pos)

PWM_T::PHCHGNXT: MSKEN0 Mask

Definition at line 8821 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN0_Pos

#define PWM_PHCHGNXT_MSKEN0_Pos (8)

PWM_T::PHCHGNXT: MSKEN0 Position

Definition at line 8820 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN1_Msk

#define PWM_PHCHGNXT_MSKEN1_Msk (0x1ul << PWM_PHCHGNXT_MSKEN1_Pos)

PWM_T::PHCHGNXT: MSKEN1 Mask

Definition at line 8824 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN1_Pos

#define PWM_PHCHGNXT_MSKEN1_Pos (9)

PWM_T::PHCHGNXT: MSKEN1 Position

Definition at line 8823 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN2_Msk

#define PWM_PHCHGNXT_MSKEN2_Msk (0x1ul << PWM_PHCHGNXT_MSKEN2_Pos)

PWM_T::PHCHGNXT: MSKEN2 Mask

Definition at line 8827 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN2_Pos

#define PWM_PHCHGNXT_MSKEN2_Pos (10)

PWM_T::PHCHGNXT: MSKEN2 Position

Definition at line 8826 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN3_Msk

#define PWM_PHCHGNXT_MSKEN3_Msk (0x1ul << PWM_PHCHGNXT_MSKEN3_Pos)

PWM_T::PHCHGNXT: MSKEN3 Mask

Definition at line 8830 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN3_Pos

#define PWM_PHCHGNXT_MSKEN3_Pos (11)

PWM_T::PHCHGNXT: MSKEN3 Position

Definition at line 8829 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN4_Msk

#define PWM_PHCHGNXT_MSKEN4_Msk (0x1ul << PWM_PHCHGNXT_MSKEN4_Pos)

PWM_T::PHCHGNXT: MSKEN4 Mask

Definition at line 8833 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN4_Pos

#define PWM_PHCHGNXT_MSKEN4_Pos (12)

PWM_T::PHCHGNXT: MSKEN4 Position

Definition at line 8832 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN5_Msk

#define PWM_PHCHGNXT_MSKEN5_Msk (0x1ul << PWM_PHCHGNXT_MSKEN5_Pos)

PWM_T::PHCHGNXT: MSKEN5 Mask

Definition at line 8836 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_MSKEN5_Pos

#define PWM_PHCHGNXT_MSKEN5_Pos (13)

PWM_T::PHCHGNXT: MSKEN5 Position

Definition at line 8835 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_TMR0TEN_Msk

#define PWM_PHCHGNXT_TMR0TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR0TEN_Pos)

PWM_T::PHCHGNXT: TMR0TEN Mask

Definition at line 8881 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_TMR0TEN_Pos

#define PWM_PHCHGNXT_TMR0TEN_Pos (30)

PWM_T::PHCHGNXT: TMR0TEN Position

Definition at line 8880 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_TMR1TEN_Msk

#define PWM_PHCHGNXT_TMR1TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR1TEN_Pos)

PWM_T::PHCHGNXT: TMR1TEN Mask

Definition at line 8860 of file Mini58Series.h.

## ◆ PWM_PHCHGNXT_TMR1TEN_Pos

#define PWM_PHCHGNXT_TMR1TEN_Pos (22)

PWM_T::PHCHGNXT: TMR1TEN Position

Definition at line 8859 of file Mini58Series.h.

## ◆ PWM_POEN_POEN0_Msk

#define PWM_POEN_POEN0_Msk (0x1ul << PWM_POEN_POEN0_Pos)

PWM_T::POEN: POEN0 Mask

Definition at line 8491 of file Mini58Series.h.

## ◆ PWM_POEN_POEN0_Pos

#define PWM_POEN_POEN0_Pos (0)

PWM_T::POEN: POEN0 Position

Definition at line 8490 of file Mini58Series.h.

## ◆ PWM_POEN_POEN1_Msk

#define PWM_POEN_POEN1_Msk (0x1ul << PWM_POEN_POEN1_Pos)

PWM_T::POEN: POEN1 Mask

Definition at line 8494 of file Mini58Series.h.

## ◆ PWM_POEN_POEN1_Pos

#define PWM_POEN_POEN1_Pos (1)

PWM_T::POEN: POEN1 Position

Definition at line 8493 of file Mini58Series.h.

## ◆ PWM_POEN_POEN2_Msk

#define PWM_POEN_POEN2_Msk (0x1ul << PWM_POEN_POEN2_Pos)

PWM_T::POEN: POEN2 Mask

Definition at line 8497 of file Mini58Series.h.

## ◆ PWM_POEN_POEN2_Pos

#define PWM_POEN_POEN2_Pos (2)

PWM_T::POEN: POEN2 Position

Definition at line 8496 of file Mini58Series.h.

## ◆ PWM_POEN_POEN3_Msk

#define PWM_POEN_POEN3_Msk (0x1ul << PWM_POEN_POEN3_Pos)

PWM_T::POEN: POEN3 Mask

Definition at line 8500 of file Mini58Series.h.

## ◆ PWM_POEN_POEN3_Pos

#define PWM_POEN_POEN3_Pos (3)

PWM_T::POEN: POEN3 Position

Definition at line 8499 of file Mini58Series.h.

## ◆ PWM_POEN_POEN4_Msk

#define PWM_POEN_POEN4_Msk (0x1ul << PWM_POEN_POEN4_Pos)

PWM_T::POEN: POEN4 Mask

Definition at line 8503 of file Mini58Series.h.

## ◆ PWM_POEN_POEN4_Pos

#define PWM_POEN_POEN4_Pos (4)

PWM_T::POEN: POEN4 Position

Definition at line 8502 of file Mini58Series.h.

## ◆ PWM_POEN_POEN5_Msk

#define PWM_POEN_POEN5_Msk (0x1ul << PWM_POEN_POEN5_Pos)

PWM_T::POEN: POEN5 Mask

Definition at line 8506 of file Mini58Series.h.

## ◆ PWM_POEN_POEN5_Pos

#define PWM_POEN_POEN5_Pos (5)

PWM_T::POEN: POEN5 Position

Definition at line 8505 of file Mini58Series.h.

## ◆ SPI_CLKDIV_DIVIDER_Msk

#define SPI_CLKDIV_DIVIDER_Msk (0xfful << SPI_CLKDIV_DIVIDER_Pos)

SPI_T::CLKDIV: DIVIDER Mask

Definition at line 9353 of file Mini58Series.h.

## ◆ SPI_CLKDIV_DIVIDER_Pos

#define SPI_CLKDIV_DIVIDER_Pos (0)

SPI_T::CLKDIV: DIVIDER Position

Definition at line 9352 of file Mini58Series.h.

## ◆ SPI_CTL_CLKPOL_Msk

#define SPI_CTL_CLKPOL_Msk (0x1ul << SPI_CTL_CLKPOL_Pos)

SPI_T::CTL: CLKPOL Mask

Definition at line 9320 of file Mini58Series.h.

## ◆ SPI_CTL_CLKPOL_Pos

#define SPI_CTL_CLKPOL_Pos (11)

SPI_T::CTL: CLKPOL Position

Definition at line 9319 of file Mini58Series.h.

## ◆ SPI_CTL_DWIDTH_Msk

#define SPI_CTL_DWIDTH_Msk (0x1ful << SPI_CTL_DWIDTH_Pos)

SPI_T::CTL: DWIDTH Mask

Definition at line 9314 of file Mini58Series.h.

## ◆ SPI_CTL_DWIDTH_Pos

#define SPI_CTL_DWIDTH_Pos (3)

SPI_T::CTL: DWIDTH Position

Definition at line 9313 of file Mini58Series.h.

## ◆ SPI_CTL_FIFOEN_Msk

#define SPI_CTL_FIFOEN_Msk (0x1ul << SPI_CTL_FIFOEN_Pos)

SPI_T::CTL: FIFOEN Mask

Definition at line 9338 of file Mini58Series.h.

## ◆ SPI_CTL_FIFOEN_Pos

#define SPI_CTL_FIFOEN_Pos (21)

SPI_T::CTL: FIFOEN Position

Definition at line 9337 of file Mini58Series.h.

## ◆ SPI_CTL_LSB_Msk

#define SPI_CTL_LSB_Msk (0x1ul << SPI_CTL_LSB_Pos)

SPI_T::CTL: LSB Mask

Definition at line 9317 of file Mini58Series.h.

## ◆ SPI_CTL_LSB_Pos

#define SPI_CTL_LSB_Pos (10)

SPI_T::CTL: LSB Position

Definition at line 9316 of file Mini58Series.h.

## ◆ SPI_CTL_REORDER_Msk

#define SPI_CTL_REORDER_Msk (0x1ul << SPI_CTL_REORDER_Pos)

SPI_T::CTL: REORDER Mask

Definition at line 9335 of file Mini58Series.h.

## ◆ SPI_CTL_REORDER_Pos

#define SPI_CTL_REORDER_Pos (19)

SPI_T::CTL: REORDER Position

Definition at line 9334 of file Mini58Series.h.

## ◆ SPI_CTL_RXEMPTY_Msk

#define SPI_CTL_RXEMPTY_Msk (0x1ul << SPI_CTL_RXEMPTY_Pos)

SPI_T::CTL: RXEMPTY Mask

Definition at line 9341 of file Mini58Series.h.

## ◆ SPI_CTL_RXEMPTY_Pos

#define SPI_CTL_RXEMPTY_Pos (24)

SPI_T::CTL: RXEMPTY Position

Definition at line 9340 of file Mini58Series.h.

## ◆ SPI_CTL_RXFULL_Msk

#define SPI_CTL_RXFULL_Msk (0x1ul << SPI_CTL_RXFULL_Pos)

SPI_T::CTL: RXFULL Mask

Definition at line 9344 of file Mini58Series.h.

## ◆ SPI_CTL_RXFULL_Pos

#define SPI_CTL_RXFULL_Pos (25)

SPI_T::CTL: RXFULL Position

Definition at line 9343 of file Mini58Series.h.

## ◆ SPI_CTL_RXNEG_Msk

#define SPI_CTL_RXNEG_Msk (0x1ul << SPI_CTL_RXNEG_Pos)

SPI_T::CTL: RXNEG Mask

Definition at line 9308 of file Mini58Series.h.

## ◆ SPI_CTL_RXNEG_Pos

#define SPI_CTL_RXNEG_Pos (1)

SPI_T::CTL: RXNEG Position

Definition at line 9307 of file Mini58Series.h.

## ◆ SPI_CTL_SLAVE_Msk

#define SPI_CTL_SLAVE_Msk (0x1ul << SPI_CTL_SLAVE_Pos)

SPI_T::CTL: SLAVE Mask

Definition at line 9332 of file Mini58Series.h.

## ◆ SPI_CTL_SLAVE_Pos

#define SPI_CTL_SLAVE_Pos (18)

SPI_T::CTL: SLAVE Position

Definition at line 9331 of file Mini58Series.h.

## ◆ SPI_CTL_SPIEN_Msk

#define SPI_CTL_SPIEN_Msk (0x1ul << SPI_CTL_SPIEN_Pos)

SPI_T::CTL: SPIEN Mask

Definition at line 9305 of file Mini58Series.h.

## ◆ SPI_CTL_SPIEN_Pos

#define SPI_CTL_SPIEN_Pos (0)

    @addtogroup SPI_CONST SPI Bit Field Definition
    Constant Definitions for SPI Controller

SPI_T::CTL: SPIEN Position

Definition at line 9304 of file Mini58Series.h.

## ◆ SPI_CTL_SUSPITV_Msk

#define SPI_CTL_SUSPITV_Msk (0xful << SPI_CTL_SUSPITV_Pos)

SPI_T::CTL: SUSPITV Mask

Definition at line 9323 of file Mini58Series.h.

## ◆ SPI_CTL_SUSPITV_Pos

#define SPI_CTL_SUSPITV_Pos (12)

SPI_T::CTL: SUSPITV Position

Definition at line 9322 of file Mini58Series.h.

## ◆ SPI_CTL_TXEMPTY_Msk

#define SPI_CTL_TXEMPTY_Msk (0x1ul << SPI_CTL_TXEMPTY_Pos)

SPI_T::CTL: TXEMPTY Mask

Definition at line 9347 of file Mini58Series.h.

## ◆ SPI_CTL_TXEMPTY_Pos

#define SPI_CTL_TXEMPTY_Pos (26)

SPI_T::CTL: TXEMPTY Position

Definition at line 9346 of file Mini58Series.h.

## ◆ SPI_CTL_TXFULL_Msk

#define SPI_CTL_TXFULL_Msk (0x1ul << SPI_CTL_TXFULL_Pos)

SPI_T::CTL: TXFULL Mask

Definition at line 9350 of file Mini58Series.h.

## ◆ SPI_CTL_TXFULL_Pos

#define SPI_CTL_TXFULL_Pos (27)

SPI_T::CTL: TXFULL Position

Definition at line 9349 of file Mini58Series.h.

## ◆ SPI_CTL_TXNEG_Msk

#define SPI_CTL_TXNEG_Msk (0x1ul << SPI_CTL_TXNEG_Pos)

SPI_T::CTL: TXNEG Mask

Definition at line 9311 of file Mini58Series.h.

## ◆ SPI_CTL_TXNEG_Pos

#define SPI_CTL_TXNEG_Pos (2)

SPI_T::CTL: TXNEG Position

Definition at line 9310 of file Mini58Series.h.

## ◆ SPI_CTL_UNITIEN_Msk

#define SPI_CTL_UNITIEN_Msk (0x1ul << SPI_CTL_UNITIEN_Pos)

SPI_T::CTL: UNITIEN Mask

Definition at line 9329 of file Mini58Series.h.

## ◆ SPI_CTL_UNITIEN_Pos

#define SPI_CTL_UNITIEN_Pos (17)

SPI_T::CTL: UNITIEN Position

Definition at line 9328 of file Mini58Series.h.

## ◆ SPI_CTL_UNITIF_Msk

#define SPI_CTL_UNITIF_Msk (0x1ul << SPI_CTL_UNITIF_Pos)

SPI_T::CTL: UNITIF Mask

Definition at line 9326 of file Mini58Series.h.

## ◆ SPI_CTL_UNITIF_Pos

#define SPI_CTL_UNITIF_Pos (16)

SPI_T::CTL: UNITIF Position

Definition at line 9325 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXOVIEN_Msk

#define SPI_FIFOCTL_RXOVIEN_Msk (0x1ul << SPI_FIFOCTL_RXOVIEN_Pos)

SPI_T::FIFOCTL: RXOVIEN Mask

Definition at line 9407 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXOVIEN_Pos

#define SPI_FIFOCTL_RXOVIEN_Pos (6)

SPI_T::FIFOCTL: RXOVIEN Position

Definition at line 9406 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXRST_Msk

#define SPI_FIFOCTL_RXRST_Msk (0x1ul << SPI_FIFOCTL_RXRST_Pos)

SPI_T::FIFOCTL: RXRST Mask

Definition at line 9395 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXRST_Pos

#define SPI_FIFOCTL_RXRST_Pos (0)

SPI_T::FIFOCTL: RXRST Position

Definition at line 9394 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXTH_Msk

#define SPI_FIFOCTL_RXTH_Msk (0x3ul << SPI_FIFOCTL_RXTH_Pos)

SPI_T::FIFOCTL: RXTH Mask

Definition at line 9413 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXTH_Pos

#define SPI_FIFOCTL_RXTH_Pos (24)

SPI_T::FIFOCTL: RXTH Position

Definition at line 9412 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXTHIEN_Msk

#define SPI_FIFOCTL_RXTHIEN_Msk (0x1ul << SPI_FIFOCTL_RXTHIEN_Pos)

SPI_T::FIFOCTL: RXTHIEN Mask

Definition at line 9401 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXTHIEN_Pos

#define SPI_FIFOCTL_RXTHIEN_Pos (2)

SPI_T::FIFOCTL: RXTHIEN Position

Definition at line 9400 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXTOIEN_Msk

#define SPI_FIFOCTL_RXTOIEN_Msk (0x1ul << SPI_FIFOCTL_RXTOIEN_Pos)

SPI_T::FIFOCTL: RXTOIEN Mask

Definition at line 9410 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_RXTOIEN_Pos

#define SPI_FIFOCTL_RXTOIEN_Pos (21)

SPI_T::FIFOCTL: RXTOIEN Position

Definition at line 9409 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_TXRST_Msk

#define SPI_FIFOCTL_TXRST_Msk (0x1ul << SPI_FIFOCTL_TXRST_Pos)

SPI_T::FIFOCTL: TXRST Mask

Definition at line 9398 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_TXRST_Pos

#define SPI_FIFOCTL_TXRST_Pos (1)

SPI_T::FIFOCTL: TXRST Position

Definition at line 9397 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_TXTH_Msk

#define SPI_FIFOCTL_TXTH_Msk (0x3ul << SPI_FIFOCTL_TXTH_Pos)

SPI_T::FIFOCTL: TXTH Mask

Definition at line 9416 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_TXTH_Pos

#define SPI_FIFOCTL_TXTH_Pos (28)

SPI_T::FIFOCTL: TXTH Position

Definition at line 9415 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_TXTHIEN_Msk

#define SPI_FIFOCTL_TXTHIEN_Msk (0x1ul << SPI_FIFOCTL_TXTHIEN_Pos)

SPI_T::FIFOCTL: TXTHIEN Mask

Definition at line 9404 of file Mini58Series.h.

## ◆ SPI_FIFOCTL_TXTHIEN_Pos

#define SPI_FIFOCTL_TXTHIEN_Pos (3)

SPI_T::FIFOCTL: TXTHIEN Position

Definition at line 9403 of file Mini58Series.h.

## ◆ SPI_RX_RX_Msk

#define SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)

SPI_T::RX: RX Mask

Definition at line 9371 of file Mini58Series.h.

## ◆ SPI_RX_RX_Pos

#define SPI_RX_RX_Pos (0)

SPI_T::RX: RX Position

Definition at line 9370 of file Mini58Series.h.

## ◆ SPI_SLVCTL_DIVMOD_Msk

#define SPI_SLVCTL_DIVMOD_Msk (0x1ul << SPI_SLVCTL_DIVMOD_Pos)

SPI_T::SLVCTL: DIVMOD Mask

Definition at line 9392 of file Mini58Series.h.

## ◆ SPI_SLVCTL_DIVMOD_Pos

#define SPI_SLVCTL_DIVMOD_Pos (31)

SPI_T::SLVCTL: DIVMOD Position

Definition at line 9391 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLV3WIRE_Msk

#define SPI_SLVCTL_SLV3WIRE_Msk (0x1ul << SPI_SLVCTL_SLV3WIRE_Pos)

SPI_T::SLVCTL: SLV3WIRE Mask

Definition at line 9377 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLV3WIRE_Pos

#define SPI_SLVCTL_SLV3WIRE_Pos (8)

SPI_T::SLVCTL: SLV3WIRE Position

Definition at line 9376 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLVABT_Msk

#define SPI_SLVCTL_SLVABT_Msk (0x1ul << SPI_SLVCTL_SLVABT_Pos)

SPI_T::SLVCTL: SLVABT Mask

Definition at line 9380 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLVABT_Pos

#define SPI_SLVCTL_SLVABT_Pos (9)

SPI_T::SLVCTL: SLVABT Position

Definition at line 9379 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLVSTIEN_Msk

#define SPI_SLVCTL_SLVSTIEN_Msk (0x1ul << SPI_SLVCTL_SLVSTIEN_Pos)

SPI_T::SLVCTL: SLVSTIEN Mask

Definition at line 9383 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLVSTIEN_Pos

#define SPI_SLVCTL_SLVSTIEN_Pos (10)

SPI_T::SLVCTL: SLVSTIEN Position

Definition at line 9382 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLVSTIF_Msk

#define SPI_SLVCTL_SLVSTIF_Msk (0x1ul << SPI_SLVCTL_SLVSTIF_Pos)

SPI_T::SLVCTL: SLVSTIF Mask

Definition at line 9386 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SLVSTIF_Pos

#define SPI_SLVCTL_SLVSTIF_Pos (11)

SPI_T::SLVCTL: SLVSTIF Position

Definition at line 9385 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SSINAIEN_Msk

#define SPI_SLVCTL_SSINAIEN_Msk (0x1ul << SPI_SLVCTL_SSINAIEN_Pos)

SPI_T::SLVCTL: SSINAIEN Mask

Definition at line 9389 of file Mini58Series.h.

## ◆ SPI_SLVCTL_SSINAIEN_Pos

#define SPI_SLVCTL_SSINAIEN_Pos (16)

SPI_T::SLVCTL: SSINAIEN Position

Definition at line 9388 of file Mini58Series.h.

## ◆ SPI_SSCTL_AUTOSS_Msk

#define SPI_SSCTL_AUTOSS_Msk (0x1ul << SPI_SSCTL_AUTOSS_Pos)

SPI_T::SSCTL: AUTOSS Mask

Definition at line 9362 of file Mini58Series.h.

## ◆ SPI_SSCTL_AUTOSS_Pos

#define SPI_SSCTL_AUTOSS_Pos (3)

SPI_T::SSCTL: AUTOSS Position

Definition at line 9361 of file Mini58Series.h.

## ◆ SPI_SSCTL_LTF_Msk

#define SPI_SSCTL_LTF_Msk (0x1ul << SPI_SSCTL_LTF_Pos)

SPI_T::SSCTL: LTF Mask

Definition at line 9368 of file Mini58Series.h.

## ◆ SPI_SSCTL_LTF_Pos

#define SPI_SSCTL_LTF_Pos (5)

SPI_T::SSCTL: LTF Position

Definition at line 9367 of file Mini58Series.h.

## ◆ SPI_SSCTL_SS_Msk

#define SPI_SSCTL_SS_Msk (0x1ul << SPI_SSCTL_SS_Pos)

SPI_T::SSCTL: SS Mask

Definition at line 9356 of file Mini58Series.h.

## ◆ SPI_SSCTL_SS_Pos

#define SPI_SSCTL_SS_Pos (0)

SPI_T::SSCTL: SS Position

Definition at line 9355 of file Mini58Series.h.

## ◆ SPI_SSCTL_SSACTPOL_Msk

#define SPI_SSCTL_SSACTPOL_Msk (0x1ul << SPI_SSCTL_SSACTPOL_Pos)

SPI_T::SSCTL: SSACTPOL Mask

Definition at line 9359 of file Mini58Series.h.

## ◆ SPI_SSCTL_SSACTPOL_Pos

#define SPI_SSCTL_SSACTPOL_Pos (2)

SPI_T::SSCTL: SSACTPOL Position

Definition at line 9358 of file Mini58Series.h.

## ◆ SPI_SSCTL_SSLTEN_Msk

#define SPI_SSCTL_SSLTEN_Msk (0x1ul << SPI_SSCTL_SSLTEN_Pos)

SPI_T::SSCTL: SSLTEN Mask

Definition at line 9365 of file Mini58Series.h.

## ◆ SPI_SSCTL_SSLTEN_Pos

#define SPI_SSCTL_SSLTEN_Pos (4)

SPI_T::SSCTL: SSLTEN Position

Definition at line 9364 of file Mini58Series.h.

## ◆ SPI_STATUS_RXCNT_Msk

#define SPI_STATUS_RXCNT_Msk (0xful << SPI_STATUS_RXCNT_Pos)

SPI_T::STATUS: RXCNT Mask

Definition at line 9431 of file Mini58Series.h.

## ◆ SPI_STATUS_RXCNT_Pos

#define SPI_STATUS_RXCNT_Pos (12)

SPI_T::STATUS: RXCNT Position

Definition at line 9430 of file Mini58Series.h.

## ◆ SPI_STATUS_RXEMPTY_Msk

#define SPI_STATUS_RXEMPTY_Msk (0x1ul << SPI_STATUS_RXEMPTY_Pos)

SPI_T::STATUS: RXEMPTY Mask

Definition at line 9440 of file Mini58Series.h.

## ◆ SPI_STATUS_RXEMPTY_Pos

#define SPI_STATUS_RXEMPTY_Pos (24)

SPI_T::STATUS: RXEMPTY Position

Definition at line 9439 of file Mini58Series.h.

## ◆ SPI_STATUS_RXFULL_Msk

#define SPI_STATUS_RXFULL_Msk (0x1ul << SPI_STATUS_RXFULL_Pos)

SPI_T::STATUS: RXFULL Mask

Definition at line 9443 of file Mini58Series.h.

## ◆ SPI_STATUS_RXFULL_Pos

#define SPI_STATUS_RXFULL_Pos (25)

SPI_T::STATUS: RXFULL Position

Definition at line 9442 of file Mini58Series.h.

## ◆ SPI_STATUS_RXOVIF_Msk

#define SPI_STATUS_RXOVIF_Msk (0x1ul << SPI_STATUS_RXOVIF_Pos)

SPI_T::STATUS: RXOVIF Mask

Definition at line 9422 of file Mini58Series.h.

## ◆ SPI_STATUS_RXOVIF_Pos

#define SPI_STATUS_RXOVIF_Pos (2)

SPI_T::STATUS: RXOVIF Position

Definition at line 9421 of file Mini58Series.h.

## ◆ SPI_STATUS_RXTHIF_Msk

#define SPI_STATUS_RXTHIF_Msk (0x1ul << SPI_STATUS_RXTHIF_Pos)

SPI_T::STATUS: RXTHIF Mask

Definition at line 9419 of file Mini58Series.h.

## ◆ SPI_STATUS_RXTHIF_Pos

#define SPI_STATUS_RXTHIF_Pos (0)

SPI_T::STATUS: RXTHIF Position

Definition at line 9418 of file Mini58Series.h.

## ◆ SPI_STATUS_SLVSTIF_Msk

#define SPI_STATUS_SLVSTIF_Msk (0x1ul << SPI_STATUS_SLVSTIF_Pos)

SPI_T::STATUS: SLVSTIF Mask

Definition at line 9428 of file Mini58Series.h.

## ◆ SPI_STATUS_SLVSTIF_Pos

#define SPI_STATUS_SLVSTIF_Pos (11)

SPI_T::STATUS: SLVSTIF Position

Definition at line 9427 of file Mini58Series.h.

## ◆ SPI_STATUS_SLVTOIF_Msk

#define SPI_STATUS_SLVTOIF_Msk (0x1ul << SPI_STATUS_SLVTOIF_Pos)

SPI_T::STATUS: SLVTOIF Mask

Definition at line 9437 of file Mini58Series.h.

## ◆ SPI_STATUS_SLVTOIF_Pos

#define SPI_STATUS_SLVTOIF_Pos (20)

SPI_T::STATUS: SLVTOIF Position

Definition at line 9436 of file Mini58Series.h.

## ◆ SPI_STATUS_TXCNT_Msk

#define SPI_STATUS_TXCNT_Msk (0xful << SPI_STATUS_TXCNT_Pos)

SPI_T::STATUS: TXCNT Mask

Definition at line 9452 of file Mini58Series.h.

## ◆ SPI_STATUS_TXCNT_Pos

#define SPI_STATUS_TXCNT_Pos (28)

SPI_T::STATUS: TXCNT Position

Definition at line 9451 of file Mini58Series.h.

## ◆ SPI_STATUS_TXEMPTY_Msk

#define SPI_STATUS_TXEMPTY_Msk (0x1ul << SPI_STATUS_TXEMPTY_Pos)

SPI_T::STATUS: TXEMPTY Mask

Definition at line 9446 of file Mini58Series.h.

## ◆ SPI_STATUS_TXEMPTY_Pos

#define SPI_STATUS_TXEMPTY_Pos (26)

SPI_T::STATUS: TXEMPTY Position

Definition at line 9445 of file Mini58Series.h.

## ◆ SPI_STATUS_TXFULL_Msk

#define SPI_STATUS_TXFULL_Msk (0x1ul << SPI_STATUS_TXFULL_Pos)

SPI_T::STATUS: TXFULL Mask

Definition at line 9449 of file Mini58Series.h.

## ◆ SPI_STATUS_TXFULL_Pos

#define SPI_STATUS_TXFULL_Pos (27)

SPI_T::STATUS: TXFULL Position

Definition at line 9448 of file Mini58Series.h.

## ◆ SPI_STATUS_TXTHIF_Msk

#define SPI_STATUS_TXTHIF_Msk (0x1ul << SPI_STATUS_TXTHIF_Pos)

SPI_T::STATUS: TXTHIF Mask

Definition at line 9425 of file Mini58Series.h.

## ◆ SPI_STATUS_TXTHIF_Pos

#define SPI_STATUS_TXTHIF_Pos (4)

SPI_T::STATUS: TXTHIF Position

Definition at line 9424 of file Mini58Series.h.

## ◆ SPI_STATUS_UNITIF_Msk

#define SPI_STATUS_UNITIF_Msk (0x1ul << SPI_STATUS_UNITIF_Pos)

SPI_T::STATUS: UNITIF Mask

Definition at line 9434 of file Mini58Series.h.

## ◆ SPI_STATUS_UNITIF_Pos

#define SPI_STATUS_UNITIF_Pos (16)

SPI_T::STATUS: UNITIF Position

Definition at line 9433 of file Mini58Series.h.

## ◆ SPI_TX_TX_Msk

#define SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)

SPI_T::TX: TX Mask

Definition at line 9374 of file Mini58Series.h.

## ◆ SPI_TX_TX_Pos

#define SPI_TX_TX_Pos (0)

SPI_T::TX: TX Position

Definition at line 9373 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODEN_Msk

#define SYS_BODCTL_BODEN_Msk (0x1ul << SYS_BODCTL_BODEN_Pos)

SYS_T::BODCTL: BODEN Mask

Definition at line 10128 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODEN_Pos

#define SYS_BODCTL_BODEN_Pos (0)

SYS_T::BODCTL: BODEN Position

Definition at line 10127 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODIF_Msk

#define SYS_BODCTL_BODIF_Msk (0x1ul << SYS_BODCTL_BODIF_Pos)

SYS_T::BODCTL: BODIF Mask

Definition at line 10137 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODIF_Pos

#define SYS_BODCTL_BODIF_Pos (4)

SYS_T::BODCTL: BODIF Position

Definition at line 10136 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODLPM_Msk

#define SYS_BODCTL_BODLPM_Msk (0x1ul << SYS_BODCTL_BODLPM_Pos)

SYS_T::BODCTL: BODLPM Mask

Definition at line 10140 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODLPM_Pos

#define SYS_BODCTL_BODLPM_Pos (5)

SYS_T::BODCTL: BODLPM Position

Definition at line 10139 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODOUT_Msk

#define SYS_BODCTL_BODOUT_Msk (0x1ul << SYS_BODCTL_BODOUT_Pos)

SYS_T::BODCTL: BODOUT Mask

Definition at line 10143 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODOUT_Pos

#define SYS_BODCTL_BODOUT_Pos (6)

SYS_T::BODCTL: BODOUT Position

Definition at line 10142 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODRSTEN_Msk

#define SYS_BODCTL_BODRSTEN_Msk (0x1ul << SYS_BODCTL_BODRSTEN_Pos)

SYS_T::BODCTL: BODRSTEN Mask

Definition at line 10134 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODRSTEN_Pos

#define SYS_BODCTL_BODRSTEN_Pos (3)

SYS_T::BODCTL: BODRSTEN Position

Definition at line 10133 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODVL_Msk

#define SYS_BODCTL_BODVL_Msk (0x3ul << SYS_BODCTL_BODVL_Pos)

SYS_T::BODCTL: BODVL Mask

Definition at line 10131 of file Mini58Series.h.

## ◆ SYS_BODCTL_BODVL_Pos

#define SYS_BODCTL_BODVL_Pos (1)

SYS_T::BODCTL: BODVL Position

Definition at line 10130 of file Mini58Series.h.

## ◆ SYS_IPRST0_CHIPRST_Msk

#define SYS_IPRST0_CHIPRST_Msk (0x1ul << SYS_IPRST0_CHIPRST_Pos)

SYS_T::IPRST0: CHIPRST Mask

Definition at line 10089 of file Mini58Series.h.

## ◆ SYS_IPRST0_CHIPRST_Pos

#define SYS_IPRST0_CHIPRST_Pos (0)

SYS_T::IPRST0: CHIPRST Position

Definition at line 10088 of file Mini58Series.h.

## ◆ SYS_IPRST0_CPURST_Msk

#define SYS_IPRST0_CPURST_Msk (0x1ul << SYS_IPRST0_CPURST_Pos)

SYS_T::IPRST0: CPURST Mask

Definition at line 10092 of file Mini58Series.h.

## ◆ SYS_IPRST0_CPURST_Pos

#define SYS_IPRST0_CPURST_Pos (1)

SYS_T::IPRST0: CPURST Position

Definition at line 10091 of file Mini58Series.h.

## ◆ SYS_IPRST1_ACMPRST_Msk

#define SYS_IPRST1_ACMPRST_Msk (0x1ul << SYS_IPRST1_ACMPRST_Pos)

SYS_T::IPRST1: ACMPRST Mask

Definition at line 10122 of file Mini58Series.h.

## ◆ SYS_IPRST1_ACMPRST_Pos

#define SYS_IPRST1_ACMPRST_Pos (22)

SYS_T::IPRST1: ACMPRST Position

Definition at line 10121 of file Mini58Series.h.

## ◆ SYS_IPRST1_ADCRST_Msk

#define SYS_IPRST1_ADCRST_Msk (0x1ul << SYS_IPRST1_ADCRST_Pos)

SYS_T::IPRST1: ADCRST Mask

Definition at line 10125 of file Mini58Series.h.

## ◆ SYS_IPRST1_ADCRST_Pos

#define SYS_IPRST1_ADCRST_Pos (28)

SYS_T::IPRST1: ADCRST Position

Definition at line 10124 of file Mini58Series.h.

## ◆ SYS_IPRST1_GPIORST_Msk

#define SYS_IPRST1_GPIORST_Msk (0x1ul << SYS_IPRST1_GPIORST_Pos)

SYS_T::IPRST1: GPIORST Mask

Definition at line 10095 of file Mini58Series.h.

## ◆ SYS_IPRST1_GPIORST_Pos

#define SYS_IPRST1_GPIORST_Pos (1)

SYS_T::IPRST1: GPIORST Position

Definition at line 10094 of file Mini58Series.h.

## ◆ SYS_IPRST1_I2C0RST_Msk

#define SYS_IPRST1_I2C0RST_Msk (0x1ul << SYS_IPRST1_I2C0RST_Pos)

SYS_T::IPRST1: I2C0RST Mask

Definition at line 10104 of file Mini58Series.h.

## ◆ SYS_IPRST1_I2C0RST_Pos

#define SYS_IPRST1_I2C0RST_Pos (8)

SYS_T::IPRST1: I2C0RST Position

Definition at line 10103 of file Mini58Series.h.

## ◆ SYS_IPRST1_I2C1RST_Msk

#define SYS_IPRST1_I2C1RST_Msk (0x1ul << SYS_IPRST1_I2C1RST_Pos)

SYS_T::IPRST1: I2C1RST Mask

Definition at line 10107 of file Mini58Series.h.

## ◆ SYS_IPRST1_I2C1RST_Pos

#define SYS_IPRST1_I2C1RST_Pos (9)

SYS_T::IPRST1: I2C1RST Position

Definition at line 10106 of file Mini58Series.h.

## ◆ SYS_IPRST1_PWM0RST_Msk

#define SYS_IPRST1_PWM0RST_Msk (0x1ul << SYS_IPRST1_PWM0RST_Pos)

SYS_T::IPRST1: PWM0RST Mask

Definition at line 10119 of file Mini58Series.h.

## ◆ SYS_IPRST1_PWM0RST_Pos

#define SYS_IPRST1_PWM0RST_Pos (20)

SYS_T::IPRST1: PWM0RST Position

Definition at line 10118 of file Mini58Series.h.

## ◆ SYS_IPRST1_SPI0RST_Msk

#define SYS_IPRST1_SPI0RST_Msk (0x1ul << SYS_IPRST1_SPI0RST_Pos)

SYS_T::IPRST1: SPI0RST Mask

Definition at line 10110 of file Mini58Series.h.

## ◆ SYS_IPRST1_SPI0RST_Pos

#define SYS_IPRST1_SPI0RST_Pos (12)

SYS_T::IPRST1: SPI0RST Position

Definition at line 10109 of file Mini58Series.h.

## ◆ SYS_IPRST1_TMR0RST_Msk

#define SYS_IPRST1_TMR0RST_Msk (0x1ul << SYS_IPRST1_TMR0RST_Pos)

SYS_T::IPRST1: TMR0RST Mask

Definition at line 10098 of file Mini58Series.h.

## ◆ SYS_IPRST1_TMR0RST_Pos

#define SYS_IPRST1_TMR0RST_Pos (2)

SYS_T::IPRST1: TMR0RST Position

Definition at line 10097 of file Mini58Series.h.

## ◆ SYS_IPRST1_TMR1RST_Msk

#define SYS_IPRST1_TMR1RST_Msk (0x1ul << SYS_IPRST1_TMR1RST_Pos)

SYS_T::IPRST1: TMR1RST Mask

Definition at line 10101 of file Mini58Series.h.

## ◆ SYS_IPRST1_TMR1RST_Pos

#define SYS_IPRST1_TMR1RST_Pos (3)

SYS_T::IPRST1: TMR1RST Position

Definition at line 10100 of file Mini58Series.h.

## ◆ SYS_IPRST1_UART0RST_Msk

#define SYS_IPRST1_UART0RST_Msk (0x1ul << SYS_IPRST1_UART0RST_Pos)

SYS_T::IPRST1: UART0RST Mask

Definition at line 10113 of file Mini58Series.h.

## ◆ SYS_IPRST1_UART0RST_Pos

#define SYS_IPRST1_UART0RST_Pos (16)

SYS_T::IPRST1: UART0RST Position

Definition at line 10112 of file Mini58Series.h.

## ◆ SYS_IPRST1_UART1RST_Msk

#define SYS_IPRST1_UART1RST_Msk (0x1ul << SYS_IPRST1_UART1RST_Pos)

SYS_T::IPRST1: UART1RST Mask

Definition at line 10116 of file Mini58Series.h.

## ◆ SYS_IPRST1_UART1RST_Pos

#define SYS_IPRST1_UART1RST_Pos (17)

SYS_T::IPRST1: UART1RST Position

Definition at line 10115 of file Mini58Series.h.

## ◆ SYS_IRCTCTL_FREQSEL_Msk

#define SYS_IRCTCTL_FREQSEL_Msk (0x1ul << SYS_IRCTCTL_FREQSEL_Pos)

SYS_T::IRCTCTL: FREQSEL Mask

Definition at line 10284 of file Mini58Series.h.

## ◆ SYS_IRCTCTL_FREQSEL_Pos

#define SYS_IRCTCTL_FREQSEL_Pos (0)

SYS_T::IRCTCTL: FREQSEL Position

Definition at line 10283 of file Mini58Series.h.

## ◆ SYS_IRCTCTL_LOOPSEL_Msk

#define SYS_IRCTCTL_LOOPSEL_Msk (0x3ul << SYS_IRCTCTL_LOOPSEL_Pos)

SYS_T::IRCTCTL: LOOPSEL Mask

Definition at line 10287 of file Mini58Series.h.

## ◆ SYS_IRCTCTL_LOOPSEL_Pos

#define SYS_IRCTCTL_LOOPSEL_Pos (4)

SYS_T::IRCTCTL: LOOPSEL Position

Definition at line 10286 of file Mini58Series.h.

## ◆ SYS_IRCTIEN_CLKEIEN_Msk

#define SYS_IRCTIEN_CLKEIEN_Msk (0x1ul << SYS_IRCTIEN_CLKEIEN_Pos)

SYS_T::IRCTIEN: CLKEIEN Mask

Definition at line 10293 of file Mini58Series.h.

## ◆ SYS_IRCTIEN_CLKEIEN_Pos

#define SYS_IRCTIEN_CLKEIEN_Pos (2)

SYS_T::IRCTIEN: CLKEIEN Position

Definition at line 10292 of file Mini58Series.h.

## ◆ SYS_IRCTIEN_TFAILIEN_Msk

#define SYS_IRCTIEN_TFAILIEN_Msk (0x1ul << SYS_IRCTIEN_TFAILIEN_Pos)

SYS_T::IRCTIEN: TFAILIEN Mask

Definition at line 10290 of file Mini58Series.h.

## ◆ SYS_IRCTIEN_TFAILIEN_Pos

#define SYS_IRCTIEN_TFAILIEN_Pos (1)

SYS_T::IRCTIEN: TFAILIEN Position

Definition at line 10289 of file Mini58Series.h.

## ◆ SYS_IRCTISTS_CLKERRIF_Msk

#define SYS_IRCTISTS_CLKERRIF_Msk (0x1ul << SYS_IRCTISTS_CLKERRIF_Pos)

SYS_T::IRCTISTS: CLKERRIF Mask

Definition at line 10302 of file Mini58Series.h.

## ◆ SYS_IRCTISTS_CLKERRIF_Pos

#define SYS_IRCTISTS_CLKERRIF_Pos (2)

SYS_T::IRCTISTS: CLKERRIF Position

Definition at line 10301 of file Mini58Series.h.

## ◆ SYS_IRCTISTS_FREQLOCK_Msk

#define SYS_IRCTISTS_FREQLOCK_Msk (0x1ul << SYS_IRCTISTS_FREQLOCK_Pos)

SYS_T::IRCTISTS: FREQLOCK Mask

Definition at line 10296 of file Mini58Series.h.

## ◆ SYS_IRCTISTS_FREQLOCK_Pos

#define SYS_IRCTISTS_FREQLOCK_Pos (0)

SYS_T::IRCTISTS: FREQLOCK Position

Definition at line 10295 of file Mini58Series.h.

## ◆ SYS_IRCTISTS_TFAILIF_Msk

#define SYS_IRCTISTS_TFAILIF_Msk (0x1ul << SYS_IRCTISTS_TFAILIF_Pos)

SYS_T::IRCTISTS: TFAILIF Mask

Definition at line 10299 of file Mini58Series.h.

## ◆ SYS_IRCTISTS_TFAILIF_Pos

#define SYS_IRCTISTS_TFAILIF_Pos (1)

SYS_T::IRCTISTS: TFAILIF Position

Definition at line 10298 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT0_Msk

#define SYS_P0_MFP_ALT0_Msk (0x1ul << SYS_P0_MFP_ALT0_Pos)

SYS_T::P0_MFP: ALT0 Mask

Definition at line 10149 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT0_Pos

#define SYS_P0_MFP_ALT0_Pos (8)

SYS_T::P0_MFP: ALT0 Position

Definition at line 10148 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT1_Msk

#define SYS_P0_MFP_ALT1_Msk (0x1ul << SYS_P0_MFP_ALT1_Pos)

SYS_T::P0_MFP: ALT1 Mask

Definition at line 10152 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT1_Pos

#define SYS_P0_MFP_ALT1_Pos (9)

SYS_T::P0_MFP: ALT1 Position

Definition at line 10151 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT4_Msk

#define SYS_P0_MFP_ALT4_Msk (0x1ul << SYS_P0_MFP_ALT4_Pos)

SYS_T::P0_MFP: ALT4 Mask

Definition at line 10155 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT4_Pos

#define SYS_P0_MFP_ALT4_Pos (12)

SYS_T::P0_MFP: ALT4 Position

Definition at line 10154 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT5_Msk

#define SYS_P0_MFP_ALT5_Msk (0x1ul << SYS_P0_MFP_ALT5_Pos)

SYS_T::P0_MFP: ALT5 Mask

Definition at line 10158 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT5_Pos

#define SYS_P0_MFP_ALT5_Pos (13)

SYS_T::P0_MFP: ALT5 Position

Definition at line 10157 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT6_Msk

#define SYS_P0_MFP_ALT6_Msk (0x1ul << SYS_P0_MFP_ALT6_Pos)

SYS_T::P0_MFP: ALT6 Mask

Definition at line 10161 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT6_Pos

#define SYS_P0_MFP_ALT6_Pos (14)

SYS_T::P0_MFP: ALT6 Position

Definition at line 10160 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT7_Msk

#define SYS_P0_MFP_ALT7_Msk (0x1ul << SYS_P0_MFP_ALT7_Pos)

SYS_T::P0_MFP: ALT7 Mask

Definition at line 10164 of file Mini58Series.h.

## ◆ SYS_P0_MFP_ALT7_Pos

#define SYS_P0_MFP_ALT7_Pos (15)

SYS_T::P0_MFP: ALT7 Position

Definition at line 10163 of file Mini58Series.h.

## ◆ SYS_P0_MFP_MFP_Msk

#define SYS_P0_MFP_MFP_Msk (0xfful << SYS_P0_MFP_MFP_Pos)

SYS_T::P0_MFP: MFP Mask

Definition at line 10146 of file Mini58Series.h.

## ◆ SYS_P0_MFP_MFP_Pos

#define SYS_P0_MFP_MFP_Pos (0)

SYS_T::P0_MFP: MFP Position

Definition at line 10145 of file Mini58Series.h.

## ◆ SYS_P0_MFP_TYPE_Msk

#define SYS_P0_MFP_TYPE_Msk (0xfful << SYS_P0_MFP_TYPE_Pos)

SYS_T::P0_MFP: TYPE Mask

Definition at line 10167 of file Mini58Series.h.

## ◆ SYS_P0_MFP_TYPE_Pos

#define SYS_P0_MFP_TYPE_Pos (16)

SYS_T::P0_MFP: TYPE Position

Definition at line 10166 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT0_Msk

#define SYS_P1_MFP_ALT0_Msk (0x1ul << SYS_P1_MFP_ALT0_Pos)

SYS_T::P1_MFP: ALT0 Mask

Definition at line 10173 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT0_Pos

#define SYS_P1_MFP_ALT0_Pos (8)

SYS_T::P1_MFP: ALT0 Position

Definition at line 10172 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT2_Msk

#define SYS_P1_MFP_ALT2_Msk (0x1ul << SYS_P1_MFP_ALT2_Pos)

SYS_T::P1_MFP: ALT2 Mask

Definition at line 10176 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT2_Pos

#define SYS_P1_MFP_ALT2_Pos (10)

SYS_T::P1_MFP: ALT2 Position

Definition at line 10175 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT3_Msk

#define SYS_P1_MFP_ALT3_Msk (0x1ul << SYS_P1_MFP_ALT3_Pos)

SYS_T::P1_MFP: ALT3 Mask

Definition at line 10179 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT3_Pos

#define SYS_P1_MFP_ALT3_Pos (11)

SYS_T::P1_MFP: ALT3 Position

Definition at line 10178 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT4_Msk

#define SYS_P1_MFP_ALT4_Msk (0x1ul << SYS_P1_MFP_ALT4_Pos)

SYS_T::P1_MFP: ALT4 Mask

Definition at line 10182 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT4_Pos

#define SYS_P1_MFP_ALT4_Pos (12)

SYS_T::P1_MFP: ALT4 Position

Definition at line 10181 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT5_Msk

#define SYS_P1_MFP_ALT5_Msk (0x1ul << SYS_P1_MFP_ALT5_Pos)

SYS_T::P1_MFP: ALT5 Mask

Definition at line 10185 of file Mini58Series.h.

## ◆ SYS_P1_MFP_ALT5_Pos

#define SYS_P1_MFP_ALT5_Pos (13)

SYS_T::P1_MFP: ALT5 Position

Definition at line 10184 of file Mini58Series.h.

## ◆ SYS_P1_MFP_MFP_Msk

#define SYS_P1_MFP_MFP_Msk (0xfful << SYS_P1_MFP_MFP_Pos)

SYS_T::P1_MFP: MFP Mask

Definition at line 10170 of file Mini58Series.h.

## ◆ SYS_P1_MFP_MFP_Pos

#define SYS_P1_MFP_MFP_Pos (0)

SYS_T::P1_MFP: MFP Position

Definition at line 10169 of file Mini58Series.h.

## ◆ SYS_P1_MFP_P12EXT_Msk

#define SYS_P1_MFP_P12EXT_Msk (0x1ul << SYS_P1_MFP_P12EXT_Pos)

SYS_T::P1_MFP: P12EXT Mask

Definition at line 10191 of file Mini58Series.h.

## ◆ SYS_P1_MFP_P12EXT_Pos

#define SYS_P1_MFP_P12EXT_Pos (26)

SYS_T::P1_MFP: P12EXT Position

Definition at line 10190 of file Mini58Series.h.

## ◆ SYS_P1_MFP_P13EXT_Msk

#define SYS_P1_MFP_P13EXT_Msk (0x1ul << SYS_P1_MFP_P13EXT_Pos)

SYS_T::P1_MFP: P13EXT Mask

Definition at line 10194 of file Mini58Series.h.

## ◆ SYS_P1_MFP_P13EXT_Pos

#define SYS_P1_MFP_P13EXT_Pos (27)

SYS_T::P1_MFP: P13EXT Position

Definition at line 10193 of file Mini58Series.h.

## ◆ SYS_P1_MFP_P14EXT_Msk

#define SYS_P1_MFP_P14EXT_Msk (0x1ul << SYS_P1_MFP_P14EXT_Pos)

SYS_T::P1_MFP: P14EXT Mask

Definition at line 10197 of file Mini58Series.h.

## ◆ SYS_P1_MFP_P14EXT_Pos

#define SYS_P1_MFP_P14EXT_Pos (28)

SYS_T::P1_MFP: P14EXT Position

Definition at line 10196 of file Mini58Series.h.

## ◆ SYS_P1_MFP_TYPE_Msk

#define SYS_P1_MFP_TYPE_Msk (0xfful << SYS_P1_MFP_TYPE_Pos)

SYS_T::P1_MFP: TYPE Mask

Definition at line 10188 of file Mini58Series.h.

## ◆ SYS_P1_MFP_TYPE_Pos

#define SYS_P1_MFP_TYPE_Pos (16)

SYS_T::P1_MFP: TYPE Position

Definition at line 10187 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT2_Msk

#define SYS_P2_MFP_ALT2_Msk (0x1ul << SYS_P2_MFP_ALT2_Pos)

SYS_T::P2_MFP: ALT2 Mask

Definition at line 10203 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT2_Pos

#define SYS_P2_MFP_ALT2_Pos (10)

SYS_T::P2_MFP: ALT2 Position

Definition at line 10202 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT3_Msk

#define SYS_P2_MFP_ALT3_Msk (0x1ul << SYS_P2_MFP_ALT3_Pos)

SYS_T::P2_MFP: ALT3 Mask

Definition at line 10206 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT3_Pos

#define SYS_P2_MFP_ALT3_Pos (11)

SYS_T::P2_MFP: ALT3 Position

Definition at line 10205 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT4_Msk

#define SYS_P2_MFP_ALT4_Msk (0x1ul << SYS_P2_MFP_ALT4_Pos)

SYS_T::P2_MFP: ALT4 Mask

Definition at line 10209 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT4_Pos

#define SYS_P2_MFP_ALT4_Pos (12)

SYS_T::P2_MFP: ALT4 Position

Definition at line 10208 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT5_Msk

#define SYS_P2_MFP_ALT5_Msk (0x1ul << SYS_P2_MFP_ALT5_Pos)

SYS_T::P2_MFP: ALT5 Mask

Definition at line 10212 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT5_Pos

#define SYS_P2_MFP_ALT5_Pos (13)

SYS_T::P2_MFP: ALT5 Position

Definition at line 10211 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT6_Msk

#define SYS_P2_MFP_ALT6_Msk (0x1ul << SYS_P2_MFP_ALT6_Pos)

SYS_T::P2_MFP: ALT6 Mask

Definition at line 10215 of file Mini58Series.h.

## ◆ SYS_P2_MFP_ALT6_Pos

#define SYS_P2_MFP_ALT6_Pos (14)

SYS_T::P2_MFP: ALT6 Position

Definition at line 10214 of file Mini58Series.h.

## ◆ SYS_P2_MFP_MFP_Msk

#define SYS_P2_MFP_MFP_Msk (0xfful << SYS_P2_MFP_MFP_Pos)

SYS_T::P2_MFP: MFP Mask

Definition at line 10200 of file Mini58Series.h.

## ◆ SYS_P2_MFP_MFP_Pos

#define SYS_P2_MFP_MFP_Pos (0)

SYS_T::P2_MFP: MFP Position

Definition at line 10199 of file Mini58Series.h.

## ◆ SYS_P2_MFP_TYPE_Msk

#define SYS_P2_MFP_TYPE_Msk (0xfful << SYS_P2_MFP_TYPE_Pos)

SYS_T::P2_MFP: TYPE Mask

Definition at line 10218 of file Mini58Series.h.

## ◆ SYS_P2_MFP_TYPE_Pos

#define SYS_P2_MFP_TYPE_Pos (16)

SYS_T::P2_MFP: TYPE Position

Definition at line 10217 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT0_Msk

#define SYS_P3_MFP_ALT0_Msk (0x1ul << SYS_P3_MFP_ALT0_Pos)

SYS_T::P3_MFP: ALT0 Mask

Definition at line 10224 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT0_Pos

#define SYS_P3_MFP_ALT0_Pos (8)

SYS_T::P3_MFP: ALT0 Position

Definition at line 10223 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT1_Msk

#define SYS_P3_MFP_ALT1_Msk (0x1ul << SYS_P3_MFP_ALT1_Pos)

SYS_T::P3_MFP: ALT1 Mask

Definition at line 10227 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT1_Pos

#define SYS_P3_MFP_ALT1_Pos (9)

SYS_T::P3_MFP: ALT1 Position

Definition at line 10226 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT2_Msk

#define SYS_P3_MFP_ALT2_Msk (0x1ul << SYS_P3_MFP_ALT2_Pos)

SYS_T::P3_MFP: ALT2 Mask

Definition at line 10230 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT2_Pos

#define SYS_P3_MFP_ALT2_Pos (10)

SYS_T::P3_MFP: ALT2 Position

Definition at line 10229 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT4_Msk

#define SYS_P3_MFP_ALT4_Msk (0x1ul << SYS_P3_MFP_ALT4_Pos)

SYS_T::P3_MFP: ALT4 Mask

Definition at line 10233 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT4_Pos

#define SYS_P3_MFP_ALT4_Pos (12)

SYS_T::P3_MFP: ALT4 Position

Definition at line 10232 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT5_Msk

#define SYS_P3_MFP_ALT5_Msk (0x1ul << SYS_P3_MFP_ALT5_Pos)

SYS_T::P3_MFP: ALT5 Mask

Definition at line 10236 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT5_Pos

#define SYS_P3_MFP_ALT5_Pos (13)

SYS_T::P3_MFP: ALT5 Position

Definition at line 10235 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT6_Msk

#define SYS_P3_MFP_ALT6_Msk (0x1ul << SYS_P3_MFP_ALT6_Pos)

SYS_T::P3_MFP: ALT6 Mask

Definition at line 10239 of file Mini58Series.h.

## ◆ SYS_P3_MFP_ALT6_Pos

#define SYS_P3_MFP_ALT6_Pos (14)

SYS_T::P3_MFP: ALT6 Position

Definition at line 10238 of file Mini58Series.h.

## ◆ SYS_P3_MFP_MFP_Msk

#define SYS_P3_MFP_MFP_Msk (0xfful << SYS_P3_MFP_MFP_Pos)

SYS_T::P3_MFP: MFP Mask

Definition at line 10221 of file Mini58Series.h.

## ◆ SYS_P3_MFP_MFP_Pos

#define SYS_P3_MFP_MFP_Pos (0)

SYS_T::P3_MFP: MFP Position

Definition at line 10220 of file Mini58Series.h.

## ◆ SYS_P3_MFP_P32EXT_Msk

#define SYS_P3_MFP_P32EXT_Msk (0x1ul << SYS_P3_MFP_P32EXT_Pos)

SYS_T::P3_MFP: P32EXT Mask

Definition at line 10245 of file Mini58Series.h.

## ◆ SYS_P3_MFP_P32EXT_Pos

#define SYS_P3_MFP_P32EXT_Pos (26)

SYS_T::P3_MFP: P32EXT Position

Definition at line 10244 of file Mini58Series.h.

## ◆ SYS_P3_MFP_TYPE_Msk

#define SYS_P3_MFP_TYPE_Msk (0xfful << SYS_P3_MFP_TYPE_Pos)

SYS_T::P3_MFP: TYPE Mask

Definition at line 10242 of file Mini58Series.h.

## ◆ SYS_P3_MFP_TYPE_Pos

#define SYS_P3_MFP_TYPE_Pos (16)

SYS_T::P3_MFP: TYPE Position

Definition at line 10241 of file Mini58Series.h.

## ◆ SYS_P4_MFP_ALT6_Msk

#define SYS_P4_MFP_ALT6_Msk (0x1ul << SYS_P4_MFP_ALT6_Pos)

SYS_T::P4_MFP: ALT6 Mask

Definition at line 10251 of file Mini58Series.h.

## ◆ SYS_P4_MFP_ALT6_Pos

#define SYS_P4_MFP_ALT6_Pos (14)

SYS_T::P4_MFP: ALT6 Position

Definition at line 10250 of file Mini58Series.h.

## ◆ SYS_P4_MFP_ALT7_Msk

#define SYS_P4_MFP_ALT7_Msk (0x1ul << SYS_P4_MFP_ALT7_Pos)

SYS_T::P4_MFP: ALT7 Mask

Definition at line 10254 of file Mini58Series.h.

## ◆ SYS_P4_MFP_ALT7_Pos

#define SYS_P4_MFP_ALT7_Pos (15)

SYS_T::P4_MFP: ALT7 Position

Definition at line 10253 of file Mini58Series.h.

## ◆ SYS_P4_MFP_MFP_Msk

#define SYS_P4_MFP_MFP_Msk (0xfful << SYS_P4_MFP_MFP_Pos)

SYS_T::P4_MFP: MFP Mask

Definition at line 10248 of file Mini58Series.h.

## ◆ SYS_P4_MFP_MFP_Pos

#define SYS_P4_MFP_MFP_Pos (0)

SYS_T::P4_MFP: MFP Position

Definition at line 10247 of file Mini58Series.h.

## ◆ SYS_P4_MFP_TYPE_Msk

#define SYS_P4_MFP_TYPE_Msk (0xfful << SYS_P4_MFP_TYPE_Pos)

SYS_T::P4_MFP: TYPE Mask

Definition at line 10257 of file Mini58Series.h.

## ◆ SYS_P4_MFP_TYPE_Pos

#define SYS_P4_MFP_TYPE_Pos (16)

SYS_T::P4_MFP: TYPE Position

Definition at line 10256 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT0_Msk

#define SYS_P5_MFP_ALT0_Msk (0x1ul << SYS_P5_MFP_ALT0_Pos)

SYS_T::P5_MFP: ALT0 Mask

Definition at line 10263 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT0_Pos

#define SYS_P5_MFP_ALT0_Pos (8)

SYS_T::P5_MFP: ALT0 Position

Definition at line 10262 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT1_Msk

#define SYS_P5_MFP_ALT1_Msk (0x1ul << SYS_P5_MFP_ALT1_Pos)

SYS_T::P5_MFP: ALT1 Mask

Definition at line 10266 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT1_Pos

#define SYS_P5_MFP_ALT1_Pos (9)

SYS_T::P5_MFP: ALT1 Position

Definition at line 10265 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT2_Msk

#define SYS_P5_MFP_ALT2_Msk (0x1ul << SYS_P5_MFP_ALT2_Pos)

SYS_T::P5_MFP: ALT2 Mask

Definition at line 10269 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT2_Pos

#define SYS_P5_MFP_ALT2_Pos (10)

SYS_T::P5_MFP: ALT2 Position

Definition at line 10268 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT3_Msk

#define SYS_P5_MFP_ALT3_Msk (0x1ul << SYS_P5_MFP_ALT3_Pos)

SYS_T::P5_MFP: ALT3 Mask

Definition at line 10272 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT3_Pos

#define SYS_P5_MFP_ALT3_Pos (11)

SYS_T::P5_MFP: ALT3 Position

Definition at line 10271 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT4_Msk

#define SYS_P5_MFP_ALT4_Msk (0x1ul << SYS_P5_MFP_ALT4_Pos)

SYS_T::P5_MFP: ALT4 Mask

Definition at line 10275 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT4_Pos

#define SYS_P5_MFP_ALT4_Pos (12)

SYS_T::P5_MFP: ALT4 Position

Definition at line 10274 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT5_Msk

#define SYS_P5_MFP_ALT5_Msk (0x1ul << SYS_P5_MFP_ALT5_Pos)

SYS_T::P5_MFP: ALT5 Mask

Definition at line 10278 of file Mini58Series.h.

## ◆ SYS_P5_MFP_ALT5_Pos

#define SYS_P5_MFP_ALT5_Pos (13)

SYS_T::P5_MFP: ALT5 Position

Definition at line 10277 of file Mini58Series.h.

## ◆ SYS_P5_MFP_MFP_Msk

#define SYS_P5_MFP_MFP_Msk (0xfful << SYS_P5_MFP_MFP_Pos)

SYS_T::P5_MFP: MFP Mask

Definition at line 10260 of file Mini58Series.h.

## ◆ SYS_P5_MFP_MFP_Pos

#define SYS_P5_MFP_MFP_Pos (0)

SYS_T::P5_MFP: MFP Position

Definition at line 10259 of file Mini58Series.h.

## ◆ SYS_P5_MFP_TYPE_Msk

#define SYS_P5_MFP_TYPE_Msk (0xfful << SYS_P5_MFP_TYPE_Pos)

SYS_T::P5_MFP: TYPE Mask

Definition at line 10281 of file Mini58Series.h.

## ◆ SYS_P5_MFP_TYPE_Pos

#define SYS_P5_MFP_TYPE_Pos (16)

SYS_T::P5_MFP: TYPE Position

Definition at line 10280 of file Mini58Series.h.

## ◆ SYS_PDID_PDID_Msk

#define SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)

SYS_T::PDID: PDID Mask

Definition at line 10065 of file Mini58Series.h.

## ◆ SYS_PDID_PDID_Pos

#define SYS_PDID_PDID_Pos (0)

    @addtogroup SYS_CONST SYS Bit Field Definition
    Constant Definitions for SYS Controller

SYS_T::PDID: PDID Position

Definition at line 10064 of file Mini58Series.h.

## ◆ SYS_REGLCTL_REGLCTL_Msk

#define SYS_REGLCTL_REGLCTL_Msk (0xfful << SYS_REGLCTL_REGLCTL_Pos)

SYS_T::REGLCTL: REGLCTL Mask

Definition at line 10305 of file Mini58Series.h.

## ◆ SYS_REGLCTL_REGLCTL_Pos

#define SYS_REGLCTL_REGLCTL_Pos (0)

SYS_T::REGLCTL: REGLCTL Position

Definition at line 10304 of file Mini58Series.h.

## ◆ SYS_RSTSTS_BODRF_Msk

#define SYS_RSTSTS_BODRF_Msk (0x1ul << SYS_RSTSTS_BODRF_Pos)

SYS_T::RSTSTS: BODRF Mask

Definition at line 10077 of file Mini58Series.h.

## ◆ SYS_RSTSTS_BODRF_Pos

#define SYS_RSTSTS_BODRF_Pos (4)

SYS_T::RSTSTS: BODRF Position

Definition at line 10076 of file Mini58Series.h.

## ◆ SYS_RSTSTS_CPULKRF_Msk

#define SYS_RSTSTS_CPULKRF_Msk (0x1ul << SYS_RSTSTS_CPULKRF_Pos)

SYS_T::RSTSTS: CPULKRF Mask

Definition at line 10086 of file Mini58Series.h.

## ◆ SYS_RSTSTS_CPULKRF_Pos

#define SYS_RSTSTS_CPULKRF_Pos (8)

SYS_T::RSTSTS: CPULKRF Position

Definition at line 10085 of file Mini58Series.h.

## ◆ SYS_RSTSTS_CPURF_Msk

#define SYS_RSTSTS_CPURF_Msk (0x1ul << SYS_RSTSTS_CPURF_Pos)

SYS_T::RSTSTS: CPURF Mask

Definition at line 10083 of file Mini58Series.h.

## ◆ SYS_RSTSTS_CPURF_Pos

#define SYS_RSTSTS_CPURF_Pos (7)

SYS_T::RSTSTS: CPURF Position

Definition at line 10082 of file Mini58Series.h.

## ◆ SYS_RSTSTS_PINRF_Msk

#define SYS_RSTSTS_PINRF_Msk (0x1ul << SYS_RSTSTS_PINRF_Pos)

SYS_T::RSTSTS: PINRF Mask

Definition at line 10071 of file Mini58Series.h.

## ◆ SYS_RSTSTS_PINRF_Pos

#define SYS_RSTSTS_PINRF_Pos (1)

SYS_T::RSTSTS: PINRF Position

Definition at line 10070 of file Mini58Series.h.

## ◆ SYS_RSTSTS_PORF_Msk

#define SYS_RSTSTS_PORF_Msk (0x1ul << SYS_RSTSTS_PORF_Pos)

SYS_T::RSTSTS: PORF Mask

Definition at line 10068 of file Mini58Series.h.

## ◆ SYS_RSTSTS_PORF_Pos

#define SYS_RSTSTS_PORF_Pos (0)

SYS_T::RSTSTS: PORF Position

Definition at line 10067 of file Mini58Series.h.

## ◆ SYS_RSTSTS_SYSRF_Msk

#define SYS_RSTSTS_SYSRF_Msk (0x1ul << SYS_RSTSTS_SYSRF_Pos)

SYS_T::RSTSTS: SYSRF Mask

Definition at line 10080 of file Mini58Series.h.

## ◆ SYS_RSTSTS_SYSRF_Pos

#define SYS_RSTSTS_SYSRF_Pos (5)

SYS_T::RSTSTS: SYSRF Position

Definition at line 10079 of file Mini58Series.h.

## ◆ SYS_RSTSTS_WDTRF_Msk

#define SYS_RSTSTS_WDTRF_Msk (0x1ul << SYS_RSTSTS_WDTRF_Pos)

SYS_T::RSTSTS: WDTRF Mask

Definition at line 10074 of file Mini58Series.h.

## ◆ SYS_RSTSTS_WDTRF_Pos

#define SYS_RSTSTS_WDTRF_Pos (2)

SYS_T::RSTSTS: WDTRF Position

Definition at line 10073 of file Mini58Series.h.

## ◆ TIMER_CAP_CAPDAT_Msk [1/2]

#define TIMER_CAP_CAPDAT_Msk (0xfffffful << TIMER_CAP_CAPDAT_Pos)

TIMER_T::CAP: CAPDAT Mask

Definition at line 10659 of file Mini58Series.h.

## ◆ TIMER_CAP_CAPDAT_Msk [2/2]

#define TIMER_CAP_CAPDAT_Msk (0xfffffful << TIMER_CAP_CAPDAT_Pos)

TIMER_T::CAP: CAPDAT Mask

Definition at line 10659 of file Mini58Series.h.

## ◆ TIMER_CAP_CAPDAT_Pos [1/2]

#define TIMER_CAP_CAPDAT_Pos (0)

TIMER_T::CAP: CAPDAT Position

Definition at line 10658 of file Mini58Series.h.

## ◆ TIMER_CAP_CAPDAT_Pos [2/2]

#define TIMER_CAP_CAPDAT_Pos (0)

TIMER_T::CAP: CAPDAT Position

Definition at line 10658 of file Mini58Series.h.

## ◆ TIMER_CMP_CMPDAT_Msk [1/2]

#define TIMER_CMP_CMPDAT_Msk (0xfffffful << TIMER_CMP_CMPDAT_Pos)

TIMER_T::CMP: CMPDAT Mask

Definition at line 10647 of file Mini58Series.h.

## ◆ TIMER_CMP_CMPDAT_Msk [2/2]

#define TIMER_CMP_CMPDAT_Msk (0xfffffful << TIMER_CMP_CMPDAT_Pos)

TIMER_T::CMP: CMPDAT Mask

Definition at line 10647 of file Mini58Series.h.

## ◆ TIMER_CMP_CMPDAT_Pos [1/2]

#define TIMER_CMP_CMPDAT_Pos (0)

TIMER_T::CMP: CMPDAT Position

Definition at line 10646 of file Mini58Series.h.

## ◆ TIMER_CMP_CMPDAT_Pos [2/2]

#define TIMER_CMP_CMPDAT_Pos (0)

TIMER_T::CMP: CMPDAT Position

Definition at line 10646 of file Mini58Series.h.

## ◆ TIMER_CNT_CNT_Msk [1/2]

#define TIMER_CNT_CNT_Msk (0xfffffful << TIMER_CNT_CNT_Pos)

TIMER_T::CNT: CNT Mask

Definition at line 10656 of file Mini58Series.h.

## ◆ TIMER_CNT_CNT_Msk [2/2]

#define TIMER_CNT_CNT_Msk (0xfffffful << TIMER_CNT_CNT_Pos)

TIMER_T::CNT: CNT Mask

Definition at line 10656 of file Mini58Series.h.

## ◆ TIMER_CNT_CNT_Pos [1/2]

#define TIMER_CNT_CNT_Pos (0)

TIMER_T::CNT: CNT Position

Definition at line 10655 of file Mini58Series.h.

## ◆ TIMER_CNT_CNT_Pos [2/2]

#define TIMER_CNT_CNT_Pos (0)

TIMER_T::CNT: CNT Position

Definition at line 10655 of file Mini58Series.h.

## ◆ TIMER_CTL_ACTSTS_Msk [1/2]

#define TIMER_CTL_ACTSTS_Msk (0x1ul << TIMER_CTL_ACTSTS_Pos)

TIMER_T::CTL: ACTSTS Mask

Definition at line 10629 of file Mini58Series.h.

## ◆ TIMER_CTL_ACTSTS_Msk [2/2]

#define TIMER_CTL_ACTSTS_Msk (0x1ul << TIMER_CTL_ACTSTS_Pos)

TIMER_T::CTL: ACTSTS Mask

Definition at line 10629 of file Mini58Series.h.

## ◆ TIMER_CTL_ACTSTS_Pos [1/2]

#define TIMER_CTL_ACTSTS_Pos (25)

TIMER_T::CTL: ACTSTS Position

Definition at line 10628 of file Mini58Series.h.

## ◆ TIMER_CTL_ACTSTS_Pos [2/2]

#define TIMER_CTL_ACTSTS_Pos (25)

TIMER_T::CTL: ACTSTS Position

Definition at line 10628 of file Mini58Series.h.

## ◆ TIMER_CTL_CAPSRC_Msk [1/2]

#define TIMER_CTL_CAPSRC_Msk (0x1ul << TIMER_CTL_CAPSRC_Pos)

TIMER_T::CTL: CAPSRC Mask

Definition at line 10620 of file Mini58Series.h.

## ◆ TIMER_CTL_CAPSRC_Msk [2/2]

#define TIMER_CTL_CAPSRC_Msk (0x1ul << TIMER_CTL_CAPSRC_Pos)

TIMER_T::CTL: CAPSRC Mask

Definition at line 10620 of file Mini58Series.h.

## ◆ TIMER_CTL_CAPSRC_Pos [1/2]

#define TIMER_CTL_CAPSRC_Pos (19)

TIMER_T::CTL: CAPSRC Position

Definition at line 10619 of file Mini58Series.h.

## ◆ TIMER_CTL_CAPSRC_Pos [2/2]

#define TIMER_CTL_CAPSRC_Pos (19)

TIMER_T::CTL: CAPSRC Position

Definition at line 10619 of file Mini58Series.h.

## ◆ TIMER_CTL_CMPCTL_Msk [1/2]

#define TIMER_CTL_CMPCTL_Msk (0x1ul << TIMER_CTL_CMPCTL_Pos)

TIMER_T::CTL: CMPCTL Mask

Definition at line 10614 of file Mini58Series.h.

## ◆ TIMER_CTL_CMPCTL_Msk [2/2]

#define TIMER_CTL_CMPCTL_Msk (0x1ul << TIMER_CTL_CMPCTL_Pos)

TIMER_T::CTL: CMPCTL Mask

Definition at line 10614 of file Mini58Series.h.

## ◆ TIMER_CTL_CMPCTL_Pos [1/2]

#define TIMER_CTL_CMPCTL_Pos (17)

TIMER_T::CTL: CMPCTL Position

Definition at line 10613 of file Mini58Series.h.

## ◆ TIMER_CTL_CMPCTL_Pos [2/2]

#define TIMER_CTL_CMPCTL_Pos (17)

TIMER_T::CTL: CMPCTL Position

Definition at line 10613 of file Mini58Series.h.

## ◆ TIMER_CTL_CNTEN_Msk [1/2]

#define TIMER_CTL_CNTEN_Msk (0x1ul << TIMER_CTL_CNTEN_Pos)

TIMER_T::CTL: CNTEN Mask

Definition at line 10641 of file Mini58Series.h.

## ◆ TIMER_CTL_CNTEN_Msk [2/2]

#define TIMER_CTL_CNTEN_Msk (0x1ul << TIMER_CTL_CNTEN_Pos)

TIMER_T::CTL: CNTEN Mask

Definition at line 10641 of file Mini58Series.h.

## ◆ TIMER_CTL_CNTEN_Pos [1/2]

#define TIMER_CTL_CNTEN_Pos (30)

TIMER_T::CTL: CNTEN Position

Definition at line 10640 of file Mini58Series.h.

## ◆ TIMER_CTL_CNTEN_Pos [2/2]

#define TIMER_CTL_CNTEN_Pos (30)

TIMER_T::CTL: CNTEN Position

Definition at line 10640 of file Mini58Series.h.

## ◆ TIMER_CTL_EXTCNTEN_Msk [1/2]

#define TIMER_CTL_EXTCNTEN_Msk (0x1ul << TIMER_CTL_EXTCNTEN_Pos)

TIMER_T::CTL: EXTCNTEN Mask

Definition at line 10626 of file Mini58Series.h.

## ◆ TIMER_CTL_EXTCNTEN_Msk [2/2]

#define TIMER_CTL_EXTCNTEN_Msk (0x1ul << TIMER_CTL_EXTCNTEN_Pos)

TIMER_T::CTL: EXTCNTEN Mask

Definition at line 10626 of file Mini58Series.h.

## ◆ TIMER_CTL_EXTCNTEN_Pos [1/2]

#define TIMER_CTL_EXTCNTEN_Pos (24)

TIMER_T::CTL: EXTCNTEN Position

Definition at line 10625 of file Mini58Series.h.

## ◆ TIMER_CTL_EXTCNTEN_Pos [2/2]

#define TIMER_CTL_EXTCNTEN_Pos (24)

TIMER_T::CTL: EXTCNTEN Position

Definition at line 10625 of file Mini58Series.h.

## ◆ TIMER_CTL_ICEDEBUG_Msk [1/2]

#define TIMER_CTL_ICEDEBUG_Msk (0x1ul << TIMER_CTL_ICEDEBUG_Pos)

TIMER_T::CTL: ICEDEBUG Mask

Definition at line 10644 of file Mini58Series.h.

## ◆ TIMER_CTL_ICEDEBUG_Msk [2/2]

#define TIMER_CTL_ICEDEBUG_Msk (0x1ul << TIMER_CTL_ICEDEBUG_Pos)

TIMER_T::CTL: ICEDEBUG Mask

Definition at line 10644 of file Mini58Series.h.

## ◆ TIMER_CTL_ICEDEBUG_Pos [1/2]

#define TIMER_CTL_ICEDEBUG_Pos (31)

TIMER_T::CTL: ICEDEBUG Position

Definition at line 10643 of file Mini58Series.h.

## ◆ TIMER_CTL_ICEDEBUG_Pos [2/2]

#define TIMER_CTL_ICEDEBUG_Pos (31)

TIMER_T::CTL: ICEDEBUG Position

Definition at line 10643 of file Mini58Series.h.

## ◆ TIMER_CTL_INTEN_Msk [1/2]

#define TIMER_CTL_INTEN_Msk (0x1ul << TIMER_CTL_INTEN_Pos)

TIMER_T::CTL: INTEN Mask

Definition at line 10638 of file Mini58Series.h.

## ◆ TIMER_CTL_INTEN_Msk [2/2]

#define TIMER_CTL_INTEN_Msk (0x1ul << TIMER_CTL_INTEN_Pos)

TIMER_T::CTL: INTEN Mask

Definition at line 10638 of file Mini58Series.h.

## ◆ TIMER_CTL_INTEN_Pos [1/2]

#define TIMER_CTL_INTEN_Pos (29)

TIMER_T::CTL: INTEN Position

Definition at line 10637 of file Mini58Series.h.

## ◆ TIMER_CTL_INTEN_Pos [2/2]

#define TIMER_CTL_INTEN_Pos (29)

TIMER_T::CTL: INTEN Position

Definition at line 10637 of file Mini58Series.h.

## ◆ TIMER_CTL_OPMODE_Msk [1/2]

#define TIMER_CTL_OPMODE_Msk (0x3ul << TIMER_CTL_OPMODE_Pos)

TIMER_T::CTL: OPMODE Mask

Definition at line 10635 of file Mini58Series.h.

## ◆ TIMER_CTL_OPMODE_Msk [2/2]

#define TIMER_CTL_OPMODE_Msk (0x3ul << TIMER_CTL_OPMODE_Pos)

TIMER_T::CTL: OPMODE Mask

Definition at line 10635 of file Mini58Series.h.

## ◆ TIMER_CTL_OPMODE_Pos [1/2]

#define TIMER_CTL_OPMODE_Pos (27)

TIMER_T::CTL: OPMODE Position

Definition at line 10634 of file Mini58Series.h.

## ◆ TIMER_CTL_OPMODE_Pos [2/2]

#define TIMER_CTL_OPMODE_Pos (27)

TIMER_T::CTL: OPMODE Position

Definition at line 10634 of file Mini58Series.h.

## ◆ TIMER_CTL_PSC_Msk [1/2]

#define TIMER_CTL_PSC_Msk (0xfful << TIMER_CTL_PSC_Pos)

TIMER_T::CTL: PSC Mask

Definition at line 10611 of file Mini58Series.h.

## ◆ TIMER_CTL_PSC_Msk [2/2]

#define TIMER_CTL_PSC_Msk (0xfful << TIMER_CTL_PSC_Pos)

TIMER_T::CTL: PSC Mask

Definition at line 10611 of file Mini58Series.h.

## ◆ TIMER_CTL_PSC_Pos [1/2]

#define TIMER_CTL_PSC_Pos (0)

    @addtogroup TIMER_CONST TIMER Bit Field Definition
    Constant Definitions for TIMER Controller

TIMER_T::CTL: PSC Position

TIMER_T::CTL: PSC Position

Definition at line 10610 of file Mini58Series.h.

## ◆ TIMER_CTL_PSC_Pos [2/2]

#define TIMER_CTL_PSC_Pos (0)

    @addtogroup TIMER_CONST TIMER Bit Field Definition
    Constant Definitions for TIMER Controller

TIMER_T::CTL: PSC Position

TIMER_T::CTL: PSC Position

Definition at line 10610 of file Mini58Series.h.

## ◆ TIMER_CTL_RSTCNT_Msk [1/2]

#define TIMER_CTL_RSTCNT_Msk (0x1ul << TIMER_CTL_RSTCNT_Pos)

TIMER_T::CTL: RSTCNT Mask

Definition at line 10632 of file Mini58Series.h.

## ◆ TIMER_CTL_RSTCNT_Msk [2/2]

#define TIMER_CTL_RSTCNT_Msk (0x1ul << TIMER_CTL_RSTCNT_Pos)

TIMER_T::CTL: RSTCNT Mask

Definition at line 10632 of file Mini58Series.h.

## ◆ TIMER_CTL_RSTCNT_Pos [1/2]

#define TIMER_CTL_RSTCNT_Pos (26)

TIMER_T::CTL: RSTCNT Position

Definition at line 10631 of file Mini58Series.h.

## ◆ TIMER_CTL_RSTCNT_Pos [2/2]

#define TIMER_CTL_RSTCNT_Pos (26)

TIMER_T::CTL: RSTCNT Position

Definition at line 10631 of file Mini58Series.h.

## ◆ TIMER_CTL_TGLPINSEL_Msk [1/2]

#define TIMER_CTL_TGLPINSEL_Msk (0x1ul << TIMER_CTL_TGLPINSEL_Pos)

TIMER_T::CTL: TGLPINSEL Mask

Definition at line 10617 of file Mini58Series.h.

## ◆ TIMER_CTL_TGLPINSEL_Msk [2/2]

#define TIMER_CTL_TGLPINSEL_Msk (0x1ul << TIMER_CTL_TGLPINSEL_Pos)

TIMER_T::CTL: TGLPINSEL Mask

Definition at line 10617 of file Mini58Series.h.

## ◆ TIMER_CTL_TGLPINSEL_Pos [1/2]

#define TIMER_CTL_TGLPINSEL_Pos (18)

TIMER_T::CTL: TGLPINSEL Position

Definition at line 10616 of file Mini58Series.h.

## ◆ TIMER_CTL_TGLPINSEL_Pos [2/2]

#define TIMER_CTL_TGLPINSEL_Pos (18)

TIMER_T::CTL: TGLPINSEL Position

Definition at line 10616 of file Mini58Series.h.

## ◆ TIMER_CTL_WKEN_Msk [1/2]

#define TIMER_CTL_WKEN_Msk (0x1ul << TIMER_CTL_WKEN_Pos)

TIMER_T::CTL: WKEN Mask

Definition at line 10623 of file Mini58Series.h.

## ◆ TIMER_CTL_WKEN_Msk [2/2]

#define TIMER_CTL_WKEN_Msk (0x1ul << TIMER_CTL_WKEN_Pos)

TIMER_T::CTL: WKEN Mask

Definition at line 10623 of file Mini58Series.h.

## ◆ TIMER_CTL_WKEN_Pos [1/2]

#define TIMER_CTL_WKEN_Pos (23)

TIMER_T::CTL: WKEN Position

Definition at line 10622 of file Mini58Series.h.

## ◆ TIMER_CTL_WKEN_Pos [2/2]

#define TIMER_CTL_WKEN_Pos (23)

TIMER_T::CTL: WKEN Position

Definition at line 10622 of file Mini58Series.h.

## ◆ TIMER_EINTSTS_CAPIF_Msk [1/2]

#define TIMER_EINTSTS_CAPIF_Msk (0x1ul << TIMER_EINTSTS_CAPIF_Pos)

TIMER_T::EINTSTS: CAPIF Mask

Definition at line 10689 of file Mini58Series.h.

## ◆ TIMER_EINTSTS_CAPIF_Msk [2/2]

#define TIMER_EINTSTS_CAPIF_Msk (0x1ul << TIMER_EINTSTS_CAPIF_Pos)

TIMER_T::EINTSTS: CAPIF Mask

Definition at line 10689 of file Mini58Series.h.

## ◆ TIMER_EINTSTS_CAPIF_Pos [1/2]

#define TIMER_EINTSTS_CAPIF_Pos (0)

TIMER_T::EINTSTS: CAPIF Position

Definition at line 10688 of file Mini58Series.h.

## ◆ TIMER_EINTSTS_CAPIF_Pos [2/2]

#define TIMER_EINTSTS_CAPIF_Pos (0)

TIMER_T::EINTSTS: CAPIF Position

Definition at line 10688 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_ACMPSSEL_Msk [1/2]

#define TIMER_EXTCTL_ACMPSSEL_Msk (0x1ul << TIMER_EXTCTL_ACMPSSEL_Pos)

TIMER_T::EXTCTL: ACMPSSEL Mask

Definition at line 10686 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_ACMPSSEL_Msk [2/2]

#define TIMER_EXTCTL_ACMPSSEL_Msk (0x1ul << TIMER_EXTCTL_ACMPSSEL_Pos)

TIMER_T::EXTCTL: ACMPSSEL Mask

Definition at line 10686 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_ACMPSSEL_Pos [1/2]

#define TIMER_EXTCTL_ACMPSSEL_Pos (9)

TIMER_T::EXTCTL: ACMPSSEL Position

Definition at line 10685 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_ACMPSSEL_Pos [2/2]

#define TIMER_EXTCTL_ACMPSSEL_Pos (9)

TIMER_T::EXTCTL: ACMPSSEL Position

Definition at line 10685 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPDBEN_Msk [1/2]

#define TIMER_EXTCTL_CAPDBEN_Msk (0x1ul << TIMER_EXTCTL_CAPDBEN_Pos)

TIMER_T::EXTCTL: CAPDBEN Mask

Definition at line 10677 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPDBEN_Msk [2/2]

#define TIMER_EXTCTL_CAPDBEN_Msk (0x1ul << TIMER_EXTCTL_CAPDBEN_Pos)

TIMER_T::EXTCTL: CAPDBEN Mask

Definition at line 10677 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPDBEN_Pos [1/2]

#define TIMER_EXTCTL_CAPDBEN_Pos (6)

TIMER_T::EXTCTL: CAPDBEN Position

Definition at line 10676 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPDBEN_Pos [2/2]

#define TIMER_EXTCTL_CAPDBEN_Pos (6)

TIMER_T::EXTCTL: CAPDBEN Position

Definition at line 10676 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEDGE_Msk [1/2]

#define TIMER_EXTCTL_CAPEDGE_Msk (0x3ul << TIMER_EXTCTL_CAPEDGE_Pos)

TIMER_T::EXTCTL: CAPEDGE Mask

Definition at line 10665 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEDGE_Msk [2/2]

#define TIMER_EXTCTL_CAPEDGE_Msk (0x3ul << TIMER_EXTCTL_CAPEDGE_Pos)

TIMER_T::EXTCTL: CAPEDGE Mask

Definition at line 10665 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEDGE_Pos [1/2]

#define TIMER_EXTCTL_CAPEDGE_Pos (1)

TIMER_T::EXTCTL: CAPEDGE Position

Definition at line 10664 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEDGE_Pos [2/2]

#define TIMER_EXTCTL_CAPEDGE_Pos (1)

TIMER_T::EXTCTL: CAPEDGE Position

Definition at line 10664 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEN_Msk [1/2]

#define TIMER_EXTCTL_CAPEN_Msk (0x1ul << TIMER_EXTCTL_CAPEN_Pos)

TIMER_T::EXTCTL: CAPEN Mask

Definition at line 10668 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEN_Msk [2/2]

#define TIMER_EXTCTL_CAPEN_Msk (0x1ul << TIMER_EXTCTL_CAPEN_Pos)

TIMER_T::EXTCTL: CAPEN Mask

Definition at line 10668 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEN_Pos [1/2]

#define TIMER_EXTCTL_CAPEN_Pos (3)

TIMER_T::EXTCTL: CAPEN Position

Definition at line 10667 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPEN_Pos [2/2]

#define TIMER_EXTCTL_CAPEN_Pos (3)

TIMER_T::EXTCTL: CAPEN Position

Definition at line 10667 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPFUNCS_Msk [1/2]

#define TIMER_EXTCTL_CAPFUNCS_Msk (0x1ul << TIMER_EXTCTL_CAPFUNCS_Pos)

TIMER_T::EXTCTL: CAPFUNCS Mask

Definition at line 10671 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPFUNCS_Msk [2/2]

#define TIMER_EXTCTL_CAPFUNCS_Msk (0x1ul << TIMER_EXTCTL_CAPFUNCS_Pos)

TIMER_T::EXTCTL: CAPFUNCS Mask

Definition at line 10671 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPFUNCS_Pos [1/2]

#define TIMER_EXTCTL_CAPFUNCS_Pos (4)

TIMER_T::EXTCTL: CAPFUNCS Position

Definition at line 10670 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPFUNCS_Pos [2/2]

#define TIMER_EXTCTL_CAPFUNCS_Pos (4)

TIMER_T::EXTCTL: CAPFUNCS Position

Definition at line 10670 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPIEN_Msk [1/2]

#define TIMER_EXTCTL_CAPIEN_Msk (0x1ul << TIMER_EXTCTL_CAPIEN_Pos)

TIMER_T::EXTCTL: CAPIEN Mask

Definition at line 10674 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPIEN_Msk [2/2]

#define TIMER_EXTCTL_CAPIEN_Msk (0x1ul << TIMER_EXTCTL_CAPIEN_Pos)

TIMER_T::EXTCTL: CAPIEN Mask

Definition at line 10674 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPIEN_Pos [1/2]

#define TIMER_EXTCTL_CAPIEN_Pos (5)

TIMER_T::EXTCTL: CAPIEN Position

Definition at line 10673 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPIEN_Pos [2/2]

#define TIMER_EXTCTL_CAPIEN_Pos (5)

TIMER_T::EXTCTL: CAPIEN Position

Definition at line 10673 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPSEL_Msk [1/2]

#define TIMER_EXTCTL_CAPSEL_Msk (0x1ul << TIMER_EXTCTL_CAPSEL_Pos)

TIMER_T::EXTCTL: CAPSEL Mask

Definition at line 10683 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPSEL_Msk [2/2]

#define TIMER_EXTCTL_CAPSEL_Msk (0x1ul << TIMER_EXTCTL_CAPSEL_Pos)

TIMER_T::EXTCTL: CAPSEL Mask

Definition at line 10683 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPSEL_Pos [1/2]

#define TIMER_EXTCTL_CAPSEL_Pos (8)

TIMER_T::EXTCTL: CAPSEL Position

Definition at line 10682 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CAPSEL_Pos [2/2]

#define TIMER_EXTCTL_CAPSEL_Pos (8)

TIMER_T::EXTCTL: CAPSEL Position

Definition at line 10682 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTDBEN_Msk [1/2]

#define TIMER_EXTCTL_CNTDBEN_Msk (0x1ul << TIMER_EXTCTL_CNTDBEN_Pos)

TIMER_T::EXTCTL: CNTDBEN Mask

Definition at line 10680 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTDBEN_Msk [2/2]

#define TIMER_EXTCTL_CNTDBEN_Msk (0x1ul << TIMER_EXTCTL_CNTDBEN_Pos)

TIMER_T::EXTCTL: CNTDBEN Mask

Definition at line 10680 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTDBEN_Pos [1/2]

#define TIMER_EXTCTL_CNTDBEN_Pos (7)

TIMER_T::EXTCTL: CNTDBEN Position

Definition at line 10679 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTDBEN_Pos [2/2]

#define TIMER_EXTCTL_CNTDBEN_Pos (7)

TIMER_T::EXTCTL: CNTDBEN Position

Definition at line 10679 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTPHASE_Msk [1/2]

#define TIMER_EXTCTL_CNTPHASE_Msk (0x1ul << TIMER_EXTCTL_CNTPHASE_Pos)

TIMER_T::EXTCTL: CNTPHASE Mask

Definition at line 10662 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTPHASE_Msk [2/2]

#define TIMER_EXTCTL_CNTPHASE_Msk (0x1ul << TIMER_EXTCTL_CNTPHASE_Pos)

TIMER_T::EXTCTL: CNTPHASE Mask

Definition at line 10662 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTPHASE_Pos [1/2]

#define TIMER_EXTCTL_CNTPHASE_Pos (0)

TIMER_T::EXTCTL: CNTPHASE Position

Definition at line 10661 of file Mini58Series.h.

## ◆ TIMER_EXTCTL_CNTPHASE_Pos [2/2]

#define TIMER_EXTCTL_CNTPHASE_Pos (0)

TIMER_T::EXTCTL: CNTPHASE Position

Definition at line 10661 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TIF_Msk [1/2]

#define TIMER_INTSTS_TIF_Msk (0x1ul << TIMER_INTSTS_TIF_Pos)

TIMER_T::INTSTS: TIF Mask

Definition at line 10650 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TIF_Msk [2/2]

#define TIMER_INTSTS_TIF_Msk (0x1ul << TIMER_INTSTS_TIF_Pos)

TIMER_T::INTSTS: TIF Mask

Definition at line 10650 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TIF_Pos [1/2]

#define TIMER_INTSTS_TIF_Pos (0)

TIMER_T::INTSTS: TIF Position

Definition at line 10649 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TIF_Pos [2/2]

#define TIMER_INTSTS_TIF_Pos (0)

TIMER_T::INTSTS: TIF Position

Definition at line 10649 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TWKF_Msk [1/2]

#define TIMER_INTSTS_TWKF_Msk (0x1ul << TIMER_INTSTS_TWKF_Pos)

TIMER_T::INTSTS: TWKF Mask

Definition at line 10653 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TWKF_Msk [2/2]

#define TIMER_INTSTS_TWKF_Msk (0x1ul << TIMER_INTSTS_TWKF_Pos)

TIMER_T::INTSTS: TWKF Mask

Definition at line 10653 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TWKF_Pos [1/2]

#define TIMER_INTSTS_TWKF_Pos (1)

TIMER_T::INTSTS: TWKF Position

Definition at line 10652 of file Mini58Series.h.

## ◆ TIMER_INTSTS_TWKF_Pos [2/2]

#define TIMER_INTSTS_TWKF_Pos (1)

TIMER_T::INTSTS: TWKF Position

Definition at line 10652 of file Mini58Series.h.

## ◆ UART_ALTCTL_ADDRDEN_Msk

#define UART_ALTCTL_ADDRDEN_Msk (0x1ul << UART_ALTCTL_ADDRDEN_Pos)

UART_T::ALTCTL: ADDRDEN Mask

Definition at line 11364 of file Mini58Series.h.

## ◆ UART_ALTCTL_ADDRDEN_Pos

#define UART_ALTCTL_ADDRDEN_Pos (15)

UART_T::ALTCTL: ADDRDEN Position

Definition at line 11363 of file Mini58Series.h.

## ◆ UART_ALTCTL_ADDRMV_Msk

#define UART_ALTCTL_ADDRMV_Msk (0xfful << UART_ALTCTL_ADDRMV_Pos)

UART_T::ALTCTL: ADDRMV Mask

Definition at line 11367 of file Mini58Series.h.

## ◆ UART_ALTCTL_ADDRMV_Pos

#define UART_ALTCTL_ADDRMV_Pos (24)

UART_T::ALTCTL: ADDRMV Position

Definition at line 11366 of file Mini58Series.h.

## ◆ UART_ALTCTL_RS485_AAD_Msk

#define UART_ALTCTL_RS485_AAD_Msk (0x1ul << UART_ALTCTL_RS485_AAD_Pos)

UART_T::ALTCTL: RS485_AAD Mask

Definition at line 11358 of file Mini58Series.h.

## ◆ UART_ALTCTL_RS485_AAD_Pos

#define UART_ALTCTL_RS485_AAD_Pos (9)

UART_T::ALTCTL: RS485_AAD Position

Definition at line 11357 of file Mini58Series.h.

## ◆ UART_ALTCTL_RS485_AUD_Msk

#define UART_ALTCTL_RS485_AUD_Msk (0x1ul << UART_ALTCTL_RS485_AUD_Pos)

UART_T::ALTCTL: RS485_AUD Mask

Definition at line 11361 of file Mini58Series.h.

## ◆ UART_ALTCTL_RS485_AUD_Pos

#define UART_ALTCTL_RS485_AUD_Pos (10)

UART_T::ALTCTL: RS485_AUD Position

Definition at line 11360 of file Mini58Series.h.

## ◆ UART_ALTCTL_RS485_NMM_Msk

#define UART_ALTCTL_RS485_NMM_Msk (0x1ul << UART_ALTCTL_RS485_NMM_Pos)

UART_T::ALTCTL: RS485_NMM Mask

Definition at line 11355 of file Mini58Series.h.

## ◆ UART_ALTCTL_RS485_NMM_Pos

#define UART_ALTCTL_RS485_NMM_Pos (8)

UART_T::ALTCTL: RS485_NMM Position

Definition at line 11354 of file Mini58Series.h.

## ◆ UART_BAUD_BAUDM0_Msk

#define UART_BAUD_BAUDM0_Msk (0x1ul << UART_BAUD_BAUDM0_Pos)

UART_T::BAUD: BAUDM0 Mask

Definition at line 11340 of file Mini58Series.h.

## ◆ UART_BAUD_BAUDM0_Pos

#define UART_BAUD_BAUDM0_Pos (28)

UART_T::BAUD: BAUDM0 Position

Definition at line 11339 of file Mini58Series.h.

## ◆ UART_BAUD_BAUDM1_Msk

#define UART_BAUD_BAUDM1_Msk (0x1ul << UART_BAUD_BAUDM1_Pos)

UART_T::BAUD: BAUDM1 Mask

Definition at line 11343 of file Mini58Series.h.

## ◆ UART_BAUD_BAUDM1_Pos

#define UART_BAUD_BAUDM1_Pos (29)

UART_T::BAUD: BAUDM1 Position

Definition at line 11342 of file Mini58Series.h.

## ◆ UART_BAUD_BRD_Msk

#define UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)

UART_T::BAUD: BRD Mask

Definition at line 11334 of file Mini58Series.h.

## ◆ UART_BAUD_BRD_Pos

#define UART_BAUD_BRD_Pos (0)

UART_T::BAUD: BRD Position

Definition at line 11333 of file Mini58Series.h.

## ◆ UART_BAUD_EDIVM1_Msk

#define UART_BAUD_EDIVM1_Msk (0xful << UART_BAUD_EDIVM1_Pos)

UART_T::BAUD: EDIVM1 Mask

Definition at line 11337 of file Mini58Series.h.

## ◆ UART_BAUD_EDIVM1_Pos

#define UART_BAUD_EDIVM1_Pos (24)

UART_T::BAUD: EDIVM1 Position

Definition at line 11336 of file Mini58Series.h.

## ◆ UART_DAT_DAT_Msk

#define UART_DAT_DAT_Msk (0xfful << UART_DAT_DAT_Pos)

UART_T::DAT: DAT Mask

Definition at line 11166 of file Mini58Series.h.

## ◆ UART_DAT_DAT_Pos

#define UART_DAT_DAT_Pos (0)

    @addtogroup UART_CONST UART Bit Field Definition
    Constant Definitions for UART Controller

UART_T::DAT: DAT Position

Definition at line 11165 of file Mini58Series.h.

## ◆ UART_FIFO_RFITL_Msk

#define UART_FIFO_RFITL_Msk (0xful << UART_FIFO_RFITL_Pos)

UART_T::FIFO: RFITL Mask

Definition at line 11205 of file Mini58Series.h.

## ◆ UART_FIFO_RFITL_Pos

#define UART_FIFO_RFITL_Pos (4)

UART_T::FIFO: RFITL Position

Definition at line 11204 of file Mini58Series.h.

## ◆ UART_FIFO_RTSTRGLV_Msk

#define UART_FIFO_RTSTRGLV_Msk (0xful << UART_FIFO_RTSTRGLV_Pos)

UART_T::FIFO: RTSTRGLV Mask

Definition at line 11211 of file Mini58Series.h.

## ◆ UART_FIFO_RTSTRGLV_Pos

#define UART_FIFO_RTSTRGLV_Pos (16)

UART_T::FIFO: RTSTRGLV Position

Definition at line 11210 of file Mini58Series.h.

## ◆ UART_FIFO_RXOFF_Msk

#define UART_FIFO_RXOFF_Msk (0x1ul << UART_FIFO_RXOFF_Pos)

UART_T::FIFO: RXOFF Mask

Definition at line 11208 of file Mini58Series.h.

## ◆ UART_FIFO_RXOFF_Pos

#define UART_FIFO_RXOFF_Pos (8)

UART_T::FIFO: RXOFF Position

Definition at line 11207 of file Mini58Series.h.

## ◆ UART_FIFO_RXRST_Msk

#define UART_FIFO_RXRST_Msk (0x1ul << UART_FIFO_RXRST_Pos)

UART_T::FIFO: RXRST Mask

Definition at line 11199 of file Mini58Series.h.

## ◆ UART_FIFO_RXRST_Pos

#define UART_FIFO_RXRST_Pos (1)

UART_T::FIFO: RXRST Position

Definition at line 11198 of file Mini58Series.h.

## ◆ UART_FIFO_TXRST_Msk

#define UART_FIFO_TXRST_Msk (0x1ul << UART_FIFO_TXRST_Pos)

UART_T::FIFO: TXRST Mask

Definition at line 11202 of file Mini58Series.h.

## ◆ UART_FIFO_TXRST_Pos

#define UART_FIFO_TXRST_Pos (2)

UART_T::FIFO: TXRST Position

Definition at line 11201 of file Mini58Series.h.

## ◆ UART_FIFOSTS_ADDRDETF_Msk

#define UART_FIFOSTS_ADDRDETF_Msk (0x1ul << UART_FIFOSTS_ADDRDETF_Pos)

UART_T::FIFOSTS: ADDRDETF Mask

Definition at line 11253 of file Mini58Series.h.

## ◆ UART_FIFOSTS_ADDRDETF_Pos

#define UART_FIFOSTS_ADDRDETF_Pos (3)

UART_T::FIFOSTS: ADDRDETF Position

Definition at line 11252 of file Mini58Series.h.

## ◆ UART_FIFOSTS_BIF_Msk

#define UART_FIFOSTS_BIF_Msk (0x1ul << UART_FIFOSTS_BIF_Pos)

UART_T::FIFOSTS: BIF Mask

Definition at line 11262 of file Mini58Series.h.

## ◆ UART_FIFOSTS_BIF_Pos

#define UART_FIFOSTS_BIF_Pos (6)

UART_T::FIFOSTS: BIF Position

Definition at line 11261 of file Mini58Series.h.

## ◆ UART_FIFOSTS_FEF_Msk

#define UART_FIFOSTS_FEF_Msk (0x1ul << UART_FIFOSTS_FEF_Pos)

UART_T::FIFOSTS: FEF Mask

Definition at line 11259 of file Mini58Series.h.

## ◆ UART_FIFOSTS_FEF_Pos

#define UART_FIFOSTS_FEF_Pos (5)

UART_T::FIFOSTS: FEF Position

Definition at line 11258 of file Mini58Series.h.

## ◆ UART_FIFOSTS_PEF_Msk

#define UART_FIFOSTS_PEF_Msk (0x1ul << UART_FIFOSTS_PEF_Pos)

UART_T::FIFOSTS: PEF Mask

Definition at line 11256 of file Mini58Series.h.

## ◆ UART_FIFOSTS_PEF_Pos

#define UART_FIFOSTS_PEF_Pos (4)

UART_T::FIFOSTS: PEF Position

Definition at line 11255 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXEMPTY_Msk

#define UART_FIFOSTS_RXEMPTY_Msk (0x1ul << UART_FIFOSTS_RXEMPTY_Pos)

UART_T::FIFOSTS: RXEMPTY Mask

Definition at line 11268 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXEMPTY_Pos

#define UART_FIFOSTS_RXEMPTY_Pos (14)

UART_T::FIFOSTS: RXEMPTY Position

Definition at line 11267 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXFULL_Msk

#define UART_FIFOSTS_RXFULL_Msk (0x1ul << UART_FIFOSTS_RXFULL_Pos)

UART_T::FIFOSTS: RXFULL Mask

Definition at line 11271 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXFULL_Pos

#define UART_FIFOSTS_RXFULL_Pos (15)

UART_T::FIFOSTS: RXFULL Position

Definition at line 11270 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXOVIF_Msk

#define UART_FIFOSTS_RXOVIF_Msk (0x1ul << UART_FIFOSTS_RXOVIF_Pos)

UART_T::FIFOSTS: RXOVIF Mask

Definition at line 11250 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXOVIF_Pos

#define UART_FIFOSTS_RXOVIF_Pos (0)

UART_T::FIFOSTS: RXOVIF Position

Definition at line 11249 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXPTR_Msk

#define UART_FIFOSTS_RXPTR_Msk (0x3ful << UART_FIFOSTS_RXPTR_Pos)

UART_T::FIFOSTS: RXPTR Mask

Definition at line 11265 of file Mini58Series.h.

## ◆ UART_FIFOSTS_RXPTR_Pos

#define UART_FIFOSTS_RXPTR_Pos (8)

UART_T::FIFOSTS: RXPTR Position

Definition at line 11264 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXEMPTY_Msk

#define UART_FIFOSTS_TXEMPTY_Msk (0x1ul << UART_FIFOSTS_TXEMPTY_Pos)

UART_T::FIFOSTS: TXEMPTY Mask

Definition at line 11277 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXEMPTY_Pos

#define UART_FIFOSTS_TXEMPTY_Pos (22)

UART_T::FIFOSTS: TXEMPTY Position

Definition at line 11276 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXEMPTYF_Msk

#define UART_FIFOSTS_TXEMPTYF_Msk (0x1ul << UART_FIFOSTS_TXEMPTYF_Pos)

UART_T::FIFOSTS: TXEMPTYF Mask

Definition at line 11286 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXEMPTYF_Pos

#define UART_FIFOSTS_TXEMPTYF_Pos (28)

UART_T::FIFOSTS: TXEMPTYF Position

Definition at line 11285 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXFULL_Msk

#define UART_FIFOSTS_TXFULL_Msk (0x1ul << UART_FIFOSTS_TXFULL_Pos)

UART_T::FIFOSTS: TXFULL Mask

Definition at line 11280 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXFULL_Pos

#define UART_FIFOSTS_TXFULL_Pos (23)

UART_T::FIFOSTS: TXFULL Position

Definition at line 11279 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXOVIF_Msk

#define UART_FIFOSTS_TXOVIF_Msk (0x1ul << UART_FIFOSTS_TXOVIF_Pos)

UART_T::FIFOSTS: TXOVIF Mask

Definition at line 11283 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXOVIF_Pos

#define UART_FIFOSTS_TXOVIF_Pos (24)

UART_T::FIFOSTS: TXOVIF Position

Definition at line 11282 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXPTR_Msk

#define UART_FIFOSTS_TXPTR_Msk (0x3ful << UART_FIFOSTS_TXPTR_Pos)

UART_T::FIFOSTS: TXPTR Mask

Definition at line 11274 of file Mini58Series.h.

## ◆ UART_FIFOSTS_TXPTR_Pos

#define UART_FIFOSTS_TXPTR_Pos (16)

UART_T::FIFOSTS: TXPTR Position

Definition at line 11273 of file Mini58Series.h.

## ◆ UART_FUNSEL_FUN_SEL_Msk

#define UART_FUNSEL_FUN_SEL_Msk (0x3ul << UART_FUNSEL_FUN_SEL_Pos)

UART_T::FUNSEL: FUN_SEL Mask

Definition at line 11370 of file Mini58Series.h.

## ◆ UART_FUNSEL_FUN_SEL_Pos

#define UART_FUNSEL_FUN_SEL_Pos (0)

UART_T::FUNSEL: FUN_SEL Position

Definition at line 11369 of file Mini58Series.h.

## ◆ UART_INTEN_ATOCTSEN_Msk

#define UART_INTEN_ATOCTSEN_Msk (0x1ul << UART_INTEN_ATOCTSEN_Pos)

UART_T::INTEN: ATOCTSEN Mask

Definition at line 11196 of file Mini58Series.h.

## ◆ UART_INTEN_ATOCTSEN_Pos

#define UART_INTEN_ATOCTSEN_Pos (13)

UART_T::INTEN: ATOCTSEN Position

Definition at line 11195 of file Mini58Series.h.

## ◆ UART_INTEN_ATORTSEN_Msk

#define UART_INTEN_ATORTSEN_Msk (0x1ul << UART_INTEN_ATORTSEN_Pos)

UART_T::INTEN: ATORTSEN Mask

Definition at line 11193 of file Mini58Series.h.

## ◆ UART_INTEN_ATORTSEN_Pos

#define UART_INTEN_ATORTSEN_Pos (12)

UART_T::INTEN: ATORTSEN Position

Definition at line 11192 of file Mini58Series.h.

## ◆ UART_INTEN_BUFERRIEN_Msk

#define UART_INTEN_BUFERRIEN_Msk (0x1ul << UART_INTEN_BUFERRIEN_Pos)

UART_T::INTEN: BUFERRIEN Mask

Definition at line 11184 of file Mini58Series.h.

## ◆ UART_INTEN_BUFERRIEN_Pos

#define UART_INTEN_BUFERRIEN_Pos (5)

UART_T::INTEN: BUFERRIEN Position

Definition at line 11183 of file Mini58Series.h.

## ◆ UART_INTEN_MODEMIEN_Msk

#define UART_INTEN_MODEMIEN_Msk (0x1ul << UART_INTEN_MODEMIEN_Pos)

UART_T::INTEN: MODEMIEN Mask

Definition at line 11178 of file Mini58Series.h.

## ◆ UART_INTEN_MODEMIEN_Pos

#define UART_INTEN_MODEMIEN_Pos (3)

UART_T::INTEN: MODEMIEN Position

Definition at line 11177 of file Mini58Series.h.

## ◆ UART_INTEN_RDAIEN_Msk

#define UART_INTEN_RDAIEN_Msk (0x1ul << UART_INTEN_RDAIEN_Pos)

UART_T::INTEN: RDAIEN Mask

Definition at line 11169 of file Mini58Series.h.

## ◆ UART_INTEN_RDAIEN_Pos

#define UART_INTEN_RDAIEN_Pos (0)

UART_T::INTEN: RDAIEN Position

Definition at line 11168 of file Mini58Series.h.

## ◆ UART_INTEN_RLSIEN_Msk

#define UART_INTEN_RLSIEN_Msk (0x1ul << UART_INTEN_RLSIEN_Pos)

UART_T::INTEN: RLSIEN Mask

Definition at line 11175 of file Mini58Series.h.

## ◆ UART_INTEN_RLSIEN_Pos

#define UART_INTEN_RLSIEN_Pos (2)

UART_T::INTEN: RLSIEN Position

Definition at line 11174 of file Mini58Series.h.

## ◆ UART_INTEN_RXTOIEN_Msk

#define UART_INTEN_RXTOIEN_Msk (0x1ul << UART_INTEN_RXTOIEN_Pos)

UART_T::INTEN: RXTOIEN Mask

Definition at line 11181 of file Mini58Series.h.

## ◆ UART_INTEN_RXTOIEN_Pos

#define UART_INTEN_RXTOIEN_Pos (4)

UART_T::INTEN: RXTOIEN Position

Definition at line 11180 of file Mini58Series.h.

## ◆ UART_INTEN_THREIEN_Msk

#define UART_INTEN_THREIEN_Msk (0x1ul << UART_INTEN_THREIEN_Pos)

UART_T::INTEN: THREIEN Mask

Definition at line 11172 of file Mini58Series.h.

## ◆ UART_INTEN_THREIEN_Pos

#define UART_INTEN_THREIEN_Pos (1)

UART_T::INTEN: THREIEN Position

Definition at line 11171 of file Mini58Series.h.

## ◆ UART_INTEN_TOCNTEN_Msk

#define UART_INTEN_TOCNTEN_Msk (0x1ul << UART_INTEN_TOCNTEN_Pos)

UART_T::INTEN: TOCNTEN Mask

Definition at line 11190 of file Mini58Series.h.

## ◆ UART_INTEN_TOCNTEN_Pos

#define UART_INTEN_TOCNTEN_Pos (11)

UART_T::INTEN: TOCNTEN Position

Definition at line 11189 of file Mini58Series.h.

## ◆ UART_INTEN_WKCTSIEN_Msk

#define UART_INTEN_WKCTSIEN_Msk (0x1ul << UART_INTEN_WKCTSIEN_Pos)

UART_T::INTEN: WKCTSIEN Mask

Definition at line 11187 of file Mini58Series.h.

## ◆ UART_INTEN_WKCTSIEN_Pos

#define UART_INTEN_WKCTSIEN_Pos (9)

UART_T::INTEN: WKCTSIEN Position

Definition at line 11186 of file Mini58Series.h.

## ◆ UART_INTSTS_BUFERRIF_Msk

#define UART_INTSTS_BUFERRIF_Msk (0x1ul << UART_INTSTS_BUFERRIF_Pos)

UART_T::INTSTS: BUFERRIF Mask

Definition at line 11304 of file Mini58Series.h.

## ◆ UART_INTSTS_BUFERRIF_Pos

#define UART_INTSTS_BUFERRIF_Pos (5)

UART_T::INTSTS: BUFERRIF Position

Definition at line 11303 of file Mini58Series.h.

## ◆ UART_INTSTS_BUFERRINT_Msk

#define UART_INTSTS_BUFERRINT_Msk (0x1ul << UART_INTSTS_BUFERRINT_Pos)

UART_T::INTSTS: BUFERRINT Mask

Definition at line 11322 of file Mini58Series.h.

## ◆ UART_INTSTS_BUFERRINT_Pos

#define UART_INTSTS_BUFERRINT_Pos (13)

UART_T::INTSTS: BUFERRINT Position

Definition at line 11321 of file Mini58Series.h.

## ◆ UART_INTSTS_CTSWKIF_Msk

#define UART_INTSTS_CTSWKIF_Msk (0x1ul << UART_INTSTS_CTSWKIF_Pos)

UART_T::INTSTS: CTSWKIF Mask

Definition at line 11325 of file Mini58Series.h.

## ◆ UART_INTSTS_CTSWKIF_Pos

#define UART_INTSTS_CTSWKIF_Pos (16)

UART_T::INTSTS: CTSWKIF Position

Definition at line 11324 of file Mini58Series.h.

## ◆ UART_INTSTS_MODEMIF_Msk

#define UART_INTSTS_MODEMIF_Msk (0x1ul << UART_INTSTS_MODEMIF_Pos)

UART_T::INTSTS: MODEMIF Mask

Definition at line 11298 of file Mini58Series.h.

## ◆ UART_INTSTS_MODEMIF_Pos

#define UART_INTSTS_MODEMIF_Pos (3)

UART_T::INTSTS: MODEMIF Position

Definition at line 11297 of file Mini58Series.h.

## ◆ UART_INTSTS_MODEMINT_Msk

#define UART_INTSTS_MODEMINT_Msk (0x1ul << UART_INTSTS_MODEMINT_Pos)

UART_T::INTSTS: MODEMINT Mask

Definition at line 11316 of file Mini58Series.h.

## ◆ UART_INTSTS_MODEMINT_Pos

#define UART_INTSTS_MODEMINT_Pos (11)

UART_T::INTSTS: MODEMINT Position

Definition at line 11315 of file Mini58Series.h.

## ◆ UART_INTSTS_RDAIF_Msk

#define UART_INTSTS_RDAIF_Msk (0x1ul << UART_INTSTS_RDAIF_Pos)

UART_T::INTSTS: RDAIF Mask

Definition at line 11289 of file Mini58Series.h.

## ◆ UART_INTSTS_RDAIF_Pos

#define UART_INTSTS_RDAIF_Pos (0)

UART_T::INTSTS: RDAIF Position

Definition at line 11288 of file Mini58Series.h.

## ◆ UART_INTSTS_RDAINT_Msk

#define UART_INTSTS_RDAINT_Msk (0x1ul << UART_INTSTS_RDAINT_Pos)

UART_T::INTSTS: RDAINT Mask

Definition at line 11307 of file Mini58Series.h.

## ◆ UART_INTSTS_RDAINT_Pos

#define UART_INTSTS_RDAINT_Pos (8)

UART_T::INTSTS: RDAINT Position

Definition at line 11306 of file Mini58Series.h.

## ◆ UART_INTSTS_RLSIF_Msk

#define UART_INTSTS_RLSIF_Msk (0x1ul << UART_INTSTS_RLSIF_Pos)

UART_T::INTSTS: RLSIF Mask

Definition at line 11295 of file Mini58Series.h.

## ◆ UART_INTSTS_RLSIF_Pos

#define UART_INTSTS_RLSIF_Pos (2)

UART_T::INTSTS: RLSIF Position

Definition at line 11294 of file Mini58Series.h.

## ◆ UART_INTSTS_RLSINT_Msk

#define UART_INTSTS_RLSINT_Msk (0x1ul << UART_INTSTS_RLSINT_Pos)

UART_T::INTSTS: RLSINT Mask

Definition at line 11313 of file Mini58Series.h.

## ◆ UART_INTSTS_RLSINT_Pos

#define UART_INTSTS_RLSINT_Pos (10)

UART_T::INTSTS: RLSINT Position

Definition at line 11312 of file Mini58Series.h.

## ◆ UART_INTSTS_RXTOIF_Msk

#define UART_INTSTS_RXTOIF_Msk (0x1ul << UART_INTSTS_RXTOIF_Pos)

UART_T::INTSTS: RXTOIF Mask

Definition at line 11301 of file Mini58Series.h.

## ◆ UART_INTSTS_RXTOIF_Pos

#define UART_INTSTS_RXTOIF_Pos (4)

UART_T::INTSTS: RXTOIF Position

Definition at line 11300 of file Mini58Series.h.

## ◆ UART_INTSTS_RXTOINT_Msk

#define UART_INTSTS_RXTOINT_Msk (0x1ul << UART_INTSTS_RXTOINT_Pos)

UART_T::INTSTS: RXTOINT Mask

Definition at line 11319 of file Mini58Series.h.

## ◆ UART_INTSTS_RXTOINT_Pos

#define UART_INTSTS_RXTOINT_Pos (12)

UART_T::INTSTS: RXTOINT Position

Definition at line 11318 of file Mini58Series.h.

## ◆ UART_INTSTS_THREIF_Msk

#define UART_INTSTS_THREIF_Msk (0x1ul << UART_INTSTS_THREIF_Pos)

UART_T::INTSTS: THREIF Mask

Definition at line 11292 of file Mini58Series.h.

## ◆ UART_INTSTS_THREIF_Pos

#define UART_INTSTS_THREIF_Pos (1)

UART_T::INTSTS: THREIF Position

Definition at line 11291 of file Mini58Series.h.

## ◆ UART_INTSTS_THREINT_Msk

#define UART_INTSTS_THREINT_Msk (0x1ul << UART_INTSTS_THREINT_Pos)

UART_T::INTSTS: THREINT Mask

Definition at line 11310 of file Mini58Series.h.

## ◆ UART_INTSTS_THREINT_Pos

#define UART_INTSTS_THREINT_Pos (9)

UART_T::INTSTS: THREINT Position

Definition at line 11309 of file Mini58Series.h.

## ◆ UART_IRDA_RXINV_Msk

#define UART_IRDA_RXINV_Msk (0x1ul << UART_IRDA_RXINV_Pos)

UART_T::IRDA: RXINV Mask

Definition at line 11352 of file Mini58Series.h.

## ◆ UART_IRDA_RXINV_Pos

#define UART_IRDA_RXINV_Pos (6)

UART_T::IRDA: RXINV Position

Definition at line 11351 of file Mini58Series.h.

## ◆ UART_IRDA_TXEN_Msk

#define UART_IRDA_TXEN_Msk (0x1ul << UART_IRDA_TXEN_Pos)

UART_T::IRDA: TXEN Mask

Definition at line 11346 of file Mini58Series.h.

## ◆ UART_IRDA_TXEN_Pos

#define UART_IRDA_TXEN_Pos (1)

UART_T::IRDA: TXEN Position

Definition at line 11345 of file Mini58Series.h.

## ◆ UART_IRDA_TXINV_Msk

#define UART_IRDA_TXINV_Msk (0x1ul << UART_IRDA_TXINV_Pos)

UART_T::IRDA: TXINV Mask

Definition at line 11349 of file Mini58Series.h.

## ◆ UART_IRDA_TXINV_Pos

#define UART_IRDA_TXINV_Pos (5)

UART_T::IRDA: TXINV Position

Definition at line 11348 of file Mini58Series.h.

## ◆ UART_LINE_BCB_Msk

#define UART_LINE_BCB_Msk (0x1ul << UART_LINE_BCB_Pos)

UART_T::LINE: BCB Mask

Definition at line 11229 of file Mini58Series.h.

## ◆ UART_LINE_BCB_Pos

#define UART_LINE_BCB_Pos (6)

UART_T::LINE: BCB Position

Definition at line 11228 of file Mini58Series.h.

## ◆ UART_LINE_EPE_Msk

#define UART_LINE_EPE_Msk (0x1ul << UART_LINE_EPE_Pos)

UART_T::LINE: EPE Mask

Definition at line 11223 of file Mini58Series.h.

## ◆ UART_LINE_EPE_Pos

#define UART_LINE_EPE_Pos (4)

UART_T::LINE: EPE Position

Definition at line 11222 of file Mini58Series.h.

## ◆ UART_LINE_NSB_Msk

#define UART_LINE_NSB_Msk (0x1ul << UART_LINE_NSB_Pos)

UART_T::LINE: NSB Mask

Definition at line 11217 of file Mini58Series.h.

## ◆ UART_LINE_NSB_Pos

#define UART_LINE_NSB_Pos (2)

UART_T::LINE: NSB Position

Definition at line 11216 of file Mini58Series.h.

## ◆ UART_LINE_PBE_Msk

#define UART_LINE_PBE_Msk (0x1ul << UART_LINE_PBE_Pos)

UART_T::LINE: PBE Mask

Definition at line 11220 of file Mini58Series.h.

## ◆ UART_LINE_PBE_Pos

#define UART_LINE_PBE_Pos (3)

UART_T::LINE: PBE Position

Definition at line 11219 of file Mini58Series.h.

## ◆ UART_LINE_SPE_Msk

#define UART_LINE_SPE_Msk (0x1ul << UART_LINE_SPE_Pos)

UART_T::LINE: SPE Mask

Definition at line 11226 of file Mini58Series.h.

## ◆ UART_LINE_SPE_Pos

#define UART_LINE_SPE_Pos (5)

UART_T::LINE: SPE Position

Definition at line 11225 of file Mini58Series.h.

## ◆ UART_LINE_WLS_Msk

#define UART_LINE_WLS_Msk (0x3ul << UART_LINE_WLS_Pos)

UART_T::LINE: WLS Mask

Definition at line 11214 of file Mini58Series.h.

## ◆ UART_LINE_WLS_Pos

#define UART_LINE_WLS_Pos (0)

UART_T::LINE: WLS Position

Definition at line 11213 of file Mini58Series.h.

## ◆ UART_MODEM_RTS_Msk

#define UART_MODEM_RTS_Msk (0x1ul << UART_MODEM_RTS_Pos)

UART_T::MODEM: RTS Mask

Definition at line 11232 of file Mini58Series.h.

## ◆ UART_MODEM_RTS_Pos

#define UART_MODEM_RTS_Pos (1)

UART_T::MODEM: RTS Position

Definition at line 11231 of file Mini58Series.h.

## ◆ UART_MODEM_RTSACTLV_Msk

#define UART_MODEM_RTSACTLV_Msk (0x1ul << UART_MODEM_RTSACTLV_Pos)

UART_T::MODEM: RTSACTLV Mask

Definition at line 11235 of file Mini58Series.h.

## ◆ UART_MODEM_RTSACTLV_Pos

#define UART_MODEM_RTSACTLV_Pos (9)

UART_T::MODEM: RTSACTLV Position

Definition at line 11234 of file Mini58Series.h.

## ◆ UART_MODEM_RTSSTS_Msk

#define UART_MODEM_RTSSTS_Msk (0x1ul << UART_MODEM_RTSSTS_Pos)

UART_T::MODEM: RTSSTS Mask

Definition at line 11238 of file Mini58Series.h.

## ◆ UART_MODEM_RTSSTS_Pos

#define UART_MODEM_RTSSTS_Pos (13)

UART_T::MODEM: RTSSTS Position

Definition at line 11237 of file Mini58Series.h.

## ◆ UART_MODEMSTS_CTSACTLV_Msk

#define UART_MODEMSTS_CTSACTLV_Msk (0x1ul << UART_MODEMSTS_CTSACTLV_Pos)

UART_T::MODEMSTS: CTSACTLV Mask

Definition at line 11247 of file Mini58Series.h.

## ◆ UART_MODEMSTS_CTSACTLV_Pos

#define UART_MODEMSTS_CTSACTLV_Pos (8)

UART_T::MODEMSTS: CTSACTLV Position

Definition at line 11246 of file Mini58Series.h.

## ◆ UART_MODEMSTS_CTSDETF_Msk

#define UART_MODEMSTS_CTSDETF_Msk (0x1ul << UART_MODEMSTS_CTSDETF_Pos)

UART_T::MODEMSTS: CTSDETF Mask

Definition at line 11241 of file Mini58Series.h.

## ◆ UART_MODEMSTS_CTSDETF_Pos

#define UART_MODEMSTS_CTSDETF_Pos (0)

UART_T::MODEMSTS: CTSDETF Position

Definition at line 11240 of file Mini58Series.h.

## ◆ UART_MODEMSTS_CTSSTS_Msk

#define UART_MODEMSTS_CTSSTS_Msk (0x1ul << UART_MODEMSTS_CTSSTS_Pos)

UART_T::MODEMSTS: CTSSTS Mask

Definition at line 11244 of file Mini58Series.h.

## ◆ UART_MODEMSTS_CTSSTS_Pos

#define UART_MODEMSTS_CTSSTS_Pos (4)

UART_T::MODEMSTS: CTSSTS Position

Definition at line 11243 of file Mini58Series.h.

## ◆ UART_TOUT_DLY_Msk

#define UART_TOUT_DLY_Msk (0xfful << UART_TOUT_DLY_Pos)

UART_T::TOUT: DLY Mask

Definition at line 11331 of file Mini58Series.h.

## ◆ UART_TOUT_DLY_Pos

#define UART_TOUT_DLY_Pos (8)

UART_T::TOUT: DLY Position

Definition at line 11330 of file Mini58Series.h.

## ◆ UART_TOUT_TOIC_Msk

#define UART_TOUT_TOIC_Msk (0xfful << UART_TOUT_TOIC_Pos)

UART_T::TOUT: TOIC Mask

Definition at line 11328 of file Mini58Series.h.

## ◆ UART_TOUT_TOIC_Pos

#define UART_TOUT_TOIC_Pos (0)

UART_T::TOUT: TOIC Position

Definition at line 11327 of file Mini58Series.h.

## ◆ WDT_ALTCTL_RSTDSEL_Msk

#define WDT_ALTCTL_RSTDSEL_Msk (0x3ul << WDT_ALTCTL_RSTDSEL_Pos)

WDT_T::ALTCTL: RSTDSEL Mask

Definition at line 11513 of file Mini58Series.h.

## ◆ WDT_ALTCTL_RSTDSEL_Pos

#define WDT_ALTCTL_RSTDSEL_Pos (0)

WDT_T::ALTCTL: RSTDSEL Position

Definition at line 11512 of file Mini58Series.h.

## ◆ WDT_CTL_ICEDEBUG_Msk

#define WDT_CTL_ICEDEBUG_Msk (0x1ul << WDT_CTL_ICEDEBUG_Pos)

WDT_T::CTL: ICEDEBUG Mask

Definition at line 11510 of file Mini58Series.h.

## ◆ WDT_CTL_ICEDEBUG_Pos

#define WDT_CTL_ICEDEBUG_Pos (31)

WDT_T::CTL: ICEDEBUG Position

Definition at line 11509 of file Mini58Series.h.

## ◆ WDT_CTL_IF_Msk

#define WDT_CTL_IF_Msk (0x1ul << WDT_CTL_IF_Pos)

WDT_T::CTL: IF Mask

Definition at line 11492 of file Mini58Series.h.

## ◆ WDT_CTL_IF_Pos

#define WDT_CTL_IF_Pos (3)

WDT_T::CTL: IF Position

Definition at line 11491 of file Mini58Series.h.

## ◆ WDT_CTL_INTEN_Msk

#define WDT_CTL_INTEN_Msk (0x1ul << WDT_CTL_INTEN_Pos)

WDT_T::CTL: INTEN Mask

Definition at line 11501 of file Mini58Series.h.

## ◆ WDT_CTL_INTEN_Pos

#define WDT_CTL_INTEN_Pos (6)

WDT_T::CTL: INTEN Position

Definition at line 11500 of file Mini58Series.h.

## ◆ WDT_CTL_RSTCNT_Msk

#define WDT_CTL_RSTCNT_Msk (0x1ul << WDT_CTL_RSTCNT_Pos)

WDT_T::CTL: RSTCNT Mask

Definition at line 11483 of file Mini58Series.h.

## ◆ WDT_CTL_RSTCNT_Pos

#define WDT_CTL_RSTCNT_Pos (0)

    @addtogroup WDT_CONST WDT Bit Field Definition
    Constant Definitions for WDT Controller

WDT_T::CTL: RSTCNT Position

Definition at line 11482 of file Mini58Series.h.

## ◆ WDT_CTL_RSTEN_Msk

#define WDT_CTL_RSTEN_Msk (0x1ul << WDT_CTL_RSTEN_Pos)

WDT_T::CTL: RSTEN Mask

Definition at line 11486 of file Mini58Series.h.

## ◆ WDT_CTL_RSTEN_Pos

#define WDT_CTL_RSTEN_Pos (1)

WDT_T::CTL: RSTEN Position

Definition at line 11485 of file Mini58Series.h.

## ◆ WDT_CTL_RSTF_Msk

#define WDT_CTL_RSTF_Msk (0x1ul << WDT_CTL_RSTF_Pos)

WDT_T::CTL: RSTF Mask

Definition at line 11489 of file Mini58Series.h.

## ◆ WDT_CTL_RSTF_Pos

#define WDT_CTL_RSTF_Pos (2)

WDT_T::CTL: RSTF Position

Definition at line 11488 of file Mini58Series.h.

## ◆ WDT_CTL_TOUTSEL_Msk

#define WDT_CTL_TOUTSEL_Msk (0x7ul << WDT_CTL_TOUTSEL_Pos)

WDT_T::CTL: TOUTSEL Mask

Definition at line 11507 of file Mini58Series.h.

## ◆ WDT_CTL_TOUTSEL_Pos

#define WDT_CTL_TOUTSEL_Pos (8)

WDT_T::CTL: TOUTSEL Position

Definition at line 11506 of file Mini58Series.h.

## ◆ WDT_CTL_WDTEN_Msk

#define WDT_CTL_WDTEN_Msk (0x1ul << WDT_CTL_WDTEN_Pos)

WDT_T::CTL: WDTEN Mask

Definition at line 11504 of file Mini58Series.h.

## ◆ WDT_CTL_WDTEN_Pos

#define WDT_CTL_WDTEN_Pos (7)

WDT_T::CTL: WDTEN Position

Definition at line 11503 of file Mini58Series.h.

## ◆ WDT_CTL_WKEN_Msk

#define WDT_CTL_WKEN_Msk (0x1ul << WDT_CTL_WKEN_Pos)

WDT_T::CTL: WKEN Mask

Definition at line 11495 of file Mini58Series.h.

## ◆ WDT_CTL_WKEN_Pos

#define WDT_CTL_WKEN_Pos (4)

WDT_T::CTL: WKEN Position

Definition at line 11494 of file Mini58Series.h.

## ◆ WDT_CTL_WKF_Msk

#define WDT_CTL_WKF_Msk (0x1ul << WDT_CTL_WKF_Pos)

WDT_T::CTL: WKF Mask

Definition at line 11498 of file Mini58Series.h.

## ◆ WDT_CTL_WKF_Pos

#define WDT_CTL_WKF_Pos (5)

WDT_T::CTL: WKF Position

Definition at line 11497 of file Mini58Series.h.

## ◆ WWDT_CNT_CNTDAT_Msk

#define WWDT_CNT_CNTDAT_Msk (0x3ful << WWDT_CNT_CNTDAT_Pos)

WWDT_T::CNT: CNTDAT Mask

Definition at line 11651 of file Mini58Series.h.

## ◆ WWDT_CNT_CNTDAT_Pos

#define WWDT_CNT_CNTDAT_Pos (0)

WWDT_T::CNT: CNTDAT Position

Definition at line 11650 of file Mini58Series.h.

## ◆ WWDT_CTL_CMPDAT_Msk

#define WWDT_CTL_CMPDAT_Msk (0x3ful << WWDT_CTL_CMPDAT_Pos)

WWDT_T::CTL: CMPDAT Mask

Definition at line 11639 of file Mini58Series.h.

## ◆ WWDT_CTL_CMPDAT_Pos

#define WWDT_CTL_CMPDAT_Pos (16)

WWDT_T::CTL: CMPDAT Position

Definition at line 11638 of file Mini58Series.h.

## ◆ WWDT_CTL_ICEDEBUG_Msk

#define WWDT_CTL_ICEDEBUG_Msk (0x1ul << WWDT_CTL_ICEDEBUG_Pos)

WWDT_T::CTL: ICEDEBUG Mask

Definition at line 11642 of file Mini58Series.h.

## ◆ WWDT_CTL_ICEDEBUG_Pos

#define WWDT_CTL_ICEDEBUG_Pos (31)

WWDT_T::CTL: ICEDEBUG Position

Definition at line 11641 of file Mini58Series.h.

## ◆ WWDT_CTL_INTEN_Msk

#define WWDT_CTL_INTEN_Msk (0x1ul << WWDT_CTL_INTEN_Pos)

WWDT_T::CTL: INTEN Mask

Definition at line 11633 of file Mini58Series.h.

## ◆ WWDT_CTL_INTEN_Pos

#define WWDT_CTL_INTEN_Pos (1)

WWDT_T::CTL: INTEN Position

Definition at line 11632 of file Mini58Series.h.

## ◆ WWDT_CTL_PSCSEL_Msk

#define WWDT_CTL_PSCSEL_Msk (0xful << WWDT_CTL_PSCSEL_Pos)

WWDT_T::CTL: PSCSEL Mask

Definition at line 11636 of file Mini58Series.h.

## ◆ WWDT_CTL_PSCSEL_Pos

#define WWDT_CTL_PSCSEL_Pos (8)

WWDT_T::CTL: PSCSEL Position

Definition at line 11635 of file Mini58Series.h.

## ◆ WWDT_CTL_WWDTEN_Msk

#define WWDT_CTL_WWDTEN_Msk (0x1ul << WWDT_CTL_WWDTEN_Pos)

WWDT_T::CTL: WWDTEN Mask

Definition at line 11630 of file Mini58Series.h.

## ◆ WWDT_CTL_WWDTEN_Pos

#define WWDT_CTL_WWDTEN_Pos (0)

WWDT_T::CTL: WWDTEN Position

Definition at line 11629 of file Mini58Series.h.

## ◆ WWDT_RLDCNT_RLDCNT_Msk

#define WWDT_RLDCNT_RLDCNT_Msk (0xfffffffful << WWDT_RLDCNT_RLDCNT_Pos)

WWDT_T::RLDCNT: RLDCNT Mask

Definition at line 11627 of file Mini58Series.h.

## ◆ WWDT_RLDCNT_RLDCNT_Pos

#define WWDT_RLDCNT_RLDCNT_Pos (0)

    @addtogroup WWDT_CONST WWDT Bit Field Definition
    Constant Definitions for WWDT Controller

WWDT_T::RLDCNT: RLDCNT Position

Definition at line 11626 of file Mini58Series.h.

## ◆ WWDT_STATUS_WWDTIF_Msk

#define WWDT_STATUS_WWDTIF_Msk (0x1ul << WWDT_STATUS_WWDTIF_Pos)

WWDT_T::STATUS: WWDTIF Mask

Definition at line 11645 of file Mini58Series.h.

## ◆ WWDT_STATUS_WWDTIF_Pos

#define WWDT_STATUS_WWDTIF_Pos (0)

WWDT_T::STATUS: WWDTIF Position

Definition at line 11644 of file Mini58Series.h.

## ◆ WWDT_STATUS_WWDTRF_Msk

#define WWDT_STATUS_WWDTRF_Msk (0x1ul << WWDT_STATUS_WWDTRF_Pos)

WWDT_T::STATUS: WWDTRF Mask

Definition at line 11648 of file Mini58Series.h.

## ◆ WWDT_STATUS_WWDTRF_Pos

#define WWDT_STATUS_WWDTRF_Pos (1)

WWDT_T::STATUS: WWDTRF Position

Definition at line 11647 of file Mini58Series.h.