| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Data Fields
GPIOBIT_T Struct Reference
NUC029FAE Control Register » General Purpose Input/Output Controller(GPIO)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | GP_BIT0
__IO uint32_t | GP_BIT1
__IO uint32_t | GP_BIT2
__IO uint32_t | GP_BIT3
__IO uint32_t | GP_BIT4
__IO uint32_t | GP_BIT5
__IO uint32_t | GP_BIT6
__IO uint32_t | GP_BIT7

## Detailed Description

Definition at line 1018 of file NUC029FAE.h.

## Field Documentation

## ◆ GP_BIT0

__IO uint32_t GPIOBIT_T::GP_BIT0

Offset: 0x0000 Px.0 Data Output Value

Definition at line 1020 of file NUC029FAE.h.

## ◆ GP_BIT1

__IO uint32_t GPIOBIT_T::GP_BIT1

Offset: 0x0004 Px.1 Data Output Value

Definition at line 1021 of file NUC029FAE.h.

## ◆ GP_BIT2

__IO uint32_t GPIOBIT_T::GP_BIT2

Offset: 0x0008 Px.2 Data Output Value

Definition at line 1022 of file NUC029FAE.h.

## ◆ GP_BIT3

__IO uint32_t GPIOBIT_T::GP_BIT3

Offset: 0x000C Px.3 Data Output Value

Definition at line 1023 of file NUC029FAE.h.

## ◆ GP_BIT4

__IO uint32_t GPIOBIT_T::GP_BIT4

Offset: 0x0010 Px.4 Data Output Value

Definition at line 1024 of file NUC029FAE.h.

## ◆ GP_BIT5

__IO uint32_t GPIOBIT_T::GP_BIT5

Offset: 0x0014 Px.5 Data Output Value

Definition at line 1025 of file NUC029FAE.h.

## ◆ GP_BIT6

__IO uint32_t GPIOBIT_T::GP_BIT6

Offset: 0x0018 Px.6 Data Output Value

Definition at line 1026 of file NUC029FAE.h.

## ◆ GP_BIT7

__IO uint32_t GPIOBIT_T::GP_BIT7

Offset: 0x001C Px.7 Data Output Value

Definition at line 1027 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nuc029faebsp/Library/Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h