| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- SEMIHOSTING_EnterSVC : semihosting.h
- SEMIHOSTING_ReportException : semihosting.h
- SEMIHOSTING_SYS_CLOCK : semihosting.h
- SEMIHOSTING_SYS_CLOSE : semihosting.h
- SEMIHOSTING_SYS_ELAPSED : semihosting.h
- SEMIHOSTING_SYS_ERRNO : semihosting.h
- SEMIHOSTING_SYS_FLEN : semihosting.h
- SEMIHOSTING_SYS_GET_CMDLINE : semihosting.h
- SEMIHOSTING_SYS_HEAPINFO : semihosting.h
- SEMIHOSTING_SYS_ISERROR : semihosting.h
- SEMIHOSTING_SYS_ISTTY : semihosting.h
- SEMIHOSTING_SYS_OPEN : semihosting.h
- SEMIHOSTING_SYS_READ : semihosting.h
- SEMIHOSTING_SYS_READC : semihosting.h
- SEMIHOSTING_SYS_REMOVE : semihosting.h
- SEMIHOSTING_SYS_RENAME : semihosting.h
- SEMIHOSTING_SYS_SEEK : semihosting.h
- SEMIHOSTING_SYS_SYSTEM : semihosting.h
- SEMIHOSTING_SYS_TICKFREQ : semihosting.h
- SEMIHOSTING_SYS_TIME : semihosting.h
- SEMIHOSTING_SYS_TMPNAM : semihosting.h
- SEMIHOSTING_SYS_WRITE : semihosting.h
- SEMIHOSTING_SYS_WRITE0 : semihosting.h
- SEMIHOSTING_SYS_WRITEC : semihosting.h
- SendChar() : retarget.c
- SendChar_ToUART() : retarget.c
- SPI : NUC029FAE.h
- SPI_ABORT_3WIRE_TRANSFER : spi.h
- SPI_BASE : NUC029FAE.h
- SPI_ClearRxFIFO() : spi.h
- SPI_ClearTxFIFO() : spi.h
- SPI_Close() : spi.h
- SPI_CLR_3WIRE_START_INT_FLAG : spi.h
- SPI_CLR_UNIT_TRANS_INT_FLAG : spi.h
- SPI_DISABLE_3WIRE_MODE : spi.h
- SPI_DISABLE_BYTE_REORDER : spi.h
- SPI_DisableAutoSS() : spi.h
- SPI_DisableFIFO() : spi.h
- SPI_DisableInt() : spi.h
- SPI_ENABLE_3WIRE_MODE : spi.h
- SPI_ENABLE_BYTE_REORDER : spi.h
- SPI_EnableAutoSS() : spi.h
- SPI_EnableFIFO() : spi.h
- SPI_EnableInt() : spi.h
- SPI_FIFO_RX_INTEN_MASK : spi.h
- SPI_FIFO_RXOV_INTEN_MASK : spi.h
- SPI_FIFO_TIMEOUT_INTEN_MASK : spi.h
- SPI_FIFO_TX_INTEN_MASK : spi.h
- SPI_GET_RX_FIFO_COUNT : spi.h
- SPI_GET_RX_FIFO_EMPTY_FLAG : spi.h
- SPI_GET_TX_FIFO_EMPTY_FLAG : spi.h
- SPI_GetBusClock() : spi.h
- SPI_IE_MASK : spi.h
- SPI_IRQn : NUC029FAE.h
- SPI_IS_BUSY : spi.h
- SPI_MASTER : spi.h
- SPI_MODE_0 : spi.h
- SPI_MODE_1 : spi.h
- SPI_MODE_2 : spi.h
- SPI_MODE_3 : spi.h
- SPI_MODULE : clk.h
- SPI_Open() : spi.h
- SPI_READ_RX : spi.h
- SPI_RST : sys.h
- SPI_SET_DATA_WIDTH() : spi.h
- SPI_SET_LSB_FIRST : spi.h
- SPI_SET_MSB_FIRST : spi.h
- SPI_SET_SS_HIGH() : spi.h
- SPI_SET_SS_LOW() : spi.h
- SPI_SET_SUSPEND_CYCLE : spi.h
- SPI_SetBusClock() : spi.h
- SPI_SLAVE : spi.h
- SPI_SS : spi.h
- SPI_SS_ACTIVE_HIGH : spi.h
- SPI_SS_ACTIVE_LOW : spi.h
- SPI_SSTA_INTEN_MASK : spi.h
- SPI_TRIGGER : spi.h
- SPI_WRITE_TX : spi.h
- SRAM_BASE : NUC029FAE.h
- stackDump() : retarget.c
- SVCall_IRQn : NUC029FAE.h
- SYS : NUC029FAE.h
- SYS_BASE : NUC029FAE.h
- SYS_BODCR_BOD_DISABLE : sys.h
- SYS_BODCR_BOD_INTERRUPT_EN : sys.h
- SYS_BODCR_BOD_RST_EN : sys.h
- SYS_BODCR_BOD_VL_2_2V : sys.h
- SYS_BODCR_BOD_VL_2_7V : sys.h
- SYS_BODCR_BOD_VL_3_7V : sys.h
- SYS_BODCR_BOD_VL_4_4V : sys.h
- SYS_CLEAR_BOD_INT_FLAG : sys.h
- SYS_CLEAR_BOD_LPM : sys.h
- SYS_CLEAR_RST_SOURCE : sys.h
- SYS_ClearResetSrc() : sys.h
- SYS_DISABLE_BOD : sys.h
- SYS_DISABLE_BOD_RST : sys.h
- SYS_DISABLE_POR : sys.h
- SYS_DisableBOD() : sys.h
- SYS_ENABLE_BOD : sys.h
- SYS_ENABLE_BOD_RST : sys.h
- SYS_ENABLE_POR : sys.h
- SYS_EnableBOD() : sys.h
- SYS_GET_BOD_INT_FLAG : sys.h
- SYS_GET_BOD_OUTPUT : sys.h
- SYS_GetBODStatus() : sys.h
- SYS_GetResetSrc() : sys.h
- SYS_IS_BOD_RST : sys.h
- SYS_IS_CPU_RST : sys.h
- SYS_IS_POR_RST : sys.h
- SYS_IS_RSTPIN_RST : sys.h
- SYS_IS_SYSTEM_RST : sys.h
- SYS_IS_WDT_RST : sys.h
- SYS_IsRegLocked() : sys.h
- SYS_LockReg() : sys.h
- SYS_MFP_ALT_Msk : sys.h
- SYS_MFP_MFP_Msk : sys.h
- SYS_MFP_P00_CTS : sys.h
- SYS_MFP_P00_GPIO : sys.h
- SYS_MFP_P00_Msk : sys.h
- SYS_MFP_P00_TXD : sys.h
- SYS_MFP_P01_GPIO : sys.h
- SYS_MFP_P01_Msk : sys.h
- SYS_MFP_P01_RTS : sys.h
- SYS_MFP_P01_RXD : sys.h
- SYS_MFP_P01_SPISS : sys.h
- SYS_MFP_P04_GPIO : sys.h
- SYS_MFP_P04_Msk : sys.h
- SYS_MFP_P04_PWM5 : sys.h
- SYS_MFP_P04_SPISS : sys.h
- SYS_MFP_P05_GPIO : sys.h
- SYS_MFP_P05_MOSI : sys.h
- SYS_MFP_P05_Msk : sys.h
- SYS_MFP_P06_GPIO : sys.h
- SYS_MFP_P06_MISO : sys.h
- SYS_MFP_P06_Msk : sys.h
- SYS_MFP_P07_GPIO : sys.h
- SYS_MFP_P07_Msk : sys.h
- SYS_MFP_P07_SPICLK : sys.h
- SYS_MFP_P10_AIN1 : sys.h
- SYS_MFP_P10_CPP0 : sys.h
- SYS_MFP_P10_GPIO : sys.h
- SYS_MFP_P10_Msk : sys.h
- SYS_MFP_P12_AIN2 : sys.h
- SYS_MFP_P12_CPP0 : sys.h
- SYS_MFP_P12_GPIO : sys.h
- SYS_MFP_P12_Msk : sys.h
- SYS_MFP_P12_RXD : sys.h
- SYS_MFP_P13_AIN3 : sys.h
- SYS_MFP_P13_CPP0 : sys.h
- SYS_MFP_P13_GPIO : sys.h
- SYS_MFP_P13_Msk : sys.h
- SYS_MFP_P13_TXD : sys.h
- SYS_MFP_P14_AIN4 : sys.h
- SYS_MFP_P14_CPN0 : sys.h
- SYS_MFP_P14_GPIO : sys.h
- SYS_MFP_P14_Msk : sys.h
- SYS_MFP_P15_AIN5 : sys.h
- SYS_MFP_P15_CPP0 : sys.h
- SYS_MFP_P15_GPIO : sys.h
- SYS_MFP_P15_Msk : sys.h
- SYS_MFP_P22_GPIO : sys.h
- SYS_MFP_P22_Msk : sys.h
- SYS_MFP_P22_PWM0 : sys.h
- SYS_MFP_P23_GPIO : sys.h
- SYS_MFP_P23_Msk : sys.h
- SYS_MFP_P23_PWM1 : sys.h
- SYS_MFP_P24_GPIO : sys.h
- SYS_MFP_P24_Msk : sys.h
- SYS_MFP_P24_PWM2 : sys.h
- SYS_MFP_P25_GPIO : sys.h
- SYS_MFP_P25_Msk : sys.h
- SYS_MFP_P25_PWM3 : sys.h
- SYS_MFP_P26_CPO1 : sys.h
- SYS_MFP_P26_GPIO : sys.h
- SYS_MFP_P26_Msk : sys.h
- SYS_MFP_P26_PWM4 : sys.h
- SYS_MFP_P30_AIN6 : sys.h
- SYS_MFP_P30_CPN1 : sys.h
- SYS_MFP_P30_GPIO : sys.h
- SYS_MFP_P30_Msk : sys.h
- SYS_MFP_P31_AIN7 : sys.h
- SYS_MFP_P31_CPP1 : sys.h
- SYS_MFP_P31_GPIO : sys.h
- SYS_MFP_P31_Msk : sys.h
- SYS_MFP_P32_CPP1 : sys.h
- SYS_MFP_P32_GPIO : sys.h
- SYS_MFP_P32_INT0 : sys.h
- SYS_MFP_P32_Msk : sys.h
- SYS_MFP_P32_STADC : sys.h
- SYS_MFP_P32_T0EX : sys.h
- SYS_MFP_P34_CPP1 : sys.h
- SYS_MFP_P34_GPIO : sys.h
- SYS_MFP_P34_Msk : sys.h
- SYS_MFP_P34_SDA : sys.h
- SYS_MFP_P34_T0 : sys.h
- SYS_MFP_P35_CPP1 : sys.h
- SYS_MFP_P35_GPIO : sys.h
- SYS_MFP_P35_Msk : sys.h
- SYS_MFP_P35_SCL : sys.h
- SYS_MFP_P35_T1 : sys.h
- SYS_MFP_P36_CKO : sys.h
- SYS_MFP_P36_CPO0 : sys.h
- SYS_MFP_P36_GPIO : sys.h
- SYS_MFP_P36_Msk : sys.h
- SYS_MFP_P36_T1EX : sys.h
- SYS_MFP_P46_GPIO : sys.h
- SYS_MFP_P46_ICE_CLK : sys.h
- SYS_MFP_P46_Msk : sys.h
- SYS_MFP_P47_GPIO : sys.h
- SYS_MFP_P47_ICE_DAT : sys.h
- SYS_MFP_P47_Msk : sys.h
- SYS_MFP_P50_GPIO : sys.h
- SYS_MFP_P50_Msk : sys.h
- SYS_MFP_P50_XTAL1 : sys.h
- SYS_MFP_P51_GPIO : sys.h
- SYS_MFP_P51_Msk : sys.h
- SYS_MFP_P51_XTAL2 : sys.h
- SYS_MFP_P52_GPIO : sys.h
- SYS_MFP_P52_INT1 : sys.h
- SYS_MFP_P52_Msk : sys.h
- SYS_MFP_P53_AIN0 : sys.h
- SYS_MFP_P53_GPIO : sys.h
- SYS_MFP_P53_Msk : sys.h
- SYS_MFP_P54_GPIO : sys.h
- SYS_MFP_P54_Msk : sys.h
- SYS_MFP_P55_GPIO : sys.h
- SYS_MFP_P55_Msk : sys.h
- SYS_MFP_TYPE_Msk : sys.h
- SYS_ReadPDID() : sys.h
- SYS_ResetChip() : sys.h
- SYS_ResetCPU() : sys.h
- SYS_ResetModule() : sys.h
- SYS_SET_BOD_LEVEL : sys.h
- SYS_SET_BOD_LPM : sys.h
- SYS_UnlockReg() : sys.h
- SystemCoreClock : system_NUC029FAE.h , system_NUC029FAE.c
- SystemCoreClockUpdate() : system_NUC029FAE.h , system_NUC029FAE.c
- SysTick_IRQn : NUC029FAE.h