| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Data Fields
GPIO_T Struct Reference
NUC029FAE Control Register » General Purpose Input/Output Controller(GPIO)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | PMD
__IO uint32_t | OFFD
__IO uint32_t | DOUT
__IO uint32_t | DMASK
__I uint32_t | PIN
__IO uint32_t | DBEN
__IO uint32_t | IMD
__IO uint32_t | IEN
__IO uint32_t | ISRC

## Detailed Description

Definition at line 928 of file NUC029FAE.h.

## Field Documentation

## ◆ DBEN

__IO uint32_t GPIO_T::DBEN

Offset: 0x0014 GPIO Port De-bounce Enable

Definition at line 935 of file NUC029FAE.h.

## ◆ DMASK

__IO uint32_t GPIO_T::DMASK

Offset: 0x000C GPIO Port Data Output Write Mask

Definition at line 933 of file NUC029FAE.h.

## ◆ DOUT

__IO uint32_t GPIO_T::DOUT

Offset: 0x0008 GPIO Port Data Output

Definition at line 932 of file NUC029FAE.h.

## ◆ IEN

__IO uint32_t GPIO_T::IEN

Offset: 0x001C GPIO Port Interrupt Enable

Definition at line 937 of file NUC029FAE.h.

## ◆ IMD

__IO uint32_t GPIO_T::IMD

Offset: 0x0018 GPIO Port Interrupt Mode Select

Definition at line 936 of file NUC029FAE.h.

## ◆ ISRC

__IO uint32_t GPIO_T::ISRC

Offset: 0x0020 GPIO Port Interrupt Source Flag

Definition at line 938 of file NUC029FAE.h.

## ◆ OFFD

__IO uint32_t GPIO_T::OFFD

Offset: 0x0004 GPIO Port Bit Off Digital Enable

Definition at line 931 of file NUC029FAE.h.

## ◆ PIN

__I uint32_t GPIO_T::PIN

Offset: 0x0010 GPIO Port Pin Value

Definition at line 934 of file NUC029FAE.h.

## ◆ PMD

__IO uint32_t GPIO_T::PMD

Offset: 0x0000 GPIO Port Bit Mode Control

Definition at line 930 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nuc029faebsp/Library/Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h