| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Data Fields
ACMP_T Struct Reference
NUC029FAE Control Register » Analog Comparator Controller(ACMP)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | CMPCR [2]
__IO uint32_t | CMPSR
__IO uint32_t | CMPRVCR

## Detailed Description

Definition at line 146 of file NUC029FAE.h.

## Field Documentation

## ◆ CMPCR

__IO uint32_t ACMP_T::CMPCR[2]

Offset: 0x0000, 0x0004 Comparator Control 0 & 1

Definition at line 148 of file NUC029FAE.h.

## ◆ CMPRVCR

__IO uint32_t ACMP_T::CMPRVCR

Offset: 0x000C Comparator Reference Voltage Control Register

Definition at line 150 of file NUC029FAE.h.

## ◆ CMPSR

__IO uint32_t ACMP_T::CMPSR

Offset: 0x0008 Comparator Status Register

Definition at line 149 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nuc029faebsp/Library/Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h