| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Data Fields
ADC_T Struct Reference
NUC029FAE Control Register » Analog to Digital Converter(ADC)

`#include <NUC029FAE.h>`

## Data Fields
__IO uint32_t | ADDR
uint32_t | RESERVED0 [7]
__IO uint32_t | ADCR
__IO uint32_t | ADCHER
__IO uint32_t | ADCMPR [2]
__IO uint32_t | ADSR
__IO uint32_t | ADTDCR
__IO uint32_t | ADSAMP

## Detailed Description

Definition at line 642 of file NUC029FAE.h.

## Field Documentation

## ◆ ADCHER

__IO uint32_t ADC_T::ADCHER

Offset: 0x0024 A/D Channel Enable Register

Definition at line 647 of file NUC029FAE.h.

## ◆ ADCMPR

__IO uint32_t ADC_T::ADCMPR[2]

Offset: 0x0028, 0x002C A/D Compare Register 0 & 1

Definition at line 648 of file NUC029FAE.h.

## ◆ ADCR

__IO uint32_t ADC_T::ADCR

Offset: 0x0020 A/D Control Register

Definition at line 646 of file NUC029FAE.h.

## ◆ ADDR

__IO uint32_t ADC_T::ADDR

Offset: 0x0000 A/D Data Register

Definition at line 644 of file NUC029FAE.h.

## ◆ ADSAMP

__IO uint32_t ADC_T::ADSAMP

Offset: 0x0048 ADC Sampling Time Counter Register

Definition at line 651 of file NUC029FAE.h.

## ◆ ADSR

__IO uint32_t ADC_T::ADSR

Offset: 0x0030 A/D Status Register

Definition at line 649 of file NUC029FAE.h.

## ◆ ADTDCR

__IO uint32_t ADC_T::ADTDCR

Offset: 0x0044 A/D Trigger Delay Control Register

Definition at line 650 of file NUC029FAE.h.

## ◆ RESERVED0

uint32_t ADC_T::RESERVED0[7]

Offset: 0x0004 ~ 0x001C Reserved

Definition at line 645 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nuc029faebsp/Library/Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h