| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Data Fields
INT_T Struct Reference
NUC029FAE Control Register » Interrupt Source Controller (INT)

`#include <NUC029FAE.h>`

## Data Fields
__I uint32_t | IRQSRC [32]
__IO uint32_t | NMICNO
__IO uint32_t | MCUIRQ

## Detailed Description

Definition at line 1155 of file NUC029FAE.h.

## Field Documentation

## ◆ IRQSRC

__I uint32_t INT_T::IRQSRC[32]

Offset: 0x0000 ~ 0x007C Interrupt Source Identity Registers

Definition at line 1157 of file NUC029FAE.h.

## ◆ MCUIRQ

__IO uint32_t INT_T::MCUIRQ

Offset: 0x0084 MCU IRQ Number Identity Register

Definition at line 1159 of file NUC029FAE.h.

## ◆ NMICNO

__IO uint32_t INT_T::NMICNO

Offset: 0x0080 NMI Source Interrupt Select Control Register

Definition at line 1158 of file NUC029FAE.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nuc029faebsp/Library/Device/Nuvoton/NUC029FAE/Include/NUC029FAE.h