| NUC029FAE BSP V3.01.002 The Board Support Package for NUC029FAE

Functions
wdt.c File Reference

NUC029FAE WDT driver source file. More...

`#include "NUC029FAE.h"`

Go to the source code of this file.

## Functions
void | WDT_Open (uint32_t u32TimeoutInterval, uint32_t u32ResetDelay, uint32_t u32EnableReset, uint32_t u32EnableWakeup)
| This function make WDT module start counting with different time-out interval. More...
void | WDT_Close (void)
| This function stops WDT counting and disable WDT module. More...
void | WDT_EnableInt (void)
| This function enables the WDT time-out interrupt. More...
void | WDT_DisableInt (void)
| This function disables the WDT time-out interrupt. More...

## Detailed Description

NUC029FAE WDT driver source file.

Version
  V1.00

Revision
  2

Date
  15/03/18 5:42p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file wdt.c.