| Nano100AN Series BSP V3.02.002 The Board Support Package for Nano100AN Series

Data Fields
s_usbd_info Struct Reference
NANO100 Device Driver » USBD Driver » USBD Exported Structs

`#include <usbd.h>`

## Data Fields
uint8_t * | gu8DevDesc
uint8_t * | gu8ConfigDesc
uint8_t ** | gu8StringDesc
uint8_t ** | gu8HidReportDesc
uint32_t * | gu32HidReportSize
uint32_t * | gu32ConfigHidDescIdx

## Detailed Description

Definition at line 26 of file usbd.h.

## Field Documentation

## ◆ gu32ConfigHidDescIdx

uint32_t* s_usbd_info::gu32ConfigHidDescIdx

Pointer for HID Descriptor start index

Definition at line 33 of file usbd.h.

## ◆ gu32HidReportSize

uint32_t* s_usbd_info::gu32HidReportSize

Pointer for HID Report descriptor Size

Definition at line 32 of file usbd.h.

## ◆ gu8ConfigDesc

uint8_t* s_usbd_info::gu8ConfigDesc

Config descriptor

Definition at line 29 of file usbd.h.

## ◆ gu8DevDesc

uint8_t* s_usbd_info::gu8DevDesc

Device descriptor

Definition at line 28 of file usbd.h.

## ◆ gu8HidReportDesc

uint8_t** s_usbd_info::gu8HidReportDesc

Pointer for HID Report descriptor

Definition at line 31 of file usbd.h.

## ◆ gu8StringDesc

uint8_t** s_usbd_info::gu8StringDesc

Pointer for USB String Descriptor pointers

Definition at line 30 of file usbd.h.

The documentation for this struct was generated from the following file:

- C:/Users/yachen/workzone/bsp/nano100absp/Library/StdDriver/inc/usbd.h